1. Before Using the Printer

1.1. Product series introduction

Product series parameters | P2210 Series | P2510 Series | P2210W Series | P2510W Series
Interface type | USB | ● | ● | ● | ●
NET |  |  |  |
WiFi |  |  | ● | ●
Print Language
GDI | ● | ● | ● | ●
Control Panel
LED | ● | ● | ● | ●
Print Speed(A4) | 20ppm | ● |  | ● |
22ppm |  | ● |  | ●
Manual duplex print | ● | ● | ● | ●

(●: Support; Blank: Unsupport)

| Note： | • This product series is subject to additions or changes without prior notice.

1.2. Supplied Accessories

When you open the package, make sure that the following parts are included in the carton:

Name | Parts
Printer |
Laser Toner Cartridge |
USB Interface Cable |
Power Cord |
CD-ROM |
Installation Manual |
Pantum Warranty |

| Note： | • The Pantum Warranty may not be attached in some regions.

1.3. Product View

| Front View

1 | Output Bin
2 | Control Panel
3 | Output Tray
4 | Automatic Feed Guide
5 | Paper Stop
6 | Feeder Tray
7 | Automatic Feeder Tray

| Rear View

| Note: | • The rear view of the printer may vary depending on the models and functions.

1 | Network Interface
2 | USB Interface
3 | Power Switch
4 | Power Interface

1.4. Laser Toner Cartridge

| Service Life of the Laser Toner Cartridge

Type | Average Print Volume
Laser Toner Cartridge with Standard Capacity | About 700 Pages (The above data is based on ISO/IEC 19752 standard)
Laser Toner Cartridge with High Capacity | About 1600 Pages (The above data is based on ISO/IEC 19752 standard)

| Note: | • The model is subject to increase without notice. • Consumables capacity may vary depending on the types used. • The Company does not recommend using consumables other than the original consumables provided, as any damages caused by non-original consumables are not covered by the scope of warranty. • Toner cartridge appearance may differ because of multiple volume and models, so the schematic diagram is only for your reference.

1.5. Easily-Refilled Laser Toner Cartridge

1.5.1. Structure of Easily-Refilled Laser Cartridge

No. | Name
1 | Waste Toner Port
2 | Toner Refilling Port
3 | Waste Toner Box
4 | Toner Box

1.5.2. Steps of Filling the Easily-Refilled Laser Cartridge

Steps | Diagram | Description
1 |  | "Hold the laser toner cartridge with the toner port side down and shake it vertically around 5-6 times."
2 |  | Open the cover of the waste toner port.
3 |  | "Pour out the waste toner from the waste toner box."
4 |  | Close the cover of the waste toner port.
5 |  | Open the cover of the toner refilling port.
6 |  | "Align the mouth of the toner bottle to the toner refilling port."
7 |  | Pour the toner into the toner box.
8 |  | Close the cover of the toner refilling port.
9 |  | The toner refilling is completed.

| Note: | • Do NOT incinerate new or waste toner or toner cartridge. Toner will combust when exposed to flame and operator may get burnt. • Do NOT use an ordinary vacuum to clean up spilled toner. The toner may be exposed to spark inside the vacuum and thus cause a fire or explosion. You can use an anti-explosion vacuum with a dust fire protection device. • If you inhaled toner, please gargle with plenty of water and go to an environment with fresh air. Go to the hospital when necessary. • If the clothes are stained with toner, wipe clothes with a dry duster and then clean them with cold water. Hot water will cause toner to penetrate fibers of clothes.