**
**
**  D-Link DFE-530TX PCI Fast Ethernet Adapter
**
**  NDIS2 Driver for PCNFS
**
**  v4.38    Feb  , 2007
**
**

Introduction:
=============

  The Ethernet NDIS2 Driver for PCNFS confirms to the Network Driver
  Interface Specification(NDIS2). This document shows you how to setup
  the driver and how to use the enhanced functions by setting the custom
  keywords in configuration file.


Contents of the Subdirectory:
=============================

    PCNFS.TXT           This file.
    DLKFET.DOS          The NDIS2 driver for PCNFS.
    PROTOCOL.INI        Sample protocol.ini file.


Installation:
=============

  Before starting with the installation process, make sure that the adapter
  is properly installed and configured. You can use the diagnostic program
  (DIAG.EXE) to make sure your connection with the network is correct.

  Installation procedure for PCNFS
  --------------------------------

    1) Run PCNFS install program and follow screen instructions.

    2) When the "Configure an Ethernet network connection" appears, Select
       "Ethernet" and press <Enter>.

    3) Choose NE2000 network adapter and select "NDIS" and press <Enter>.

    4) Follow the screen instructions to complete the installation.

    5) Two subdirectory will be created after installation, default in C:\NFS
       and C:\LANMAN.

    6) Copy A:\PCNFS\DLKFET.DOS to C:\NFS.

    7) Edit CONFIG.SYS to replace the line

                DEVICE=C:\LANMAN\NE2000.DOS
       with
                DEVICE=C:\LANMAN\DLKFET.DOS

    8) Edit PROTOCOL.INI file in C:\LANMAN directory, add the following section

       [FETND_NIF]
             Drivername    = DLKFET$
         
    9) Find [NFS-NDIS] section in PROTOCOL.INI file in C:\LANMAN directory, add
       the following line after "Drivername = NFSLINK$" line:

             Bindings   = FETND_NIF

   10) Restart the computer.


Configuration Files:
====================

    Sample of configuration file:
    -----------------------------

    File Name:          C:\CONFIG.SYS
    ----------
        DEVICE=C:\LANMAN\PROTMAN.SYS /I:C:\LANMAN
        DEVICE=C:\LANMAN\DLKFET.DOS
        DEVICE=C:\LANMAN\NFS-NDIS.SYS
        DEVICE=C:\NFS\PCNFS.SYS
        DEVICE=C:\NFS\SOCKDRV.SYS
        DEVICE=C:\DOS\ANSI.SYS

    File Name:          C:\AUTOEXEC.BAT
    ----------
        C:\LANMAN\NETBIND
        SET NFSDRIVE=C
        SET NFSPATH=C:\NFS
        PRT *
        CALL C:\NFS\NETWORK
        CALL C:\NFS\DRIVES
        LH C:\DOS\SHARE.EXE /l:500 /f:5100
        RTM

    File Name:          C:\LANMAN\PROTOCOL.INI
    ----------
        [protocol manager]
              drivername = PROTMAN$
        [FETND_NIF]
              Drivername    = DLKFET$
        [NFS-NDIS]
              Drivername = NFSLINK$
              Bindings   = FETND_NIF


    Custom Keywords:
    ----------------
        FULLDUPLEX                      This keyword is used to enable full
                                        duplex mode.
                                        (suggest use CONNECTIONTYPE instead of this keyword)

        SPEED                           This keyword is used to force the
                                        adapter at 10Mbps or 100Mbps speed.
                                        (suggest use CONNECTIONTYPE instead of this keyword)

        AUTO                            This keyword is used to force the
                                        chip at Auto-Negotiation mode.
                                        (suggest use CONNECTIONTYPE instead of this keyword)

        DEVICENO                        This keyword is used to force device number
                                        for specified NIC card

        BUSNO                           This keyword is used to force bus number for
                                        specified NIC card
 
        CONNECTIONTYPE                  This keyword is used to specify duplex 
                                        and speed mode. The strings are :
                                        
                                        AUTOSENSE
                                        _10BaseT  
                                        _10BaseTFD
                                        _100BaseTX   
                                        _100BaseTXFD 
                                        
        FLOWCTRL                        This keyword is used to specify flow contro
                                        ability. The strings are :
                                        
                                        HARDWARE_DEFAULT (Auto Mode)
                                        ENABLE
                                        DISABLE

                                        Driver doesn't care the result of auto-negotiate if 
                                        the value of this keyword, FLOWCTRL , is ENALBE or
                                        DISABLE. It just enables or disable flow control
                                        ability according your setting.

        NETWORKADDRESS                  This keyword is used to override the network address
                                        of the network adapter. Its type is :
                                        
                                        "000123456789"

        Note: If you want to specify NIC card, the DEVICENO is necessary, but BUSNO is optional
              When the NIC cards in the system have the same device number, you can use 
              BUSNO to specify.
              If there are two or more NIC cards in the system and you don't specify anyone,
              driver will display the menu for selection. You can get the information about 
              bus number and device number form this menu.
                                        