SUMO
Simulation of Urban MObility

- Home
- Download
- Documentation
- Wiki
- Trac
- Blog
- Contact
- SF-Project

# Simulation/Output/Lane- or Edge-based Noise Measures

The edge/lane based noise output based on Harmonoise writes information about the noise produced on edges/lanes. The model was generated within the EC-project Imagine. Its description can be found in the deliverable 18 of this project (D18 The Harmonoise Engineering model).

Missing:
Add a model description here

## Instantiating within the Simulation

### Edge-Based Noise Output

An edge-based noise emissions output is defined way within an additional file as following:

<edgeData id="<DETECTOR_ID>" type="harmonoise" freq="<FREQUENCY>" file="<OUTPUT_FILE>" [excludeEmpty="true"]/>

### Lane-Based Noise Output

An edge-based noise emissions output is defined way within an additional file as following:

<laneData id="<DETECTOR_ID>" type="harmonoise" freq="<FREQUENCY>" file="<OUTPUT_FILE>" [excludeEmpty="true"]/>

### Attributes, for both Edge- and Lane-Based Noise Output

Attribute Name | Value Type | Description
--- | --- | ---
id | id (string) | The id of the detector
freq | int (time) | The aggregation period the values the detector collects shall be summed up.
file | filename | The path to the output file. The path may be relative.
begin | int (time) | The time to start writing (intervals starting before this time are discarded). If not given, the simulation's begin is used.
end | int (time) | The time to end writing (intervals starting at or after this time are discarded). If not given the simulation's end is used.
excludeEmpty | bool | If set, edges/lanes which were not use by a vehicle during this period will not be written; default: false.

## Generated Output

### Edge-Based Network States

### Lane-Based Network States

### Value Descriptions

Name | Type | Description
--- | --- | ---
begin | (simulation) seconds | The first time step the values were collected in
end | (simulation) seconds | The last time step + DELTA_T in which the reported values were collected
edge@id | (edge) id | The name of the reported edge
lane@id | (lane) id | The name of the reported lane
sampledSeconds | s | Number seconds vehicles were measured on the edge/lane (may be subseconds if a vehicle enters/leaves the edge/lane)
noise | dBA | The noise generated by the vehicles on the edge/lane during the interval

## Notes

Notes:

- Per default, all edges are written, even those on which no vehicle drove. It can be disabled setting the excludeEmpty attribute to true.
- The interval end is the interval begin + aggregation time, meaning that values were collected within these steps excluding the end time itself. If the simulation ends before the last interval is over, the interval will be prunned.
- The output file will be generated, does not have to exist earlier and will be overwritten if existing without any warning. The folder the output file shall be generated in must exist.
- If you need only information about the network states during certain time periods, you may constraint generation of the dumps by giving attributes "begin="<TIME>[,<TIME>]+"" and "end="<TIME>[,<TIME>]+"". When at least one combination is given, dumps will be written only if an according begin/end-pair exists for the current time. This means, only those intervals will be saved for which begin[x]<=INTERVAL_END and end[x]>=INTERVAL_BEGIN. All dumps will cover the complete simulation if no values for begin/end are given.

## See Also

- edge/lane-based network performace measures output and edge/lane-based vehicular pollutant emission output which have similar formats
- The mpl_dump_onNet.py script can display values of this output as a colored net (and further visualization tools exist).

This page was last modified on 20 February 2012, at 09:26.