SUMO
Simulation of Urban MObility

- Home
- Download
- Documentation
- Wiki
- Trac
- Blog
- Contact
- SF-Project

# Z/Changes from Version 0.10.1 to Version 0.10.2

- All
  - If configuration is written using --write-config, the application stops after this step
  - The devices now also allow "NUL" or "/dev/NULL" as output file name. In this case, the output is redirected to NUL (MS Windows) or /dev/null (Linux)

- GUISIM
  - solved bug 2519476: vss are not shown properly
  - solved bug 2510002: Crash on vss manipulator
  - debugged size info ("legend") drawing
  - solved bug 2519761: guisim crashes on "show all routes"
  - changed how decals are aligned (see SUMO-GUI#Using_Decals_within_SUMO-GUI)
  - Consolidated the startup-options --suppress-end-info and --quit-on-end: --suppress-end-info was removed, the application quits after performing the simulation when --quit-on-end is given. This is also done even if errors occured
  - added the possibility to copy the cursor position to clipboard
  - debugged false position information within the popup-menu of a lane
  - Tests based on SUMO tests are now also performed for GUISIM. Thanks to Michael Behrisch for this very nice work

- Simulation
  - solved bug 2524031: sumo xml parser relies on sequence order instead IDs; thanks to Andrey Gursky for supplying the example
  - solved bug 2519762: rerouter are not shown properly
  - solved bug 2105526: Subsecond simulation does not compile
  - changed default simulation end time to INT_MAX
  - simulation stops on running empty only if there is no end time specified
  - closed work on pollutant emission modelling based on HBEFA

- Netconvert / Netgen
  - trying to deal with problems on network building; networks are more correct for most cases, but may look weird sometimes
  - solved defect 38: speed instead of length while importing XML
  - changed the tls-guessing procedure (unverified, yet); tls which span over multiple junctions can now been "guessed" if both, nodes are marked as being controlled by traffic lights or not within the imported data; see also: task 42: (TAPAS) add possibility to generate joined tls if tls are given

- Polyconvert
  - solved defect 14: polyconvert does not report about double ids
  - renamed option --xml-points to --xml
  - renamed option --shape-files to --shape-file

- Tools
  - Rebuilt traceExporter; added tests

- Documentation
  - solved bug 1993983: Errors in User Documentation

- TAPAS
  - see TAPASCologne Change Log

This page was last modified on 27 October 2011, at 07:40.