SUMO
Simulation of Urban MObility

- Home
- Download
- Documentation
- Wiki
- Trac
- Blog
- Contact
- SF-Project

# TraCI/Change Route State

# Command 0xc6: Change Route State

ubyte | string | ubyte | <value_type>
Variable | Route ID | Type of the value | New Value
--- | --- | --- | ---

Changes the state of a route. Because it is possible to change different values of a route, the given value may have different types. The following values can be changed, the type of the value to given is also shown in the table.

Overview Changeable Route Variables
Variable | ValueType | Description
--- | --- | ---
add (0x80) | stringList | Adds a new route; the route gets the given id and follows the given edges.

This page was last modified on 8 October 2012, at 11:31.