SUMO
Simulation of Urban MObility

- Home
- Download
- Documentation
- Wiki
- Trac
- Blog
- Contact
- SF-Project

# Tutorials/OSMActivityGen/eichstaett.net.xml

eichstaett.net.xml

SUMO network of the German city Eichstätt. It is based on an optimized OpenStreetMap file following the Tutorials/Import from OpenStreetMap. The netconvert call was:

    netconvert --xml-type-files ../../edge-type-templates/osm-urban-de.typ.xml --guess-ramps --remove-edges.by-vclass hov,taxi,bus,delivery,transport,lightrail,cityrail,rail_slow,rail_fast,motorcycle,bicycle,pedestrian --remove-geometry --remove-isolated --try-join-tls --verbose --seed 1 --osm-files eichstaett.osm --output-file eichstaett.net.xml

You can use this file if you need a road network of a town with about 13,000 inhabitants. All roads were verified to have the right highway type, speed limit and one-way attribute. All traffic lights of cars (not all pedestrian lights) were also verified. See also Tutorials/OSMActivityGen/eichstaett.osm.

Author | W. Bamberger
Source | Tutorials/OSMActivityGen/eichstaett.osm by W. Bamberger. Map data © OpenStreetMap contributors, CC-BY-SA
History | This file is located in the SUMO Subversion repository. See the log there.
License | This work is licensed under a Creative Commons Attribution-ShareAlike 3.0 Unported License. The authors are listed in the history.

This page was last modified on 4 October 2012, at 12:45.