SUMO
Simulation of Urban MObility

- Home
- Download
- Documentation
- Wiki
- Trac
- Blog
- Contact
- SF-Project

# Z/Changes from Version 0.11.1 to Version 0.12.0

Release date: 27.05.2010

- Simulation
  - solved regarding red light late blocks vehicles
  - corrected the documentation on using an abstract vehicle class; the attribute which defines it is named vclass not class.
  - introducing flows as replacement for vehicles with repno and period
  - introducing stops in routes
  - corrected unmotivated deceleration in front of intersections reported by Björn Hendriks (thanks!)
  - added option --sloppy-emit for not trying to emit on full edges (speeds up the simulation a lot)

- TraCI
  - moved to representation of time in milliseconds
  - Induction Loop occupancy is now given in % as defined

- SUMO-GUI
  - Improved layering (correct order of element drawing)
  - solved bug 2872900: same title/naming for different dialog boxes
  - solved bug 2872824: fox related sumo crash
  - Viewport settings can now be saved/loaded
  - Added new visualisation options
    - lanes: by vclass
    - vehicles: HSV by depart position/arrival position/direction and distance

- ROUTER
  - removed random routes generation; introduced a script for generating random trips instead

- NETCONVERT
  - removed the --tls-poi-output; instead, poi_atTLS.py can be used
  - OpenStreetMap import
    - removal of edges and nodes which have the attribute action='delete'
    - recognition and removal of duplicate edges (all values but ids are same) added
    - opposite direction edge is built if oneway==-1
  - edge and node attributes can be overridden

- Tools
  - tools for easier open street map import added

This page was last modified on 23 September 2011, at 07:36.