;DrIvEr DeScRiPtIoN
; VeRsIoN=1.11 Novell LAN Installation Information File for BCM570X.
; CoPyRiGhT=(c) Copyright 2000-2007 Broadcom Corporation. All rights reserved.
; B57.ldi
; Broadcom Corporation

VER:	1.11
SYN:	1.00

DR BCM570X_XG
{

   DES: 	$bcm_1
   HELP:	$bcm_5
   PAR: 	2.00

   FILE: 	B57.LAN

   PROD:    'PCI.14E4.1644.*.*.*',	;5700
            'PCI.14E4.1645.*.*.*',	;5701
            'PCI.14E4.1646.*.*.*',	;5702
            'PCI.14E4.16A6.*.*.*',	;5702s
            'PCI.14E4.1647.*.*.*',	;5703
            'PCI.14E4.16A7.*.*.*',	;5703s
            'PCI.14E4.1648.*.*.*',	;5704
            'PCI.14E4.16A8.*.*.*',	;5704s
            'PCI.14E4.164d.*.*.*',	;5702fe
            'PCI.14E4.1653.*.*.*',	;5705
            'PCI.14E4.1654.*.*.*',	;5705
            'PCI.14E4.165d.*.*.*',	;5705m
            'PCI.14E4.165e.*.*.*',	;5705m
            'PCI.14E4.166d.*.*.*',	;5705mfe
            'PCI.14E4.1696.*.*.*',	;5782
            'PCI.14E4.16c6.*.*.*',	;5702a3
            'PCI.14E4.16c7.*.*.*',	;5702a3
            'PCI.14E4.1676.*.*.*',	;5750
            'PCI.14E4.167c.*.*.*',	;5750m
            'PCI.14E4.1677.*.*.*',	;5751
            'PCI.14E4.167d.*.*.*',	;5751m
            'PCI.14E4.1658.*.*.*',	;5720
            'PCI.14E4.1659.*.*.*',	;5721
            'PCI.14E4.16f7.*.*.*',	;5753
            'PCI.14E4.16fd.*.*.*',	;5753m
            'PCI.14e4.1600.*.*.*',	;5752
            'PCI.14e4.1601.*.*.*',	;5752m
            'PCI.14e4.1668.*.*.*',	;5714
            'PCI.14e4.1669.*.*.*',	;5714s
            'PCI.14e4.1678.*.*.*',	;5715
            'PCI.14e4.1679.*.*.*',	;5715s
            'PCI.14e4.167a.*.*.*',  ;5754
            'PCI.14e4.1672.*.*.*',  ;5754m
            'PCI.14e4.166a.*.*.*',	;5780
            'PCI.14e4.166b.*.*.*',	;5780s
            'PCI.14e4.1673.*.*.*',	;5755m
            'PCI.14e4.167b.*.*.*',	;5755
            'PCI.14e4.1674.*.*.*',	;5756me
            'PCI.14e4.165a.*.*.*',	;5722
            'PCI.14e4.16ff.*.*.*',	;5903M
            'PCI.14e4.1680.*.*.*',	;5761e
            'PCI.14e4.1681.*.*.*',	;5761
            'PCI.14e4.1684.*.*.*',	;5764
            'PCI.14e4.1698.*.*.*',	;5784
            'PCI.14e4.165b.*.*.*'   ;5723
                                    
   ;@#	 SPROD: 'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#          'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#          'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Gigabit Ethernet Adapter'

   ;@#   CLIENT:B57.LAN
   ;@#	 ALIAS: B57.LAN


   PR	SLOT OPT
   {
	DES:	$bcm_6
	HELP:	$bcm_7
	default: UND
   }

   FR	FrameSelect
   {
	DES:	$bcm_8
	HELP:	$bcm_9

	CD:	$bcm_10
	CH:	'Ethernet_802.2'

	CD:	$bcm_11
	CH:	'Ethernet_802.3'

	CD:	$bcm_12
	CH:	'Ethernet_SNAP'

	CD:	$bcm_13
	CH:	'Ethernet_II'

	Default: 1,2,3,4
   }

   LIST SPEED OPT
   {
		DES: $bcm_14

		HELP: $bcm_15 

		CD: $bcm_16 
		CH: $bcm_17 

		CD: $bcm_18 
		CH: $bcm_19 

		CD: $bcm_20 
		CH: $bcm_21 

		CD: $bcm_22 
		CH: $bcm_23 

		CD: $bcm_24 
		CH: $bcm_25 

		Default: 1

		OutputFormat: 'Speed=%s'
   }

   PR RXBUFFERS OPT
   {
	  DES:  $bcm_26 

	  HELP: $bcm_34 

	  TYPE:    DECIMAL(3)
	  VAL:     2-512

	  Default: 200
	  OutputFormat: 'RxBuffers=%s'
   }

}


DR BCM570X_XF
{

   DES: 	$bcm_2
   HELP:	$bcm_5
   PAR: 	2.00

   FILE: 	B57.LAN

   PROD: 	'PCI.14E4.170d.*.*.*',	;5901
            'PCI.14E4.170e.*.*.*',      ;5901
           	'PCI.14E4.167e.*.*.*',	;5751f
         	'PCI.14E4.16fe.*.*.*',	;5753f
         	'PCI.14E4.1712.*.*.*',	;5906
         	'PCI.14E4.1713.*.*.*'	;5906m


   ;@#	 SPROD: 'Broadcom~NetXtreme Fast Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Fast Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Fast Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Fast Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Fast Ethernet Adapter',
   ;@#	        'Broadcom~NetXtreme Fast Ethernet Adapter'


   ;@#   CLIENT:B57.LAN
   ;@#	 ALIAS: B57.LAN


   PR	SLOT OPT
   {
	DES:	$bcm_6
	HELP:	$bcm_7
	default: UND
   }

   FR	FrameSelect
   {
	DES:	$bcm_8
	HELP:	$bcm_9

	CD:	$bcm_10
	CH:	'Ethernet_802.2'

	CD:	$bcm_11
	CH:	'Ethernet_802.3'

	CD:	$bcm_12
	CH:	'Ethernet_SNAP'

	CD:	$bcm_13
	CH:	'Ethernet_II'

	Default: 1,2,3,4
   }

   LIST SPEED OPT
   {
		DES: $bcm_14

		HELP: $bcm_15 

		CD: $bcm_16 
		CH: $bcm_17 

		CD: $bcm_18 
		CH: $bcm_19 

		CD: $bcm_20 
		CH: $bcm_21 

		CD: $bcm_22 
		CH: $bcm_23 

		CD: $bcm_24 
		CH: $bcm_25 

		Default: 1

		OutputFormat: 'Speed=%s'
   }

   PR RXBUFFERS OPT
   {
	  DES:  $bcm_26 

	  HELP: $bcm_34 

	  TYPE:    DECIMAL(3)
	  VAL:     2-512

	  Default: 200
	  OutputFormat: 'RxBuffers=%s'
   }

}


DR BCM570X_LG
{

   DES: 	$bcm_3
   HELP:	$bcm_35
   PAR: 	2.00

   FILE: 	B57.LAN

   PROD: 	'PCI.14E4.169c.*.*.*',	;5788
          	'PCI.14E4.169d.*.*.*',	;5789
    		'PCI.14E4.16dd.*.*.*',	;5781
         	'PCI.14e4.169b.*.*.*',	;5787
         	'PCI.14e4.1693.*.*.*',	;5787M
         	'PCI.14e4.169a.*.*.*'	;5786



   ;@#	 SPROD: 'Broadcom~NetLink Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetLink Gigabit Ethernet Adapter',
   ;@#          'Broadcom~NetLink Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetLink Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetLink Gigabit Ethernet Adapter',
   ;@#	        'Broadcom~NetLink Gigabit Ethernet Adapter'


   ;@#   CLIENT:B57.LAN
   ;@#	 ALIAS: B57.LAN


   PR	SLOT OPT
   {
	DES:	$bcm_3
	HELP:	$bcm_4
	default: UND
   }

   FR	FrameSelect
   {
	DES:	$bcm_5
	HELP:	$bcm_6

	CD:	$bcm_7
	CH:	'Ethernet_802.2'

	CD:	$bcm_8
	CH:	'Ethernet_802.3'

	CD:	$bcm_9
	CH:	'Ethernet_SNAP'

	CD:	$bcm_10
	CH:	'Ethernet_II'

	Default: 1,2,3,4
   }

   LIST SPEED OPT
   {
		DES: $bcm_11

		HELP: $bcm_12 

		CD: $bcm_13 
		CH: $bcm_14 

		CD: $bcm_15 
		CH: $bcm_16 

		CD: $bcm_17 
		CH: $bcm_18 

		CD: $bcm_19 
		CH: $bcm_20 

		CD: $bcm_21 
		CH: $bcm_22 

		Default: 1

		OutputFormat: 'Speed=%s'
   }

   PR RXBUFFERS OPT
   {
	  DES:  $bcm_23 

	  HELP: $bcm_34 

	  TYPE:    DECIMAL(3)
	  VAL:     2-512

	  Default: 200
	  OutputFormat: 'RxBuffers=%s'
   }

}


DR BCM570X_LF
{

   DES: 	$bcm_4
   HELP:	$bcm_35
   PAR: 	2.00

   FILE: 	B57.LAN

   PROD: 	'PCI.14e4.167f.*.*.*'       ;5787f


   ;@#	 SPROD: 'Broadcom~NetLink Fast Ethernet Adapter'


   ;@#   CLIENT:B57.LAN
   ;@#	 ALIAS: B57.LAN


   PR	SLOT OPT
   {
	DES:	$bcm_3
	HELP:	$bcm_4
	default: UND
   }

   FR	FrameSelect
   {
	DES:	$bcm_5
	HELP:	$bcm_6

	CD:	$bcm_7
	CH:	'Ethernet_802.2'

	CD:	$bcm_8
	CH:	'Ethernet_802.3'

	CD:	$bcm_9
	CH:	'Ethernet_SNAP'

	CD:	$bcm_10
	CH:	'Ethernet_II'

	Default: 1,2,3,4
   }

   LIST SPEED OPT
   {
		DES: $bcm_11

		HELP: $bcm_12 

		CD: $bcm_13 
		CH: $bcm_14 

		CD: $bcm_15 
		CH: $bcm_16 

		CD: $bcm_17 
		CH: $bcm_18 

		CD: $bcm_19 
		CH: $bcm_20 

		CD: $bcm_21 
		CH: $bcm_22 

		Default: 1

		OutputFormat: 'Speed=%s'
   }

   PR RXBUFFERS OPT
   {
	  DES:  $bcm_23 

	  HELP: $bcm_34 

	  TYPE:    DECIMAL(3)
	  VAL:     2-512

	  Default: 200
	  OutputFormat: 'RxBuffers=%s'
   }

}


DLANG:	4
;English
	$bcm_1 = "Broadcom NetXtreme Gigabit Ethernet Driver "
	$bcm_2 = "Broadcom NetXtreme Fast Ethernet Driver "
	$bcm_3 = "Broadcom NetLink Gigabit Ethernet Driver "
	$bcm_4 = "Broadcom NetLink Fast Ethernet Driver "
	$bcm_5 = "This driver supports all Broadcom NetXtreme Ethernet Adapters."
	$bcm_6 = "Slot Number"
	$bcm_7 = "Select a slot number. If unsure which slot the adapter is in, choose an arbitrary slot number."
	$bcm_8 = "Frame Types"
	$bcm_9 = "Select a frame."
	$bcm_10 = "802.2"
	$bcm_11 = "802.3"
	$bcm_12 = "802.2 SNAP"
	$bcm_13 = "Ethernet II"
	$bcm_14 = "Line Speed"
	$bcm_15 = "Automatic Detection mode is the default, preferred and reliable mode.
			   To force the media access mode, select a Speed and Duplex mode."
	$bcm_16 = "Automatic Detection"
	$bcm_17 = "AUTO"
	$bcm_18 = "100 Mbs Full Duplex"
	$bcm_19 = '100FD'
	$bcm_20 = "100 Mbs Half Duplex"
	$bcm_21 = '100HD'
	$bcm_22 = "10 Mbs Full Duplex"
	$bcm_23 = '10FD'
	$bcm_24 = "10 Mbs Half Duplex"
	$bcm_25 = '10HD'
	$bcm_26 = "Receive Buffers"
	$bcm_34 = "To change the default amount of receive buffers the adapter uses, enter a value within the allowable range."
	$bcm_35 = "This driver supports all Broadcom NetLink Ethernet Adapters."


LANG:	6
;French
	$bcm_1 = "Broadcom NetXtreme Gigabit Ethernet Driver "
	$bcm_2 = "Broadcom NetXtreme Fast Ethernet Driver "
	$bcm_3 = "Broadcom NetLink Gigabit Ethernet Driver "
	$bcm_4 = "Broadcom NetLink Fast Ethernet Driver "
	$bcm_5 = "This driver supports all Broadcom NetXtreme Ethernet Adapters."
	$bcm_6 = "Slot Number"
	$bcm_7 = "Select a slot number. If unsure which slot the adapter is in, choose an arbitrary slot number."
	$bcm_8 = "Frame Types"
	$bcm_9 = "Select a frame."
	$bcm_10 = "802.2"
	$bcm_11 = "802.3"
	$bcm_12 = "802.2 SNAP"
	$bcm_13 = "Ethernet II"
	$bcm_14 = "Line Speed"
	$bcm_15 = "Automatic Detection mode is the default, preferred and reliable mode.
			   To force the media access mode, select a Speed and Duplex mode."
	$bcm_16 = "Automatic Detection"
	$bcm_17 = "AUTO"
	$bcm_18 = "100 Mbs Full Duplex"
	$bcm_19 = '100FD'
	$bcm_20 = "100 Mbs Half Duplex"
	$bcm_21 = '100HD'
	$bcm_22 = "10 Mbs Full Duplex"
	$bcm_23 = '10FD'
	$bcm_24 = "10 Mbs Half Duplex"
	$bcm_25 = '10HD'
	$bcm_26 = "Receive Buffers"
	$bcm_34 = "To change the default amount of receive buffers the adapter uses, enter a value within the allowable range."
	$bcm_35 = "This driver supports all Broadcom NetLink Ethernet Adapters."

LANG:	7
;German
	$bcm_1 = "Broadcom NetXtreme Gigabit Ethernet Driver "
	$bcm_2 = "Broadcom NetXtreme Fast Ethernet Driver "
	$bcm_3 = "Broadcom NetLink Gigabit Ethernet Driver "
	$bcm_4 = "Broadcom NetLink Fast Ethernet Driver "
	$bcm_5 = "This driver supports all Broadcom NetXtreme Ethernet Adapters."
	$bcm_6 = "Slot Number"
	$bcm_7 = "Select a slot number. If unsure which slot the adapter is in, choose an arbitrary slot number."
	$bcm_8 = "Frame Types"
	$bcm_9 = "Select a frame."
	$bcm_10 = "802.2"
	$bcm_11 = "802.3"
	$bcm_12 = "802.2 SNAP"
	$bcm_13 = "Ethernet II"
	$bcm_14 = "Line Speed"
	$bcm_15 = "Automatic Detection mode is the default, preferred and reliable mode.
			   To force the media access mode, select a Speed and Duplex mode."
	$bcm_16 = "Automatic Detection"
	$bcm_17 = "AUTO"
	$bcm_18 = "100 Mbs Full Duplex"
	$bcm_19 = '100FD'
	$bcm_20 = "100 Mbs Half Duplex"
	$bcm_21 = '100HD'
	$bcm_22 = "10 Mbs Full Duplex"
	$bcm_23 = '10FD'
	$bcm_24 = "10 Mbs Half Duplex"
	$bcm_25 = '10HD'
	$bcm_26 = "Receive Buffers"
	$bcm_34 = "To change the default amount of receive buffers the adapter uses, enter a value within the allowable range."
	$bcm_35 = "This driver supports all Broadcom NetLink Ethernet Adapters."


LANG:	8
;Italian
	$bcm_1 = "Broadcom NetXtreme Gigabit Ethernet Driver "
	$bcm_2 = "Broadcom NetXtreme Fast Ethernet Driver "
	$bcm_3 = "Broadcom NetLink Gigabit Ethernet Driver "
	$bcm_4 = "Broadcom NetLink Fast Ethernet Driver "
	$bcm_5 = "This driver supports all Broadcom NetXtreme Ethernet Adapters."
	$bcm_6 = "Slot Number"
	$bcm_7 = "Select a slot number. If unsure which slot the adapter is in, choose an arbitrary slot number."
	$bcm_8 = "Frame Types"
	$bcm_9 = "Select a frame."
	$bcm_10 = "802.2"
	$bcm_11 = "802.3"
	$bcm_12 = "802.2 SNAP"
	$bcm_13 = "Ethernet II"
	$bcm_14 = "Line Speed"
	$bcm_15 = "Automatic Detection mode is the default, preferred and reliable mode.
			   To force the media access mode, select a Speed and Duplex mode."
	$bcm_16 = "Automatic Detection"
	$bcm_17 = "AUTO"
	$bcm_18 = "100 Mbs Full Duplex"
	$bcm_19 = '100FD'
	$bcm_20 = "100 Mbs Half Duplex"
	$bcm_21 = '100HD'
	$bcm_22 = "10 Mbs Full Duplex"
	$bcm_23 = '10FD'
	$bcm_24 = "10 Mbs Half Duplex"
	$bcm_25 = '10HD'
	$bcm_26 = "Receive Buffers"
	$bcm_34 = "To change the default amount of receive buffers the adapter uses, enter a value within the allowable range."
	$bcm_35 = "This driver supports all Broadcom NetLink Ethernet Adapters."

LANG:	14
;Spanish
	$bcm_1 = "Broadcom NetXtreme Gigabit Ethernet Driver "
	$bcm_2 = "Broadcom NetXtreme Fast Ethernet Driver "
	$bcm_3 = "Broadcom NetLink Gigabit Ethernet Driver "
	$bcm_4 = "Broadcom NetLink Fast Ethernet Driver "
	$bcm_5 = "This driver supports all Broadcom NetXtreme Ethernet Adapters."
	$bcm_6 = "Slot Number"
	$bcm_7 = "Select a slot number. If unsure which slot the adapter is in, choose an arbitrary slot number."
	$bcm_8 = "Frame Types"
	$bcm_9 = "Select a frame."
	$bcm_10 = "802.2"
	$bcm_11 = "802.3"
	$bcm_12 = "802.2 SNAP"
	$bcm_13 = "Ethernet II"
	$bcm_14 = "Line Speed"
	$bcm_15 = "Automatic Detection mode is the default, preferred and reliable mode.
			   To force the media access mode, select a Speed and Duplex mode."
	$bcm_16 = "Automatic Detection"
	$bcm_17 = "AUTO"
	$bcm_18 = "100 Mbs Full Duplex"
	$bcm_19 = '100FD'
	$bcm_20 = "100 Mbs Half Duplex"
	$bcm_21 = '100HD'
	$bcm_22 = "10 Mbs Full Duplex"
	$bcm_23 = '10FD'
	$bcm_24 = "10 Mbs Half Duplex"
	$bcm_25 = '10HD'
	$bcm_26 = "Receive Buffers"
	$bcm_34 = "To change the default amount of receive buffers the adapter uses, enter a value within the allowable range."
	$bcm_35 = "This driver supports all Broadcom NetLink Ethernet Adapters."

LANG:	1
;Chinese-Simplified
	$bcm_1 = "Broadcom NetXtreme Gigabit Ethernet Driver "
	$bcm_2 = "Broadcom NetXtreme Fast Ethernet Driver "
	$bcm_3 = "Broadcom NetLink Gigabit Ethernet Driver "
	$bcm_4 = "Broadcom NetLink Fast Ethernet Driver "
	$bcm_5 = "This driver supports all Broadcom NetXtreme Ethernet Adapters."
	$bcm_6 = "Slot Number"
	$bcm_7 = "Select a slot number. If unsure which slot the adapter is in, choose an arbitrary slot number."
	$bcm_8 = "Frame Types"
	$bcm_9 = "Select a frame."
	$bcm_10 = "802.2"
	$bcm_11 = "802.3"
	$bcm_12 = "802.2 SNAP"
	$bcm_13 = "Ethernet II"
	$bcm_14 = "Line Speed"
	$bcm_15 = "Automatic Detection mode is the default, preferred and reliable mode.
			   To force the media access mode, select a Speed and Duplex mode."
	$bcm_16 = "Automatic Detection"
	$bcm_17 = "AUTO"
	$bcm_18 = "100 Mbs Full Duplex"
	$bcm_19 = '100FD'
	$bcm_20 = "100 Mbs Half Duplex"
	$bcm_21 = '100HD'
	$bcm_22 = "10 Mbs Full Duplex"
	$bcm_23 = '10FD'
	$bcm_24 = "10 Mbs Half Duplex"
	$bcm_25 = '10HD'
	$bcm_26 = "Receive Buffers"
	$bcm_34 = "To change the default amount of receive buffers the adapter uses, enter a value within the allowable range."
	$bcm_35 = "This driver supports all Broadcom NetLink Ethernet Adapters."

LANG:	9
;Japanese
	$bcm_1 = "Broadcom NetXtreme Gigabit Ethernet Driver "
	$bcm_2 = "Broadcom NetXtreme Fast Ethernet Driver "
	$bcm_3 = "Broadcom NetLink Gigabit Ethernet Driver "
	$bcm_4 = "Broadcom NetLink Fast Ethernet Driver "
	$bcm_5 = "This driver supports all Broadcom NetXtreme Ethernet Adapters."
	$bcm_6 = "Slot Number"
	$bcm_7 = "Select a slot number. If unsure which slot the adapter is in, choose an arbitrary slot number."
	$bcm_8 = "Frame Types"
	$bcm_9 = "Select a frame."
	$bcm_10 = "802.2"
	$bcm_11 = "802.3"
	$bcm_12 = "802.2 SNAP"
	$bcm_13 = "Ethernet II"
	$bcm_14 = "Line Speed"
	$bcm_15 = "Automatic Detection mode is the default, preferred and reliable mode.
			   To force the media access mode, select a Speed and Duplex mode."
	$bcm_16 = "Automatic Detection"
	$bcm_17 = "AUTO"
	$bcm_18 = "100 Mbs Full Duplex"
	$bcm_19 = '100FD'
	$bcm_20 = "100 Mbs Half Duplex"
	$bcm_21 = '100HD'
	$bcm_22 = "10 Mbs Full Duplex"
	$bcm_23 = '10FD'
	$bcm_24 = "10 Mbs Half Duplex"
	$bcm_25 = '10HD'
	$bcm_26 = "Receive Buffers"
	$bcm_34 = "To change the default amount of receive buffers the adapter uses, enter a value within the allowable range."
	$bcm_35 = "This driver supports all Broadcom NetLink Ethernet Adapters."

LANG:	10
;Korean
	$bcm_1 = "Broadcom NetXtreme Gigabit Ethernet Driver "
	$bcm_2 = "Broadcom NetXtreme Fast Ethernet Driver "
	$bcm_3 = "Broadcom NetLink Gigabit Ethernet Driver "
	$bcm_4 = "Broadcom NetLink Fast Ethernet Driver "
	$bcm_5 = "This driver supports all Broadcom NetXtreme Ethernet Adapters."
	$bcm_6 = "Slot Number"
	$bcm_7 = "Select a slot number. If unsure which slot the adapter is in, choose an arbitrary slot number."
	$bcm_8 = "Frame Types"
	$bcm_9 = "Select a frame."
	$bcm_10 = "802.2"
	$bcm_11 = "802.3"
	$bcm_12 = "802.2 SNAP"
	$bcm_13 = "Ethernet II"
	$bcm_14 = "Line Speed"
	$bcm_15 = "Automatic Detection mode is the default, preferred and reliable mode.
			   To force the media access mode, select a Speed and Duplex mode."
	$bcm_16 = "Automatic Detection"
	$bcm_17 = "AUTO"
	$bcm_18 = "100 Mbs Full Duplex"
	$bcm_19 = '100FD'
	$bcm_20 = "100 Mbs Half Duplex"
	$bcm_21 = '100HD'
	$bcm_22 = "10 Mbs Full Duplex"
	$bcm_23 = '10FD'
	$bcm_24 = "10 Mbs Half Duplex"
	$bcm_25 = '10HD'
	$bcm_26 = "Receive Buffers"
	$bcm_34 = "To change the default amount of receive buffers the adapter uses, enter a value within the allowable range."
	$bcm_35 = "This driver supports all Broadcom NetLink Ethernet Adapters."

LANG:	13
;Russian
	$bcm_1 = "Broadcom NetXtreme Gigabit Ethernet Driver "
	$bcm_2 = "Broadcom NetXtreme Fast Ethernet Driver "
	$bcm_3 = "Broadcom NetLink Gigabit Ethernet Driver "
	$bcm_4 = "Broadcom NetLink Fast Ethernet Driver "
	$bcm_5 = "This driver supports all Broadcom NetXtreme Ethernet Adapters."
	$bcm_6 = "Slot Number"
	$bcm_7 = "Select a slot number. If unsure which slot the adapter is in, choose an arbitrary slot number."
	$bcm_8 = "Frame Types"
	$bcm_9 = "Select a frame."
	$bcm_10 = "802.2"
	$bcm_11 = "802.3"
	$bcm_12 = "802.2 SNAP"
	$bcm_13 = "Ethernet II"
	$bcm_14 = "Line Speed"
	$bcm_15 = "Automatic Detection mode is the default, preferred and reliable mode.
			   To force the media access mode, select a Speed and Duplex mode."
	$bcm_16 = "Automatic Detection"
	$bcm_17 = "AUTO"
	$bcm_18 = "100 Mbs Full Duplex"
	$bcm_19 = '100FD'
	$bcm_20 = "100 Mbs Half Duplex"
	$bcm_21 = '100HD'
	$bcm_22 = "10 Mbs Full Duplex"
	$bcm_23 = '10FD'
	$bcm_24 = "10 Mbs Half Duplex"
	$bcm_25 = '10HD'
	$bcm_26 = "Receive Buffers"
	$bcm_34 = "To change the default amount of receive buffers the adapter uses, enter a value within the allowable range."
	$bcm_35 = "This driver supports all Broadcom NetLink Ethernet Adapters."

LANG:	16
;Chinese-Traditional
	$bcm_1 = "Broadcom NetXtreme Gigabit Ethernet Driver "
	$bcm_2 = "Broadcom NetXtreme Fast Ethernet Driver "
	$bcm_3 = "Broadcom NetLink Gigabit Ethernet Driver "
	$bcm_4 = "Broadcom NetLink Fast Ethernet Driver "
	$bcm_5 = "This driver supports all Broadcom NetXtreme Ethernet Adapters."
	$bcm_6 = "Slot Number"
	$bcm_7 = "Select a slot number. If unsure which slot the adapter is in, choose an arbitrary slot number."
	$bcm_8 = "Frame Types"
	$bcm_9 = "Select a frame."
	$bcm_10 = "802.2"
	$bcm_11 = "802.3"
	$bcm_12 = "802.2 SNAP"
	$bcm_13 = "Ethernet II"
	$bcm_14 = "Line Speed"
	$bcm_15 = "Automatic Detection mode is the default, preferred and reliable mode.
			   To force the media access mode, select a Speed and Duplex mode."
	$bcm_16 = "Automatic Detection"
	$bcm_17 = "AUTO"
	$bcm_18 = "100 Mbs Full Duplex"
	$bcm_19 = '100FD'
	$bcm_20 = "100 Mbs Half Duplex"
	$bcm_21 = '100HD'
	$bcm_22 = "10 Mbs Full Duplex"
	$bcm_23 = '10FD'
	$bcm_24 = "10 Mbs Half Duplex"
	$bcm_25 = '10HD'
	$bcm_26 = "Receive Buffers"
	$bcm_34 = "To change the default amount of receive buffers the adapter uses, enter a value within the allowable range."
	$bcm_35 = "This driver supports all Broadcom NetLink Ethernet Adapters."

