; Copyright 2001-2005 Broadcom Corporation.
; INF for Windows Me, and 98SE

; InfVersion   10.26.0.0.D

[Version]
Signature   = "$Chicago$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
CatalogFile = b57win32.cat
Compatible  = 1
Provider    = %BRCM%
DriverVer   = 03/06/2007,10.26.0.0

[Manufacturer]
%BRCM% = Broadcom

[ControlFlags]
ExcludeFromSelect = *

[Broadcom]
%BCM5700%   = BCM5700.Inst,   PCI\VEN_14e4&DEV_1644
%BCM5701%   = BCM5701.Inst,   PCI\VEN_14e4&DEV_1645
%BCM5702%   = BCM5702.Inst,   PCI\VEN_14e4&DEV_1646
%BCM5702%   = BCM5702.Inst,   PCI\VEN_14e4&DEV_16A6
%BCM5702%   = BCM5702A3.Inst, PCI\VEN_14e4&DEV_16C6
%BCM5703%   = BCM5703.Inst,   PCI\VEN_14e4&DEV_1647
%BCM5703%   = BCM5703.Inst,   PCI\VEN_14e4&DEV_16A7
%BCM5703%   = BCM5703A3.Inst, PCI\VEN_14e4&DEV_16C7
%BCM5704%   = BCM5704.Inst,   PCI\VEN_14e4&DEV_1648
%BCM5705%   = BCM5705.Inst,   PCI\VEN_14e4&DEV_1653
%BCM5705M%  = BCM5705M.Inst,  PCI\VEN_14e4&DEV_165D
%BCM5705%   = BCM5705A2.Inst, PCI\VEN_14e4&DEV_1654
%BCM5705M%  = BCM5705MA2.Inst,PCI\VEN_14e4&DEV_165e
%BCM5705F%  = BCM5705F.Inst,  PCI\VEN_14e4&DEV_166e

%BCM5705M%  = BCM5705MA2.Inst,PCI\VEN_14e4&DEV_165e&SUBSYS_0890103c
%BCM5705M%  = BCM5705MA2.Inst,PCI\VEN_14e4&DEV_165e&SUBSYS_0894103c
%BCM5705M%  = BCM5705MA2.Inst,PCI\VEN_14e4&DEV_165e&SUBSYS_088c103c
%BCM5705M%  = BCM5705MA2.Inst,PCI\VEN_14e4&DEV_165e&SUBSYS_08bc103c
%BCM5705M%  = BCM5705MA2.Inst,PCI\VEN_14e4&DEV_165e&SUBSYS_3000103c
%BCM5705M%  = BCM5705MA2.Inst,PCI\VEN_14e4&DEV_165e&SUBSYS_099c103c
%BCM5705M%  = BCM5705MA2.Inst,PCI\VEN_14e4&DEV_165e&SUBSYS_0727152d

%BCM5750%   = BCM5750.Inst,   PCI\VEN_14e4&DEV_1658&REV_00
%BCM5750%   = BCM5750.Inst,   PCI\VEN_14e4&DEV_1659&REV_00
%BCM5750%   = BCM5750.Inst,   PCI\VEN_14e4&DEV_1676&REV_00
%BCM5750%   = BCM5750.Inst,   PCI\VEN_14e4&DEV_1677&REV_00
%BCM5750%   = BCM5750.Inst,   PCI\VEN_14e4&DEV_167C&REV_00
%BCM5750%   = BCM5750.Inst,   PCI\VEN_14e4&DEV_167D&REV_00

%BCM5750A1%   = BCM5750A1.Inst,     PCI\VEN_14e4&DEV_1658
%BCM5750A1%   = BCM5750A1.Inst,     PCI\VEN_14e4&DEV_1659
%BCM5750A1%   = BCM5750A1M.Inst,   PCI\VEN_14e4&DEV_1672
%BCM5750A1%   = BCM5750A1M.Inst,   PCI\VEN_14e4&DEV_1673
%BCM5750A1%   = BCM5750A1.Inst,     PCI\VEN_14e4&DEV_1676
%BCM5750A1%   = BCM5750A1.Inst,     PCI\VEN_14e4&DEV_1677
%BCM5750A1%   = BCM5750A1.Inst,     PCI\VEN_14e4&DEV_167A
%BCM5750A1%   = BCM5750A1.Inst,     PCI\VEN_14e4&DEV_167B
%BCM5750A1%   = BCM5750A1.Inst,     PCI\VEN_14e4&DEV_167C
%BCM5750A1%   = BCM5750A1M.Inst,   PCI\VEN_14e4&DEV_167D
%BCM5750A1F%  = BCM5750A1F.Inst,   PCI\VEN_14e4&DEV_167F
%BCM5750A1%   = BCM5750A1M.Inst,   PCI\VEN_14e4&DEV_1693
%BCM5786%       = BCM5750A1.Inst,     PCI\VEN_14e4&DEV_169A
%BCM5786%       = BCM5750A1F3.Inst,     PCI\VEN_14e4&DEV_169A&SUBSYS_13ee10cf
%BCM5750A1%   = BCM5750A1.Inst,     PCI\VEN_14e4&DEV_169B
%BCM5750A1%   = BCM5750A1M.Inst,   PCI\VEN_14e4&DEV_16FF

%BCM5750A1%   = BCM5750A1M.Inst,   PCI\VEN_14e4&DEV_167D&SUBSYS_0934103c
%BCM5750A1%   = BCM5750A1M.Inst,   PCI\VEN_14e4&DEV_167D&SUBSYS_0938103c
%BCM5750A1%   = BCM5750A1M.Inst,   PCI\VEN_14e4&DEV_167D&SUBSYS_0940103c
%BCM5750A1%   = BCM5750A1M.Inst,   PCI\VEN_14e4&DEV_167D&SUBSYS_0944103c

%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_105D1734
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1659&SUBSYS_10611734
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_10961734

%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1659&SUBSYS_02C61014

%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_267610f1



%BCM5755%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_167B&SUBSYS_100F17AA
%BCM5755%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_167B&SUBSYS_101017AA
%BCM5755%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_167B&SUBSYS_101117AA
%BCM5755%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_167B&SUBSYS_101317AA
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_169B&SUBSYS_100C17AA
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_169B&SUBSYS_100D17AA
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_169B&SUBSYS_100E17AA



%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3001103c
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3002103c
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3003103c
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3004103c
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3005103c
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3006103c
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3007103c
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3008103c
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_3009103c
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_12f2103c
%BCM5788%     = BCM5788F1.Inst,   PCI\VEN_14e4&DEV_169c&SUBSYS_099c103c
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3010103c
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3011103c
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3012103c
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3013103c
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3014103c
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3015103c
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1600&SUBSYS_3016103c

%BCM5901%   = BCM5901.Inst,   PCI\VEN_14e4&DEV_170D
%BCM5901%   = BCM5901.Inst,   PCI\VEN_14e4&DEV_170e
%BCM5906%   = BCM5750A1.Inst,     PCI\VEN_14e4&DEV_1712
%BCM5906%   = BCM5750A1M.Inst,   PCI\VEN_14e4&DEV_1713

%BCM5782%   = BCM5782.Inst,   PCI\VEN_14e4&DEV_1696
%BCM5788%   = BCM5788.Inst,   PCI\VEN_14e4&DEV_169c
%BCM5789%   = BCM5789.Inst,   PCI\VEN_14e4&DEV_169d
%BCM5789%   = BCM5789.Inst,   PCI\VEN_14e4&DEV_169d&SUBSYS_100317AA

%BCM5788%   = BCM5788.Inst,   PCI\VEN_14e4&DEV_169c&SUBSYS_c016144d
%BCM5788%   = BCM5788F1.Inst,   PCI\VEN_14e4&DEV_169c&SUBSYS_123c10cf
%BCM5788%   = BCM5788F1.Inst,   PCI\VEN_14e4&DEV_169d&SUBSYS_83101033

%BCM5705M%  = BCM5705MA2F2.Inst,PCI\VEN_14e4&DEV_165e&SUBSYS_127910cf
%BCM5750A1%   = BCM5750A1F3.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_128810cf
%BCM5750A1%   = BCM5750A1F3M.Inst,   PCI\VEN_14e4&DEV_167D&SUBSYS_130010cf
%BCM5750A1%   = BCM5750A1F3M.Inst,   PCI\VEN_14e4&DEV_167D&SUBSYS_82c31033
%BCM5750A1%   = BCM5750A1F3.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_82d31033
%BCM5750A1%   = BCM5750A1F3.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_82ee1033

%BCM5705M%  = BCM5705MA2F2.Inst,PCI\VEN_14e4&DEV_1654&SUBSYS_82581033
%BCM5705M%  = BCM5705MA2F2.Inst,PCI\VEN_14e4&DEV_1654&SUBSYS_825c1033
%BCM5705M%  = BCM5705MA2F2.Inst,PCI\VEN_14e4&DEV_165e&SUBSYS_82c51033
%BCM5788%   = BCM5788F1.Inst,   PCI\VEN_14e4&DEV_169c&SUBSYS_82fa1033
%BCM5788%   = BCM5788F1.Inst,   PCI\VEN_14e4&DEV_169c&SUBSYS_83011033

%BCM5700FB% = BCM5700FB.Inst, PCI\VEN_14e4&DEV_1644&SUBSYS_000214e4
%BCM5700FA% = BCM5700FA.Inst, PCI\VEN_14e4&DEV_1644&SUBSYS_000314e4
%BCM5701FA% = BCM5701FA.Inst, PCI\VEN_14e4&DEV_1645&SUBSYS_000714e4
%BCM5703S%  = BCM5703S.Inst,  PCI\VEN_14e4&DEV_16A7&SUBSYS_000a14e4
%BCM5703S%  = BCM5703S.Inst,  PCI\VEN_14e4&DEV_1647&SUBSYS_000a14e4
%BCM5703SW% = BCM5703SW.Inst, PCI\VEN_14e4&DEV_16A7&SUBSYS_02811014
%BCM5703S%  = BCM5703SA3.Inst,PCI\VEN_14e4&DEV_16C7&SUBSYS_000a14e4
%BCM5704S%  = BCM5704S.Inst,  PCI\VEN_14e4&DEV_16A8


; BB  0x167D AX Revs
%BCM5750%   = BCM5750.Inst,   PCI\VEN_14e4&DEV_167D&SUBSYS_05771014&REV_01

; BB  0x167D BX, CX, XX  Revs
%BCM5750A1%   = BCM5750B0M.Inst,   PCI\VEN_14e4&DEV_167D&SUBSYS_05771014

; BB  0x167E AX Revs
%BCM5750A1F%   = BCM5750A1F.Inst,   PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014&REV_01

; BB  0x167E BX, CX, XX  Revs
%BCM5750A1F%   = BCM5750B0MF.Inst,   PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014


%BCM5750A1F%   = BCM5750A1F.Inst,   PCI\VEN_14e4&DEV_167E&SUBSYS_02F71014

%BCM5750A1F%   = BCM5750A1F.Inst,   PCI\VEN_14e4&DEV_167E&SUBSYS_01E41028

%BCM5704SW% = BCM5704SW.Inst, PCI\VEN_14e4&DEV_16A8&SUBSYS_029c1014
%BCM5704SW% = BCM5704SW.Inst, PCI\VEN_14e4&DEV_16A8&SUBSYS_02a81014
%BCM5704SW% = BCM5704SW.Inst, PCI\VEN_14e4&DEV_16A8&SUBSYS_03011014

%BCM5705%   = BCM5705A2.Inst, PCI\VEN_14e4&DEV_1654&SUBSYS_02b51014
%BCM5705%   = BCM5705A2.Inst, PCI\VEN_14e4&DEV_1654&SUBSYS_02b61014
%BCM5705%   = BCM5705A2.Inst, PCI\VEN_14e4&DEV_1654&SUBSYS_02D81014
%BCM5705%   = BCM5705A2.Inst, PCI\VEN_14e4&DEV_1654&SUBSYS_02D91014
%BCM5705%   = BCM5705A2.Inst, PCI\VEN_14e4&DEV_1654&SUBSYS_02F81014
%BCM5750A1% = BCM5750A1.Inst, PCI\VEN_14e4&DEV_1677&SUBSYS_02F71014

%BCM5705M%    = BCM5705MA2.Inst,PCI\VEN_14e4&DEV_165e&SUBSYS_05721014
%BCM5750A1%   = BCM5750A1M.Inst,   PCI\VEN_14e4&DEV_167D&SUBSYS_05771014
%BCM5750A1F%   = BCM5750A1F.Inst,   PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014
%BCM5750A1F%   = BCM5750A1F.Inst,   PCI\VEN_14e4&DEV_167E&SUBSYS_02F71014



%OEM1_DEV1% = OEM1_DEV1.Inst, PCI\VEN_14e4&DEV_1644&SUBSYS_102814e4
%OEM1_DEV1% = OEM1_DEV1.Inst, PCI\VEN_14e4&DEV_1644&SUBSYS_00d11028
%OEM1_DEV2% = OEM1_DEV2.Inst, PCI\VEN_14e4&DEV_1644&SUBSYS_01091028
%OEM1_DEV3% = OEM1_DEV3.Inst, PCI\VEN_14e4&DEV_1644&SUBSYS_010A1028
%OEM1_DEV4% = OEM1_DEV4.Inst, PCI\VEN_14e4&DEV_16A6&SUBSYS_81261028

%OEM1_DEV5% = OEM1_DEV5.Inst, PCI\VEN_14e4&DEV_165D&SUBSYS_865d1028
%OEM1_DEV5% = OEM1_DEV5.Inst, PCI\VEN_14e4&DEV_165D&SUBSYS_019c1028
%OEM1_DEV5% = OEM1_DEV5.Inst, PCI\VEN_14e4&DEV_165D&SUBSYS_20031028
%OEM1_DEV6% = OEM1_DEV6.Inst, PCI\VEN_14e4&DEV_1653&SUBSYS_86531028

%OEM1_DEV7% = BCM5705MA2.Inst, PCI\VEN_14e4&DEV_165e&SUBSYS_01711028
%OEM1_DEV7% = BCM5705MA2.Inst, PCI\VEN_14e4&DEV_165e&SUBSYS_015a1028
%OEM1_DEV7% = BCM5705MA2.Inst, PCI\VEN_14e4&DEV_165e&SUBSYS_017c1028
%OEM1_DEV7% = BCM5705MA2.Inst, PCI\VEN_14e4&DEV_165e&SUBSYS_01AA1028

%BCM5750A1DDT%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01751028
%BCM5750A1DDT%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01761028
%BCM5750A1DDT%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01771028
%BCM5750A1DDT%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01781028
%BCM5750A1DDT%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01791028
%BCM5750A1DDT%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_167a&SUBSYS_01da1028
%BCM5750A1DDT%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_167a&SUBSYS_01de1028


;%OEM1_DEV6%     = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01801028
;%OEM1_DEV6%     = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1659&SUBSYS_01851028
;%OEM1_DEV6%     = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1659&SUBSYS_01841028

%BCM5750A1DMOBILE%         =  BCM5750A1DMOBILE.Inst,      PCI\VEN_14e4&DEV_1672&SUBSYS_02021028
%BCM5750A1DMOBILE%         =  BCM5750A1DMOBILE.Inst,      PCI\VEN_14e4&DEV_1673&SUBSYS_01f91028
%BCM5750A1DMOBILE%         =  BCM5750A1DMOBILE.Inst,      PCI\VEN_14e4&DEV_1673&SUBSYS_01fa1028
%BCM5750A1DMOBILE%         =  BCM5750A1DMOBILE.Inst,      PCI\VEN_14e4&DEV_1673&SUBSYS_01fe1028
%BCM5750A1DMOBILE%         =  BCM5750A1DMOBILE.Inst,      PCI\VEN_14e4&DEV_1673&SUBSYS_01ff1028
%BCM5750A1DMOBILE%         =  BCM5750A1DMOBILE.Inst,      PCI\VEN_14e4&DEV_1673&SUBSYS_02061028

%BCM5750A1DMOBILE%     = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01AD1028
%BCM5750A1DMOBILE%     = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1600&SUBSYS_01AD1028
%BCM5750A1DMOBILE%     = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01A81028
%BCM5750A1DMOBILE%     = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1600&SUBSYS_01A81028
%BCM5750A1DMOBILE%     = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1600&SUBSYS_01A71028
%BCM5750A1DMOBILE%     = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01A91028


%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01821028
%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01861028
%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01871028
%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01881028
%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_018f1028
%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01a01028
%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01a31028
%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_02071028

%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1659&SUBSYS_3260103C

%BCM5705M%  = BCM5705MA2.Inst,          PCI\VEN_14e4&DEV_165E&SUBSYS_05721014
%BCM5901%   = BCM5901.Inst,             PCI\VEN_14e4&DEV_170D&SUBSYS_05451014
%BCM5901%   = BCM5901.Inst,             PCI\VEN_14e4&DEV_170E&SUBSYS_05451014

;12x12
%BCM5750A1%   = BCM5750A1.Inst,    PCI\VEN_14e4&DEV_16F7
%BCM5750A1%   = BCM5750A1M.Inst,  PCI\VEN_14e4&DEV_16FD
%BCM5788%        = BCM5781.Inst,   PCI\VEN_14e4&DEV_16DD

; hamil
%BCM5714%    = BCM5714.Inst,     PCI\VEN_14e4&DEV_1668
%BCM5714%    = BCM5714.Inst,     PCI\VEN_14e4&DEV_1678
%BCM5714%    = BCM5780.Inst,     PCI\VEN_14e4&DEV_166A
%BCM5714S%   = BCM5714S.Inst,    PCI\VEN_14e4&DEV_166B


%BCM5750A1%   = BCM5750A1.Inst,    PCI\VEN_14e4&DEV_1600


;..............................................................................................................................

; Win 9x Install sections.
[BCM5700.Inst]
DelReg    = DelReg.WolS
AddReg    = BCM5700.W9xAddReg, W9xAddReg2, BCM5700.Params, ParamsW9x, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5700.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_1644"
HKR, Ndi\Install,   ndis3,  , "BCM5700.Inst"

[BCM5701.Inst]
AddReg    = BCM5701.W9xAddReg, W9xAddReg2, BCM5701.Params, ParamsW9x, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5701.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_1645"
HKR, Ndi\Install,   ndis3,  , "BCM5701.Inst"

[BCM5702.Inst]
AddReg    = BCM5702.W9xAddReg, W9xAddReg2, BCM5702.Params, ParamsW9x, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5702.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_16a6"
HKR, Ndi\Install,   ndis3,  , "BCM5702.Inst"

[BCM5702A3.Inst]
AddReg    = BCM5702A3.W9xAddReg, W9xAddReg2, BCM5702.Params, ParamsW9x, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5702A3.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_16C6"
HKR, Ndi\Install,   ndis3,  , "BCM5702A3.Inst"

[BCM5703.Inst]
AddReg    = BCM5703.W9xAddReg, W9xAddReg2, BCM5703.Params, ParamsW9x, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5703.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_16a7"
HKR, Ndi\Install,   ndis3,  , "BCM5703.Inst"

[BCM5703A3.Inst]
AddReg    = BCM5703A3.W9xAddReg, W9xAddReg2, BCM5703.Params, ParamsW9x, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5703A3.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_16C7"
HKR, Ndi\Install,   ndis3,  , "BCM5703A3.Inst"

[BCM5704.Inst]
DelReg    = DelReg.WolS
AddReg    = BCM5704.W9xAddReg, W9xAddReg2, BCM5704.Params, ParamsW9x, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, ParamsWireSpeed
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5704.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_1648"
HKR, Ndi\Install,   ndis3,  , "BCM5704.Inst"

[BCM5705.Inst]
DelReg    = DelReg.Jumbo
AddReg    = BCM5705.W9xAddReg, W9xAddReg2, BCM5705.Params, ParamsW9x, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5705.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_1653"
HKR, Ndi\Install,   ndis3,  , "BCM5705.Inst"

[BCM5705A2.Inst]
DelReg    = DelReg.Jumbo, DelReg.WireSpeed
AddReg    = BCM5705A2.W9xAddReg, W9xAddReg2, BCM5705A2.Params, ParamsW9x, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5705A2.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_1654"
HKR, Ndi\Install,   ndis3,  , "BCM5705A2.Inst"

[BCM5705M.Inst]
DelReg    = DelReg.Jumbo
AddReg    = BCM5705M.W9xAddReg, W9xAddReg2, BCM5705M.Params, ParamsW9x, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5705M.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_165d"
HKR, Ndi\Install,   ndis3,  , "BCM5705M.Inst"

[BCM5705MA2.Inst]
DelReg    = DelReg.Jumbo, DelReg.WireSpeed
AddReg    = BCM5705MA2.W9xAddReg, W9xAddReg2, BCM5705MA2.Params, ParamsW9x, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5705MA2.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_165e"
HKR, Ndi\Install,   ndis3,  , "BCM5705MA2.Inst"

[BCM5705MA2F2.Inst]
DelReg    = DelReg.Jumbo, DelReg.WireSpeed
AddReg    = BCM5705MA2F2.W9xAddReg, W9xAddReg2, BCM5705MA2.Params, ParamsW9x, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLogOptions
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5705MA2F2.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_165e"
HKR, Ndi\Install,   ndis3,  , "BCM5705MA2.Inst"

[BCM5901.Inst]
DelReg    = DelReg.Jumbo
AddReg    = BCM5901.W9xAddReg, W9xAddReg2, BCM5901.Params, ParamsW9x, ParamsNtW9x, ParamsC100, ParamsWOL
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5901.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_170D"
HKR, Ndi\Install,   ndis3,  , "BCM5901.Inst"

[BCM5705F.Inst]
DelReg    = DelReg.Jumbo
AddReg    = BCM5705F.W9xAddReg, W9xAddReg2, BCM5705F.Params, ParamsW9x, ParamsNtW9x, ParamsC100, ParamsWOL
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5705F.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_166e"
HKR, Ndi\Install,   ndis3,  , "BCM5705F.Inst"

[BCM5782.Inst]
DelReg    = DelReg.Jumbo, DelReg.WireSpeed
AddReg    = BCM5782.W9xAddReg, W9xAddReg2, BCM5782.Params, ParamsW9x, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5782.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_1696"
HKR, Ndi\Install,   ndis3,  , "BCM5782.Inst"

[BCM5788.Inst]
DelReg    = DelReg.Jumbo, DelReg.WireSpeed
AddReg    = BCM5788.W9xAddReg, W9xAddReg2, BCM5788.Params, ParamsW9x, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5788.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_169c"
HKR, Ndi\Install,   ndis3,  , "BCM5788.Inst"


[BCM5789.Inst]
DelReg    = DelReg.Jumbo, DelReg.WireSpeed
AddReg    = BCM5788.W9xAddReg, W9xAddReg2, BCM5788.Params, ParamsW9x, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5789.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_169d"
HKR, Ndi\Install,   ndis3,  , "BCM5788.Inst"


[BCM5781.Inst]
DelReg    = DelReg.Jumbo, DelReg.WireSpeed
AddReg    = BCM5781.W9xAddReg, W9xAddReg2, BCM5788.Params, ParamsW9x, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5781.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_16dd"
HKR, Ndi\Install,   ndis3,  , "BCM5781.Inst"


[BCM5788F1.Inst]
DelReg    = DelReg.Jumbo, DelReg.WireSpeed
AddReg    = BCM5788.W9xAddReg, W9xAddReg2, BCM5788.Params, ParamsW9x, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLogOptions
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5788F1.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_169c"
HKR, Ndi\Install,   ndis3,  , "BCM5788F1.Inst"

[BCM5700FB.Inst]
DelReg    = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg    = BCM5700FB.W9xAddReg, W9xAddReg2, BCM5700.Params, ParamsW9x, ParamsNtW9x, ParamsJumbo
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5700FB.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_1644"
HKR, Ndi\Install,   ndis3,  , "BCM5700FB.Inst"

[BCM5700FA.Inst]
DelReg    = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg    = BCM5700FA.W9xAddReg, W9xAddReg2, BCM5700.Params, ParamsW9x, ParamsNtW9x, ParamsJumbo
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5700FA.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_1644"
HKR, Ndi\Install,   ndis3,  , "BCM5700FA.Inst"

[BCM5701FA.Inst]
DelReg    = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg    = BCM5701FA.W9xAddReg, W9xAddReg2, BCM5701.Params, ParamsW9x, ParamsNtW9x, ParamsJumbo
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5701FA.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_1645"
HKR, Ndi\Install,   ndis3,  , "BCM5701FA.Inst"

[BCM5703S.Inst]
DelReg    = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg    = BCM5703S.W9xAddReg, W9xAddReg2, BCM5703.Params, ParamsW9x, ParamsNtW9x, ParamsJumbo
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5703S.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_16a7"
HKR, Ndi\Install,   ndis3,  , "BCM5703S.Inst"

[BCM5703SA3.Inst]
DelReg    = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg    = BCM5703SA3.W9xAddReg, W9xAddReg2, BCM5703.Params, ParamsW9x, ParamsNtW9x, ParamsJumbo
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5703SA3.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_16C7"
HKR, Ndi\Install,   ndis3,  , "BCM5703SA3.Inst"

[BCM5703SW.Inst]
DelReg    = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg    = BCM5703SW.W9xAddReg, W9xAddReg2, BCM5703.Params, ParamsW9x, ParamsNtW9x, ParamsJumbo, ParamsWOLTbi
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5703SW.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_16a7"
HKR, Ndi\Install,   ndis3,  , "BCM5703SW.Inst"

[BCM5704S.Inst]
DelReg    = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg    = BCM5704S.W9xAddReg, W9xAddReg2, BCM5704.Params, ParamsW9x, ParamsNtW9x, ParamsJumbo
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5704S.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_16a8"
HKR, Ndi\Install,   ndis3,  , "BCM5704S.Inst"

[BCM5704SW.Inst]
DelReg    = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg    = BCM5704SW.W9xAddReg, W9xAddReg2, BCM5704.Params, ParamsW9x, ParamsNtW9x, ParamsJumbo, ParamsWOLTbi
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5704SW.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_16a8"
HKR, Ndi\Install,   ndis3,  , "BCM5704SW.Inst"

[OEM1_DEV1.Inst]
DelReg    = DelReg.WolS
AddReg    = OEM1_DEV1.W9xAddReg, W9xAddReg2, BCM5700.Params, ParamsW9x, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS
CopyFiles = CopyFile.W9xSys
BusType   = 5

[OEM1_DEV1.W9xAddReg]
HKR, Ndi, DeviceID,         0, "PCI\VEN_14e4&DEV_1644"
HKR, Ndi\Install,    ndis3,  , "OEM1_DEV1.Inst"

[OEM1_DEV2.Inst]
DelReg    = DelReg.WolS
AddReg    = OEM1_DEV2.W9xAddReg, W9xAddReg2, BCM5700.Params, ParamsW9x, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS
CopyFiles = CopyFile.W9xSys
BusType   = 5

[OEM1_DEV2.W9xAddReg]
HKR, Ndi, DeviceID,         0, "PCI\VEN_14e4&DEV_1644"
HKR, Ndi\Install,    ndis3,  , "OEM1_DEV2.Inst"

[OEM1_DEV3.Inst]
DelReg    = DelReg.WolS
AddReg    = OEM1_DEV3.W9xAddReg, W9xAddReg2, BCM5700.Params, ParamsW9x, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS
CopyFiles = CopyFile.W9xSys
BusType   = 5

[OEM1_DEV3.W9xAddReg]
HKR, Ndi, DeviceID,         0, "PCI\VEN_14e4&DEV_1644"
HKR, Ndi\Install,    ndis3,  , "OEM1_DEV3.Inst"

[OEM1_DEV4.Inst]
AddReg    = OEM1_DEV4.W9xAddReg, W9xAddReg2, BCM5702.Params, OEM1_DEV4.Params, ParamsW9x, ParamsC, ParamsWOLNS, ParamsFlow
CopyFiles = CopyFile.W9xSys
BusType   = 5

[OEM1_DEV4.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_16a6"
HKR, Ndi\Install,   ndis3,  , "OEM1_DEV4.Inst"

[OEM1_DEV5.Inst]
AddReg    = OEM1_DEV5.W9xAddReg, W9xAddReg2, BCM5705M.Params, OEM1_DEV5.Params, ParamsW9x, ParamsC, ParamsWOLNS, ParamsFlow
CopyFiles = CopyFile.W9xSys
BusType   = 5

[OEM1_DEV5.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_165d"
HKR, Ndi\Install,   ndis3,  , "OEM1_DEV5.Inst"

[OEM1_DEV6.Inst]
AddReg    = OEM1_DEV6.W9xAddReg, W9xAddReg2, BCM5705.Params, OEM1_DEV6.Params, ParamsW9x, ParamsC, ParamsWOLNS, ParamsFlow
CopyFiles = CopyFile.W9xSys
BusType   = 5

[OEM1_DEV6.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_1653"
HKR, Ndi\Install,   ndis3,  , "OEM1_DEV6.Inst"

[OEM1_DEV7.Inst]
AddReg    = OEM1_DEV7.W9xAddReg, W9xAddReg2, BCM5705.Params, OEM1_DEV7.Params, ParamsW9x, ParamsC, ParamsWOLNS, ParamsFlow
CopyFiles = CopyFile.W9xSys
BusType   = 5

[OEM1_DEV7.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_165e"
HKR, Ndi\Install,   ndis3,  , "OEM1_DEV7.Inst"

[BCM5750.Inst]
DelReg    = DelReg.Jumbo
AddReg    = BCM5750.W9xAddReg, W9xAddReg2, BCM5750.Params, ParamsW9x, ParamsNtW9x, ParamsC, ParamsWOLMagic, ParamsWireSpeed
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5750.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_1676"
HKR, Ndi\Install,   ndis3,  , "BCM5750.Inst"

[BCM5750A1.Inst]
DelReg    = DelReg.Jumbo
AddReg    = BCM5750A1.W9xAddReg, W9xAddReg2, BCM5750.Params, ParamsW9x, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5750A1.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_1677"
HKR, Ndi\Install,   ndis3,  , "BCM5750A1.Inst"

[BCM5754.Inst]
DelReg    = DelReg.Jumbo
AddReg    = BCM5754.W9xAddReg, W9xAddReg2, BCM5750.Params, ParamsW9x, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5754.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_167a"
HKR, Ndi\Install,   ndis3,  , "BCM5754.Inst"


[BCM5714.Inst]
DelReg    = DelReg.Jumbo, DelReg.Wol
AddReg    = BCM5714.W9xAddReg, W9xAddReg2, BCM5750.Params, ParamsW9x, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsJumbo
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5714.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_1668"
HKR, Ndi\Install,   ndis3,  , "BCM5714.Inst"

[BCM5780.Inst]
DelReg    = DelReg.Jumbo
AddReg    = BCM5780.W9xAddReg, W9xAddReg2, BCM5750.Params, ParamsW9x, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsJumbo
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5780.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_166A"
HKR, Ndi\Install,   ndis3,  , "BCM5780.Inst"


[BCM5714S.Inst]
DelReg    = DelReg.Jumbo
AddReg    = BCM5714.W9xAddReg, W9xAddReg2, BCM5750.Params, ParamsW9x, ParamsNtW9x, ParamsWOL, ParamsWireSpeed, ParamsJumbo
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5714S.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_1669"
HKR, Ndi\Install,   ndis3,  , "BCM5714S.Inst"



[BCM5750A1M.Inst]
DelReg    = DelReg.Jumbo
AddReg    = BCM5750A1.W9xAddReg, W9xAddReg2, BCM5750.Params, ParamsW9x, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsM
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5750A1M.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_1677"
HKR, Ndi\Install,   ndis3,  , "BCM5750A1M.Inst"

[BCM5750A1F.Inst]
DelReg    = DelReg.Jumbo
AddReg    = BCM5750A1F.W9xAddReg, W9xAddReg2, BCM5750.Params, ParamsW9x, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsWireSpeed
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5750A1F.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_167e"
HKR, Ndi\Install,   ndis3,  , "BCM5750A1F.Inst"


[BCM5750B0M.Inst]
DelReg    = DelReg.Jumbo
AddReg    = BCM5750B0M.W9xAddReg, W9xAddReg2, BCM5750.Params, ParamsW9x, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsM, ParamsWOLLink
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5750B0M.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_1677"
HKR, Ndi\Install,   ndis3,  , "BCM5750B0M.Inst"

[BCM5750B0MF.Inst]
DelReg    = DelReg.Jumbo
AddReg    = BCM5750B0MF.W9xAddReg, W9xAddReg2, BCM5750.Params, ParamsW9x, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsWireSpeed, ParamsM, ParamsWOLLink
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5750B0MF.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_167e"
HKR, Ndi\Install,   ndis3,  , "BCM5750B0MF.Inst"




[BCM5750A1DMOBILE.Inst]
DelReg    = DelReg.Jumbo
AddReg    = BCM5750A1DMOBILE.W9xAddReg, W9xAddReg2, BCM5750.Params, ParamsW9x, ParamsNtW9xMOBILE, ParamsC, ParamsWOLNS, DMobile.Params
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5750A1DMOBILE.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_1677"
HKR, Ndi\Install,   ndis3,  , "BCM5750A1DMOBILE.Inst"

[BCM5750A1F3.Inst]
DelReg    = DelReg.Jumbo
AddReg    = BCM5750A1F3.W9xAddReg, W9xAddReg2, BCM5750.Params, ParamsW9x, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLogOptions
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5750A1F3.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_1676"
HKR, Ndi\Install,   ndis3,  , "BCM5750A1.Inst"


[BCM5750A1F3M.Inst]
DelReg    = DelReg.Jumbo
DelReg    = DelReg.ClockControl
AddReg    = BCM5750A1F3M.W9xAddReg, W9xAddReg2, BCM5750.Params, ParamsW9x, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLogOptions, ParamsM
CopyFiles = CopyFile.W9xSys
BusType   = 5

[BCM5750A1F3M.W9xAddReg]
HKR, Ndi, DeviceID,        0, "PCI\VEN_14e4&DEV_167D"
HKR, Ndi\Install,   ndis3,  , "BCM5750A1.Inst"


; Win9x common sections.
[W9xAddReg2]
HKR, , DevLoader,  0, *ndis
HKR, , DeviceVxDs, 0, b57w2k.sys

;Windows 95 does not support Ndis5 upper range.
HKR, Ndi\Interfaces, DefUpper,   0, "ndis3"
HKR, Ndi\Interfaces, DefLower,   0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

HKR, NDIS, LogDriverName,    0, "b57w2k"
HKR, NDIS, MajorNdisVersion, 1, 04
HKR, NDIS, MinorNdisVersion, 1, 00

; Registry parameters.
[BCM5700.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "360"
HKR, , TxCoalescingTicks,        0, "360"
HKR, , RxMaxCoalescedFrames,     0, "15"
HKR, , TxMaxCoalescedFrames,     0, "75"

[BCM5701.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5702.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5703.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5704.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705A2.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5782.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5788.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705M.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705MA2.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5901.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705F.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5750.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"
        
[OEM1_DEV4.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1500"
HKR, , WolSpeed,                 0, "0"
HKR, , WireSpeed,                0, "1"

[OEM1_DEV5.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1500"
HKR, , WolSpeed,                 0, "0"
HKR, , WireSpeed,                0, "1"

[OEM1_DEV6.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1500"
HKR, , WolSpeed,                 0, "0"
HKR, , WireSpeed,                0, "1"

[OEM1_DEV7.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1500"
HKR, , WolSpeed,                 0, "0"
HKR, , WireSpeed,                0, "1"

[DMobile.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1500"
HKR, , WireSpeed,                0, "1"

[ParamsNt]
HKR, Ndi\Params\TaskOffloadCap,      ParamDesc, , %TaskOffload%
HKR, Ndi\Params\TaskOffloadCap,      default,   , "63"
HKR, Ndi\Params\TaskOffloadCap,      type,      , "enum"
HKR, Ndi\Params\TaskOffloadCap\enum, 0,         , %TaskOffload_None%
HKR, Ndi\Params\TaskOffloadCap\enum, 42,        , %TaskOffload_Rx_Chksum%
HKR, Ndi\Params\TaskOffloadCap\enum, 21,        , %TaskOffload_Tx_Chksum%
HKR, Ndi\Params\TaskOffloadCap\enum, 63,        , %TaskOffload_Rx_Tx_Chksum%

[ParamsNt8021p]
HKR, Ndi\Params\Enable8021p,      ParamDesc, , %QOS_8021p%
HKR, Ndi\Params\Enable8021p,      default,   , "0"
HKR, Ndi\Params\Enable8021p,      type,      , "enum"
HKR, Ndi\Params\Enable8021p\enum, 0,         , %QOS_8021p_Disable%
HKR, Ndi\Params\Enable8021p\enum, 1,         , %QOS_8021p_Enable%

[ParamsW9x]
HKR, , IsWin9x, 0, "1"

[ParamsNtW9x]
HKR, Ndi\Params\FlowControlCap,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\FlowControlCap,      default,    , "2147483648"
HKR, Ndi\Params\FlowControlCap,      type,       , "enum"
HKR, Ndi\Params\FlowControlCap\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\FlowControlCap\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2147483648, , %FlowControl_Auto%

HKR, Ndi\params\NetworkAddress,        ParamDesc,  0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress,        Default,    0, ""
HKR, Ndi\params\NetworkAddress,        type,       0, "edit"
HKR, NDI\params\NetworkAddress,        LimitText,  0, "12"
HKR, NDI\params\NetworkAddress,        UpperCase,  0, "1"
HKR, NDI\params\NetworkAddress,        optional,   0, "1"


[ParamsNtW9xFJ]
HKR, Ndi\Params\FlowControlCap,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\FlowControlCap,      default,    , "0"
HKR, Ndi\Params\FlowControlCap,      type,       , "enum"
HKR, Ndi\Params\FlowControlCap\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\FlowControlCap\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2147483648, , %FlowControl_Auto%

HKR, Ndi\params\NetworkAddress,        ParamDesc,  0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress,        Default,    0, ""
HKR, Ndi\params\NetworkAddress,        type,       0, "edit"
HKR, NDI\params\NetworkAddress,        LimitText,  0, "12"
HKR, NDI\params\NetworkAddress,        UpperCase,  0, "1"
HKR, NDI\params\NetworkAddress,        optional,   0, "1"


[ParamsNtW9xMOBILE]
HKR, Ndi\Params\FlowControlCap,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\FlowControlCap,      default,    , "2147483648"
HKR, Ndi\Params\FlowControlCap,      type,       , "enum"
HKR, Ndi\Params\FlowControlCap\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\FlowControlCap\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2147483648, , %FlowControl_Auto%

[ParamsJumbo]
HKR, Ndi\Params\RxMtu, ParamDesc, , %JumboMtu%
HKR, Ndi\Params\RxMtu, default,   , "1500"
HKR, Ndi\Params\RxMtu, type,      , "dword"
HKR, Ndi\Params\RxMtu, min,       , "1500"
HKR, Ndi\Params\RxMtu, max,       , "9000"
HKR, Ndi\Params\RxMtu, step,      , "500"
HKR, Ndi\Params\RxMtu, base,      , "10"

[ParamsWireSpeed]
HKR, Ndi\Params\WireSpeed,        ParamDesc, , %WireSpeed%
HKR, Ndi\Params\WireSpeed,        default,   , "1"
HKR, Ndi\Params\WireSpeed,        type,      , "enum"
HKR, Ndi\Params\WireSpeed\enum,   0,         , %WireSpeed_Disable%
HKR, Ndi\Params\WireSpeed\enum,   1,         , %WireSpeed_Enable%

[ParamsLogOptions]
HKR, Ndi\Params\LogLevelInfo,        ParamDesc, , %LogLevelInfo%
HKR, Ndi\Params\LogLevelInfo,        default,   , "0"
HKR, Ndi\Params\LogLevelInfo,        type,      , "enum"
HKR, Ndi\Params\LogLevelInfo\enum,   0,         , %LogLevelInfo_Disable%
HKR, Ndi\Params\LogLevelInfo\enum,   1,         , %LogLevelInfo_Enable%
HKR, Ndi\Params\LogLevelWarn,        ParamDesc, , %LogLevelWarn%
HKR, Ndi\Params\LogLevelWarn,        default,   , "0"
HKR, Ndi\Params\LogLevelWarn,        type,      , "enum"
HKR, Ndi\Params\LogLevelWarn\enum,   0,         , %LogLevelWarn_Disable%
HKR, Ndi\Params\LogLevelWarn\enum,   1,         , %LogLevelWarn_Enable%

[ParamsC]
HKR, Ndi\Params\RequestedMediaType,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\RequestedMediaType,      default,   , "0"
HKR, Ndi\Params\RequestedMediaType,      type,      , "enum"
HKR, Ndi\Params\RequestedMediaType\enum, 0,         , %Speed_Duplex_Auto%
HKR, Ndi\Params\RequestedMediaType\enum, 3,         , %Speed_Duplex_10Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 4,         , %Speed_Duplex_10Mb_Fd%
HKR, Ndi\Params\RequestedMediaType\enum, 5,         , %Speed_Duplex_100Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 6,         , %Speed_Duplex_100Mb_Fd%

[ParamsC100]
HKR, Ndi\Params\RequestedMediaType,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\RequestedMediaType,      default,   , "0"
HKR, Ndi\Params\RequestedMediaType,      type,      , "enum"
HKR, Ndi\Params\RequestedMediaType\enum, 0,         , %Speed_Duplex_Auto%
HKR, Ndi\Params\RequestedMediaType\enum, 3,         , %Speed_Duplex_10Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 4,         , %Speed_Duplex_10Mb_Fd%
HKR, Ndi\Params\RequestedMediaType\enum, 5,         , %Speed_Duplex_100Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 6,         , %Speed_Duplex_100Mb_Fd%

[ParamsWOL]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "0"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%


[ParamsWOLTbi]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "1"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, , TbiWol,                   0, "1"

[ParamsWOLNS]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

[ParamsFlow]
HKR, Ndi\Params\FlowControlCap,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\FlowControlCap,      default,    , "2147483648"
HKR, Ndi\Params\FlowControlCap,      type,       , "enum"
HKR, Ndi\Params\FlowControlCap\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\FlowControlCap\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2147483648, , %FlowControl_Auto%

[ParamsM]
HKR, , ClockControl,          0, "1"

[ParamsWOLLink]
HKR, Ndi\Params\WakeOnLink,        ParamDesc, , %WakeOnLink%
HKR, Ndi\Params\WakeOnLink,        default,   , "1"
HKR, Ndi\Params\WakeOnLink,        type,      , "enum"
HKR, Ndi\Params\WakeOnLink\enum,   0,         , %WakeOnLink_Disable%
HKR, Ndi\Params\WakeOnLink\enum,   1,         , %WakeOnLink_Enable%

[ParamsWOLMagic]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "1"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "0"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%


; Keys to remove.
[DelReg.RequestedMediaType]
HKR, Ndi\Params\RequestedMediaType

[DelReg.Wol]
HKR, Ndi\Params\WakeUpModeCap
HKR, Ndi\Params\WolSpeed

[DelReg.WolS]
HKR, Ndi\Params\WolSpeed

[DelReg.Jumbo]
HKR, Ndi\Params\RxMtu

[DelReg.WireSpeed]
HKR, Ndi\Params\WireSpeed

[DelReg.ClockControl]
HKR, Ndi\Params\ClockControl

; Destination directories
[DestinationDirs]
DefaultDestDir  = 11
CopyFile.NtSys  = 12
CopyFile.W9xSys = 11

[SourceDisksNames]
1 = %DISK_DESC%,,,

[SourceDisksFiles]
b57w2k.sys = 1

[CopyFile.NtSys]
b57w2k.sys,,,1

[CopyFile.W9xSys]
b57w2k.sys,,,1

; Localizable strings
[Strings]
BRCM                = "Broadcom"
DISK_DESC           = "Broadcom NetXtreme Installation Media"
BCM5700             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5701             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5702             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5703             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5704             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705M            = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705F            = "Broadcom 570x 10/100 Integrated Controller"
BCM5750             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5750A1           = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5750A1F          = "Broadcom NetXtreme Fast Ethernet"
BCM5750B0           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5750B0F          = "Broadcom NetXtreme Fast Ethernet"
BCM5754             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5755           = "Broadcom NetXtreme Gigabit Ethernet"

BCM5901             = "Broadcom NetXtreme Fast Ethernet"
BCM5906             = "Broadcom NetLink (TM) Fast Ethernet"
BCM5782             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5786             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5788             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5789             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5700FB           = "Broadcom NetXtreme Gigabit Fiber"
BCM5700FA           = "Broadcom NetXtreme Gigabit Fiber"
BCM5701FA           = "Broadcom NetXtreme Gigabit Fiber"
BCM5703S            = "Broadcom NetXtreme Gigabit Fiber"
BCM5703SW           = "Broadcom NetXtreme Gigabit Fiber WOL"
BCM5704S            = "Broadcom NetXtreme Gigabit Fiber"
BCM5704SW           = "Broadcom NetXtreme Gigabit Fiber WOL"
OEM1_DEV1           = "Broadcom NetXtreme Gigabit Ethernet"
OEM1_DEV2           = "Broadcom NetXtreme Gigabit Ethernet"
OEM1_DEV3           = "Broadcom NetXtreme Gigabit Ethernet"
OEM1_DEV4           = "Broadcom 570x Gigabit Integrated Controller"
OEM1_DEV5           = "Broadcom 570x Gigabit Integrated Controller"
OEM1_DEV6           = "Broadcom NetXtreme Gigabit Ethernet"
OEM1_DEV7           = "Broadcom 570x Gigabit Integrated Controller"
OEM2_DEV1           = "Broadcom NetXtreme Gigabit Ethernet"
OEM2_DEV3           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV1           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV2           = "Broadcom NetXtreme Gigabit Ethernet"
OEM3_DEV3           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5750A1DSF      = "Broadcom NetXtreme 5751 Gigabit Controller"
BCM5750A1DSSF    = "Broadcom NetXtreme 5721 Gigabit Controller"
BCM5750A1DDT      = "Broadcom NetXtreme 57xx Gigabit Controller"
BCM5750A1DMOBILE =  "Broadcom NetXtreme 57xx Gigabit Controller"
BCM5714               = "Broadcom NetXtreme Gigabit Ethernet"
BCM5714S            = "Broadcom NetXtreme Gigabit Fiber"


JumboMtu = "Jumbo Mtu"
FlowControl             = "Flow Control"
FlowControl_Disable     = "Disable"
FlowControl_Rx_Pause    = "Rx PAUSE"
FlowControl_Tx_Pause    = "Tx PAUSE"
FlowControl_Rx_Tx_Pause = "Rx/Tx PAUSE"
FlowControl_Auto        = "Auto"
Speed_Duplex          = "Speed & Duplex"
Speed_Duplex_Auto     = "Auto"
Speed_Duplex_10Mb_Hd  = "10 Mb Half"
Speed_Duplex_10Mb_Fd  = "10 Mb Full"
Speed_Duplex_100Mb_Hd = "100 Mb Half"
Speed_Duplex_100Mb_Fd = "100 Mb Full"
Speed_Duplex_1000Mb_Fd = "1000 Mb Full"
QOS_8021p         = "802.1p QOS"
QOS_8021p_Disable = "Disable"
QOS_8021p_Enable  = "Enable"
WireSpeed         = "Ethernet@WireSpeed"
WireSpeed_Disable = "Disable"
WireSpeed_Enable  = "Enable"
TaskOffload              = "Checksum Offload"
TaskOffload_None         = "None"
TaskOffload_Rx_Chksum    = "Rx TCP/IP Checksum"
TaskOffload_Tx_Chksum    = "Tx TCP/IP Checksum"
TaskOffload_Rx_Tx_Chksum = "Tx/Rx TCP/IP Checksum"
WakeUpMode         = "Wake Up Capabilities"
WakeUpMode_None    = "None"
WakeUpMode_Magic   = "Magic Packet"
WakeUpMode_Pattern = "Wake Up Frame"
WakeUpMode_Both    = "Both"
WolSpeed       = "WOL Speed"
WolSpeed_Auto  = "Auto"
WolSpeed_10mb  = "10 Mb"
WolSpeed_100mb = "100 Mb"
WolSpeed_1000mb = "1000 Mb"
NetworkAddress           = "Locally Administered Address"
LogLevelInfo    = "Log Information Messages"
LogLevelWarn  = "Log Warning Messages"
LogLevelInfo_Disable  =  "Disable"
LogLevelInfo_Enable  =  "Enable"
LogLevelWarn_Disable  =  "Disable"
LogLevelWarn_Enable  =  "Enable"
WakeOnLink         = "Wake On Link"
WakeOnLink_Disable = "Disable"
WakeOnLink_Enable  = "Enable"

