Release Note

[Version 0.0.1]
1.提交版本进行系统测试，其中对Flash total size获取和获得平台资源文件是否存在状态列为本版本限制。

[Version 0.0.2]
1.由于集成测试采用Debug进行，导致未覆盖Release版出现的问题。重新对Release版进行修改，使用静态库，发布此版本进行第一轮系统测试。

[Version0.0.3] 09/28/2006
1.修改了第一轮系统测试中的bug，发布版本进行第二轮系统测试。

[Version0.1.0] 10/08/2006
1.修改第二轮系统测试中的bug:
  Set Size时对所有平台进行Program All的问题；
  存在同名资源文件时取文件size只针对第一个设备的问题；
  fw图标刷新消失的问题。

[Version0.2.0]10/11/2006
1.完成debug工作，提交QA进行回归测试。

[version0.3.0] 10/16/2006
1.添加Mass版本可以让用户设置设备顺序的功能到Pro，在Advanced页中所对应的设备为用户设置设备号中最靠前的设备。

[version1.0.0] 10/17/2006
1.修正资源文件超过1000后进度条无法正常更新的bug。
2.添加F2为clear log window的快捷键。

[version1.1.0] 11/09/2006
1.添加card isp的功能。

[version1.1.5] 12/19/2006
1.添加disk image的功能。

[version1.1.6] 12/25/2006
1.update user guide for SPMP3050
2.fixed bug of pre size judge.

[version1.1.7] 01/13/2007
update MLC nand driver.

[version1.1.7a] 01/22/2007
fixed bugs of MLC nand driver update(include swap blk added).

[version1.1.8] 01/24/2007
add blk size detected before create disk image.

[version1.1.8a] 01/25/2007
slove some bug of blk size get added in v1.1.8.

[version1.1.8b] 02/01/2007
1.AP: fixed read verify bug for res files & firmware.
2.isp: fixed paritial res update and fw program error in nand.c

[version1.1.9] 02/08/2007
1. fixed other read verify bugs in "Program All" & "FW + Partial Rsv".
2. add fw(bin0 & bin1) read verify(can disable in FRM_Setting.ini) after "Program All" & "Fw + Partial Rsv". 
3. create customize folder after "Program All", folder name can customize in FRM_Setting.ini.
4. modify the Fw program flow the same as current SPCA5000 isp flow.

[version1.1.9a] 02/09/2007
1. add Unmount & Mount before fw(bin0 & bin1) read verify to force FAT table update.

[version1.1.9b] 03/08/2007
1. fixed bugs in ispsr.bin of fw and resource partial update.(this version for sys test)