;***********************************************************************
; 3C154G72.INF
;
;   This installation script supports Windows 98, Me, 2000 and XP for the
;   3Com OfficeConnect Wireless 11g PC Card(3CRWE154G72).
;
;   Copyright (c) 2003 3Com Corporation.
;   All Rights Reserved.
;***********************************************************************

[Version]
 DriverVer = 11/18/2003, 2.1.13.0
 Signature           = "$Chicago$"
 Compatible          = 1
 Class               = Net
 ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
 Provider            = %VER_VENDOR_STR%
 CatalogFile         = 3C154G72.cat
 MillenniumPreferred = .ME

[ControlFlags]
;Exclude all PNP adapters from user selection
 ExcludeFromSelect   = *

[Manufacturer]
 %VER_VENDOR_NAME_STR% = DeviceList

[DeviceList]
 %A001_DESC_STR%     = PRISM_A001,     PCI\VEN_10b7&DEV_6001&SUBSYS_600110b7 

;==========================================
[PRISM_A001]       ; Win9x
 AddReg         = PRISM_A001.reg, PRISM_A001.reg1, COMMON_A00.reg, COMMON_NDIS.reg, COMMON.reg
 DelReg         = COMMON_A00_DEL.reg
 CopyFiles      = PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
 DelFiles       = PRISM_FWA00.del

[PRISM_A001.ME]    ; WinMe
 AddReg         = PRISM_A001.reg, PRISM_A001.reg1, COMMON_A00.reg, COMMON_NDIS.reg.ME, COMMON.reg
 DelReg         = COMMON_A00_DEL.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
 DelFiles       = PRISM_FWA00.del.ME

[PRISM_A001.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
 AddReg         = PRISM_A001.reg, PRISM_A001.reg1, COMMON_A00.reg, COMMON_NDIS.reg.ME, COMMON.reg
 DelReg         = COMMON_A00_DEL.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
 DelFiles       = PRISM_FWA00.del.ME

[PRISM_A001.NT]    ; Win2k
 AddReg         = PRISM_A001.reg, PRISM_A001.reg1, COMMON_A00.reg, COMMON_NDIS.reg.NT, COMMON.reg
 DelReg         = COMMON_A00_DEL.reg
 CopyFiles      = PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT,PRISM_NDI.copy
 DelFiles       = PRISM_FWA00.del.NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_A001.NT.Services]
 AddService     = "3C154G", 2, PRISM_DRIVER_A00.Service, PRISM_DRIVER.EventLog

[PRISM_A001.NT.CoInstallers]
 CopyFiles      = PRISM_COINSTALL.copy.NT
 AddReg         = PRISM_COINSTALL.reg.NT

[PRISM_A001.reg1]
 HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\RunOnce, "3C154G",, "%11%\CCU3C154.exe"

[PRISM_A001.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_10b7&DEV_6001&SUBSYS_600110b7"
; 0x3890 = 14480
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%A001_DESC_STR%
 HKR,,11dMode,0,0
 HKR,,EnableRadio,0,0

;###############################################################################
[PRISM_COINSTALL.reg.NT]
 HKR,           ,CoInstallers32         ,0x00010000     ,"CCU3C154.DLL,CoCCU"

[PRISM_DRIVER_A00.Service]
 DisplayName    = %A00_SERVICE_STR%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\3C154G72.sys
 LoadOrderGroup = NDIS

[PRISM_DRIVER.EventLog]
 AddReg         = PRISM_DRIVER.EventLog.reg

[PRISM_DRIVER.EventLog.reg]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

;###############################################################################
[COMMON_A00.reg]
 HKR,NDI                ,Service                    ,0  ,"3C154G72"
 HKR,                   ,BusType                    ,0  ,"5"
 HKR,                   ,DeviceVxDs                 ,0  ,"3C154G72.sys"
 HKR,                   ,CardBusBridgeLatencyTimer  ,0  ,"32"
 HKR,                   ,CardBusBridgeCacheLineSize ,0  ,"8"

[COMMON_A00_DEL.reg]
 HKR,                   ,FWFileName

[COMMON_NDIS.reg]
; Win9X
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
;; HKR,NDI                ,NdiInstaller           ,0      ,"CCU3C154.dll,CoCCU"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"3C154G72"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

[COMMON_NDIS.reg.ME]
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
;; HKR,NDI                ,NdiInstaller           ,0      ,"CCU3C154.DLL,CoCCU"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"3C154G72"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

[COMMON_NDIS.reg.NT]
;; HKR,                   ,EnumPropPages32        ,0      ,"CCU3C154.dll,NetPropPageProvider"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

[COMMON.reg]
 HKR,                   ,PRISMIOC               ,0      ,"1"
 HKR,                   ,SilentInstall          ,0      ,"1"
;Uncomment the line above to install without user interface prompts

 HKR,NDI\params\RTSThresh,,0,2347
 HKR,Ndi\params\RTSThresh,default,0,2347
 HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
 HKR,NDI\params\RTSThresh,type,0,int
 HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
 HKR,NDI\params\RTSThresh,min,0,0
 HKR,NDI\params\RTSThresh,max,0,2347
 HKR,NDI\params\RTSThresh,step,0,1
 HKR,NDI\params\RTSThresh,optional,0,1

 HKR,NDI\params\FragThresh,,0,2346
 HKR,Ndi\params\FragThresh,default,0,2346
 HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
 HKR,NDI\params\FragThresh,type,0,int
 HKR,NDI\params\FragThresh,flag,1,20,00,00,00
 HKR,NDI\params\FragThresh,min,0,256
 HKR,NDI\params\FragThresh,max,0,2346
 HKR,NDI\params\FragThresh,step,0,2
 HKR,NDI\params\FragThresh,optional,0,1

 HKR,NDI\params\ShortRetryLimit,,0,7
 HKR,NDI\params\ShortRetryLimit,default,0,7
 HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
 HKR,NDI\params\ShortRetryLimit,type,,int
 HKR,NDI\params\ShortRetryLimit,min,0,1
 HKR,NDI\params\ShortRetryLimit,max,0,255
 HKR,NDI\params\ShortRetryLimit,step,0,1
 HKR,NDI\params\ShortRetryLimit,optional,0,1

 HKR,NDI\params\LongRetryLimit,,0,4
 HKR,NDI\params\LongRetryLimit,default,0,4
 HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
 HKR,NDI\params\LongRetryLimit,type,0,int
 HKR,NDI\params\LongRetryLimit,min,0,1
 HKR,NDI\params\LongRetryLimit,max,0,255
 HKR,NDI\params\LongRetryLimit,step,0,1
 HKR,NDI\params\LongRetryLimit,optional,0,1

 HKR,,ConfigProfile,0,256
 HKR,NDI\params\ConfigProfile,,0,256
 HKR,NDI\params\ConfigProfile,default,0,256
 HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
 HKR,NDI\params\ConfigProfile,type,,enum
 HKR,NDI\params\ConfigProfile,flag,1,30,00,00,00
 HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
 HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
 HKR,NDI\params\ConfigProfile\enum,2,,%CONFIG_PROF_MIXED_LONG%
 HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
 HKR,NDI\params\ConfigProfile\enum,4,,%CONFIG_PROF_TEST%
 HKR,NDI\params\ConfigProfile\enum,5,,%CONFIG_PROF_B_WIFI%
 HKR,NDI\params\ConfigProfile\enum,6,,%CONFIG_PROF_MIXED_SHORT%
 HKR,NDI\params\ConfigProfile\enum,256,,%CONFIG_PROF_WIFI_SPEC%
 HKR,NDI\params\ConfigProfile,optional,0,1

 HKR,,NitroMode,0,"1"
 HKR,NDI\params\NitroMode,,0,1
 HKR,NDI\params\NitroMode,default,0,1
 HKR,NDI\params\NitroMode,ParamDesc,,%NITRO_MODE%
 HKR,NDI\params\NitroMode,type,,enum
 HKR,NDI\params\NitroMode,flag,1,30,00,00,00
 HKR,NDI\params\NitroMode\enum,0,,%OFF_STR%
 HKR,NDI\params\NitroMode\enum,1,,%ON_STR%
 HKR,NDI\params\NitroMode,optional,0,1

 HKR,,PSMode,0,1
 HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
 HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
 HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
 HKR,NDI\params\PSMode,optional,0,1

;###############################################################################
[DestinationDirs]
;CopyFiles Section      = Destination Directory ID -- see layout.inf
;-----------------        ------------------------
 DefaultDestDir         = 11 ; Win9x=%windir%\system Win2k=%windir%\system32
 PRISM_DRIVER.copy      = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.ME   = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.NT   = 12 ; Win2k=%windir%\system32\drivers
 PRISM_NDI.copy         = 11 ; Win9x=%windir%\system
 PRISM_FWA00.del        = 11 ; Win9x=%windir%\system
 PRISM_FWA00.del.ME     = 11 ; Win9x=%windir%\system
 PRISM_FWA00.del.NT     = 12 ; Win2k=%windir%\system32\drivers

[PRISM_NDI.copy]
 CCU3C154.exe

[PRISM_NDI.copy.ME]
 CCU3C154.exe

[PRISM_COINSTALL.copy.NT]
 CCU3C154.dll

[PRISM_DRIVER.copy]
 3C154G72.sys

[PRISM_DRIVER.copy.ME]
 3C154G72.sys

[PRISM_DRIVER.copy.NT]
 3C154G72.sys

[PRISM_FWA00.del]
 3C154G72.arm

[PRISM_FWA00.del.ME]
 3C154G72.arm

[PRISM_FWA00.del.NT]
 3C154G72.arm

[PRISM_APPLET.copy]

[PRISM_APPLET.copy.ME]

[PRISM_APPLET.copy.NT]

[SourceDisksNames]
;Source Disk ID         = Disk Name
;--------------           ---------
 1                      = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]      ; Win9x
;File Name              = Source Disk ID
;---------                --------------
 3C154G72.sys           = 1
 CCU3C154.exe		= 1

[SourceDisksFiles.ME]   ; WinMe
 3C154G72.sys           = 1
 CCU3C154.exe		= 1

[SourceDisksFiles.X86]  ; Win2k/Xp
 3C154G72.sys           = 1,winxp
 CCU3C154.dll		= 1
 CCU3C154.exe		= 1

;###############################################################################
[Strings]
;String ID               = String Text
;---------                 -----------
 VER_VENDOR_STR          = "3Com"
 VER_VENDOR_NAME_STR     = "3Com Corporation"
 INSTALL_DISK_STR        = "3Com OfficeConnect 802.11g PC Card Install Disk"

 A001_DESC_STR           = "3Com OfficeConnect Wireless 11g PC Card (3CRWE154G72)"
 A00_SERVICE_STR         = "3Com OfficeConnect 802.11g PC Card Driver"

 ON_STR                  = "On"
 OFF_STR                 = "Off"
 RTSTHRESH_STR           = "RTS Threshold"
 FRAGTHRESH_STR          = "Fragmentation Threshold"
 AUTHENT_TYPE_STR        = "Authentication Algorithm"
 POWER_SAVE_STR          = "Power Save Mode"
 POWER_SAVE_OFF_STR      = "Disabled"
 POWER_SAVE_DYN_STR      = "Dynamic"
 POWER_SAVE_MAX_STR      = "Maximum"
 SHORT_RETRY_STR         = "Short Retry Limit"
 LONG_RETRY_STR          = "Long Retry Limit"
 CONFIG_PROFILE          = "Configuration Profile"
 CONFIG_PROF_B_ONLY      = "B only"
 CONFIG_PROF_MIXED       = "Mixed"
 CONFIG_PROF_MIXED_LONG  = "Mixed Long"
 CONFIG_PROF_G_ONLY      = "G only"
 CONFIG_PROF_TEST        = "Test"
 CONFIG_PROF_B_WIFI      = "B WiFi"
 CONFIG_PROF_MIXED_SHORT = "Mixed Short"
 CONFIG_PROF_WIFI_SPEC   = "WiFi Spec"
 NITRO_MODE              = "Nitro Mode"

