;; NETRTLXP.INF (WindowsXP inf for NDIS5.1 driver)
;;
;; Realtek RTL8139/810x/8169/8110 all in one INF file
;;
;; Copyright 2003, Realtek Semiconductor Corporation
;;
;; .this release is primarily for motherboard OEM for WHQL test.

[version]
Signature	= "$Chicago$"
Compatible	= 1
Class		= Net
ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
Provider	= %Realtek%                                
CatalogFile	= netrtlxp.cat	;; for WHQL certified
DriverVer	= 12/31/2003,5.611.1231.2003

[Manufacturer]
%Realtek%   = Realtek

[ControlFlags]
ExcludeFromSelect = PCI\VEN_10EC&DEV_8139
ExcludeFromSelect = PCI\VEN_10EC&DEV_8169

[Realtek]
; DisplayName		Section		   DeviceID
; -----------		-------		   --------
%RTL8169.DeviceDesc%	= RTL8169.ndi,	   PCI\VEN_10EC&DEV_8169
%RTL8139.DeviceDesc%	= RTL8139.ndi,     PCI\VEN_10EC&DEV_8139&REV_10
%RTL8139P.DeviceDesc%	= RTL8139P.ndi,    PCI\VEN_10EC&DEV_8139&REV_20
%RTL8169.DeviceDesc%	= RTL8169.ndi,     PCI\VEN_10EC&DEV_8169&SUBSYS_816910EC
%RTL8139.DeviceDesc%	= RTL8139_TOS.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_813610EC
%RTL8139.DeviceDesc%	= RTL8139.ndi,     PCI\VEN_10EC&DEV_8139&SUBSYS_813910EC&REV_10
%RTL8139P.DeviceDesc%	= RTL8139P.ndi,    PCI\VEN_10EC&DEV_8139&SUBSYS_813910EC&REV_20

;----------------
; RTL8139 Family
;----------------
[RTL8139.ndi.NT]
DelReg          = PreParams.DelReg
AddReg          = Rtlnic.common.reg, RTL8139.common.reg, RTL8023.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFiles

[RTL8139.ndi.NT.Services]
AddService = RTL8023, 2, rtsnt.Service, common.EventLog

[RTL8139_TOS.ndi.NT]
DelReg          = PreParams.DelReg
AddReg          = RTL8139TOS.common.reg, RTL8023.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFiles

[RTL8139_TOS.ndi.NT.Services]
AddService = RTL8023, 2, rtsnt.Service, common.EventLog

;-----------
; RTL8139c+
;-----------
[RTL8139P.ndi.NT]
DelReg          = CpPreParams.DelReg
AddReg          = Rtlnic.common.reg, RTL8139P.common.reg, RTL8023.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = Rtlnic.CopyFiles

[RTL8139P.ndi.NT.Services]
AddService = RTL8023, 2, rtsnt.Service, common.EventLog

;---------
; RTL8169
;---------
[RTL8169.ndi.NT]
Characteristics = 0x84
BusType         = 5
AddReg          = RTL8169.common.reg, RTL8023.reg
CopyFiles       = Rtlnic.CopyFiles

[RTL8169.ndi.NT.Services]
AddService = RTL8023, 2, rtsnt.Service, common.EventLog

[Rtlnic.CopyFiles]
Rtlnic51.sys,,,2

;;****************************************************************************
;; common parameters
;;****************************************************************************
[Rtlnic.common.reg]
HKR,Ndi\params\DuplexMode,        ParamDesc,   0, %SpeedDuplexMode%
HKR,Ndi\params\DuplexMode,        type,        0, "enum"
HKR,Ndi\params\DuplexMode,        default,     0, "1"
HKR,Ndi\params\DuplexMode\enum,   1,           0, %auto_nego%
HKR,Ndi\params\DuplexMode\enum,   2,           0, %sd10half%
HKR,Ndi\params\DuplexMode\enum,   3,           0, %sd10full%
HKR,Ndi\params\DuplexMode\enum,   4,           0, %sd100half%
HKR,Ndi\params\DuplexMode\enum,   5,           0, %sd100full%

HKR,Ndi\params\NetworkAddress,    ParamDesc,  0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,    type,       0, "edit"
HKR,Ndi\params\NetworkAddress,    default,    0, "000000000000"
HKR,Ndi\params\NetworkAddress,    LimitText,  0, "12"
HKR,Ndi\params\NetworkAddress,    UpperCase,  0, "1"
HKR,Ndi\params\NetworkAddress,    Optional,   0, "1"

HKR,Ndi\params\WakeUpFrame,       ParamDesc,  0, %WOLCapability%
HKR,Ndi\params\WakeUpFrame,       default,    0, "1"
HKR,Ndi\params\WakeUpFrame,       type,       0, "enum"
HKR,Ndi\params\WakeUpFrame\enum,  "1",        0, "Enable"
HKR,Ndi\params\WakeUpFrame\enum,  "0",        0, "Disable"
HKR,,WakeUpFrame, 0, "1"  

HKR,Ndi\params\LinkUp,            ParamDesc,  0, %WOLLinkChange%
HKR,Ndi\params\LinkUp,            default,    0, "0"
HKR,Ndi\params\LinkUp,            type,       0, "enum"
HKR,Ndi\params\LinkUp\enum,       "1",        0, "Enable"
HKR,Ndi\params\LinkUp\enum,       "0",        0, "Disable"

HKR,Ndi\params\EnableLDPS,        ParamDesc,  0, %LDPSCapability%
HKR,Ndi\params\EnableLDPS,        default,    0, "0"
HKR,Ndi\params\EnableLDPS,        type,       0, "enum"
HKR,Ndi\params\EnableLDPS\enum,   "1",        0, "Enable"
HKR,Ndi\params\EnableLDPS\enum,   "0",        0, "Disable"

HKR,Ndi\params\OptimalPerf,        ParamDesc, 0, %OptimalPerf%
HKR,Ndi\params\OptimalPerf,        default,   0, "0"
HKR,Ndi\params\OptimalPerf,        type,      0, "enum"
HKR,Ndi\params\OptimalPerf\enum,   "1",       0, "Enable"
HKR,Ndi\params\OptimalPerf\enum,   "0",       0, "Disable"

;----------------
; RTL8139 Family
;----------------
[RTL8139.common.reg]
HKR,Ndi\params\RxBufLen,	  ParamDesc,  0, "Receive Buffer Size"
HKR,Ndi\params\RxBufLen,	  type,       0, "enum"
HKR,Ndi\params\RxBufLen,	  default,    0, "3"
HKR,Ndi\params\RxBufLen\enum,	  "0",	      0, "8K bytes"
HKR,Ndi\params\RxBufLen\enum,	  "1",	      0, "16K bytes"
HKR,Ndi\params\RxBufLen\enum,	  "2",	      0, "32K bytes"
HKR,Ndi\params\RxBufLen\enum,	  "3",	      0, "64K bytes"

HKR,Ndi\params\RTPME,             ParamDesc,  0, "WakeUp using APM Mode"
HKR,Ndi\params\RTPME,             default,    0, "0"
HKR,Ndi\params\RTPME,             type,       0, "enum"
HKR,Ndi\params\RTPME\enum,        "1",        0, "Enable"
HKR,Ndi\params\RTPME\enum,        "0",        0, "Disable"

;-----------
; RTL8139c+
;-----------
[RTL8139P.common.reg]
HKR,Ndi\Params\NumCoalesce,       ParamDesc,  0, "Number of Tx Coalesce Buffer"
HKR,Ndi\Params\NumCoalesce,       Type,       0, "int"
HKR,Ndi\Params\NumCoalesce,       Default,    0, "16"
HKR,Ndi\Params\NumCoalesce,       Min,        0, "0"
HKR,Ndi\Params\NumCoalesce,       Max,        0, "32"
HKR,Ndi\Params\NumCoalesce,       Step,       0, "1"
HKR,Ndi\Params\NumCoalesce,       Base,       0, "10"

HKR,Ndi\params\Offload,           ParamDesc,  0, "Task Offload"
HKR,Ndi\params\Offload,           default,    0, "1"
HKR,Ndi\params\Offload,           type,       0, "enum"
HKR,Ndi\params\Offload\enum,      "0",        0, "All Disable"
HKR,Ndi\params\Offload\enum,      "1",        0, "Checksum"
HKR,Ndi\params\Offload\enum,      "2",        0, "Chksum & TCP_Segment"

HKR,Ndi\params\Support8021p,      ParamDesc,  0, "802.1Q/1p VLAN Tagging"
HKR,Ndi\params\Support8021p,      default,    0, "0"
HKR,Ndi\params\Support8021p,      type,       0, "enum"
HKR,Ndi\params\Support8021p\enum, "0",        0, "Disable"
HKR,Ndi\params\Support8021p\enum, "1",        0, "Enable"

[PreParams.DelReg]
HKR,Ndi\Params\PME
HKR,,PME
HKR,Ndi\Params\EarlyTxThreshold
HKR,,EarlyTxThreshold

[CpPreParams.DelReg]
HKR,Ndi\Params\PME
HKR,,PME
HKR,Ndi\Params\RTPME
HKR,,RTPME
HKR,Ndi\Params\RxBufLen
HKR,,RxBufLen
HKR,Ndi\Params\EarlyTxThreshold
HKR,,EarlyTxThreshold

[RTL8139TOS.common.reg] 
HKR,Ndi\params\DuplexMode,        ParamDesc,   0, %SpeedDuplexMode%
HKR,Ndi\params\DuplexMode,        type,        0, "enum"
HKR,Ndi\params\DuplexMode,        default,     0, "1"
HKR,Ndi\params\DuplexMode\enum,   1,           0, %auto_nego%
HKR,Ndi\params\DuplexMode\enum,   2,           0, %sd10half%
HKR,Ndi\params\DuplexMode\enum,   3,           0, %sd10full%
HKR,Ndi\params\DuplexMode\enum,   4,           0, %sd100half%
HKR,Ndi\params\DuplexMode\enum,   5,           0, %sd100full%

HKR,Ndi\params\NetworkAddress,     ParamDesc,  0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,     type,       0, "edit"
HKR,Ndi\params\NetworkAddress,     default,    0, "000000000000"
HKR,Ndi\params\NetworkAddress,     LimitText,  0, "12"
HKR,Ndi\params\NetworkAddress,     UpperCase,  0, "1"
HKR,Ndi\params\NetworkAddress,     Optional,   0, "1"

HKR,Ndi\params\RxBufLen,           ParamDesc,  0, "Receive Buffer Size"
HKR,Ndi\params\RxBufLen,           type,       0, "enum"
HKR,Ndi\params\RxBufLen,           default,    0, "3"
HKR,Ndi\params\RxBufLen\enum,      "0",        0, "8K bytes"
HKR,Ndi\params\RxBufLen\enum,      "1",        0, "16K bytes"
HKR,Ndi\params\RxBufLen\enum,      "2",        0, "32K bytes"
HKR,Ndi\params\RxBufLen\enum,      "3",        0, "64K bytes"

HKR, Ndi\params\LinkUp,            ParamDesc,  0, %WOLLinkChange%
HKR, Ndi\params\LinkUp,            default,    0, "0"
HKR, Ndi\params\LinkUp,            type,       0, "enum"
HKR, Ndi\params\LinkUp\enum,       "1",        0, "Enable"
HKR, Ndi\params\LinkUp\enum,       "0",        0, "Disable"

HKR, Ndi\params\WakeUpFrame,       ParamDesc,  0, %WOLCapability%        
HKR, Ndi\params\WakeUpFrame,       default,    0, "1"                          
HKR, Ndi\params\WakeUpFrame,       type,       0, "enum"                       
HKR, Ndi\params\WakeUpFrame\enum,  "1",        0, "Enable"                     
HKR, Ndi\params\WakeUpFrame\enum,  "0",        0, "Disable"                   

HKR, Ndi\params\RTPME,             ParamDesc,  0, "WakeUp using APM Mode"     
HKR, Ndi\params\RTPME,             default,    0, "0"                         
HKR, Ndi\params\RTPME,             type,       0, "enum"                     
HKR, Ndi\params\RTPME\enum,        "1",        0, "Enable"                 
HKR, Ndi\params\RTPME\enum,        "0",        0, "Disable"                   

HKR, Ndi\params\EnableLDPS,        ParamDesc,  0, %LDPSCapability%
HKR, Ndi\params\EnableLDPS,        default,    0, "1"
HKR, Ndi\params\EnableLDPS,        type,       0, "enum"
HKR, Ndi\params\EnableLDPS\enum,   "1",        0, "Enable"
HKR, Ndi\params\EnableLDPS\enum,   "0",        0, "Disable"

HKR,Ndi\params\TxMaxDMABurst,      ParamDesc,  0, "Transmit DMA burst size"  
HKR,Ndi\params\TxMaxDMABurst,      type,       0, "enum"                           
HKR,Ndi\params\TxMaxDMABurst,      default,    0, "6"       
HKR,Ndi\params\TxMaxDMABurst\enum, 0,          0, "16 bytes" 
HKR,Ndi\params\TxMaxDMABurst\enum, 1,          0, "32 bytes"
HKR,Ndi\params\TxMaxDMABurst\enum, 2,          0, "64 bytes" 
HKR,Ndi\params\TxMaxDMABurst\enum, 3,          0, "128 bytes"
HKR,Ndi\params\TxMaxDMABurst\enum, 4,          0, "256 bytes"  
HKR,Ndi\params\TxMaxDMABurst\enum, 5,          0, "512 bytes"     
HKR,Ndi\params\TxMaxDMABurst\enum, 6,          0, "1024 bytes"  
HKR,Ndi\params\TxMaxDMABurst\enum, 7,          0, "2048 bytes"  

HKR,Ndi\params\RxMaxDMABurst,      ParamDesc,  0, "Receive DMA burst size"   
HKR,Ndi\params\RxMaxDMABurst,      type,       0, "enum"                            
HKR,Ndi\params\RxMaxDMABurst,      default,    0, "6"                            
HKR,Ndi\params\RxMaxDMABurst\enum, 0,          0, "16 bytes"                  
HKR,Ndi\params\RxMaxDMABurst\enum, 1,          0, "32 bytes"                 
HKR,Ndi\params\RxMaxDMABurst\enum, 2,          0, "64 bytes"                 
HKR,Ndi\params\RxMaxDMABurst\enum, 3,          0, "128 bytes"                 
HKR,Ndi\params\RxMaxDMABurst\enum, 4,          0, "256 bytes"                 
HKR,Ndi\params\RxMaxDMABurst\enum, 5,          0, "512 bytes"                 
HKR,Ndi\params\RxMaxDMABurst\enum, 6,          0, "1024 bytes"                
HKR,Ndi\params\RxMaxDMABurst\enum, 7,          0, "unlimitted"               

HKR,Ndi\params\EarlyRxThreshold,     ParamDesc,0, "Receive FIFO threshold"   
HKR,Ndi\params\EarlyRxThreshold,     type,     0, "enum"
HKR,Ndi\params\EarlyRxThreshold,     default,  0, "2"                    
HKR,Ndi\params\EarlyRxThreshold\enum,0,        0, "16 bytes"                  
HKR,Ndi\params\EarlyRxThreshold\enum,1,        0, "32 bytes"                  
HKR,Ndi\params\EarlyRxThreshold\enum,2,        0, "64 bytes"                  
HKR,Ndi\params\EarlyRxThreshold\enum,3,        0, "128 bytes"                 
HKR,Ndi\params\EarlyRxThreshold\enum,4,        0, "256 bytes"                 
HKR,Ndi\params\EarlyRxThreshold\enum,5,        0, "512 bytes"                 
HKR,Ndi\params\EarlyRxThreshold\enum,6,        0, "1024 bytes"                
HKR,Ndi\params\EarlyRxThreshold\enum,7,        0, "No threshold"              

HKR,,EnableLDPS,        0,   "1"
HKR,,WakeUpFrame,       0,   "1"          
HKR,,RTPME,             0,   "0"          
HKR,,LinkUp,            0,   "0"
HKR,,RxBufLen,          0,   "3"
HKR,,EarlyRxThreshold,  0,   "2"                   
HKR,,RxMaxDMABurst,     0,   "6"                  
HKR,,TxMaxDMABurst,     0,   "6"    
  
;---------
; RTL8169
;---------
[RTL8169.common.reg]
HKR, Ndi\params\DuplexMode,       ParamDesc,  0, %SpeedDuplexMode%
HKR, Ndi\params\DuplexMode,       type,       0, "enum"
HKR, Ndi\params\DuplexMode,       default,    0, "1"
HKR, Ndi\params\DuplexMode\enum,  1,          0, %auto_nego%
HKR, Ndi\params\DuplexMode\enum,  2,          0, %sd10half%
HKR, Ndi\params\DuplexMode\enum,  3,          0, %sd10full%
HKR, Ndi\params\DuplexMode\enum,  4,          0, %sd100half%
HKR, Ndi\params\DuplexMode\enum,  5,          0, %sd100full%
HKR, Ndi\params\DuplexMode\enum,  6,          0, %sd1000full%

HKR,Ndi\params\NetworkAddress,    ParamDesc,  0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,    type,       0, "edit"
HKR,Ndi\params\NetworkAddress,    default,    0, "000000000000"
HKR,Ndi\params\NetworkAddress,    LimitText,  0, "12"
HKR,Ndi\params\NetworkAddress,    UpperCase,  0, "1"
HKR,Ndi\params\NetworkAddress,    Optional,   0, "1"

HKR,Ndi\Params\NumTxDesc,         ParamDesc,  0, %TxDescNumber%
HKR,Ndi\Params\NumTxDesc,         Type,       0, "int"
HKR,Ndi\Params\NumTxDesc,         Default,    0, "256"
HKR,Ndi\Params\NumTxDesc,         Min,        0, "64"
HKR,Ndi\Params\NumTxDesc,         Max,        0, "512"
HKR,Ndi\Params\NumTxDesc,         Step,       0, "1"
HKR,Ndi\Params\NumTxDesc,         Base,       0, "10"

HKR,Ndi\Params\NumRxDesc,         ParamDesc,  0, %RxDescNumber%
HKR,Ndi\Params\NumRxDesc,         Type,       0, "int"
HKR,Ndi\Params\NumRxDesc,         Default,    0, "256"
HKR,Ndi\Params\NumRxDesc,         Min,        0, "64"
HKR,Ndi\Params\NumRxDesc,         Max,        0, "512"
HKR,Ndi\Params\NumRxDesc,         Step,       0, "1"
HKR,Ndi\Params\NumRxDesc,         Base,       0, "10"

HKR,Ndi\Params\NumTxDescHPQ,      ParamDesc,  0, %TxHPQDescNumber%
HKR,Ndi\Params\NumTxDescHPQ,      Type,       0, "int"
HKR,Ndi\Params\NumTxDescHPQ,      Default,    0, "256"
HKR,Ndi\Params\NumTxDescHPQ,      Min,        0, "64"
HKR,Ndi\Params\NumTxDescHPQ,      Max,        0, "512"
HKR,Ndi\Params\NumTxDescHPQ,      Step,       0, "1"
HKR,Ndi\Params\NumTxDescHPQ,      Base,       0, "10"

HKR,Ndi\params\WakeUpFrame,       ParamDesc,  0, %WOLCapability%
HKR,Ndi\params\WakeUpFrame,       default,    0, "1"
HKR,Ndi\params\WakeUpFrame,       type,       0, "enum"
HKR,Ndi\params\WakeUpFrame\enum,  "0",        0, "Disable"
HKR,Ndi\params\WakeUpFrame\enum,  "1",        0, "Enable"

HKR,Ndi\params\CksOffload,        ParamDesc,  0, %ChecksumOffload%
HKR,Ndi\params\CksOffload,        default,    0, "1"
HKR,Ndi\params\CksOffload,        type,       0, "enum"
HKR,Ndi\params\CksOffload\enum,   "0",        0, "Disable"
HKR,Ndi\params\CksOffload\enum,   "1",        0, "Tx/Rx Checksum"
HKR,Ndi\params\CksOffload\enum,   "3",        0, "Rx Checksum"
HKR,Ndi\params\CksOffload\enum,   "4",        0, "Tx Checksum"

HKR,Ndi\params\Largesend,         ParamDesc,  0, %LargesendOffload%
HKR,Ndi\params\Largesend,         default,    0, "0"
HKR,Ndi\params\Largesend,         type,       0, "enum"
HKR,Ndi\params\Largesend\enum,    "1",        0, "Enable"
HKR,Ndi\params\Largesend\enum,    "0",        0, "Disable"

HKR,Ndi\params\Support8021p,      ParamDesc,  0, %VLanTagging%
HKR,Ndi\params\Support8021p,      default,    0, "0"
HKR,Ndi\params\Support8021p,      type,       0, "enum"
HKR,Ndi\params\Support8021p\enum, "0",        0, "Disable"
HKR,Ndi\params\Support8021p\enum, "1",        0, "Enable"

HKR,Ndi\params\FlowControl,      ParamDesc,  0, %FlowControl%
HKR,Ndi\params\FlowControl,      default,    0, "0"
HKR,Ndi\params\FlowControl,      type,       0, "enum"
HKR,Ndi\params\FlowControl\enum, "0",        0, "Disable"
HKR,Ndi\params\FlowControl\enum, "1",        0, "Enable"

HKR,Ndi\Params\RegVlanid,   ParamDesc,  0, %VLanID%
HKR,Ndi\Params\RegVlanid,   Type,       0, "int"
HKR,Ndi\Params\RegVlanid,   Default,    0, "0"
HKR,Ndi\Params\RegVlanid,   Min,        0, "0"
HKR,Ndi\Params\RegVlanid,   Max,        0, "4094"
HKR,Ndi\Params\RegVlanid,   Step,       0, "1"
HKR,Ndi\Params\RegVlanid,   Base,       0, "10"

HKR,Ndi\params\Jumboframe,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\Jumboframe,        default,    0, "0"
HKR,Ndi\params\Jumboframe,        type,       0, "enum"
HKR,Ndi\params\Jumboframe\enum,   "0",        0, "Disable"
HKR,Ndi\params\Jumboframe\enum,   "1",        0, "2KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "2",        0, "3KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "3",        0, "4KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "4",        0, "5KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "5",        0, "6KB MTU"
HKR,Ndi\params\Jumboframe\enum,   "6",        0, "7KB MTU"

HKR,,WakeUpFrame,0,"1" 
HKR,,CksOffload,0,"1" 
HKR,,Largesend,0,"0" 

;;****************************************************************************
;; NT 5.0 parameters
;;****************************************************************************
[RTL8023.reg]
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi,            Service,    0, "RTL8023"

[rtsnt.Service]
DisplayName     = %Rtlnic.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtlnic51.sys
LoadOrderGroup  = NDIS

[common.EventLog]
Addreg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
Rtlnic.CopyFiles           = 12
DefaultDestDir             = 11        ; LDID_SYS

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
Rtlnic51.sys  = 1

;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p VLAN Tagging"
VLanID			= "802.1Q VLAN ID"
ChecksumOffload		= "Offload Checksum"
LargesendOffload	= "Offload TCP_LargeSend"
SpeedDuplexMode		= "Link Speed/Duplex Mode"
auto_nego		= "Auto Negotiation"
sd10half		= "10Mbps/Half Duplex"
sd10full		= "10Mbps/Full Duplex"
sd100half		= "100Mbps/Half Duplex"
sd100full		= "100Mbps/Full Duplex"
sd1000full		= "1000Mbps/Full Duplex"
NetworkAddress		= "Network Address"
JumboFrame		= "Jumbo Frame"
TxDescNumber		= "Number of Tx Descriptor"
RxDescNumber		= "Number of Rx Descriptor"
TxHPQDescNumber		= "Number of High Priority Tx Descriptor"
WOLCapability		= "WakeUp on ARP/PING"
WOLLinkChange		= "WakeUp on Link Change"
LDPSCapability		= "Link Down Power Saving"
OptimalPerf		= "Optimal Performance"
FlowControl		= "Flow Control"

;;Source disk name
DISKNAME = "Realtek RTL8139/810x/8169/8110 all in one NDIS Driver"

RTL8169.DeviceDesc        = "Realtek RTL8169/8110 Family Gigabit Ethernet NIC"
RTL8139.DeviceDesc        = "Realtek RTL8139/810x Family Fast Ethernet NIC"
RTL8139P.DeviceDesc       = "Realtek RTL8139C+ Fast Ethernet NIC"

;;NT service name
Rtlnic.Service.DispName    = "Realtek RTL8139/810x/8169/8110 all in one NDIS NT Driver"
