;***********************************************************************
;
; NETWPX96.INF
;
;   This installation script supportted Windows 2000 and XP for the
;   3COM Wireless LAN PCI Adapter.
;
;   Copyright (c) 2001-2002 Gemtek Corporation
;   All Rights Reserved.
;   
;   
;***********************************************************************

[Version]
 DriverVer = 05/08/2002, 1.07.37.1037
 Signature           = "$Chicago$"
 Compatible          = 1
 Class               = Net
 ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
 Provider            = %VER_VENDOR_STR%
 CatalogFile         = NETWPX96.cat

[ControlFlags]
 ExcludeFromSelect   = PCMCIA\WIRELESS_LAN-11MBPS_PC_CARD-207D
 ExcludeFromSelect   = PCI\VEN_1260&DEV_3873&SUBSYS_000110B7


[Manufacturer]
 %VER_VENDOR_NAME_STR% = DeviceList,NTx86.5.1
 
[DeviceList.NTx86.5.1]
 %PRISM_PCMCIA7_STR% = PRISM_PCMCIA7.NT, PCMCIA\WIRELESS_LAN-11MBPS_PC_CARD-207D
 %PRISM_PCI1_STR%    = PRISM_PCI1.NT,    PCI\VEN_1260&DEV_3873&SUBSYS_000110B7
 

[DeviceList]
 
 %PRISM_PCMCIA7_STR% = PRISM_PCMCIA7, PCMCIA\WIRELESS_LAN-11MBPS_PC_CARD-207D
 %PRISM_PCI1_STR%    = PRISM_PCI1,    PCI\VEN_1260&DEV_3873&SUBSYS_000110B7




;==========================================
[PRISM_PCMCIA7]         ; Win9x
 AddReg         = PRISM_PCMCIA7.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy

[PRISM_PCMCIA7.NT]      ; Win2k
 AddReg         = PRISM_PCMCIA7.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.NT
 BusType        = 8     ; PCMCIA
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_PCMCIA7.NT.Services]
 AddService     = "PRISM", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog

; This is to start CoHelper.exe afer driver installs on Win2K systems.
; RunOnce will not work because Win2K does not require reboot after driver install.
; [PRISM_PCMCIA7.NT.CoInstallers]
; CopyFiles = PRISM_DRIVER.copy
; AddReg = PRISM_DRIVER.CoInstallers_AddReg

[PRISM_PCMCIA7.reg]
 HKR,Ndi        ,DeviceID,0,"PCMCIA\WIRELESS_LAN-11MBPS_PC_CARD-207D"


;==========================================
[PRISM_PCI1]            ; Win9x
 AddReg         = PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy

[PRISM_PCI1.NT]         ; Win2k
 AddReg         = PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_PCI1.NT.Services]
 AddService     = "PRISM", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog

; This is to start CoHelper.exe afer driver installs on Win2K systems.
; RunOnce will not work because Win2K does not require reboot after driver install.
; [PRISM_PCI1.NT.CoInstallers]
; CopyFiles = PRISM_DRIVER.copy
; AddReg = PRISM_DRIVER.CoInstallers_AddReg

[PRISM_PCI1.reg]
 HKR,Ndi        ,DeviceID,0,"PCI\VEN_1260&DEV_3873&SUBSYS_000110B7"




;###############################################################################

[PRISM_DRIVER.Service]
 DisplayName    = %PRISM_SERVICE_DISPLAY%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\PRISMNDS.sys
 LoadOrderGroup = NDIS

;*******************************************************************************
; Add Service section for CoInstaller
;*******************************************************************************

; [PRISM_DRIVER.CoInstallers_AddReg]
; HKR,,CoInstallers32,0x00010000,"coinst.dll, SrwlCoInstaller"

[PRISM_DRIVER.EventLog]
 AddReg         = PRISM_DRIVER.EventLog.reg

[PRISM_DRIVER.EventLog.reg]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

;###############################################################################
[COMMON_PCMCIA.reg]
;RegKey,SubKey          ,Name                   ,Type   ,Value
;-------------          -----                   -----   ------
 HKR,NDI                ,Service                ,0      ,"PRISM"
 HKR,NDI                ,CardType               ,0      ,"PCMCIA"
 HKR,                   ,BusType                ,0      ,"8"
 HKR,                   ,DeviceVxDs             ,0      ,"PRISMNDS.sys"
 HKR,                   ,EnableIRQSharing       ,1      ,01,00,00,00
 HKR,                   ,IOBaseAddress          ,1      ,02,00,00,00
 HKR,                   ,InterruptNumber        ,1      ,04,00,00,00

[COMMON_PCI.reg]
 HKR,NDI                ,Service                ,0      ,"PRISM"
 HKR,NDI                ,CardType               ,0      ,"PCI"
 HKR,                   ,BusType                ,0      ,"5"
 HKR,                   ,DeviceVxDs             ,0      ,"PRISMNDS.sys"
 HKR,                   ,EnableIRQSharing       ,1      ,01,00,00,00
 HKR,                   ,IOBaseAddress          ,1      ,02,00,00,00
 HKR,                   ,InterruptNumber        ,1      ,04,00,00,00



[COMMON_NDIS.reg]
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 HKR,NDI                ,NdiInstaller           ,0      ,"PRISMCFG.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"PRISM"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

 HKR,defaults,PSMode,0,1
 HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode,optional,0,1


[COMMON_NDIS.reg.NT]
 HKR,                   ,EnumPropPages32        ,0      ,"PRISMCFG.cpl,NetPropPageProvider"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

 HKR,defaults,PSMode,0,1
 HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode\enum,3,,"Auto Enable"
 HKR,NDI\params\PSMode,optional,0,1

[COMMON.reg]
 HKR,                   ,GTKSIOC               ,0      ,"1"
 HKR,                   ,PRISMIOC               ,0      ,"1"
 HKR,                   ,SilentInstall          ,0      ,"1"
;Uncomment the line above to install without user interface prompts

 HKR,defaults,ListenInterval,0,3
 HKR,NDI\params\ListenInterval,,0,3
 HKR,Ndi\params\ListenInterval,default,0,3
 HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
 HKR,NDI\params\ListenInterval,type,,int
 HKR,NDI\params\ListenInterval,flag,1,30,00,00,00
 HKR,NDI\params\ListenInterval,min,0,0
 HKR,NDI\params\ListenInterval,max,0,77
 HKR,NDI\params\ListenInterval,step,0,1
 HKR,NDI\params\ListenInterval,optional,0,1

 HKR,defaults,RTSThresh,0,2432
 HKR,NDI\params\RTSThresh,,0,2432
 HKR,Ndi\params\RTSThresh,default,0,2432
 HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
 HKR,NDI\params\RTSThresh,type,0,int
 HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
 HKR,NDI\params\RTSThresh,min,0,0
 HKR,NDI\params\RTSThresh,max,0,2432
 HKR,NDI\params\RTSThresh,step,0,64
 HKR,NDI\params\RTSThresh,optional,0,1

 HKR,defaults,FragThresh,0,2432
 HKR,NDI\params\FragThresh,,0,2432
 HKR,Ndi\params\FragThresh,default,0,2432
 HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
 HKR,NDI\params\FragThresh,type,0,int
 HKR,NDI\params\FragThresh,flag,1,20,00,00,00
 HKR,NDI\params\FragThresh,min,0,256
 HKR,NDI\params\FragThresh,max,0,2432
 HKR,NDI\params\FragThresh,step,0,128
 HKR,NDI\params\FragThresh,optional,0,1

 HKR,defaults,PreambleMode,0,1
 HKR,NDI\params\PreambleMode,,0,1
 HKR,Ndi\params\PreambleMode,default,0,1
 HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
 HKR,NDI\params\PreambleMode,type,,enum
 HKR,NDI\params\PreambleMode,flag,1,30,00,00,00
 HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
 HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
 HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
 HKR,NDI\params\PreambleMode,optional,0,1

 HKR,defaults,AuthentAlg,0,65535
 HKR,NDI\params\AuthentAlg,,0,65535
 HKR,NDI\params\AuthentAlg,default,0,65535
 HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
 HKR,NDI\params\AuthentAlg,type,,enum
 HKR,NDI\params\AuthentAlg,flag,1,30,00,00,00
 HKR,NDI\params\AuthentAlg\enum,1,,"WECA Compliant (always use Open)"
 HKR,NDI\params\AuthentAlg\enum,2,,"Must use Shared with WEP"
 HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
 HKR,NDI\params\AuthentAlg,optional,0,1

 HKR,defaults,AdhocDemoMode,0,0
 HKR,NDI\params\AdhocDemoMode,,0,0
 HKR,Ndi\params\AdhocDemoMode,default,0,0
 HKR,NDI\params\AdhocDemoMode,ParamDesc,,%ADHOC_DEMO_STR%
 HKR,NDI\params\AdhocDemoMode,type,,enum
 HKR,NDI\params\AdhocDemoMode,flag,1,30,00,00,00
 HKR,NDI\params\AdhocDemoMode\enum,0,,"Disable"
 HKR,NDI\params\AdhocDemoMode\enum,1,,"Enable"
 HKR,NDI\params\AdhocDemoMode,optional,0,1

;###############################################################################
[DestinationDirs]
;CopyFiles Section      = Destination Directory ID -- see layout.inf
;-----------------        ------------------------
 DefaultDestDir         = 11 ; Win9x=%windir%\system Win2k=%windir%\system32
 PRISM_DRIVER.copy      = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.NT   = 12 ; Win2k=%windir%\system32\drivers
 
 
[PRISM_DRIVER.copy]
 PRISMNDS.sys
; cohelper.exe,,,2
; coinst.dll,,,2


[PRISM_DRIVER.copy.NT]
 PRISMNDS.sys
 



[SourceDisksNames]
;Source Disk ID         = Disk Name
;--------------           ---------
 1                      = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]      ; Win9x
;File Name              = Source Disk ID
;---------                --------------
 PRISMNDS.sys           = 1

[SourceDisksFiles.X86]  ; Win2k/Xp
 PRISMNDS.sys		= 1,SYS
 

;###############################################################################
[Strings]
;String ID              = String Text
;---------                -----------
 VER_VENDOR_STR         = "3Com"
 VER_VENDOR_NAME_STR    = "3Com Corporation"

 
 PRISM_PCMCIA7_STR      = "3Com 3CRDW696 Wireless LAN PC Card"
 PRISM_PCI1_STR         = "3Com 3CRDW696 Wireless LAN PCI Adapter"
 PRISM_PCI2_STR         = "3Com 3CRDW696 Wireless LAN PCI Adapter"
 PRISM_SERVICE_DISPLAY  = "3Com 3CRDW696 Wireless LAN PCI Adapter LAN Driver"
 INSTALL_DISK_STR       = "3Com 3CRDW696 Wireless LAN PCI Adapter Install Disk"


 ADHOC_DEMO_STR         = "Adhoc Demo Mode"
 SHORT_PREAM_STR        = "Preamble Mode"
 RTSTHRESH_STR          = "RTS Threshold"
 FRAGTHRESH_STR         = "Fragmentation Threshold"
 AUTHENT_TYPE_STR       = "Authentication Algorithm"
 LISTENINTERVAL_STR     = "Listen Interval"
 POWER_SAVE_STR         = "Power Save Mode"
 POWER_LEVEL_STR        = "Power Save Level"
 

