;; Windows .INF file for NDIS driver
;;
;; Realtek RTL8187 Wireless USB 2.0 Adapter
;;
;; Copyright (C) 2007 Realtek Semiconductor Corp.
;;
;; this release is primarily for WHQL test.

[Version]
Signature	= "$Chicago$"
Compatible	= 1
Class		= Net
ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
Provider	= %Realtek%
CatalogFile.NT	= netrtuw.cat		;; for WHQL certified
DriverVer	= 05/18/2007,5.1293.0518.2007

[Manufacturer]
%Realtek%    = Realtek

[ControlFlags]
ExcludeFromSelect = USB\VID_0BDA&PID_8187&REV_0100
ExcludeFromSelect = USB\VID_0769&PID_11F2&REV_0100

[Realtek]
%RTL8187.DeviceDesc% = RTL8187.ndi,USB\VID_0BDA&PID_8187&REV_0100

;;****************************************************************************
;; IDs for OEM.
;;****************************************************************************
%RTL8187.DeviceDesc% = RTL8187.ndi,USB\VID_13D1&PID_ABE6&REV_0100 ; 
%RTL8187.DeviceDesc% = RTL8187.ndi,USB\VID_1371&PID_9401&REV_0100 ;
%RTL8187.DeviceDesc% = RTL8187.ndi,USB\VID_114B&PID_0150&REV_0100 ;
%RTL8187.DeviceDesc% = RTL8187.ndi,USB\VID_18E8&PID_6232&REV_0100 ;
%RTL8187.DeviceDesc% = RTL8187.ndi,USB\VID_0789&PID_010C&REV_0100 ;

%RTL8187.DeviceDesc.Surecom% = RTL8187.ndi,USB\VID_0769&PID_11F2&REV_0100 ;
%RTL8187.DeviceDesc.Sitecom% = RTL8187.ndi,USB\VID_0DF6&PID_000D&REV_0100 ;

; by Owen on 04/12/04
;;****************************************************************************
;; Windows 98
;;****************************************************************************
[RTL8187.ndi]
DriverVer       = 05/18/2007,1293
AddReg = RTL8187.Reg, RTL8187.common.reg
CopyFiles       = RTL8187.CopyFiles98
;
;;****************************************************************************
;; Windows XP
;;****************************************************************************
[RTL8187.ndi.NT]
AddReg		= RTL8187.NT.Reg, RTL8187.common.reg
Characteristics = 0x84
BusType         = 15 
CopyFiles       = RTL8187.CopyFiles


[RTL8187.ndi.NT.Services]
AddService = RTLWUSB, 2, rtsnt.Service, RTL8187.EventLog

; by Owen on 04/12/04
;*******************************************************************************
; Windows 98
;*******************************************************************************
[RTL8187.Reg]
HKR, Ndi, DeviceID, 0, USB\VID_0BDA&PID_8187&REV_0100

HKR,Ndi,CardType,,"PNP"

HKR, , DriverDesc, 0, "Realtek RTL8187 Wireless USB 2.0 Adapter"
HKR, , DevLoader,,*ndis,*ntkern,*ndis
HKR, , DeviceVxDs,,RTL8187.sys
HKR, , EnumPropPages, 0, netdi.dll, EnumPropPages

; NDIS Info
HKR,NDIS,MajorNdisVersion,1,03
HKR,NDIS,MinorNdisVersion,1,0a
HKR,NDIS,LogDriverName,,RTLWUSB

; Interfaces
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
;
;*******************************************************************************
; RTL8187 common paramters
;*******************************************************************************
[RTL8187.common.reg]
HKR,Ndi\params\SSID,   	      ParamDesc,  0, %SSID_STR%
HKR,Ndi\params\SSID,   	      type,       0, "edit"
HKR,Ndi\params\SSID,   	      default,    0, "ANY"
HKR,Ndi\params\SSID,   	      LimitText,  0, "32"
HKR,defaults,SSID,0,"ANY"
HKR,,SSID,0,"ANY"

HKR,Ndi\params\Channel,       ParamDesc,  0, %CHANNEL_STR%
HKR,Ndi\params\Channel,       type,       0, "int"
HKR,Ndi\params\Channel,       default,    0, "1"
HKR,Ndi\params\Channel,       Min,        0, "1"
HKR,Ndi\params\Channel,       Max,        0, "14"
HKR,Ndi\params\Channel,       Step,       0, "1"
HKR,Ndi\params\Channel,       Base,       0, "10"
HKR,defaults,Channel,0,"1"
HKR,,Channel,0,"1"

HKR,Ndi\params\NetworkType,        ParamDesc,  0, %NETWORK_TYPE_STR%
HKR,Ndi\params\NetworkType,        type,       0, "enum"
HKR,Ndi\params\NetworkType,        default,    0, "1"
HKR,Ndi\params\NetworkType\enum,   "0",        0, "Ad Hoc"
HKR,Ndi\params\NetworkType\enum,   "1",        0, "Infrastructure"
HKR,Ndi\params\NetworkType\enum,   "2",        0, "Auto select"
HKR,defaults,NetworkType,0,"1"
HKR,,NetworkType,0,"1"

HKR,Ndi\params\LedCtrl,        ParamDesc,  0, %LED_CONTROL_STR%
HKR,Ndi\params\LedCtrl,        type,       0, "enum"
HKR,Ndi\params\LedCtrl,        default,    0, "1"
HKR,Ndi\params\LedCtrl\enum,   "0",        0, "Disable"
HKR,Ndi\params\LedCtrl\enum,   "1",        0, "Enable"
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,NDI\params\PowerSaveMode,      ParamDesc,  0, %POWER_SAVE_STR%
HKR,NDI\params\PowerSaveMode,      type,       0, "enum"
HKR,Ndi\params\PowerSaveMode,      default,    0, "0"
HKR,NDI\params\PowerSaveMode\enum, "0",        0, "CAM"
HKR,NDI\params\PowerSaveMode\enum, "1",        0, "MAX_PSP"
HKR,NDI\params\PowerSaveMode\enum, "2",        0, "Fast_PSP"
HKR,defaults,PowerSaveMode,0,"0"
HKR,,PowerSaveMode,0,"0"

HKR,Ndi\params\WiFi11bIbss,        ParamDesc,  0, %WIFI_IBSS_STR%
HKR,Ndi\params\WiFi11bIbss,        type,       0, "enum"
HKR,Ndi\params\WiFi11bIbss,        default,    0, "0"
HKR,Ndi\params\WiFi11bIbss\enum,   "0",        0, "Disable"
HKR,Ndi\params\WiFi11bIbss\enum,   "1",        0, "Enable"
HKR,defaults,WiFi11bIbss,0,"0"
HKR,,WiFi11bIbss,0,"0"

HKR,Ndi\params\bRateAdaptive,        ParamDesc,  0, %RATE_ADAPTIVE_STR%
HKR,Ndi\params\bRateAdaptive,        type,       0, "enum"
HKR,Ndi\params\bRateAdaptive,        default,    0, "1"
HKR,Ndi\params\bRateAdaptive\enum,   "0",        0, "Disable"
HKR,Ndi\params\bRateAdaptive\enum,   "1",        0, "Enable"
HKR,defaults,bRateAdaptive,0,"1"
HKR,,bRateAdaptive,0,"1"

HKR,Ndi\params\MaxPktSize, ParamDesc, 0, %MAX_PKTSIZE_STR%
HKR,Ndi\params\MaxPktSize, type, 0, "int"
HKR,Ndi\params\MaxPktSize, default, 0, "1514"
HKR,Ndi\params\MaxPktSize, min, 0, "256"
HKR,Ndi\params\MaxPktSize, max, 0, "2304"
HKR,Ndi\params\MaxPktSize, step, 0, "1"
HKR,defaults,MaxPktSize, 0, "1514"
HKR,,MaxPktSize, 0, "1514"

HKR,Ndi\params\ChannelPlan, ParamDesc, 0, %CHANNEL_PLAN_STR%
HKR,Ndi\params\ChannelPlan, type, 0, "enum"
HKR,Ndi\params\ChannelPlan, default, 0, "15"
HKR,Ndi\params\ChannelPlan\enum, "0", 0, "FCC"
HKR,Ndi\params\ChannelPlan\enum, "1", 0, "IC"
HKR,Ndi\params\ChannelPlan\enum, "2", 0, "ETSI"
HKR,Ndi\params\ChannelPlan\enum, "3", 0, "Spain"
HKR,Ndi\params\ChannelPlan\enum, "4", 0, "France"
HKR,Ndi\params\ChannelPlan\enum, "5", 0, "MKK"
HKR,Ndi\params\ChannelPlan\enum, "6", 0, "MKK1"
HKR,Ndi\params\ChannelPlan\enum, "7", 0, "Israel"
HKR,Ndi\params\ChannelPlan\enum, "8", 0, "TELEC"
HKR,Ndi\params\ChannelPlan\enum, "15", 0, "DOMAIN_FROM_EEPROM"
HKR,defaults,ChannelPlan, 0, "15"
HKR,,ChannelPlan, 0, "15"

HKR,Ndi\params\ShortRetryLimit, ParamDesc, 0, %SHORT_RETRY_LIMIT%
HKR,Ndi\params\ShortRetryLimit, default, 0, "7"
HKR,Ndi\params\ShortRetryLimit, type, 0, "int"
HKR,Ndi\params\ShortRetryLimit, min, 0, "0"
HKR,Ndi\params\ShortRetryLimit, max, 0, "255"
HKR,Ndi\params\ShortRetryLimit, step, 0, "1"
HKR,defaults,ShortRetryLimit, 0, "7"
HKR,,ShortRetryLimit, 0, "7"

HKR,Ndi\params\LongRetryLimit, ParamDesc, 0, %LONG_RETRY_LIMIT%
HKR,Ndi\params\LongRetryLimit, default, 0, "7"
HKR,Ndi\params\LongRetryLimit, type, 0, "int"
HKR,Ndi\params\LongRetryLimit, min, 0, "0"
HKR,Ndi\params\LongRetryLimit, max, 0, "255"
HKR,Ndi\params\LongRetryLimit, step, 0, "1"
HKR,defaults,LongRetryLimit, 0, "7"
HKR,,LongRetryLimit, 0, "7"

HKR,Ndi\params\FragThresh, ParamDesc, 0, %FRAGTHRESH_STR%
HKR,Ndi\params\FragThresh, default, 0, "2346"
HKR,Ndi\params\FragThresh, type, 0, "int"
HKR,Ndi\params\FragThresh, min, 0, "256"
HKR,Ndi\params\FragThresh, max, 0, "2346"
HKR,Ndi\params\FragThresh, step, 0, "1"
HKR,defaults,FragThresh, 0, "2346"
HKR,,FragThresh, 0, "2346"

HKR,Ndi\params\RTSThresh, ParamDesc, 0, %RTSTHRESH_STR%
HKR,Ndi\params\RTSThresh, default, 0, "2347"
HKR,Ndi\params\RTSThresh, type, 0, "int"
HKR,Ndi\params\RTSThresh, min, 0, "0"
HKR,Ndi\params\RTSThresh, max, 0, "2347"
HKR,Ndi\params\RTSThresh, step, 0, "1"
HKR,defaults,RTSThresh, 0, "2347"
HKR,,RTSThresh, 0, "2347"

HKR,Ndi\params\PSPXlinkMode,        ParamDesc,  0, %PSP_XLINK_STR%
HKR,Ndi\params\PSPXlinkMode,        type,       0, "enum"
HKR,Ndi\params\PSPXlinkMode,        default,    0, "0"
HKR,Ndi\params\PSPXlinkMode\enum,   "0",        0, "Disable"
HKR,Ndi\params\PSPXlinkMode\enum,   "1",        0, "Enable"
HKR,defaults,PSPXlinkMode,0,"0"
HKR,,PSPXlinkMode,0,"0"

HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""

; by Owen on 04/12/04
[RTL8187.CopyFiles98]
RTL8187.sys,,,2
;
;*******************************************************************************
; Windows XP
;*******************************************************************************
[RTL8187.NT.Reg]
HKR, Ndi\Interfaces,	UpperRange, 0, "ndis5,mdcwifi"
HKR, Ndi\Interfaces,    LowerRange, 0, "ethernet"
HKR, Ndi,            	Service,    0, "RTLWUSB"

[rtsnt.Service]
DisplayName    = %RTL8187.DeviceDesc.DispName%
ServiceType    = 1		; %SERVICE_KERNEL_DRIVER%
StartType      = 3		; %SERRVICE_DEMAND_START%
ErrorControl   = 1		; %SERRVICE_ERROR_NORMAL%
ServiceBinary  = %12%\RTL8187.sys
LoadOrderGroup = NDIS

[RTL8187.EventLog]
AddReg = RTL8187.AddEventLog.reg

[RTL8187.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported  , 0x00010001, 7

[RTL8187.CopyFiles]
RTL8187.sys,,,2

;*******************************************************************************
; Destination Directory
;*******************************************************************************
[DestinationDirs]
; by Owen on 04/12/04
RTL8187.CopyFiles98	= 11
;
RTL8187.CopyFiles	= 12

[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
RTL8187.sys = 1

;*******************************************************************************
; Strings
;*******************************************************************************
[Strings]
Realtek 			= "Realtek Semiconductor Corp."
SSID_STR			= "SSID"
CHANNEL_STR			= "Channel"
NETWORK_TYPE_STR	= "Network Type"
LED_CONTROL_STR		= "LED Control"
POWER_SAVE_STR		= "Power Save Mode"
WIFI_IBSS_STR		= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR	= "Rate Adaptive"
MAX_PKTSIZE_STR		= "Maximum Packet Size"
CHANNEL_PLAN_STR	= "Channel Plan"
SHORT_RETRY_LIMIT	= "Short Retry Limit"
LONG_RETRY_LIMIT	= "Long Retry Limit"
FRAGTHRESH_STR		= "Fragmentation Threshold"
RTSTHRESH_STR		= "RTS Threshold"
PSP_XLINK_STR		= "PSP XLink Mode"

;; Source disk name
DISKNAME					= "Realtek RTL8187 Wireless 802.11g 54Mbps USB 2.0 Network Adapter Driver Disk"
RTL8187.DeviceDesc			= "Realtek RTL8187 Wireless 802.11g 54Mbps USB 2.0 Network Adapter"
RTL8187.DeviceDesc.DispName	= "Realtek RTL8187 Wireless 802.11g 54Mbps USB 2.0 Network Adapter"
RTL8187.DeviceDesc.Surecom	= "SURECOM EP-9001-g 802.11g 54M WLAN USB Adapter"
RTL8187.DeviceDesc.Sitecom	= "SITECOM WL-168 Wireless Network USB Adapter 54g"
