;===========================================================================
; 
; Windows XP (32bit), 2000 NDIS driver INF for TOPDOG 802.11n/g/b Wireless
; Copyright (C) 2006 Marvell Semiconductor, Inc.
;
;=========================================================================== 
 
 
[Version] 
Signature = "$Windows NT$" 
Compatible  = 1
Class=Net
ClassGUID={4D36E972-E325-11CE-BFC1-08002BE10318} 
Provider=%MRVL% 
CatalogFile=MRVW245.cat
DriverVer=11/27/2006,1.0.4.9

;===========================================================================
; Source Media Information Sections
;===========================================================================
[SourceDisksNames]
1 = %DriverDisk%,,,

[SourceDisksFiles]
; On Marvell installation disk 1 
MRVW245.sys = 1
MRVW243.sys = 1

[DestinationDirs]
W8360USB.XP.CopyFiles  = 12 
W8360USB.2K.CopyFiles  = 12 
DefaultDestDir = 11

[Manufacturer] 
%MRVL%=Marvell,NT.5.1

[Marvell]
%MRVL8360USB.DeviceDesc% = W8360USB.ndi.NT,USB\VID_1286&PID_2006
%BelkinN1USB.DeviceDesc% = W8360USB.ndi.NT,USB\VID_1799&PID_8051
%LinksysNUSB.DeviceDesc% = W8360USB.ndi.NT,USB\VID_13B1&PID_0029
%WN121TUSB.DeviceDesc%   = W8360USB.ndi.NT,USB\VID_0846&PID_7100
%N130USB.DeviceDesc%     = W8360USB.ndi.NT,USB\VID_07D1&PID_3B11
%N650USB.DeviceDesc%     = W8360USB.ndi.NT,USB\VID_07D1&PID_3B10
%AsusUSB1.DeviceDesc%    = W8360USB.ndi.NT,USB\VID_0B05&PID_172A
%AsusUSB2.DeviceDesc%    = W8360USB.ndi.NT,USB\VID_0B05&PID_172B
%BuffaloUSB.DeviceDesc%  = W8360USB.ndi.NT,USB\VID_0411&PID_00CA

[Marvell.NT.5.1]
%MRVL8360USB.DeviceDesc% = W8360USBXP.ndi,USB\VID_1286&PID_2006
%BelkinN1USB.DeviceDesc% = W8360USBXP.ndi,USB\VID_1799&PID_8051
%LinksysNUSB.DeviceDesc% = W8360USBXP.ndi,USB\VID_13B1&PID_0029
%WN121TUSB.DeviceDesc%   = W8360USBXP.ndi,USB\VID_0846&PID_7100
%N130USB.DeviceDesc%     = W8360USBXP.ndi,USB\VID_07D1&PID_3B11
%N650USB.DeviceDesc%     = W8360USBXP.ndi,USB\VID_07D1&PID_3B10
%AsusUSB1.DeviceDesc%    = W8360USBXP.ndi,USB\VID_0B05&PID_172A
%AsusUSB2.DeviceDesc%    = W8360USBXP.ndi,USB\VID_0B05&PID_172B
%BuffaloUSB.DeviceDesc%  = W8360USBXP.ndi,USB\VID_0411&PID_00CA


;===========================================================================
; ControlFlags section
;===========================================================================
[ControlFlags]
ExcludeFromSelect = *


;***************************************************************************
;**         
;**          Win XP DDInstall section
;**          
;***************************************************************************
;***************************************************************************
[W8360USBXP.ndi]
; "Characteristics" is (NCF_PHYSICAL | NCF_HAS_UI)
Characteristics = 0x84 
; "BusType" is USB
BusType         = 15 ;Is USB
AddReg          = W8360USBWXP.reg, W8360USB.reg, W8360USBXP.reg
CopyFiles       = W8360USB.XP.CopyFiles

[W8360USBXP.ndi.Services]
AddService = MRVW245, 2, W8360USBXP.Service, CommonXP.EventLog

;===========================================================================
; W8360 USB WinXP registers
;===========================================================================
[W8360USBXP.reg]
HKR, Ndi,            Service,    0, "MRVW245"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"


[W8360USB.XP.CopyFiles]
MRVW245.sys,,,2 

[W8360USBXP.Service]
DisplayName    = %W8360USBXP.Service.DispName%
ServiceType    = 1 ;%SERVICE_KERNEL_DRIVER%
StartType      = 3 ;%SERVICE_DEMAND_START%
ErrorControl   = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\MRVW245.sys
LoadOrderGroup = NDIS

[CommonXP.EventLog]
AddReg = CommonXP.AddEventLog.reg

[CommonXP.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


;***************************************************************************
;***************************************************************************
;**         
;**          Win 2K DDInstall section
;**          
;***************************************************************************
;***************************************************************************

[W8360USB.ndi.NT]
; "Characteristics" is (NCF_PHYSICAL | NCF_HAS_UI)
Characteristics = 0x84 
; "BusType" is USB
BusType         = 15; Is USB.
AddReg          = W8360USBW2K.reg, W8360USB.reg, W8360USB2K.reg, W8360USB2K.devID.reg
CopyFiles       = W8360USB.2K.CopyFiles 

[W8360USB.ndi.NT.Services]
AddService = MRVW243, 2, W8360USB2K.Service, Common.EventLog

;===========================================================================
; W8360 USB Win2K registers
;===========================================================================
[W8360USB2K.reg]
HKR, Ndi,            Service,    0, "MRVW243"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

[W8360USB2K.devID.reg]
;HKR, Ndi, DeviceID, 0, "USB\VID_1286&PID_2006"
HKR, Ndi, DeviceID, 0, "USB\VID_07D1&PID_3B11"

[W8360USB.2K.CopyFiles]
MRVW243.sys,,,2 

[W8360USB2K.Service]
DisplayName    = %W8360USB2K.Service.DispName%
ServiceType    = 1 ;%SERVICE_KERNEL_DRIVER%
StartType      = 3 ;%SERVICE_DEMAND_START%
ErrorControl   = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\MRVW243.sys
LoadOrderGroup = NDIS

[Common.EventLog]
AddReg = Common.AddEventLog.reg

[Common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


;===========================================================================
; W8360 USB Common registers
;===========================================================================
[W8360USB.reg]
HKR,, OpMode, 			0x00002, 0	;//STA Mode

;
; LED Control
;
; Mode 1 (Default)
HKR,, LED0PowerOn,		0x00002, "0100ff00"
HKR,, LED1PowerOn,		0x00002, "0101fe00"
HKR,, LED0PowerOff,		0x00002, "0100fe00"
HKR,, LED1PowerOff,		0x00002, "0101fe00"
HKR,, LED0Scan,			0x00002, "0100ff00"
HKR,, LED1Scan,			0x00002, "01010200"
HKR,, LED0Associated,		0x00002, "0100ff00"
HKR,, LED1Associated,		0x00002, "0101fe00"
HKR,, LED0Joined,		0x00002, "0100ff00"
HKR,, LED1Joined,		0x00002, "0101fe00"
HKR,, LED0Started,		0x00002, "0100ff00"
HKR,, LED1Started,		0x00002, "0101fe00"
HKR,, LED0Tx,			0x00002, "0100ff00"
HKR,, LED1Tx,			0x00002, "01010200"
HKR,, LED0Rx,			0x00002, "0100ff00"
HKR,, LED1Rx,			0x00002, "01010200"
;HKR,, LED0TxMiddle,		0x00002, "0100ff00"
;HKR,, LED1TxMiddle,		0x00002, "01010200"
;HKR,, LED0RxMiddle,		0x00002, "0100ff00"
;HKR,, LED1RxMiddle,		0x00002, "01010200"
HKR,, LED0TxHigh,		0x00002, "0100ff00"
HKR,, LED1TxHigh,		0x00002, "01010200"
HKR,, LED0RxHigh,		0x00002, "0100ff00"
HKR,, LED1RxHigh,		0x00002, "01010200"

HKR,, LEDOffAfterRadioOff,	0x00002, "1" 

HKR, Ndi\params\AdhocMode,ParamDesc,,"%AdhocMode%"
HKR, Ndi\params\AdhocMode,default,,"1"
HKR, Ndi\params\AdhocMode,type,,enum
HKR, Ndi\params\AdhocMode\enum,"0",,"%AdhocMode_GMode%"
HKR, Ndi\params\AdhocMode\enum,"1",,"%AdhocMode_BMode%" 
HKR, Ndi\params\AdhocMode\enum,"4",,"%AdhocMode_NMode%" 

HKR, Ndi\xparams\DesiredSSID,ParamDesc,,"%SSID%"
HKR, Ndi\xparams\DesiredSSID,default,,""
HKR, Ndi\xparams\DesiredSSID,type,,"edit" 
HKR, Ndi\xparams\DesiredSSID,LimitText,,"32"
HKR, Ndi\xparams\DesiredSSID,UpperCase,,"0" 
HKR, Ndi\xparams\DesiredSSID,Optional,,"1" 

HKR, Ndi\xparams\AuthMode,ParamDesc,,"%AuthMode%"
HKR, Ndi\xparams\AuthMode,default,,"0"
HKR, Ndi\xparams\AuthMode,type,,enum
HKR, Ndi\xparams\AuthMode\enum,"0",,"%AuthMode_Open%"
HKR, Ndi\xparams\AuthMode\enum,"1",,"%AuthMode_Shared%"

HKR, Ndi\xparams\NetworkMode,ParamDesc,,"%NetworkMode%"
HKR, Ndi\xparams\NetworkMode,default,,"1"
HKR, Ndi\xparams\NetworkMode,type,,enum
HKR, Ndi\xparams\NetworkMode\enum,"0",,"%NetworkMode_AdHoc%"
HKR, Ndi\xparams\NetworkMode\enum,"1",,"%NetworkMode_Infra%"

HKR, Ndi\params\FragThsd,  ParamDesc,0 , "%FragThsds%"
HKR, Ndi\params\FragThsd,  default, 0 , "2346"
HKR, Ndi\params\FragThsd,  min, 0 , "256"
HKR, Ndi\params\FragThsd,  max, 0 , "2346"
HKR, Ndi\params\FragThsd,  step, 0 , "1"
HKR, Ndi\params\FragThsd,  Base, 0 , "10"
HKR, Ndi\params\FragThsd,  type, 0 ,"dword"

HKR, Ndi\xparams\Channel,  ParamDesc,0 , "%Channel%"
HKR, Ndi\xparams\Channel,  default, 0 , "36"
HKR, Ndi\xparams\Channel,  min, 0 , "1"
HKR, Ndi\xparams\Channel,  max, 0 , "165"
HKR, Ndi\xparams\Channel,  step, 0 , "1"
HKR, Ndi\xparams\Channel,  Base, 0 , "10"
HKR, Ndi\xparams\Channel,  type, 0 ,"dword"

HKR, Ndi\xparams\TxAntenna,  ParamDesc,0 , "%TxAntennaStr%"
HKR, Ndi\xparams\TxAntenna,  default, 0 , "2"
HKR, Ndi\xparams\TxAntenna,  min, 0 , "1"
HKR, Ndi\xparams\TxAntenna,  max, 0 , "ffff"
HKR, Ndi\xparams\TxAntenna,  step, 0 , "1"
HKR, Ndi\xparams\TxAntenna,  Base, 0 , "16"
HKR, Ndi\xparams\TxAntenna,  type, 0 ,"dword"

HKR, Ndi\xparams\RxAntenna,  ParamDesc,0 , "%RxAntennaStr%"
HKR, Ndi\xparams\RxAntenna,  default, 0 , "ffff"
HKR, Ndi\xparams\RxAntenna,  min, 0 , "1"
HKR, Ndi\xparams\RxAntenna,  max, 0 , "ffff"
HKR, Ndi\xparams\RxAntenna,  step, 0 , "1"
HKR, Ndi\xparams\RxAntenna,  Base, 0 , "16"
HKR, Ndi\xparams\RxAntenna,  type, 0 ,"dword"

HKR, Ndi\params\RTSThsd,  ParamDesc, 0, "%RTSThsds%"
HKR, Ndi\params\RTSThsd,  default, 0, "2346"
HKR, Ndi\params\RTSThsd,  min, 0, "0"
HKR, Ndi\params\RTSThsd,  max, 0, "2346"
HKR, Ndi\params\RTSThsd,  step, 0, "1"
HKR, Ndi\params\RTSThsd,  Base, 0, "10"
HKR, Ndi\params\RTSThsd,  type, 0, "dword"

HKR, Ndi\params\PowerMode,ParamDesc,,"%PowerMode%"
HKR, Ndi\params\PowerMode,default,,"0"
HKR, Ndi\params\PowerMode,type,,enum
HKR, Ndi\params\PowerMode\enum,"0",,"%PowerMode_CAM%"
HKR, Ndi\params\PowerMode\enum,"1",,"%PowerMode_Max%"

HKR, Ndi\xparams\DataRate,ParamDesc,,"%DataRate%"
HKR, Ndi\xparams\DataRate,default,,"FF"
HKR, Ndi\xparams\DataRate,type,,enum
HKR, Ndi\xparams\DataRate\enum,"FF",,"%DataRate_Auto%"
HKR, Ndi\xparams\DataRate\enum,"2",,"%DataRate_1Mbps%"
HKR, Ndi\xparams\DataRate\enum,"4",,"%DataRate_2Mbps%"
HKR, Ndi\xparams\DataRate\enum,"b",,"%DataRate_5_5Mbps%"
HKR, Ndi\xparams\DataRate\enum,"16",,"%DataRate_11Mbps%"
HKR, Ndi\xparams\DataRate\enum,"C",,"%DataRate_6Mbps%" 
HKR, Ndi\xparams\DataRate\enum,"12",,"%DataRate_9Mbps%" 
HKR, Ndi\xparams\DataRate\enum,"18",,"%DataRate_12Mbps%" 
HKR, Ndi\xparams\DataRate\enum,"24",,"%DataRate_18Mbps%" 
HKR, Ndi\xparams\DataRate\enum,"30",,"%DataRate_24Mbps%" 
HKR, Ndi\xparams\DataRate\enum,"48",,"%DataRate_36Mbps%" 
HKR, Ndi\xparams\DataRate\enum,"60",,"%DataRate_48Mbps%" 
HKR, Ndi\xparams\DataRate\enum,"6C",,"%DataRate_54Mbps%"

HKR, Ndi\xparams\WepStatus,ParamDesc,,"%WepStatus%"
HKR, Ndi\xparams\WepStatus,default,,"1"
HKR, Ndi\xparams\WepStatus,type,,enum
HKR, Ndi\xparams\WepStatus\enum,"0",,"%Enabled%"
HKR, Ndi\xparams\WepStatus\enum,"1",,"%Disabled%"

HKR, Ndi\params\Preamble,ParamDesc,,"%PreambleStr%"
HKR, Ndi\params\Preamble,default,,"3"
HKR, Ndi\params\Preamble,type,,enum 
HKR, Ndi\params\Preamble\enum,"1",,"%PreambleStr_Auto%"
HKR, Ndi\params\Preamble\enum,"2",,"%PreambleStr_Short%" 
HKR, Ndi\params\Preamble\enum,"3",,"%PreambleStr_Long%"

;HKR, Ndi\params\DefaultAdhocMediaMode,ParamDesc,,"%DefaultAdhocMediaModeStr%"
;HKR, Ndi\params\DefaultAdhocMediaMode,default,,"0"
;HKR, Ndi\params\DefaultAdhocMediaMode,type,,enum 
;HKR, Ndi\params\DefaultAdhocMediaMode\enum,"0",,"%DefaultAdhocMediaModeStr_11b%"
;HKR, Ndi\params\DefaultAdhocMediaMode\enum,"1",,"%DefaultAdhocMediaModeStr_11g%" 
;HKR, Ndi\params\DefaultAdhocMediaMode\enum,"2",,"%DefaultAdhocMediaModeStr_11a%"
;HKR,, DefaultAdhocMediaMode, 2, "2" 


HKR,, TxWepKey, 2, "" 
HKR,, WepKey1, 2, "" 
HKR,, WepKey2, 2, "" 
HKR,, WepKey3, 2, "" 
HKR,, WepKey4, 2, "" 

HKR,, RadioOn,2, "1"

HKR,, DriverRel, 2, "11/27/2006"

HKR,, AMSDUCompatible,2, "1"
HKR,, AMPDUCompatible,2, "1"
HKR,, SSIDScanOnce,2, "0"

HKR, Ndi\params\BlockAckMode,ParamDesc,,"%AMPDUSettings%"
HKR, Ndi\params\BlockAckMode,default,,"2"
HKR, Ndi\params\BlockAckMode,type,,enum 
HKR, Ndi\params\BlockAckMode\enum,"2",,"%Partial%" 
HKR, Ndi\params\BlockAckMode\enum,"3",,"%Full%"

;HKR, Ndi\params\AmpduFactor,ParamDesc,,"%AmpduFactor%"
;HKR, Ndi\params\AmpduFactor,default,,"0"
;HKR, Ndi\params\AmpduFactor,type,,enum 
;HKR, Ndi\params\AmpduFactor\enum,"0",,"%8k%"
;HKR, Ndi\params\AmpduFactor\enum,"1",,"%16k%" 
;HKR, Ndi\params\AmpduFactor\enum,"2",,"%32k%"
;HKR, Ndi\params\AmpduFactor\enum,"3",,"%64k%"

HKR, Ndi\params\EncryptionType,ParamDesc,,"%EncryptionType%"
HKR, Ndi\params\EncryptionType,default,,"0"
HKR, Ndi\params\EncryptionType,type,,enum 
HKR, Ndi\params\EncryptionType\enum,"0",,"%HwEncryption%" 
HKR, Ndi\params\EncryptionType\enum,"1",,"%SwEncryption%"

HKR, Ndi\params\EWCTurboMode,ParamDesc,,"%EWCTurboMode%"
HKR, Ndi\params\EWCTurboMode,default,,"1"
HKR, Ndi\params\EWCTurboMode,type,,enum 
HKR, Ndi\params\EWCTurboMode\enum,"0",,"%Disabled%"
HKR, Ndi\params\EWCTurboMode\enum,"1",,"%Enabled%" 

HKR, Ndi\params\HTModeEnabled
HKR, Ndi\params\HTModeEnabled, ParamDesc,,"%HTModeEnabled%"
HKR, Ndi\params\HTModeEnabled, default,,"1"
HKR, Ndi\params\HTModeEnabled, type,,enum
HKR, Ndi\params\HTModeEnabled\enum,"0",,"%Disabled%" 
HKR, Ndi\params\HTModeEnabled\enum,"1",,"%Enabled%"

HKR, Ndi\params\ChannelWidth, ParamDesc,,"%ChannelWidth%"
HKR, Ndi\params\ChannelWidth, default,,"-1"
HKR, Ndi\params\ChannelWidth, type,,enum
HKR, Ndi\params\ChannelWidth\enum,"0",,"%20MHz%" 
HKR, Ndi\params\ChannelWidth\enum,"1",,"%40MHz%"
HKR, Ndi\params\ChannelWidth\enum,"-1",,"%Auto%"

HKR, Ndi\params\ExtChannelOffset, ParamDesc,,"%ExtChannelOffset%"
HKR, Ndi\params\ExtChannelOffset, default,,"-1"
HKR, Ndi\params\ExtChannelOffset, type,,enum
HKR, Ndi\params\ExtChannelOffset\enum,"0",,"%Below%" 
HKR, Ndi\params\ExtChannelOffset\enum,"1",,"%Above%"
HKR, Ndi\params\ExtChannelOffset\enum,"2",,"%None%"
HKR, Ndi\params\ExtChannelOffset\enum,"-1",,"%Auto%"

HKR, Ndi\params\GuardInterval, ParamDesc,,"%GuardInterval%"
HKR, Ndi\params\GuardInterval, default,,"-1"
HKR, Ndi\params\GuardInterval, type,,enum
HKR, Ndi\params\GuardInterval\enum,"0",,"%LongGI%" 
HKR, Ndi\params\GuardInterval\enum,"1",,"%ShortGI%"
HKR, Ndi\params\GuardInterval\enum,"-1",,"%Auto%"

HKR, Ndi\params\RegistryMimoCfg, ParamDesc,,"%Antenna%"
HKR, Ndi\params\RegistryMimoCfg, default,,"-1"
HKR, Ndi\params\RegistryMimoCfg, type,,enum
HKR, Ndi\params\RegistryMimoCfg\enum,"0",,"%2by3%" 
HKR, Ndi\params\RegistryMimoCfg\enum,"1",,"%Antenna_A%"
HKR, Ndi\params\RegistryMimoCfg\enum,"2",,"%Antenna_B%"
HKR, Ndi\params\RegistryMimoCfg\enum,"3",,"%2by2%"
HKR, Ndi\params\RegistryMimoCfg\enum,"4",,"%Aby2%"
HKR, Ndi\params\RegistryMimoCfg\enum,"5",,"%Bby2%"
HKR, Ndi\params\RegistryMimoCfg\enum,"-1",,"%Auto%"

HKR, Ndi\params\RateAdaptMode, ParamDesc,,"%RateAdaptMode%"
HKR, Ndi\params\RateAdaptMode, default,,"0"
HKR, Ndi\params\RateAdaptMode, type,,enum
HKR, Ndi\params\RateAdaptMode\enum,"0",,"%In%" 
HKR, Ndi\params\RateAdaptMode\enum,"1",,"%Out%"

HKR, Ndi\params\CSMode, ParamDesc,,"%LinkAdaptCSMode%"
HKR, Ndi\params\CSMode, default,,"0"
HKR, Ndi\params\CSMode, type,,enum
HKR, Ndi\params\CSMode\enum,"0",,"%Conservative%" 
HKR, Ndi\params\CSMode\enum,"1",,"%Aggressive%"
HKR, Ndi\params\CSMode\enum,"2",,"%Auto%"


;===========================================================================
; W8360 USB Win2k registers
;===========================================================================
[W8360USBW2K.reg]
HKR, Ndi\params\AMSDUEnabled,ParamDesc,,"%AMSDUEnabled%"
HKR, Ndi\params\AMSDUEnabled,default,,"1"
HKR, Ndi\params\AMSDUEnabled,type,,enum 
HKR, Ndi\params\AMSDUEnabled\enum,"0",,"%Disabled%"
HKR, Ndi\params\AMSDUEnabled\enum,"1",,"%AMSDUEnabled_3839Bytes%" 

HKLM,System\CurrentControlSet\Services\Tcpip\Parameters,TcpWindowSize,0x00010001,00065535

;===========================================================================
; W8360 USB WinXP 32 bit registers
;===========================================================================
[W8360USBWXP.reg]
HKR, Ndi\params\AMSDUEnabled,ParamDesc,,"%AMSDUEnabled%"
HKR, Ndi\params\AMSDUEnabled,default,,"2"
HKR, Ndi\params\AMSDUEnabled,type,,enum 
HKR, Ndi\params\AMSDUEnabled\enum,"0",,"%Disabled%"
HKR, Ndi\params\AMSDUEnabled\enum,"1",,"%AMSDUEnabled_3839Bytes%" 
HKR, Ndi\params\AMSDUEnabled\enum,"2",,"%AMSDUEnabled_Max%" 

HKLM,System\CurrentControlSet\Services\Tcpip\Parameters,Tcp1323Opts,0x00010001,00000001
HKLM,System\CurrentControlSet\Services\Tcpip\Parameters,TcpWindowSize,0x00010001,00262144


;===========================================================================
; English Strings section
;===========================================================================
[Strings]
MRVL = "Marvell"
Enabled = "Enabled"
Disabled = "Disabled"
Off = "Off"
On = "On"
TxAntennaStr = "Tx Antenna Select"
RxAntennaStr = "Rx Antenna Select" 
Channel = "Channel"
FragThsds = "Fragmentation Threshold"
DataRate = "Data Rate"
DataRate_Auto = "Auto"
DataRate_1Mbps = "1 Mbps"
DataRate_2Mbps = "2 Mbps"
DataRate_5_5Mbps = "5.5 Mbps"
DataRate_11Mbps = "11 Mbps"
DataRate_6Mbps = "6 Mbps"
DataRate_9Mbps = "9 Mbps"
DataRate_12Mbps = "12 Mbps"
DataRate_18Mbps = "18 Mbps"
DataRate_24Mbps = "24 Mbps"
DataRate_36Mbps = "36 Mbps"
DataRate_48Mbps = "48 Mbps"
DataRate_54Mbps = "54 Mbps"
RTSThsds = "RTS Threshold"
AuthMode = "Authentication Mode"
AuthMode_Open = "Open"
AuthMode_Shared = "Shared"
;WirelessM = "Wireless Mode"
NetworkMode = "Operation Mode"
NetworkMode_AdHoc = "Ad-Hoc"
NetworkMode_Infra = "Infrastructure"
WepStatus = "WEP Status"
SSID = "SSID"
PreambleStr = "Preamble Select"
PreambleStr_Auto = "Auto"
PreambleStr_Short = "Short Preamble"
PreambleStr_Long = "Long Preamble"
PowerMode = "Power Save Mode"
PowerMode_CAM = "CAM-Constantly Awake Mode"
PowerMode_Max = "MaxPSP-Max Power Savings"
PowerMode_Fast = "FastPSP-Fast Power Savings"
AdhocMode = "Ad-Hoc Mode"
AdhocMode_GMode = "Ad-Hoc G Mode"
AdhocMode_BMode = "Ad-Hoc B Mode only"
AdhocMode_NMode = "Ad-Hoc N Mode"
DefaultAdhocMediaModeStr = "Default Ad-Hoc Media Mode"
DefaultAdhocMediaModeStr_11b = "11b"
DefaultAdhocMediaModeStr_11g = "11g"
DefaultAdhocMediaModeStr_11a = "11a"
AMSDUEnabled = "MSDU Aggregation"
AMSDUEnabled_3839Bytes = "Enabled (3839 Bytes)" 
AMSDUEnabled_Max = "Enabled (Device Max)" 
EWCTurboMode = "802.11n Turbo Mode"
AMPDUSettings= "Packet Aggregation (A-MPDU)"
HTModeEnabled = "802.11n Network"
ChannelWidth = "Channel Width"
20MHz  = "20 MHz"
40MHz = "40 MHz"
Auto = "Auto"
ExtChannelOffset = "Extension Channel"
Below = "Lower"
Above = "Upper"
None = "None"
GuardInterval = "Guard Interval"
LongGI = "Standard"
ShortGI = "Short"
Antenna = "Antenna"
2by3 = "2by3"
Antenna_A = "Antenna A"
Antenna_B = "Antenna B"
2by2 = "2by2"
Aby2 = "A by 2"
Bby2 = "B by 2"
RateAdaptMode= "Rate adapt mode"
In = "Indoor"
Out = "Outdoor"
LinkAdaptCSMode = "Link Adapt CS Mode"
Conservative = "Conservative"
Aggressive = "Aggressive"
Full = "Full"
Partial = "Partial"
;AmpduFactor= "MaxRx AMPDU Factor"
;8k = "8k"
;16k = "16k"
;32k = "32k"
;64k = "64k"
EncryptionType= "Encryption Type"
SwEncryption = "Sw Encryption"
HwEncryption = "Hw Encryption"

DriverDisk = "Marvell installation disk 1"

MRVL8360USB.DeviceDesc      = "Marvell TOPDOG 802.11n WLAN Client Adaptors - USB"
BelkinN1USB.DeviceDesc      = "N1 Wireless USB Network Adapter"
LinksysNUSB.DeviceDesc      = "Wireless-N USB Network Adapter"
WN121TUSB.DeviceDesc        = "NETGEAR WN121T Wireless USB 2.0 Adapter"
N130USB.DeviceDesc          = "D-Link Wireless N USB Adapter DWA-130"
N650USB.DeviceDesc          = "D-Link RangeBooster N USB Adapter"
AsusUSB1.DeviceDesc         = "ASUS 802.11n Network Adapter"
AsusUSB2.DeviceDesc         = "802.11n Network Adapter"
BuffaloUSB.DeviceDesc       = "802.11n Network Adapter"

W8360USBXP.Service.DispName = "D-Link Wireless N USB Adapter DWA-130 Driver for Windows XP"
W8360USB2K.Service.DispName = "D-Link Wireless N USB Adapter DWA-130 Driver for Windows 2K"
