;/*++
;
;Copyright (c) 2005 SMC Networks, Inc. All Rights Reserved
;
;Module Name:
;
;    SMCWCBTG.inf
;
;Abstract:
;    INF file for installing  Wireless Network Adapter
;
;    Installs SMCWPCIG.SYS (NDIS 5/5.1 driver) on NT platforms (2000, XP and greater)
;    Installs SMCWPCIG.sys (NDIS 5 driver) on 9x platforms 
;
;--*/

[Version]
Signature   = "$CHICAGO$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Vendor%
Compatible  = 1
DriverVer   = 04/19/2005,4.0.0.167
Catalogfile = SMCWPCIG.CAT

[Manufacturer]
%Vendor%     = DeviceList

[ControlFlags]
ExcludeFromSelect = *

[DeviceList]
%DeviceList.DeviceDesc.0001%      = NIC_4201D.ndi,        PCI\VEN_168C&DEV_001A&SUBSYS_EE241113

; Windows 9X specific entries

[NIC_4201D.ndi]
AddReg          = NIC_4201D.id.reg, NIC.common.reg, NIC.win.reg, NIC.bgmp.reg
CopyFiles       = NIC.win.CopyFiles, DEFAULTDESTDIRS
DelFiles        = NIC.DelIniFiles
DelReg          = NIC.DelReg

; Windows NT specific entries

[NIC_4201D.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
DelReg          = NIC.DelReg
AddReg          = NIC.common.reg, NIC.reg, NIC.bgmp.reg
CopyFiles       = NIC.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = NIC.DelIniFiles

[NIC_4201D.ndi.NT.Services]
AddService      = SMCWPCIG, 2, NIC.Service, common.EventLog

;----------------------------------------------------------------------------
; Win9x id registry sections
; These are not needed by NT

[NIC_4201D.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001A&SUBSYS_EE241113"
;
; NIC Enumerated Types
;

[NIC.bgmp.reg]
HKR, ,                                  NetBand,                        0x00002,  "12"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  2
HKR, ,                                  radioEnable,                    0x00002,  "1"

;-----------------------------------------------------------------------------

;
; NIC common
;
[NIC.DelReg]
HKR,,NetBand
HKR,,ssid
HKR,,ssid2
HKR,,ssid3
HKR,,prefBssid1
HKR,,prefBssid2
HKR,,prefBssid3
HKR,,prefBssid4
HKR,Ndi\Params\tpc
HKR,,tpc
HKR,Ndi\Params\authTypeUseOnly
HKR,,authTypeUseOnly
HKR,,AdHocBand
HKR,,AwakeTimePerf
HKR,,beaconInterval
HKR,,bkScanEnable
HKR,,bssType
HKR,,clist
HKR,,defaultKey
HKR,,EncryptionAlg
HKR,,FragThreshold
HKR,,HwTxRetries
HKR,,privacyInvoked
HKR,,QoS
HKR,,rateCtrlEnable
HKR,,RTSThreshold
HKR,,scanType
HKR,,SwTxRetryScale
HKR,,SmeEnable
HKR,,aifs
HKR,,cwmin

[NIC.common.reg]
HKR, Ndi\params\MapRegisters,           ParamDesc,                      0,  %MapRegisters%
HKR, Ndi\params\MapRegisters,           default,                        0,  "256"
HKR, Ndi\params\MapRegisters,           min,                            0,  "32"
HKR, Ndi\params\MapRegisters,           max,                            0,  "512"
HKR, Ndi\params\MapRegisters,           step,                           0,  "8"
HKR, Ndi\params\MapRegisters,           base,                           0,  "10"
HKR, Ndi\params\MapRegisters,           type,                           0,  "int"

HKR, Ndi\params\NetworkAddress,         ParamDesc,                      0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,         default,                        0,  ""
HKR, Ndi\params\NetworkAddress,         LimitText,                      0,  "12"
HKR, Ndi\params\NetworkAddress,         UpperCase,                      0,  "1"
HKR, Ndi\params\NetworkAddress,         optional,                       0,  "1"
HKR, Ndi\params\NetworkAddress,         type,                           0,  "edit"

HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "2"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  "1"
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,  %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,  "10"
HKR, Ndi\params\radioEnable,            default,                        0,  "1"
HKR, Ndi\params\radioEnable,            type,                           0,  "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,  %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,  %radioEnableOff%

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"

HKR, ,                                  AdHocBand,                      0x00002,  "0"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"
HKR, ,                                  beaconInterval,                 0x00002,  "100"
HKR, ,                                  bkScanEnable,                   0x00002,  "1"
HKR, ,                                  bssType,                        0x00002,  "1"
HKR, ,                                  clist,                          0x00002,  ""
HKR, ,                                  defaultKey,                     0x00002,  "0"
HKR, ,                                  EncryptionAlg,                  0x00002,  "2"
HKR, ,                                  FragThreshold,                  0x00002,  "2346"
HKR, ,                                  HwTxRetries,                    0x00002,  "4"
HKR, ,                                  privacyInvoked,                 0x00002,  "0"
HKR, ,                                  QoS,                            0x00002,  "0"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                                  RTSThreshold,                   0x00002,  "2346"
HKR, ,                                  scanType,                       0x00002,  "2"
HKR, ,                                  SwTxRetryScale,                 0x00002,  "6"
HKR, ,                                  SmeEnable,                      0x00002,  "1"


HKR, CustomParams\Configurations,       MajorVersion,                   0x10003,  2
HKR, CustomParams\Configurations,       MinorVersion,                   0x10003,  0

HKR, CustomParams\Configurations,       SelectedConfigurationIndex,     0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationName,      0x00002,  "Default"

;-----------------------------------------------------------------------------
; NT specific
;

[NIC.reg]
HKR, Ndi,             Service,      0, "SMCWPCIG"
HKR, Ndi\Interfaces,  UpperRange,   0, "ndis5"
HKR, Ndi\Interfaces,  LowerRange,   0, "ethernet"

[NIC.Service]
DisplayName     = %NIC.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\SMCWPCIG.sys
LoadOrderGroup  = NDIS

;-----------------------------------------------------------------------------
; NT/XP common
;
[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, ,                  EventMessageFile,   0x00020000,   "%%SystemRoot%%\System32\netevent.dll"
HKR, ,                  TypesSupported,     0x00010001,   7

;----------------------------------------------------------------------------
; Win9x specific
;
[NIC.win.reg]
HKR, ,                  DevLoader,          0,            "*ndis"
HKR, ,                  DeviceVxDs,         0,            "SMCWPCIG.sys"
HKR, ,                  EnumPropPages,      0,            "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,    DefUpper,           0,            "ndis3"
HKR, Ndi\Interfaces,    DefLower,           0,            "ethernet"
HKR, Ndi\Interfaces,    UpperRange,         0,            "ndis3"
HKR, Ndi\Interfaces,    LowerRange,         0,            "ethernet"


HKR, NDIS,              LogDriverName,      0,            "SMCWPCIG"
HKR, NDIS,              MajorNdisVersion,   1,            03
HKR, NDIS,              MinorNdisVersion,   1,            0A

HKR, Ndi\Install,       ndis3,              0,            "NIC.install"


;----------------------------------------------------------------------------
; Win9x Files to Copy
[NIC.win.CopyFiles]
SMCWPCIG.sys,,,2
;----------------------------------------------------------------------------
; NT Files to Copy
[NIC.CopyFiles.nt]
SMCWPCIG.sys,,,2

[NIC.DelIniFiles]
Athnic.ini,,,1

[SourceDisksNames]
;
; diskid = description[, [tagfile] [, <unused>, subdir]]
;
1 = %NIC_Disk%,,,

;----------------------------------------------------------------------------
; Source Files
[SourceDisksFiles]
SMCWPCIG.sys                 = 1,, ; on distribution disk 1

[DestinationDirs]
NIC.CopyFiles.nt           = 12
NIC.win.CopyFiles          = 10,system32\drivers ; %SystemRoot%\system32\drivers
NIC.DelIniFiles            = 10,system32\drivers ; %SystemRoot%\system32\drivers
DefaultDestDir               = 11

[DEFAULTDESTDIRS]
;


[Strings]
Vendor                       = "SMC"
MapRegisters                 = "Map Registers"
NetworkAddress               = "Network Address"
sleepMode                    = "Power Save Mode"
scanTimeValid                = "Scan Valid Interval"
sleepModeOff                 = "Off"
sleepModeNormal              = "Normal"
sleepModeMax                 = "Maximum"
shortPreamble                = "802.11b Preamble"
shortPreambleEnable          = "Long and Short"
shortPreambleDisable         = "Long only"
radioEnable                  = "Radio On/Off"
radioEnableOn                = "On"
radioEnableOff               = "Off"

NIC_Disk                 = "SMCWPCI-G 54Mbps Wireless PCI adapter Driver Disk"
NIC.Service.DispName       = "SMCWPCI-G 54Mbps Wireless PCI adapter Service"
DeviceList.DeviceDesc.0001   = "SMCWPCI-G 54Mbps Wireless PCI adapter"
