;****************************************************************************************
;
; RT2400.inf
;
;   This installation script supports Windows 98,Me,2000 & XP for the
;   Ralink RT2400 series Wireless LAN Card.
;
;   Copyright (c)2002, Ralink Technology Corp., All Rights Reserved
;   All Rights Reserved.
;   Developed by RaLink Technology, Corp. -- http://www.ralinktech.com
;
;****************************************************************************************

[Version]
DriverVer=02/24/2004, 2.01.00.0001
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Provider%
;CatalogFile=RT2400.CAT            ;;for WHQL certified


[ControlFlags]

;***********Ralink 802.11b board  ***********
;ExcludeFromSelect = PCI\VEN_1814&DEV_0101


[Manufacturer]
%V_Provider%=Adapters


[Adapters]
; DisplayName                	Section                	DeviceID
; -----------                	-------                	--------
%RT2400.DeviceDesc%=		RT2400.ndi,      	PCI\VEN_1814&DEV_0101&SUBSYS_24601814
%ASUS.DeviceDesc%=		RT2400.ndi,      	PCI\VEN_1814&DEV_0101&SUBSYS_01071043
%ASUS.DeviceDesc%=		RT2400.ndi,      	PCI\VEN_1814&DEV_0101&SUBSYS_01261043
%ASUS.DeviceDesc%=		RT2400.ndi,      	PCI\VEN_1814&DEV_0101&SUBSYS_01271043
%ASUSGEN.DeviceDesc%=		RT2400.ndi,      	PCI\VEN_1814&DEV_0101&SUBSYS_01251043



;*******************************************************************************************
; Windows 9X specific entries
;*******************************************************************************************

[RT2400.ndi]
AddReg=Common.reg, RT2400.ndi.reg
CopyFiles=win9x.CopyFiles


;*******************************************************************************************
; NT specific entries
;*******************************************************************************************

[RT2400.ndi.NT]
AddReg=Common.reg, RT2400.ndi.NT.reg
Characteristics=0x84              ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=5
CopyFiles=NT.CopyFiles

; NT services sections
[RT2400.ndi.NT.Services]
AddService=RT2400, 2, RT2400.Service, common.EventLog



[RT2400.ndi.reg]
HKR, ,                            NTMPDriver,      0, RT2400.sys
HKR, Ndi,                         DeviceID,        0, "PCI\VEN_1814&DEV_0101&SUBSYS_24601814"

HKR, ,                            RunningWin9X,    0, "1"
HKR, ,                            DevLoader,       0, *ndis
HKR, ,                            DeviceVxDs,      0, RT2400.sys
HKR, ,                            EnumPropPages,   0, "netdi.dll,EnumPropPages"

;
; NDIS Info
;
HKR, NDIS,                        LogDriverName,   0, "RT2400"
HKR, NDIS,                        MajorNdisVersion,1, 03
HKR, NDIS,                        MinorNdisVersion,1, 0A

HKR, ,                            BusType,         0, 5
HKR, NDI,                         CardType,        0, "PCI"

;
; Interfaces
;
HKR, Ndi\Interfaces,              DefUpper,        0, "ndis3"
HKR, Ndi\Interfaces,              DefLower,        0, "ethernet"
HKR, Ndi\Interfaces,              UpperRange,      0, "ndis3"
HKR, Ndi\Interfaces,              LowerRange,      0, "ethernet"

;
; Install sections
;HKR,Ndi\Install,ndis3,,"RT2400.install"


[win9x.CopyFiles]
RT2400.sys ; Win9x Installation

;*******************************************************************************************
; common regs for NT and W9x
;*******************************************************************************************

[Common.reg]

;
; SSID
;
HKR, ,                            SSID,            0, %SSID_DEF_STR%
HKR, Default,                     SSID,            0, %SSID_DEF_STR%
HKR, NDI\params\SSID,             ParamDesc,       0, "SSID"
HKR, NDI\params\SSID,             type,            0, "edit"
HKR, NDI\params\SSID,             limitText,       0, "32"
HKR, NDI\params\SSID,             default,         0, %SSID_DEF_STR%

;
; Network Type
;
HKR, ,                            NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, Default,                     NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType,      ParamDesc,       0, "Network Type"
HKR, NDI\params\NetworkType,      type,            0, "enum"
HKR, NDI\params\NetworkType,      default,         0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType\enum, 0,               0, "802.11 Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1,               0, "Infrastructure"

;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%
HKR, NDI\params\Channel,          ParamDesc,       0, "Channel"
HKR, NDI\params\Channel,          type,            0, "enum"
HKR, NDI\params\Channel,          default,         0, %CHANNEL%
HKR, NDI\params\Channel\enum,     1,               0, "01"
HKR, NDI\params\Channel\enum,     2,               0, "02"
HKR, NDI\params\Channel\enum,     3,               0, "03"
HKR, NDI\params\Channel\enum,     4,               0, "04"
HKR, NDI\params\Channel\enum,     5,               0, "05"
HKR, NDI\params\Channel\enum,     6,               0, "06"
HKR, NDI\params\Channel\enum,     7,               0, "07"
HKR, NDI\params\Channel\enum,     8,               0, "08"
HKR, NDI\params\Channel\enum,     9,               0, "09"
HKR, NDI\params\Channel\enum,     10,              0, "10"
HKR, NDI\params\Channel\enum,     11,              0, "11"


;*******************************************************************************************
; System Configuration Page

;
; Local Administration MAC Network Address
;
HKR, ,                            NetworkAddress,  0, ""
HKR, Default,                     NetworkAddress,  0, ""
HKR, NDI\params\NetworkAddress,   ParamDesc,       0, "Local Administration MAC Network Address"
HKR, NDI\params\NetworkAddress,   type,            0, "edit"
HKR, NDI\params\NetworkAddress,   limitText,       0, "12"
HKR, NDI\params\NetworkAddress,   default,         0, ""

;
; Select Config Utility
;
HKR, ,                            RaConfig,	   0, "1"      ;1=RaConfig , 0=ZeroConfig for MiniPCI

;
; Country Region
;
HKR, ,                            	CountryRegion,		0, "0"
;HKR, Default,                     	CountryRegion,      	0, "0"
HKR, NDI\params\CountryRegion,          ParamDesc,       	0, "Country Region"
HKR, NDI\params\CountryRegion,          type,            	0, "enum"
HKR, NDI\params\CountryRegion,          default,         	0, "0"
HKR, NDI\params\CountryRegion\enum,     0,               	0, "FCC (Channel 1 - 11)"
HKR, NDI\params\CountryRegion\enum,	1,               	0, "IC (Channel 1 - 11)"
HKR, NDI\params\CountryRegion\enum,     2,               	0, "ETSI (Channel 1 - 13)"
HKR, NDI\params\CountryRegion\enum,     3,               	0, "Spain (Channel 10 - 11)"
HKR, NDI\params\CountryRegion\enum,	4,               	0, "France (Channel 10 - 13)"
HKR, NDI\params\CountryRegion\enum,     5,               	0, "MKK (Channel 14)"
HKR, NDI\params\CountryRegion\enum,     6,               	0, "MKK1 (Channel 1 - 14)"
HKR, NDI\params\CountryRegion\enum,	7,               	0, "Israel (Channel 3 - 9)"


;
; Power Saving Mode
;
HKR, ,                            PSMode,          0, "0"
HKR, Default,                     PSMode,          0, "0"
HKR, NDI\params\PSMode,           ParamDesc,       0, "Power Saving Mode"
HKR, NDI\params\PSMode,           type,            0, "enum"
HKR, NDI\params\PSMode,           default,         0, "0"
HKR, NDI\params\PSMode\enum,      0,               0, "CAM (Constantly Awake Mode)"
HKR, NDI\params\PSMode\enum,      1,               0, "Max_PSP (Max Power Savings)"
HKR, NDI\params\PSMode\enum,      2,               0, "Fast_PSP (Power Save Mode)"

;
; CAM when AC Power
;
HKR, ,                            ACPowerCam,      0, "0"
HKR, Default,                     ACPowerCam,      0, "0"
HKR, NDI\params\ACPowerCam,       ParamDesc,       0, "CAM when AC Power"
HKR, NDI\params\ACPowerCam,       type,            0, "enum"
HKR, NDI\params\ACPowerCam,       default,         0, "0"
HKR, NDI\params\ACPowerCam\enum,  0,               0, "Disable"
HKR, NDI\params\ACPowerCam\enum,  1,               0, "Enable"

;
; Antenna Tx Diversity 
;
HKR, ,                            AntennaTx,       0, "0"
HKR, Default,                     AntennaTx,       0, "0"
HKR, NDI\params\AntennaTx,        ParamDesc,       0, "Antenna Tx Diversity"
HKR, NDI\params\AntennaTx,        type,            0, "enum"
HKR, NDI\params\AntennaTx,        default,         0, "0"
HKR, NDI\params\AntennaTx\enum,   0,               0, "Diversity"
HKR, NDI\params\AntennaTx\enum,   1,               0, "Antenna A Only"
HKR, NDI\params\AntennaTx\enum,   2,               0, "Antenna B Only"

;
; Antenna Rx Diversity 
;
HKR, ,                            AntennaRx,       0, "0"
HKR, Default,                     AntennaRx,       0, "0"
HKR, NDI\params\AntennaRx,        ParamDesc,       0, "Antenna Rx Diversity"
HKR, NDI\params\AntennaRx,        type,            0, "enum"
HKR, NDI\params\AntennaRx,        default,         0, "0"
HKR, NDI\params\AntennaRx\enum,   0,               0, "Diversity"
HKR, NDI\params\AntennaRx\enum,   1,               0, "Antenna A Only"
HKR, NDI\params\AntennaRx\enum,   2,               0, "Antenna B Only"

;
; Transmit Rate
;
HKR, ,                            TransRate,       0, "0"
HKR, Default,                     TransRate,       0, "0"
HKR, NDI\params\TransRate,        ParamDesc,       0, "Transmit Rate"
HKR, NDI\params\TransRate,        type,            0, "enum"
HKR, NDI\params\TransRate,        default,         0, "0"
HKR, NDI\params\TransRate\enum,   0,               0, "Auto"
HKR, NDI\params\TransRate\enum,   1,               0, "11 Mb/s"
HKR, NDI\params\TransRate\enum,   2,               0, "5.5 Mb/s"
HKR, NDI\params\TransRate\enum,   3,               0, "2 Mb/s"
HKR, NDI\params\TransRate\enum,   4,               0, "1 Mb/s"


;
; Preamble Type
;
HKR, ,                            PreambleType,    0, "2"
HKR, Default,                     PreambleType,    0, "2"
HKR, NDI\params\PreambleType,     ParamDesc,       0, "Preamble Type"
HKR, NDI\params\PreambleType,     type,            0, "enum"
HKR, Ndi\params\PreambleType,     default,         0, "2"
HKR, NDI\params\PreambleType\enum,0,               0, "Long"
HKR, NDI\params\PreambleType\enum,1,               0, "Short"
HKR, NDI\params\PreambleType\enum,2,               0, "Auto"
HKR, NDI\params\PreambleType,     optional,        0, "0"

;
; RTS Threshold
;
HKR, ,                            RTSThresh,       0, "2347"
HKR, Default,                     RTSThresh,       0, "2347"
HKR, NDI\params\RTSThresh,        ParamDesc,       0, "RTS Threshold"
HKR, NDI\params\RTSThresh,        type,            0, "int"
HKR, Ndi\params\RTSThresh,        default,         0, "2347"
HKR, NDI\params\RTSThresh,        min,             0, "0"
HKR, NDI\params\RTSThresh,        max,             0, "2347"
HKR, NDI\params\RTSThresh,        step,            0, "32"
HKR, NDI\params\RTSThresh,        optional,        0, "0"

;
; Fragment Threshold
;
HKR, ,                            FragThresh,      0, "2346"
HKR, Default,                     FragThresh,      0, "2346"
HKR, NDI\params\FragThresh,       ParamDesc,       0, "Fragment Threshold"
HKR, NDI\params\FragThresh,       type,            0, "int"
HKR, Ndi\params\FragThresh,       default,         0, "2346"
HKR, NDI\params\FragThresh,       min,             0, "256"
HKR, NDI\params\FragThresh,       max,             0, "2346"
HKR, NDI\params\FragThresh,       step,            0, "32"
HKR, NDI\params\FragThresh,       optional,        0, "0"

;
; Radio Status
;
HKR, ,                       Radio,      0, "0"
HKR, NDI\params\Radio,       ParamDesc,       0, "Radio Status"
HKR, NDI\params\Radio,       type,            0, "enum"
HKR, NDI\params\Radio,       default,         0, "0"
HKR, NDI\params\Radio\enum,  1,               0, "Disable"
HKR, NDI\params\Radio\enum,  0,               0, "Enable"

;
; Auto Reconnect Mode
;
HKR, ,                       		 AutoReconnect,   0, "1"
HKR, NDI\params\AutoReconnect,       ParamDesc,       0, "Auto Reconnect Mode"
HKR, NDI\params\AutoReconnect,       type,            0, "enum"
HKR, NDI\params\AutoReconnect,       default,         0, "1"
HKR, NDI\params\AutoReconnect\enum,  0,               0, "Disable"
HKR, NDI\params\AutoReconnect\enum,  1,               0, "Enable"

;*******************************************************************************************
; Authentication & Security Page

;
; Authentication Type
;
HKR, ,				  AuthenType,      0, "0" ; Open System
HKR, Default,			  AuthenType,      0, "0"

;
; Encryption
;
HKR, ,                            Encryption,      0, "1" ; Disable
HKR, Default,                     Encryption,      0, "1"

;
; WEP Keys Length
;
HKR, ,                            WEPKeyLen,       0, "0"
HKR, Default,                     WEPKeyLen,       0, "0"

;
; WEP Key to use
;
HKR, ,                            WEPKeyUse,       0,"1"
HKR, Default,                     WEPKeyUse,       0,"1"

;
; WEP Key1
;
HKR, , 				  WEPKey1,         0,""
HKR, Default, 			  WEPKey1,         0,""

;
; WEP Key2
;
HKR, , 				  WEPKey2,         0,""
HKR, Default, 			  WEPKey2,         0,""

;
; WEP Key3
;
HKR, , 				  WEPKey3,         0,""
HKR, Default, 			  WEPKey3,         0,""

;
; WEP Key4
;
HKR, , 				  WEPKey4,         0,""
HKR, Default, 			  WEPKey4,         0,""

;
; Current Profile
;
HKR, , 				  CurProfile,      0,""
HKR, Default, 			  CurProfile,      0,""

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************

[DestinationDirs]
NT.CopyFiles=12    ; system32\drivers subdirectory on NT
win9x.CopyFiles=11    ; system32 subdirectory on win9x

[NT.CopyFiles]
RT2400.sys ; NT Installation

[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,

[SourceDisksFiles] 
RT2400.sys=1


;*******************************************************************************************
; NT specific
;*******************************************************************************************

[RT2400.ndi.NT.reg]
HKR, Ndi,                         Service,         0, "RT2400"
HKR, Ndi\Interfaces,              UpperRange,      0, "ndis5"
HKR, Ndi\Interfaces,              LowerRange,      0, "ethernet"

[RT2400.Service]
DisplayName=%RT2400.Service.DispName%
ServiceType=1                	;%SERVICE_KERNEL_DRIVER%
StartType=3                	;%SERVICE_AUTO_START%
ErrorControl=1                	;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\RT2400.sys
LoadOrderGroup=NDIS

[common.EventLog]
AddReg=common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\RT2400.sys"
HKR, , TypesSupported,   0x00010001, 7


;*******************************************************************************************
; Strings
;*******************************************************************************************

[strings]
Provider=			"Ralink"
V_Provider=			"Ralink Technology Corp."

RT2400.DeviceDesc=		"RT2400 Wireless LAN Card"
ASUS.DeviceDesc=  		"ASUS 802.11b Wireless LAN Card"
ASUSGEN.DeviceDesc=  		"802.11b Wireless LAN Card"


RT2400.Service.DispName=	"RT2400 Wireless Driver"
INSTALL_DISK_STR=		"RT2400 Wireless LAN Installation Disk"

;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
SSID_DEF_STR		= ""
NETWORK_TYPE_DEF_STR	= "1"
CHANNEL			= "1"
