;;
;; bcmwl5.inf
;;
;; Copyright 1998-2002, Broadcom Corporation.
;; All Rights Reserved.
;;
;; This is UNPUBLISHED PROPRIETARY SOURCE CODE of Broadcom Corporation;
;; the contents of this file may not be disclosed to third parties, copied or
;; duplicated in any form, in whole or in part, without the prior written
;; permission of Broadcom Corporation.
;;

[version]
	Signature	= "$Windows NT$"
	Class=Net
	ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
	Provider	= %V_BCM%
DriverVer=07/09/2002, 3.08.27.0
	CatalogFile=BCM43XX.CAT

[Manufacturer]
	%V_BCM% = BROADCOM

[ControlFlags] 
	ExcludeFromSelect = *

[BROADCOM]
	%BCM430X.DeviceDesc% = BCM43XX, PCI\VEN_14E4&DEV_4301&SUBSYS_00011028
	%BCM430X.DeviceDesc% = BCM43XX, PCI\VEN_14E4&DEV_4301

[BCM43XX.NT]
	Characteristics	= 0x84	; NCF_PHYSICAL | NCF_HAS_UI
	BusType		= 5			; PCI bus
	AddReg		= BCM43XX.reg, common.reg
	CopyFiles	= BCM43XX.files.NT
DriverVer=07/09/2002, 3.08.27.0

[BCM43XX.NT.Services]
	AddService = BCM43XX, 2, BCM43XX.Service, common.EventLog

[BCM43XX.reg]
	HKR,	Ndi,	Service,		0,	"BCM43XX"
	; Ndis Info
	; Interfaces
	HKR,	Ndi\Interfaces,	UpperRange,	,	"ndis5"
	HKR,	Ndi\Interfaces,	LowerRange,	,	"ethernet"
	HKR,	Ndi,	HelpText,		,	%BCM43XX_HELP%

[BCM43XX.Service]
	DisplayName	= %BCM43XX.Service.DispName%
	ServiceType	= 1			; %SERVICE_KERNEL_DRIVER%
	StartType	= 3			; %SERVICE_DEMAND_START%
	ErrorControl	= 1			; %SERVICE_ERROR_NORMAL%
	ServiceBinary	= %12%\bcmwl5.sys
	LoadOrderGroup	= NDIS

[common.EventLog]
	AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
	HKR,	,	EventMessageFile,	0x00020000,	"%%SystemRoot%%\System32\netevent.dll"
	HKR,	,	TypesSupported,		0x00010001,	7

[BCM43XX.files.NT]
	BCMWL5.SYS,,,2

[common.reg]
	; Properties added to the advanced tab 
	HKR,,	MaxParamIndex, 0, "5"

	HKR,	Ndi\params\RadioState, ParamDesc,	0,	"Radio Enable/Disable"
	HKR,	Ndi\params\RadioState, type,		0,	"enum"
	HKR,	Ndi\params\RadioState\enum, "1",		0,	"Disabled"
	HKR,	Ndi\params\RadioState\enum, "0",		0,	"Enabled"
	HKR,    Ndi\params\RadioState,default,,"0"	

	HKR,	Ndi\params\Channel, ParamDesc, 0, "IBSS Channel Number"
	HKR,	Ndi\params\Channel, default,   0, "11"
	HKR,	Ndi\params\Channel, min,       0, "1"
	HKR,	Ndi\params\Channel, max,       0, "11"
	HKR,	Ndi\params\Channel, step,      0, "1"
	HKR,	Ndi\params\Channel, base,      0, "10"
	HKR,	Ndi\params\Channel, type,      0, "int"

	HKR,	Ndi\params\PowerSaveMode, ParamDesc,	0,	"Power Save Mode"
	HKR,	Ndi\params\PowerSaveMode, type,		0,	"enum"
	HKR,	Ndi\params\PowerSaveMode\enum, "0",		0,	"Disabled"
	HKR,	Ndi\params\PowerSaveMode\enum, "1",		0,	"Enabled"
	HKR,    Ndi\params\PowerSaveMode,default,,"0"	

	HKR,	Ndi\params\Rate, ParamDesc,	0,	"Rate"
	HKR,	Ndi\params\Rate, type,		0,	"enum"
	HKR,	Ndi\params\Rate\enum, "0",	0,	"Use best rate"
	HKR,	Ndi\params\Rate\enum, "2",	0,	"1"
	HKR,	Ndi\params\Rate\enum, "4",	0,	"2"
	HKR,	Ndi\params\Rate\enum, "11",	0,	"5.5"
	HKR,	Ndi\params\Rate\enum, "22",	0,	"11"
	HKR,	Ndi\params\Rate,default,,"0"

	HKR,	Ndi\params\PLCPHeader, ParamDesc,	0,	"PLCP Header"
	HKR,	Ndi\params\PLCPHeader, type,		0,	"enum"
	HKR,	Ndi\params\PLCPHeader\enum, "-1",	0,	"Long"
	HKR,	Ndi\params\PLCPHeader\enum, "0",	0,	"Auto (Short/Long)"
	HKR,	Ndi\params\PLCPHeader,default,,"0"

	HKR,	Ndi\params\antdiv, ParamDesc,	0,	"Antenna Diversity"
	HKR,	Ndi\params\antdiv, type,	0,	"enum"
	HKR,	Ndi\params\antdiv\enum, "-1",	0,	"Default"
	HKR,	Ndi\params\antdiv\enum, "0",	0,	"Disabled"
	HKR,	Ndi\params\antdiv\enum, "3",	0,	"Enabled"
	HKR,	Ndi\params\antdiv,default,,"-1"

	HKR,	Ndi\params\frag, ParamDesc,	0,	"Fragmentation Threshold"
	HKR,	Ndi\params\frag,type,0,"dword"
	HKR,	Ndi\params\frag,min,,"256"
	HKR,	Ndi\params\frag,max,,"2346"
	HKR,	Ndi\params\frag,default,,"2346"

	HKR,	Ndi\params\rts, ParamDesc,	0,	"RTS Threshold"
	HKR,	Ndi\params\rts,type,0,"dword"
	HKR,	Ndi\params\rts,min,,"0"
	HKR,	Ndi\params\rts,max,,"2347"
	HKR,	Ndi\params\rts,default,,"2347"

	HKR,	Ndi\params\NetworkAddress, ParamDesc,	0, "Locally Administered MAC Address"
	HKR,	Ndi\params\NetworkAddress, type,	0, "edit"
	HKR,	Ndi\params\NetworkAddress, LimitText,	0, "12"
	HKR,	Ndi\params\NetworkAddress, UpperCase,  0, "1"
	HKR,	Ndi\params\NetworkAddress, default,	0, ""
	HKR,	Ndi\params\NetworkAddress, optional,	0, "1"

[DestinationDirs]
	DefaultDestDir=12
	BCM43XX.files.NT = 12

[SourceDisksNames]
	1=%BCM43XX.DiskName%,,

[SourceDisksFiles]
	BCMWL5.SYS=1

[strings]
	; Provider
	V_BCM = "Broadcom"
	; PNP Devices
	BCM430X.DeviceDesc	= "Dell TrueMobile 1180 Internal 802.11b Mini PCI Card"
	; General Strings
	BCM43XX_HELP		= "The TrueMobile 1180 Internal 802.11b Mini PCI Network Adapter provides local area networking over thin air."
	BCM43XX.Service.DispName = "Dell TrueMobile 1180 Internal 802.11b Mini PCI Adapter Driver"
	BCM43XX.DiskName = "Dell TrueMobile 1180 Internal 802.11b Mini PCI Adapter Install Disk"
