;/*++
;
;Copyright (c), All Rights Reserved
;
;
;--*/

[Version]
Signature   = "$CHICAGO$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %OEM%
Compatible  = 1
DriverVer   = 10/22/2003,2.1.3.1
;Catalogfile = net5211.cat

[Manufacturer]
%OEM%     = OEM

[ControlFlags]
ExcludeFromSelect = *

[OEM]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
; Generic
; For G 9013
%ATHER.DeviceDesc.0013_1%  = ATHER_DEV_9013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_710116AB
%ATHER.DeviceDesc.0013_3%  = ATHER_DEV_9013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_710216AB
%ATHER.DeviceDesc.0013_1%  = ATHER_DEV_9013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_710316AB
%ATHER.DeviceDesc.0013_3%  = ATHER_DEV_9013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_710416AB
%ATHER.DeviceDesc.0013_3%  = ATHER_DEV_9013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_730216AB
%ATHER.DeviceDesc.0013_1%  = ATHER_DEV_9013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1025168C
%ATHER.DeviceDesc.0013_3%  = ATHER_DEV_9013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2027168C
%ATHER.DeviceDesc.0013_1%  = ATHER_DEV_9013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1030168C
%ATHER.DeviceDesc.0013_3%  = ATHER_DEV_9013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2030168C
%ATHER.DeviceDesc.0013_1%  = ATHER_DEV_9013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2041168C
%ATHER.DeviceDesc.0013_3%  = ATHER_DEV_9013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1041168C
%ATHER.DeviceDesc.0013_1%  = ATHER_DEV_9013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1043168C
%ATHER.DeviceDesc.0013_1%  = ATHER_DEV_9013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_F040168C

; For A+G 8013
%ATHER.DeviceDesc.0013_2%  = ATHER_DEV_8013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_720116AB
%ATHER.DeviceDesc.0013_4%  = ATHER_DEV_8013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_720216AB
%ATHER.DeviceDesc.0013_2%  = ATHER_DEV_8013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_720316AB
%ATHER.DeviceDesc.0013_4%  = ATHER_DEV_8013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_720416AB
%ATHER.DeviceDesc.0013_4%  = ATHER_DEV_8013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_740216AB
%ATHER.DeviceDesc.0013_2%  = ATHER_DEV_8013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1031168C
%ATHER.DeviceDesc.0013_4%  = ATHER_DEV_8013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2031168C
%ATHER.DeviceDesc.0013_2%  = ATHER_DEV_8013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1026168C
%ATHER.DeviceDesc.0013_4%  = ATHER_DEV_8013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2026168C
%ATHER.DeviceDesc.0013_2%  = ATHER_DEV_8013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_1042168C
%ATHER.DeviceDesc.0013_4%  = ATHER_DEV_8013.ndi,    PCI\VEN_168C&DEV_0013&SUBSYS_2042168C





; Windows 9X specific entries
[ATHER_DEV_0012.ndi]
AddReg          = ATHER_DEV_0012.id.reg, 5211.reg, ATHER.win.reg, 5211.acb.reg
CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1021.ndi]
AddReg          = ATHER_DEV_1021.id.reg, 5211.reg, ATHER.win.reg, 5211.acb.reg
CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1022.ndi]
AddReg          = ATHER_DEV_1022.id.reg, 5211.reg, ATHER.win.reg, 5211.abcb.reg
CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2022.ndi]
AddReg          = ATHER_DEV_2022.id.reg, 5211.reg, ATHER.win.reg, 5211.abmp.reg
CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_0013.ndi]
AddReg          = ATHER_DEV_0013.id.reg, 5211.reg, ATHER.win.reg, 5212.abg.reg
CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

; G
[ATHER_DEV_9013.ndi]
AddReg          = ATHER_DEV_0013.id.reg, 5211.reg, ATHER.win.reg, 5212_1.abg.reg
CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

; A+G
[ATHER_DEV_8013.ndi]
AddReg          = ATHER_DEV_0013.id.reg, 5211.reg, ATHER.win.reg, 5212_2.abg.reg
CopyFiles       = ATHER.win.CopyFiles, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles


; Windows NT specific entries

[ATHER_DEV_0012.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5211.acb.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1021.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5211.acb.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_1022.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5211.abcb.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_2022.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5211.abmp.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

[ATHER_DEV_0013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212.abg.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

; G
[ATHER_DEV_9013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212_1.abg.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles

; A+G
[ATHER_DEV_8013.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = 5211.reg, ATHER.reg, 5211.reg, 5212_2.abg.reg
CopyFiles       = ATHER.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = ATHER.DelIniFiles




[ATHER_DEV_0012.ndi.NT.Services]
AddService      = AR5211, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1021.ndi.NT.Services]
AddService      = AR5211, 2, ATHER.Service, common.EventLog

[ATHER_DEV_1022.ndi.NT.Services]
AddService      = AR5211, 2, ATHER.Service, common.EventLog

[ATHER_DEV_2022.ndi.NT.Services]
AddService      = AR5211, 2, ATHER.Service, common.EventLog

[ATHER_DEV_0013.ndi.NT.Services]
AddService      = AR5211, 2, ATHER.Service, common.EventLog

; G
[ATHER_DEV_9013.ndi.NT.Services]
AddService      = AR5211, 2, ATHER.Service, common.EventLog

; A+G
[ATHER_DEV_8013.ndi.NT.Services]
AddService      = AR5211, 2, ATHER.Service, common.EventLog


;----------------------------------------------------------------------------
; Win9x id registry sections
; These are not needed by NT

[ATHER_DEV_0012.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0012"

[ATHER_DEV_1021.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0012&SUBSYS_1021168C"

[ATHER_DEV_1022.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0012&SUBSYS_1022168C"

[ATHER_DEV_2022.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0012&SUBSYS_2022168C"

[ATHER_DEV_0013.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013"



;
; 5211 Enumerated Types
;
[5211.acb.reg]
HKR, ,                                  NetBand,                        0x00002,  "3"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  0
HKR, CustomParams\Configurations\Cfg0,  NetBand,                        0x10003,  3

[5211.abcb.reg]
HKR, ,                                  NetBand,                        0x00002,  "7"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, CustomParams\Configurations\Cfg0,  NetBand,                        0x10003,  7

[5211.abmp.reg]
HKR, ,                                  NetBand,                        0x00002,  "7"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  2
HKR, CustomParams\Configurations\Cfg0,  NetBand,                        0x10003,  7

; 
[5212.abg.reg]
HKR, ,                                  NetBand,                        0x00002,  "31"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, CustomParams\Configurations\Cfg0,  NetBand,                        0x10003,  31

; G
[5212_1.abg.reg]
HKR, ,                                  NetBand,                        0x00002,  "28"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, CustomParams\Configurations\Cfg0,  NetBand,                        0x10003,  28

; A+G
[5212_2.abg.reg]
HKR, ,                                  NetBand,                        0x00002,  "31"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, CustomParams\Configurations\Cfg0,  NetBand,                        0x10003,  31



;-----------------------------------------------------------------------------

;
; 5211 common
;

[5211.reg]

HKR, Ndi\params\MapRegisters,           ParamDesc,                      0,  %MapRegisters%
HKR, Ndi\params\MapRegisters,           default,                        0,  "256"
HKR, Ndi\params\MapRegisters,           min,                            0,  "32"
HKR, Ndi\params\MapRegisters,           max,                            0,  "512"
HKR, Ndi\params\MapRegisters,           step,                           0,  "8"
HKR, Ndi\params\MapRegisters,           base,                           0,  "10"
HKR, Ndi\params\MapRegisters,           type,                           0,  "int"

HKR, Ndi\params\NetworkAddress,         ParamDesc,                      0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,         default,                        0,  ""
HKR, Ndi\params\NetworkAddress,         LimitText,                      0,  "12"
HKR, Ndi\params\NetworkAddress,         UpperCase,                      0,  "1"
HKR, Ndi\params\NetworkAddress,         optional,                       0,  "1"
HKR, Ndi\params\NetworkAddress,         type,                           0,  "edit"

HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "0"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%


; Antenna Tx
HKR, Ndi\params\AntennaTx,                    ParamDesc,                      0,  "Antenna Tx"
HKR, Ndi\params\AntennaTx,                    Base,                           0,  "10"
HKR, Ndi\params\AntennaTx,                    default,                        0,  "0"
HKR, Ndi\params\AntennaTx,                    type,                           0,  "enum"
HKR, Ndi\params\AntennaTx\enum,               "0",                            0,  "Both"
HKR, Ndi\params\AntennaTx\enum,               "1",                            0,  "Antenna 1"
HKR, Ndi\params\AntennaTx\enum,               "2",                            0,  "Anteena 2"


; Antenna Tx 03.17.2003
HKR, Ndi\params\antennaSwitch,                    ParamDesc,                      0,  "Antenna Switch"
HKR, Ndi\params\antennaSwitch,                    Base,                           0,  "10"
HKR, Ndi\params\antennaSwitch,                    default,                        0,  "0"
HKR, Ndi\params\antennaSwitch,                    type,                           0,  "enum"
HKR, Ndi\params\antennaSwitch\enum,               "0",                            0,  "Both"
HKR, Ndi\params\antennaSwitch\enum,               "1",                            0,  "Antenna 1"
HKR, Ndi\params\antennaSwitch\enum,               "2",                            0,  "Anteena 2"






HKR, Ndi\params\tpc,                    ParamDesc,                      0,  %tpc%
HKR, Ndi\params\tpc,                    Base,                           0,  "10"
HKR, Ndi\params\tpc,                    default,                        0,  "0"
HKR, Ndi\params\tpc,                    type,                           0,  "enum"
HKR, Ndi\params\tpc\enum,               "0",                            0,  %tpc100%
HKR, Ndi\params\tpc\enum,               "1",                            0,  %tpc50%
HKR, Ndi\params\tpc\enum,               "2",                            0,  %tpc25%
HKR, Ndi\params\tpc\enum,               "3",                            0,  %tpc12%
HKR, Ndi\params\tpc\enum,               "4",                            0,  %tpcLowest%

HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  "1"
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,  %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,  "10"
HKR, Ndi\params\radioEnable,            default,                        0,  "1"
HKR, Ndi\params\radioEnable,            type,                           0,  "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,  %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,  %radioEnableOff%


HKR, ,                                  AdHocBand,                      0x00002,  "0"
HKR, ,                                  AdHocChannel,                   0x00002,  "2437"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"
HKR, ,                                  beaconInterval,                 0x00002,  "100"

; 03.12.2003  
; 0 - don't del bssid list
HKR, ,                                  DelBSSIDList,                   0x00002,  "0"

; Disable back scan
; 0 - don't back scan
HKR, ,                                  bkScanEnable,                   0x00002,  "0"

; Check Our Card
HKR, ,                                  CheckOurCard,                   0x00002,  "1"

; ssid 03.25.2003
HKR, ,                                  ssid,                           0x00002,  "default"

; 108G
HKR, ,                                  abolt,                          0x00002,  "63"

; WiFi 11g Adhoc
HKR, ,                                  WiFiAdhoc,			0x00002,  "1"


HKR, ,                                  bssType,                        0x00002,  "1"
HKR, ,                                  ccode,                          0x00002,  "US"
HKR, ,                                  clist,                          0x00002,  ""
HKR, ,                                  defaultKey,                     0x00002,  "0"
HKR, ,                                  EncryptionAlg,                  0x00002,  "2"
HKR, ,                                  FragThreshold,                  0x00002,  "2346"
HKR, ,                                  HwTxRetries,                    0x00002,  "4"
HKR, ,                                  privacyInvoked,                 0x00002,  "0"
HKR, ,                                  QoS,                            0x00002,  "0"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                                  RTSThreshold,                   0x00002,  "2346"
HKR, ,                                  scanType,                       0x00002,  "2"
HKR, ,                                  SwTxRetryScale,                 0x00002,  "6"
HKR, ,                                  SmeEnable,                      0x00002,  "1"

HKR, CustomParams\Configurations,       MajorVersion,                   0x10003,  2
HKR, CustomParams\Configurations,       MinorVersion,                   0x10003,  0

HKR, CustomParams\Configurations,       SelectedConfigurationIndex,     0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationName,      0x00002,  "Default"
HKR, CustomParams\Configurations\Cfg0,  AdHocBand,                      0x10003,  1
HKR, CustomParams\Configurations\Cfg0,  ConfigurationName,              0x00002,  "Default"
HKR, CustomParams\Configurations\Cfg0,  DefaultKey,                     0x10003,  0
HKR, CustomParams\Configurations\Cfg0,  EnableMacAddress,               0x10003,  0
HKR, CustomParams\Configurations\Cfg0,  EnableSecurity,                 0x10003,  0
HKR, CustomParams\Configurations\Cfg0,  EncryptionAlg,                  0x10003,  4
HKR, CustomParams\Configurations\Cfg0,  HexEntry,                       0x10003,  1
HKR, CustomParams\Configurations\Cfg0,  leapEnabled,                    0x10003,  0
HKR, CustomParams\Configurations\Cfg0,  MacAddress,                     0x00002,  ""
HKR, CustomParams\Configurations\Cfg0,  NetworkConnectionType,          0x10003,  1
HKR, CustomParams\Configurations\Cfg0,  NetworkName,                    0x00002,  ""
HKR, CustomParams\Configurations\Cfg0,  PowerManagement,                0x10003,  1
HKR, CustomParams\Configurations\Cfg0,  Preamble,                       0x10003,  1
HKR, CustomParams\Configurations\Cfg0,  QoS,                            0x10003,  0
HKR, CustomParams\Configurations\Cfg0,  scanType,                       0x10003,  2
HKR, CustomParams\Configurations\Cfg0,  tpc,                            0x10003,  0

; Allow non admin uses to switch profiles
[5211.reg.security]
"D:ARAI(A;;GA;;;BA)(A;;GA;;;SY)(A;CI;GA;;;IU)"

;-----------------------------------------------------------------------------
; ATHER NT specific
;

[ATHER.reg]
HKR, Ndi,             Service,      0, "AR5211"
HKR, Ndi\Interfaces,  UpperRange,   0, "ndis5"
HKR, Ndi\Interfaces,  LowerRange,   0, "ethernet"
HKR, ,                aifs,         0, "2"
HKR, ,                cwmin,        0, "15"


[ATHER.Service]
DisplayName     = %ATHER.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\ar5211.sys
LoadOrderGroup  = NDIS

;-----------------------------------------------------------------------------
; ATHER NT/XP common
;
[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, ,                  EventMessageFile,   0x00020000,   "%%SystemRoot%%\System32\netevent.dll"
HKR, ,                  TypesSupported,     0x00010001,   7

;----------------------------------------------------------------------------
; ATHER Win9x specific
;
[ATHER.win.reg]
HKR, ,                  DevLoader,          0,    "*ndis"
HKR, ,                  DeviceVxDs,         0,    "ar52119x.sys"
HKR, ,                  EnumPropPages,      0,    "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,    DefUpper,           0,    "ndis3"
HKR, Ndi\Interfaces,    DefLower,           0,    "ethernet"
HKR, Ndi\Interfaces,    UpperRange,         0,    "ndis3"
HKR, Ndi\Interfaces,    LowerRange,         0,    "ethernet"


HKR, NDIS,              LogDriverName,      0,    "AR52119X"
HKR, NDIS,              MajorNdisVersion,   1,    03
HKR, NDIS,              MinorNdisVersion,   1,    0A
HKR, ,                  aifs,               0,    "2"
HKR, ,                  cwmin,              0,    "15"

HKR, Ndi\Install,       ndis3,              0,    "ATHER.install"

;----------------------------------------------------------------------------
; Win9x Files to Copy
[ATHER.win.CopyFiles]
ar52119x.sys,,,2

;----------------------------------------------------------------------------
; NT Files to Copy
[ATHER.CopyFiles.nt]
ar5211.sys,,,2

[ATHER.DelIniFiles]
Athnic.ini,,,1

[SourceDisksNames]
;
; diskid = description[, [tagfile] [, <unused>, subdir]]
;
1 = %OEM_Disk%,,,

;----------------------------------------------------------------------------
; Source Files
[SourceDisksFiles]
ar52119x.sys                 = 1,, ; on distribution disk 1
ar5211.sys                   = 1,, ; on distribution disk 1


[DestinationDirs]
ATHER.CopyFiles.nt           = 12
ATHER.win.CopyFiles          = 10,system32\drivers ; %SystemRoot%\system32\drivers 
ATHER.DelIniFiles            = 10,system32\drivers ; %SystemRoot%\system32\drivers 
DefaultDestDir               = 11

[DEFAULTDESTDIRS]
;


[Strings]
OEM                        = ""
MapRegisters                 = "Map Registers"
NetworkAddress               = "Network Address"
sleepMode                    = "Power Save Mode"
sleepModeOff                 = "Off"
sleepModeNormal              = "Normal"
sleepModeMax                 = "Maximum"
tpc                          = "Transmit Power"
tpcLowest                    = "Lowest"
tpc12                        = "12.5%"
tpc25                        = "25%"
tpc50                        = "50%"
tpc100                       = "100%"
shortPreamble                = "802.11b Preamble"
shortPreambleEnable          = "Long and Short"
shortPreambleDisable         = "Long only"
radioEnable                  = "Radio On/Off"
radioEnableOn                = "On"
radioEnableOff               = "Off"

OEM_Disk                 = "Wireless LAN Adapter Install Disk"
ATHER.DeviceDesc.0013_1        = "108Mbps High Speed Wireless Network Adapter"
ATHER.DeviceDesc.0013_2        = "108Mbps High Speed Wireless Network Adapter"
ATHER.DeviceDesc.0013_3        = "108Mbps High Speed Wireless Network Adapter"
ATHER.DeviceDesc.0013_4        = "108Mbps High Speed Wireless Network Adapter"
;ATHER.DeviceDesc.0013_1        = "802.11g Wireless LAN CardBus Adapter"
;ATHER.DeviceDesc.0013_2        = "802.11a+g Multimode Wireless LAN Cardbus Adapter"
;ATHER.DeviceDesc.0013_3        = "802.11g Wireless LAN PCI Adapter"
;ATHER.DeviceDesc.0013_4        = "802.11a+g Multimode Wireless LAN PCI Adapter"


ATHER.Service.DispName       = "Wireless LAN Adapter"
