;(c) Copyright 2006 ASUSTek Computer Inc. All rights reserved.                         

[version]
Signature   = "$Chicago$"
Compatible  = 1
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %ICPlus%
CatalogFile    = ip100sn.cat
DriverVer   = 02/02/2005,4.5.50202

[Manufacturer]
%ICPlus%  = ICPlus, NT.5.1

[ControlFlags]
ExcludeFromSelect = PCI\VEN_13f0&DEV_0200

[ICPlus]
%IP100.DeviceDesc%      = ip100.ndi, PCI\VEN_13f0&DEV_0200
%IP100.DeviceDesc%      = ip100.ndi, PCI\VEN_13F0&DEV_0200&SUBSYS_82131043
%IP100.DeviceDesc%      = ip100.ndi, PCI\VEN_13F0&DEV_0200&SUBSYS_020113F0
[ICPlus.NT.5.1]
%IP100XP.DeviceDesc%    = ip100xp.ndi, PCI\VEN_13F0&DEV_0200
%IP100XP.DeviceDesc%    = ip100xp.ndi, PCI\VEN_13F0&DEV_0200&SUBSYS_82131043
%IP100XP.DeviceDesc%    = ip100xp.ndi, PCI\VEN_13F0&DEV_0200&SUBSYS_020113F0
;-----------------------------------------------------------------------------
;   W i n d o w s   9 x
;-----------------------------------------------------------------------------
[ip100.ndi]
CopyFiles   = ip100.win9x.CopyFiles, ip100.inf.CopyFiles
AddReg      = ip100.win9x.reg, ip100.common.reg

;-----------------------------------------------------------------------------
[ip100.win9x.reg]
HKR, ,                              BusType,            0,  5
HKR, ,                              DevLoader,          0,  *ndis
HKR, ,                              DeviceVxDs,         0,  ipfnd5.sys
HKR, ,				    EnumPropPages,      0,  netdi.dll,	EnumPropPages

HKR, NDIS,                          LogDriverName,      0,  "ip100"
HKR, NDIS,                          MajorNdisVersion,   1,  03
HKR, NDIS,                          MinorNdisVersion,   1,  0a

HKR, Ndi,                            DeviceID,           0,  "PCI\VEN_13f0&DEV_0200"  

HKR, Ndi\Interfaces,                DefLower,           ,   "ethernet"
HKR, Ndi\Interfaces,                LowerRange,         ,   "ethernet"
HKR, Ndi\Interfaces,                DefUpper,           ,   "ndis3"
HKR, Ndi\Interfaces,                UpperRange,         ,   "ndis3"

HKR, Ndi\params\RxBuffer,                   flag,       1,  "20","00","00","00"
HKR, Ndi\params\TxBuffer,                   flag,       1,  "20","00","00","00"
HKR, Ndi\params\NoCableIndication,          flag,       1,  "20","00","00","00"
HKR, Ndi\params\NetworkAddress,             flag,       1,  "20","00","00","00"
HKR, Ndi\params\ConnectionType,             flag,       1,  "20","00","00","00"

[ip100.win9x.CopyFiles]
ipfnd5.sys,,,2
[ip100.inf.CopyFiles]
netipf.inf,,,2

;--------------------------------------------------------------------------
;   W i n d o w s   2 0 0 0
;--------------------------------------------------------------------------
[ip100.ndi.nt]
Characteristics = 0x84  ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5     ; PCI
AddReg          = ip100.nt.reg, ip100.common.reg
CopyFiles       = ip100.nt.CopyFiles

[ip100.ndi.nt.Services]
AddService = IP100, 2, ip100.Service, ip100.EventLog


[ip100.nt.reg]
HKR, Ndi,                           Service,            ,   "IP100"
HKR, Ndi\Interfaces,                LowerRange,         ,   "ethernet"
HKR, Ndi\Interfaces,                UpperRange,         ,   "ndis5"

[ip100.Service]
DisplayName     = %ip100.Service.DispName%
ServiceType     = 1 ; %SERVICE_KERNEL_DRIVER%
StartType       = 3 ; %SERVICE_AUTO_START%
ErrorControl    = 1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\ipfnd5.sys
LoadOrderGroup  = NDIS

[ip100.EventLog]
AddReg = ip100.AddEventLog.reg

[ip100.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystenRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

[ip100.nt.CopyFiles]
ipfnd5.sys,,,2

;-----------------------------------------------------------------------------
;   W i n d o w s   XP
;-----------------------------------------------------------------------------
[ip100xp.ndi.nt]
Characteristics = 0x84  ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 5     ; PCI
AddReg          = ip100xp.nt.reg, ip100.common.reg
CopyFiles       = ip100xp.nt.CopyFiles

[ip100xp.ndi.nt.Services]
AddService = ip100xp, 2, ip100xp.Service, ip100xp.EventLog

[ip100xp.nt.reg]
HKR, Ndi,                           Service,            ,   "ip100xp"
HKR, Ndi\Interfaces,                LowerRange,         ,   "ethernet"
HKR, Ndi\Interfaces,                UpperRange,         ,   "ndis5"

[ip100xp.Service]
DisplayName     = %ip100xp.Service.DispName%
ServiceType     = 1 ; %SERVICE_KERNEL_DRIVER%
StartType       = 3 ; %SERVICE_AUTO_START%
ErrorControl    = 1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\ipfnd51.sys
LoadOrderGroup  = NDIS

[ip100xp.EventLog]
AddReg = ip100xp.AddEventLog.reg

[ip100xp.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystenRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

[ip100xp.nt.CopyFiles]
ipfnd51.sys,,,2

;-----------------------------------------------------------------------------
;Both Windows 2000 & 9x
;-----------------------------------------------------------------------------
[ip100.common.reg]
HKR, ,                              AdapterCFID,        0,  "020013f0"
HKR, ,                              AdapterType,        0,  "5"
HKR, ,                              MediaType,          0,  "1"

; Connection Type
HKR, Ndi\params\ConnectionType,             ParamDesc,  ,   %ConnectionType%
HKR, Ndi\params\ConnectionType,             default,    ,   "0"
HKR, Ndi\params\ConnectionType,             type,       ,   "enum"
HKR, Ndi\params\ConnectionType\enum,        0,          ,   %Autosense%
;HKR, Ndi\params\ConnectionType\enum,        1,          ,   %10BaseT%
;HKR, Ndi\params\ConnectionType\enum,        2,          ,   %10BaseTFD%
;HKR, Ndi\params\ConnectionType\enum,        3,          ,   %100BaseTx%
;HKR, Ndi\params\ConnectionType\enum,        4,          ,   %100BaseTxFD%
HKR, Ndi\params\ConnectionType\enum,        6,          ,   %N10BaseT%
HKR, Ndi\params\ConnectionType\enum,        7,          ,   %N10BaseTFD%
HKR, Ndi\params\ConnectionType\enum,        8,          ,   %N100BaseTx%
HKR, Ndi\params\ConnectionType\enum,        9,          ,   %N100BaseTxFD%

; Receive Buffers
HKR, Ndi\params\RxBuffer,                   ParamDesc,  ,   %RxBuffer%
HKR, Ndi\params\RxBuffer,                   default,    ,   "96"
HKR, Ndi\params\RxBuffer,                   type,       ,   "enum"
HKR, Ndi\params\RxBuffer\enum,              16,         ,   "16"
HKR, Ndi\params\RxBuffer\enum,              32,         ,   "32"
HKR, Ndi\params\RxBuffer\enum,              48,         ,   "48"
HKR, Ndi\params\RxBuffer\enum,              64,         ,   "64"
HKR, Ndi\params\RxBuffer\enum,              80,         ,   "80"
HKR, Ndi\params\RxBuffer\enum,              96,         ,   "96"
HKR, Ndi\params\RxBuffer\enum,              112,         ,   "112"
HKR, Ndi\params\RxBuffer\enum,              128,         ,   "128"

; Transmit Buffers
HKR, Ndi\params\TxBuffer,                   ParamDesc,  ,   %TxBuffer%
HKR, Ndi\params\TxBuffer,                   default,    ,   "96"
HKR, Ndi\params\TxBuffer,                   type,       ,   "enum"
HKR, Ndi\params\TxBuffer\enum,              16,         ,   "16"
HKR, Ndi\params\TxBuffer\enum,              32,         ,   "32"
HKR, Ndi\params\TxBuffer\enum,              48,         ,   "48"
HKR, Ndi\params\TxBuffer\enum,              64,         ,   "64"
HKR, Ndi\params\TxBuffer\enum,              80,         ,   "80"
HKR, Ndi\params\TxBuffer\enum,              96,         ,   "96"
HKR, Ndi\params\TxBuffer\enum,              112,         ,   "112"
HKR, Ndi\params\TxBuffer\enum,              128,         ,   "128"

; No Cable Indication
HKR, Ndi\params\NoCableIndication,          ParamDesc,  ,   %NoCableIndication%
HKR, Ndi\params\NoCableIndication,          default,    ,   "0"
HKR, Ndi\params\NoCableIndication,          type,       ,   "enum"
HKR, Ndi\params\NoCableIndication\enum,     0,          ,   %Disabled%
HKR, Ndi\params\NoCableIndication\enum,     1,          ,   %Enabled%

; Network Address
HKR, Ndi\params\NetworkAddress,             ParamDesc,  ,   %NetworkAddress%
HKR, Ndi\params\NetworkAddress,             type,       ,   "edit"
HKR, Ndi\params\NetworkAddress,             LimitText,  ,   "12"
HKR, Ndi\params\NetworkAddress,             UpperCase,  ,   "1"
HKR, Ndi\params\NetworkAddress,             default,    ,   ""
HKR, Ndi\params\NetworkAddress,             optional,   ,   "1"

;-----------------------------------------------------------------------------
; DestinationDirs
;
[DestinationDirs]
DefaultDestDir 	= 11
ip100.win9x.CopyFiles = 11
ip100.inf.CopyFiles = 17
ip100.nt.CopyFiles = 12
ip100xp.nt.CopyFiles = 12
;-----------------------------------------------------------------------------
; Source Disk layout
;
[SourceDisksNames]
3=%DriverDisketteName%,"netipf.inf",		

[SourceDisksFiles]
ipfnd51.sys = 3
ipfnd5.sys = 3
ipfnd4.sys = 3
ipfnd3.sys = 3
netipf.inf = 3


;-----------------------------------------------------------------------------
; Localizable Strings
;
[Strings]
ICPlus              = "ASUSTek Computer Inc."

RxBuffer            = "Receive Buffers"
TxBuffer            = "Transmit Buffers"
NoCableIndication   = "No Cable Indication"
NetworkAddress      = "Network Address"
ConnectionType      = "Connection Type"
Disabled            = "Disabled"
Enabled             = "Enabled"
Autosense           = "AutoSense"
10BaseT             = "10Half (Force)"
10BaseTFD           = "10Full (Force)"
100BaseTx           = "100Half(Force)"
100BaseTxFD         = "100Full(Force)"
N10BaseT             = "10Half (Nway)"
N10BaseTFD           = "10Full (Nway)"
N100BaseTx           = "100Half(Nway)"
N100BaseTxFD         = "100Full(Nway)"

IP100.DeviceDesc	 = "ASUS NX1001 Network Adapter"
IP100.Service.DispName   = "ASUS NX1001 Network Adapter NT Driver"
IP100xp.DeviceDesc	 = "ASUS NX1001 Network Adapter"
IP100xp.Service.DispName   = "ASUS NX1001 Network Adapter NT Driver"

DriverDisketteName	 = "ASUS NX1001 Network Adapter Driver Diskette""