;; FETHCB.inf (NT 5.0 & Win98 combined inf for NDIS5 driver)
;;
;; CardBus PCI/Cardbus Fast Ethernet Network Interface Cards.
;;
;; Copyright 1996-2001, CardBus Semiconductor Corporation
;;


[version]
Signature      = "$Chicago$"
Compatible     = 1
Class          = Net
ClassGUID      = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider       = %CardBus%                                 ;;
CatalogFile    = FETHCB.cat                               ;; for WHQL certified
                            
DriverVer      = 08/23/2001,5.397.0823.2001

[Manufacturer]
%CardBus%   = CardBus

[ControlFlags]
ExcludeFromSelect     = PCI\VEN_10ec&DEV_8138
ExcludeFromSelect     = PCI\VEN_10ec&DEV_8139
ExcludeFromSelect     = PCI\VEN_10ec&DEV_8138&SUBSYS_020014cb                        
ExcludeFromSelect     = PCI\VEN_10ec&DEV_8139&SUBSYS_020014cb  

[CardBus]
%FETHCB.DeviceDesc%  = FETHCB.ndi, PCI\VEN_10ec&DEV_8138
%FETHCB.DeviceDesc%  = FETHCB.ndi, PCI\VEN_10ec&DEV_8139
%FETHCB_A.DeviceDesc%  = FETHCB_A.ndi, PCI\VEN_10ec&DEV_8138&SUBSYS_020014cb
%FETHCB_A.DeviceDesc%  = FETHCB_A.ndi, PCI\VEN_10ec&DEV_8139&SUBSYS_020014cb


;;****************************************************************************
;; Windows 9x
;;****************************************************************************
[FETHCB.ndi]
DriverVer       = 08/23/2001,397
AddReg          = FETHCB.id.reg, FETHCB.common.reg, FETHCB.win.reg, FETHCB.oncbs.reg
CopyFiles       = FETHCB.CopyFiles98
;DeviceID        = "PCI\VEN_10ec&DEV_8139"
;LogConfig       = DefaultConfig

[FETHCB_A.ndi]
DriverVer       = 08/23/2001,397
AddReg          = FETHCB.id.reg, FETHCB.common.reg, FETHCB.win.reg, FETHCB.oncbs.reg
CopyFiles       = FETHCB.CopyFiles98
;DeviceID        = "PCI\VEN_10ec&DEV_8139&SUBSYS_020014cb"
;LogConfig       = DefaultConfig


;;****************************************************************************
;; NT 5.0
;;****************************************************************************
[FETHCB.ndi.NT]
AddReg          = FETHCB.common.reg, FETHCB.reg, FETHCB.oncbs.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = FETHCB.CopyFiles

[FETHCB.ndi.NT.Services]
AddService = FETHCB, 2, rtsnt.Service, FETHCB.EventLog

[FETHCB_A.ndi.NT]
AddReg          = FETHCB.common.reg, FETHCB.reg, FETHCB.oncbs.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = FETHCB.CopyFiles

[FETHCB_A.ndi.NT.Services]
AddService = FETHCB, 2, rtsnt.Service, FETHCB.EventLog

[FETHCB.CopyFiles]
FETHCB.sys,,,2

[FETHCB.CopyFiles98]
FETHCB.sys,,,2

;;----------------------------------------------------------------------------
;; FETHCB Parameters
;;----------------------------------------------------------------------------
;;***************************************************************************
;; Windows 9x parameters
;;***************************************************************************
[FETHCB.id.reg]
HKR, Ndi,       DeviceID,       0,      "PCI\VEN_10ec&DEV_8139"

HKR, Ndi\Install,                       ,       0,      rtsnt.install
HKR, NDI\Params\DuplexMode,             flag,   1,      30, 00, 00, 00
HKR, Ndi\Params\EarlyTxThreshold,       flag,   1,      20, 00, 00, 00
HKR, NDI\Params\NetworkAddress,         flag,   1,      30, 00, 00, 00
HKR, NDI\Params\WakeUpFrame,            flag,   1,      30, 00, 00, 00

[FETHCB.win.reg]
;; key,subkey,valuname,type,value
HKR, ,  DriverDesc,     0,      "Fast Ethernet CardBus PC Card"
HKR, ,  DevLoader,      0,      *ndis
HKR, ,  DeviceVxDs,     0,      FETHCB.sys
HKR, ,  EnumPropPages,  0,      netdi.dll,      EnumPropPages

;;params
HKR, ,  MediaType,      0,      1
HKR, ,  AdapterType,    0,      5
HKR, ,  BusType,        0,      5

;; NDIS Info
HKR, NDIS,              MajorNdisVersion,       1,      03
HKR, NDIS,              MinorNdisVersion,       1,      0a
HKR, NDIS,              LogDriverName,          0,      "FETHCB"

;; Interfaces
HKR, Ndi\Interfaces,    DefLower,               ,       "ethernet"
HKR, Ndi\Interfaces,    LowerRange,             ,       "ethernet"
HKR, Ndi\Interfaces,    DefUpper,               ,       "ndis3"
HKR, Ndi\Interfaces,    UpperRange,             ,       "ndis3"

;; Install sections
HKR, Ndi\Install,       ndis3,                  0,      "rtl139.ndis5"

;;****************************************************************************
;; FETHCB common parameters
;;****************************************************************************
[FETHCB.oncbs.reg]
HKR,,ChipOnCardbus,,"0"

[FETHCB.common.reg]
HKR, Ndi\params\DuplexMode,      ParamDesc, 0, %DuplexMode%
HKR, Ndi\params\DuplexMode,      type,      0, "enum"
HKR, Ndi\params\DuplexMode,      default,   0, "1"
HKR, Ndi\params\DuplexMode\enum, 1,         0, %dmAutoMode%
HKR, Ndi\params\DuplexMode\enum, 2,         0, %dm10HalfMode%
HKR, Ndi\params\DuplexMode\enum, 3,         0, %dm10FullMode%
HKR, Ndi\params\DuplexMode\enum, 4,         0, %dm100HalfMode%
HKR, Ndi\params\DuplexMode\enum, 5,         0, %dm100FullMode%

HKR,Ndi\Params\EarlyTxThreshold, ParamDesc, 0, %EarlyTxThreshold%
HKR,Ndi\Params\EarlyTxThreshold, Type,      0, "int"
HKR,Ndi\Params\EarlyTxThreshold, Default,   0, "15"
HKR,Ndi\Params\EarlyTxThreshold, Min,       0, "0"
HKR,Ndi\Params\EarlyTxThreshold, Max,       0, "63"
HKR,Ndi\Params\EarlyTxThreshold, Step,      0, "1"
HKR,Ndi\Params\EarlyTxThreshold, Base,      0, "10"

HKR,Ndi\params\NetworkAddress,   ParamDesc, 0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,   type,      0, "edit"
HKR,Ndi\params\NetworkAddress,   default,   0, "000000000000"
HKR,Ndi\params\NetworkAddress,   LimitText, 0, "12"
HKR,Ndi\params\NetworkAddress,   UpperCase, 0, "1"
HKR,Ndi\params\NetworkAddress,   Optional,  0, "1"

;HKR,NDI\Params\TxMaxDMABurst,flag,1,30,00,00,00
;HKR,Ndi\params\TxMaxDMABurst,ParamDesc,0,"Transmit DMA burst size"
;HKR,Ndi\params\TxMaxDMABurst,type,0,enum
;HKR,Ndi\params\TxMaxDMABurst,default,0,6
;HKR,Ndi\params\TxMaxDMABurst\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,7,0,"7:2048 bytes"

;HKR,NDI\Params\RxMaxDMABurst,flag,1,30,00,00,00
;HKR,Ndi\params\RxMaxDMABurst,ParamDesc,0,"Receive DMA burst size"
;HKR,Ndi\params\RxMaxDMABurst,type,0,enum
;HKR,Ndi\params\RxMaxDMABurst,default,0,6
;HKR,Ndi\params\RxMaxDMABurst\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,7,0,"7:unlimitted"

;HKR,NDI\Params\EarlyRxThreshold,flag,1,30,00,00,00
;HKR,Ndi\params\EarlyRxThreshold,ParamDesc,0,"Receive FIFO threshold"
;HKR,Ndi\params\EarlyRxThreshold,type,0,enum
;HKR,Ndi\params\EarlyRxThreshold,default,0,2
;HKR,Ndi\params\EarlyRxThreshold\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,7,0,"7:No threshold"

;HKR,NDI\Params\TxInterFrameGap,flag,1,30,00,00,00
;HKR,Ndi\params\TxInterFrameGap,ParamDesc,0,"Tx IFG(10M/100M)"
;HKR,Ndi\params\TxInterFrameGap,type,0,enum
;HKR,Ndi\params\TxInterFrameGap,default,0,3
;HKR,Ndi\params\TxInterFrameGap\enum,0,0,"8.4us/840ns"
;HKR,Ndi\params\TxInterFrameGap\enum,1,0,"8.8us/880ns"
;HKR,Ndi\params\TxInterFrameGap\enum,2,0,"9.2us/920ns"
;HKR,Ndi\params\TxInterFrameGap\enum,3,0,"9.6us/960ns"

;HKR, Ndi\params\WakeOnLan,         ParamDesc,  0, "Smart Power Saving"
;HKR, Ndi\params\WakeOnLan,         default,    0, "0"  
;HKR, Ndi\params\WakeOnLan,         type,       0, "enum"
;HKR, Ndi\params\WakeOnLan\enum,    "0",        0, "Disable"
;HKR, Ndi\params\WakeOnLan\enum,    "1",        0, "Enable (No WakeUp)"

HKR,Ndi\params\RxBufLen,	   ParamDesc,  0, "Receive Buffer Size"
HKR,Ndi\params\RxBufLen,	   type,       0, "enum"
HKR,Ndi\params\RxBufLen,	   default,    0, "3"
HKR,Ndi\params\RxBufLen\enum,	   "0",	       0, "8K bytes"
HKR,Ndi\params\RxBufLen\enum,	   "1",	       0, "16K bytes"
HKR,Ndi\params\RxBufLen\enum,	   "2",	       0, "32K bytes"
HKR,Ndi\params\RxBufLen\enum,	   "3",	       0, "64K bytes"

HKR, Ndi\params\LinkUp,            ParamDesc,  0, "WakeUp on Link Change"
HKR, Ndi\params\LinkUp,            default,    0, "0"
HKR, Ndi\params\LinkUp,            type,       0, "enum"
HKR, Ndi\params\LinkUp\enum,       "1",        0, "Enable"
HKR, Ndi\params\LinkUp\enum,       "0",        0, "Disable"

HKR, Ndi\params\WakeUpFrame,       ParamDesc,  0, "WakeUp on ARP/PING"
HKR, Ndi\params\WakeUpFrame,       default,    0, "0"
HKR, Ndi\params\WakeUpFrame,       type,       0, "enum"
HKR, Ndi\params\WakeUpFrame\enum,  "0",        0, "Enable"
HKR, Ndi\params\WakeUpFrame\enum,  "1",        0, "Disable"

HKR, Ndi\params\PME,               ParamDesc,  0, "WakeUp using APM Mode"
HKR, Ndi\params\PME,               default,    0, "1"
HKR, Ndi\params\PME,               type,       0, "enum"
HKR, Ndi\params\PME\enum,          "0",        0, "Enable"
HKR, Ndi\params\PME\enum,          "1",        0, "Disable"

HKR, Ndi\params\EnableLDPS,        ParamDesc,  0, "Link Down Power Saving"
HKR, Ndi\params\EnableLDPS,        default,    0, "0"
HKR, Ndi\params\EnableLDPS,        type,       0, "enum"
HKR, Ndi\params\EnableLDPS\enum,   "0",        0, "Disable"
HKR, Ndi\params\EnableLDPS\enum,   "1",        0, "Enable"


;;****************************************************************************
;; NT 5.0 parameters
;;****************************************************************************
[FETHCB.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "FETHCB"

[rtsnt.Service]
DisplayName     = %FETHCB.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\FETHCB.sys
LoadOrderGroup  = NDIS

[FETHCB.EventLog]
Addreg = FETHCB.AddEventLog.reg

[FETHCB.AddEventLog.reg]
HKR,    ,   EventMessageFile,   0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR,    ,   TypesSupported,     0x00010001, 7

;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
FETHCB.CopyFiles           = 12
FETHCB.CopyFiles98         = 11
DefaultDestDir              = 11        ; LDID_SYS

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
FETHCB.sys  = 1
;FETHCB.inf  = 1
;FETHCB.cat  = 1
                 

;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
;Msft                      = "Microsoft"
CardBus                   = "CardBus"

;;Source disk name
DISKNAME = " Fast Ethernet CardBus PC Card Driver Disk "

NetworkAddress            = "Network Address"
EarlyTxThreshold          = "Early Tx Threshold"
DuplexMode                = "Link Speed/Duplex Mode"
dmAutoMode                = "Auto Mode"
dm10HalfMode              = "10 Half Mode"
dm10FullMode              = "10 Full Mode"
dm100HalfMode             = "100 Half Mode"
dm100FullMode             = "100 Full Mode"

FETHCB.DeviceDesc        = "Fast Ethernet CardBus PC Card"
FETHCB.Service.DispName  = "Fast Ethernet CardBus PC Card NT Driver"
FETHCB_A.DeviceDesc      = "Fast Ethernet CardBus PC Card"

