; netA504.INF
;
; Install driver for 802.11a/b radio on Win98, WinME, Win2K, WinXP
;
; Copyright 2002, Cisco Systems, Inc.
;
[version]
signature   = "$CHICAGO$"
Compatible  = 1
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
provider    = %V_CISCO%
MillenniumPreferred = .ME
DriverVer   = 04/29/2005, 3.10.7
CatalogFile = neta504.cat



[SourceDisksNames]
;diskid = disk-description[,[tag-or-cab-file],[unused,path][,flags]]
1= %Disk_1_Desc%,,,,



[SourceDisksFiles]
;filename = diskid[,[subdir][,size]]
PCX504.sys    =1,,
PCX504.51     =1,,
vxdx500.vxd   =1,,
pcx504a.img   =1,,
pcx504b.img   =1,,
CInsX500.dll  =1,,
CInst16.dll   =1,,
CUtil16.exe   =1,,



[DestinationDirs]
CopySys_NT               = 12 ; Drivers directory (%windir%\system32\drivers)
CopySys_XP               = 12 ; Drivers directory (%windir%\system32\drivers)
CopyFW_a_NT              = 12 ; Drivers directory (%windir%\system32\drivers)
CopyFW_b_NT              = 12 ; Drivers directory (%windir%\system32\drivers)
CopyCoInst_NT            = 11
;
; win9x
;
CopySys_9x               = 11 ; Win9x Only (%windir%\system)
CopyFW_a_9x              = 11 ; Win9x Only (%windir%\system)
CopyFW_b_9x              = 11 ; Win9x Only (%windir%\system)
CopyCoInst_9x            = 11 ; Win9x Only (%windir%\system)
DefaultDestDir           = 11 ; Win9x Only (%windir%\system)



[Manufacturer]
%V_CISCO%  = CISCO,NT.5.1



[ControlFlags]
ExcludeFromSelect = *



[CISCO]
; DisplayName           Section             DeviceID
; -----------           -------             --------
%PCX504_b.DevDesc%      = PCX504_b.ndi,     PCI\VEN_14B9&DEV_A504&SUBSYS_500014B9
%PCX504_a.DevDesc%      = PCX504_a.ndi,     PCI\VEN_14B9&DEV_A505&SUBSYS_640014B9


[CISCO.NT.5.1]
; DisplayName           Section             DeviceID
; -----------           -------             --------
%PCX504_b.DevDesc%      = PCX504_b_XP.ndi,  PCI\VEN_14B9&DEV_A504&SUBSYS_500014B9
%PCX504_a.DevDesc%      = PCX504_a_XP.ndi,  PCI\VEN_14B9&DEV_A505&SUBSYS_640014B9



;------------------------------------------------------------------------------
; 802.11b -- 2.4 GHz 
;------------------------------------------------------------------------------
[PCX504_b_XP.ndi]
AddReg          =   NDI5, COMMON, DATARATE_b, SSID, RADIONAME_b, BUSPCI
Characteristics =   0x84
BusType         =   5
CopyFiles       =   CopySys_XP, CopyFW_b_NT

[PCX504_b_XP.ndi.Services]
AddService      =   PCX504, 2, PCX504.Service, common.AddEventLog

[PCX504_b_XP.ndi.CoInstallers]
AddReg          =   CoInstaller.NT.AddReg
CopyFiles       =   CopyCoInst_NT



[PCX504_b.ndi.NT]
AddReg          =   NDI5, COMMON, DATARATE_b, SSID, RADIONAME_b, BUSPCI
Characteristics =   0x84
BusType         =   5
CopyFiles       =   CopySys_NT, CopyFW_b_NT

[PCX504_b.ndi.NT.Services]
AddService      =   PCX504, 2, PCX504.Service, common.AddEventLog

[PCX504_b.ndi.NT.CoInstallers]
AddReg          =   CoInstaller.NT.AddReg
CopyFiles       =   CopyCoInst_NT



[PCX504_b.ndi.ME]
AddReg          =   NDI5_ME, COMMON, DATARATE_b, SSID, RADIONAME_b, BUSPCI, DEVID_b
Characteristics =   0x84
BusType         =   5
CopyFiles       =   CopyCoInst_9x,CopySys_9x,CopyFW_b_9x

[PCX504_b.ndi.ME.Services]
AddService      =   PCX504, 2, PCX504.Service, common.AddEventLog



[PCX504_b.ndi]
AddReg          =   NDI3, COMMON, DATARATE_b, SSID, RADIONAME_b, BUSPCI, DEVID_b
CopyFiles       =   CopyCoInst_9x,CopySys_9x,CopyFW_b_9x



;------------------------------------------------------------------------------
; 802.11a -- 5.0 GHz 
;------------------------------------------------------------------------------
[PCX504_a_XP.ndi]
AddReg          =   NDI5, COMMON, DATARATE_a, SSID, RADIONAME_a, BUSCARDBUS
Characteristics =   0x84
BusType         =   5
CopyFiles       =   CopySys_XP, CopyFW_a_NT

[PCX504_a_XP.ndi.Services]
AddService      =   PCX504, 2, PCX504.Service, common.AddEventLog

[PCX504_a_XP.ndi.CoInstallers]
AddReg          =   CoInstaller.NT.AddReg
CopyFiles       =   CopyCoInst_NT



[PCX504_a.ndi.NT]
AddReg          =   NDI5, COMMON, DATARATE_a, SSID, RADIONAME_a, BUSCARDBUS
Characteristics =   0x84
BusType         =   5
CopyFiles       =   CopySys_NT, CopyFW_a_NT

[PCX504_a.ndi.NT.Services]
AddService      =   PCX504, 2, PCX504.Service, common.AddEventLog

[PCX504_a.ndi.NT.CoInstallers]
AddReg          =   CoInstaller.NT.AddReg
CopyFiles       =   CopyCoInst_NT



[PCX504_a.ndi.ME]
AddReg          =   NDI5_ME, COMMON, DATARATE_a, SSID, RADIONAME_a, BUSCARDBUS, DEVID_a
Characteristics =   0x84
BusType         =   5
CopyFiles       =   CopyCoInst_9x,CopySys_9x,CopyFW_a_9x

[PCX504_a.ndi.ME.Services]
AddService      =   PCX504, 2, PCX504.Service, common.AddEventLog



[PCX504_a.ndi]
AddReg          =   NDI3, COMMON, DATARATE_a, SSID, RADIONAME_a, BUSCARDBUS, DEVID_a
CopyFiles       =   CopyCoInst_9x,CopySys_9x,CopyFW_a_9x



[DEVID_b]
HKR,Ndi,DeviceID,,"PCI\VEN_14B9&DEV_A504"



[DEVID_a]
HKR,Ndi,DeviceID,,"PCI\VEN_14B9&DEV_A505"



[NDI5]
HKR,Ndi,Service,0,"PCX504"
HKR,Ndi\Interfaces,DefUpper,0,"ndis5"
HKR,Ndi\Interfaces,DefLower,0,"ethernet"
HKR,Ndi\Interfaces,UpperRange,0,"ndis5"
HKR,Ndi\Interfaces,LowerRange,0,"ethernet"
HKR,,MediaDisconnectDamper,,"10"
HKR,,AdapterType,,"1"



[NDI5_ME]
HKR,Ndi,Service,0,"PCX504"
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,PCX504.sys
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"
;
; NDIS Info
;
HKR,NDIS,LogDriverName,,"PCX504"
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
;
; Interfaces
;
HKR,Ndi\Interfaces,DefUpper,,"ndis5"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis5"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,,AdapterType,,1
; Co-installer
HKR,Ndi,NdiInstaller,0,"CINST16.DLL,CiscoNdiProc"



[NDI3]
HKR,,PnPCapabilities,0x10001,0x138
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,PCX504.sys
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"
;
; NDIS Info
;
HKR,NDIS,LogDriverName,,"PCX504"
HKR,NDIS,MajorNdisVersion,1,03
HKR,NDIS,MinorNdisVersion,1,0A
;
; Interfaces
;
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,,AdapterType,,1
; Co-installer
HKR,Ndi,NdiInstaller,0,"CINST16.DLL,CiscoNdiProc"



[BUSPCI]
HKR,,FormFactor,,"PCI"



[BUSCARDBUS]
HKR,,FormFactor,,"CARDBUS"



[COMMON]
HKR,,NodeName,2,""
HKR,NDI\params\NodeName,ParamDesc,,%ClientName%
HKR,NDI\params\NodeName,flag,1,30,00,00,00
HKR,NDI\params\NodeName,type,,"edit"
HKR,NDI\params\NodeName,LimitText,,"16"
HKR,NDI\params\NodeName,default,2,""
HKR,NDI\params\NodeName,optional,0,"1"

HKR,,InfrastructureMode,2,"1"
HKR,NDI\params\InfrastructureMode,ParamDesc,,%InfraMode%
HKR,NDI\params\InfrastructureMode,flag,1,30,00,00,00
HKR,NDI\params\InfrastructureMode,type,,"enum"
HKR,NDI\params\InfrastructureMode,default,,"1" 
HKR,NDI\params\InfrastructureMode\enum,0,0,%No%
HKR,NDI\params\InfrastructureMode\enum,1,0,%Yes%

HKR,,PowerSaveMode,2,"0"
HKR,NDI\params\PowerSaveMode,ParamDesc,,%PSP%
HKR,NDI\params\PowerSaveMode,flag,1,30,00,00,00
HKR,NDI\params\PowerSaveMode,type,,"enum"
HKR,NDI\params\PowerSaveMode,default,,"0" 
HKR,NDI\params\PowerSaveMode\enum,0,,%CAM%
HKR,NDI\params\PowerSaveMode\enum,2,,%PSP-CAM%
HKR,NDI\params\PowerSaveMode\enum,3,,%MAXPSP%


[SSID]
HKR,, SSID1,2,""
HKR,NDI\params\SSID1,ParamDesc,0,"SSID"
HKR,NDI\params\SSID1,type,0,"edit"
HKR,NDI\params\SSID1,flag,1,30,0,0,0
HKR,NDI\params\SSID1,optional,0,"1"
HKR,NDI\params\SSID1,default,2,""



[DATARATE_b]
;
; 2.4 GHz data rates
;
HKR,,SupportedRates,2,"0"
HKR,NDI\params\SupportedRates,ParamDesc,,%DataRates%    
HKR,NDI\params\SupportedRates,flag,1,30,00,00,00
HKR,NDI\params\SupportedRates,type,,"enum"
HKR,NDI\params\SupportedRates,default,,"0" 
HKR,NDI\params\SupportedRates\enum,0,,%Auto%            
HKR,NDI\params\SupportedRates\enum,2,,%1Mb%                 
HKR,NDI\params\SupportedRates\enum,4,,%2Mb%         
HKR,NDI\params\SupportedRates\enum,B,,%5Mb%         
HKR,NDI\params\SupportedRates\enum,16,,%11Mb%       
HKR,NDI\params\SupportedRates,base,0,"16"



[DATARATE_a]
;
; 5 GHz data rates
;
HKR,,SupportedRates,2,"0"
HKR,NDI\params\SupportedRates,ParamDesc,,%DataRates%    
HKR,NDI\params\SupportedRates,flag,1,30,00,00,00
HKR,NDI\params\SupportedRates,type,,"enum"
HKR,NDI\params\SupportedRates,default,,"0" 
HKR,NDI\params\SupportedRates\enum,0,,%Auto%            
HKR,NDI\params\SupportedRates\enum,C,,%6Mb%                 
HKR,NDI\params\SupportedRates\enum,12,,%9Mb%                 
HKR,NDI\params\SupportedRates\enum,18,,%12Mb%                 
HKR,NDI\params\SupportedRates\enum,24,,%18Mb%                 
HKR,NDI\params\SupportedRates\enum,30,,%24Mb%                 
HKR,NDI\params\SupportedRates\enum,48,,%36Mb%                 
HKR,NDI\params\SupportedRates\enum,60,,%48Mb%                 
HKR,NDI\params\SupportedRates\enum,6C,,%54Mb%                 
HKR,NDI\params\SupportedRates,base,0,"16"



[RADIONAME_b] 
HKR,,RadioName,,"PCX504"



[RADIONAME_a] 
HKR,,RadioName,,"PCX5045G"



[PCX504.Service]
DisplayName     = %PCX504.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\PCX504.sys
LoadOrderGroup  = NDIS



[CoInstaller.NT.AddReg]
HKR,,CoInstallers32,0x00010000,"CInsX500.dll,CiscoX500CoInstaller"



[common.AddEventLog]
AddReg = common.AddEventLog.reg



[common.AddEventLog.reg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\netevent.dll"
HKR,,TypesSupported,0x00010001,7



[CopySys_NT]
PCX504.sys,,,2



[CopySys_XP]
PCX504.sys,pcx504.51,,2



[CopyFW_b_NT]
pcx504b.img



[CopyFW_a_NT]
pcx504a.img



[CopySys_9x]
PCX504.sys,,,2
vxdX500.vxd,,,2



[CopyFW_a_9x]
pcx504a.img



[CopyFW_b_9x]
pcx504b.img



[CopyCoInst_NT]
CInsX500.dll,,,2



[CopyCoInst_9x]
CUtil16.exe,,,2
CInst16.dll,,,2



[strings]
V_CISCO                     = "Cisco"
ClientName                  = "Client Name"
InfraMode                   = "Infrastructure Mode"
No                          = "No"
Yes                         = "Yes"
Disabled                    = "Disabled"
Enabled                     = "Enabled"
PSP                         = "Power Saving Mode(PSP)"
CAM                         = "CAM"
PSP-CAM                     = "PSP-CAM (FASTPSP)"
MAXPSP                      = "Max Power Save/PSP"
DataRates                   = "Data Rates"
Auto                        = "Auto"
;
; 802.11b -- 2.4 GHz data rates
;
1Mb                         = " 1 Mb"            
2Mb                         = " 2 Mb"
5Mb                         = " 5.5 Mb"
11Mb                        = "11 Mb"
;
; 802.11a -- 5.0 GHz data rates
;
6Mb                         = " 6 Mb"
9Mb                         = " 9 Mb"
12Mb                        = "12 Mb"
18Mb                        = "18 Mb"
24Mb                        = "24 Mb"
36Mb                        = "36 Mb"
48Mb                        = "48 Mb"
54Mb                        = "54 Mb"
;
; descriptions
;
Disk_1_Desc                 = "Cisco Systems Wireless LAN Adapter Installation Disk"
PCX504.Service.DispName     = "Cisco Systems Wireless LAN Adapter Driver"
PCX504_b.DevDesc            = "Cisco Systems PCI Wireless LAN Adapter"
PCX504_a.DevDesc            = "Cisco Systems AIR-CB20A 802.11a Wireless LAN Adapter"
