;''''''''''''''''''''''''''''''''''''''''''''''''''''''''''''''''''''''''''''''
; WN-B11/PCMx Setup File
; File Name : WNPCMX.INF
; Operating System : Windows 95 / 98 / 98SE / Me / 2000 / XP
; Platform Type : PC98-NX Series, DOS/V
; Copyright (C) 2002 I-O DATA DEVICE,INC.
;,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,

[Version]
 DriverVer = 01/17/2002, 1.7.37
 Signature           = "$Chicago$"
 Compatible          = 1
 Class               = Net
 ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
 Provider            = %VER_VENDOR_STR%
;CatalogFile         = WNPCMX.CAT
 MillenniumPreferred = .ME

[ControlFlags]
;Exclude all PNP adapters from user selection
 ExcludeFromSelect   = PCMCIA\IO_DATA-WNB11PCMH-E412	;I-O DATA WN-B11/PCMH
 ExcludeFromSelect   = PCMCIA\IO_DATA-WNB11PCM-9DE7	;I-O DATA WN-B11/PCM

[Manufacturer]
 %VER_VENDOR_NAME_STR% = DeviceList

[DeviceList]
 %PRISM_PCMCIA1_STR% = PRISM_PCMCIA1, PCMCIA\IO_DATA-WNB11PCMH-E412
 %PRISM_PCMCIA2_STR% = PRISM_PCMCIA2, PCMCIA\IO_DATA-WNB11PCM-9DE7

;==========================================
[PRISM_PCMCIA1]         ; Win9x
 AddReg         = PRISM_PCMCIA1.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy

[PRISM_PCMCIA1.ME]      ; WinMe
 AddReg         = PRISM_PCMCIA1.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME

[PRISM_PCMCIA1.ME.ME]   ; WinMe - Same as .ME (Needed for Update Driver)
 AddReg         = PRISM_PCMCIA1.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME

[PRISM_PCMCIA1.NT]      ; Win2k
 AddReg         = PRISM_PCMCIA1.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
 BusType        = 8     ; PCMCIA
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_PCMCIA1.NT.Services]
 AddService     = "PRISM", 2, PRISM1_DRIVER.Service, PRISM_DRIVER.EventLog

[PRISM_PCMCIA1.NT.CoInstallers]
 CopyFiles      = PRISM_COINSTALL.copy.NT
 AddReg         = PRISM_COINSTALL.reg.NT

[PRISM_PCMCIA1.reg]
 HKR,Ndi        ,DeviceID,0,"PCMCIA\IO_DATA-WNB11PCMH-E412"

;==========================================
[PRISM_PCMCIA2]         ; Win9x
 AddReg         = PRISM_PCMCIA2.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy

[PRISM_PCMCIA2.ME]      ; WinMe
 AddReg         = PRISM_PCMCIA2.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME

[PRISM_PCMCIA2.ME.ME]   ; WinMe - Same as .ME (Needed for Update Driver)
 AddReg         = PRISM_PCMCIA2.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME

[PRISM_PCMCIA2.NT]      ; Win2k
 AddReg         = PRISM_PCMCIA2.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
 BusType        = 8     ; PCMCIA
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_PCMCIA2.NT.Services]
 AddService     = "PRISM", 2, PRISM2_DRIVER.Service, PRISM_DRIVER.EventLog

[PRISM_PCMCIA2.NT.CoInstallers]
 CopyFiles      = PRISM_COINSTALL.copy.NT
 AddReg         = PRISM_COINSTALL.reg.NT

[PRISM_PCMCIA2.reg]
 HKR,Ndi        ,DeviceID,0,"PCMCIA\IO_DATA-WNB11PCM-9DE7"


;###############################################################################

[PRISM_COINSTALL.reg.NT]
; HKR,           ,CoInstallers32         ,0x00010000     ,"PRISMCFG.cpl,NdiProc"

[PRISM1_DRIVER.Service]
 DisplayName    = %PRISM1_SERVICE_DISPLAY%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\PRISMNDS.sys
 LoadOrderGroup = NDIS

[PRISM2_DRIVER.Service]
 DisplayName    = %PRISM2_SERVICE_DISPLAY%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\PRISMNDS.sys
 LoadOrderGroup = NDIS

[PRISM_DRIVER.EventLog]
 AddReg         = PRISM_DRIVER.EventLog.reg

[PRISM_DRIVER.EventLog.reg]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

;###############################################################################
[COMMON_PCMCIA.reg]
;RegKey,SubKey          ,Name                   ,Type   ,Value
;-------------          -----                   -----   ------
 HKR,NDI                ,Service                ,0      ,"PRISM"
 HKR,NDI                ,CardType               ,0      ,"PCMCIA"
 HKR,                   ,BusType                ,0      ,"8"
 HKR,                   ,DeviceVxDs             ,0      ,"PRISMNDS.sys"
 HKR,                   ,EnableIRQSharing       ,1      ,01,00,00,00
 HKR,                   ,IOBaseAddress          ,1      ,02,00,00,00
 HKR,                   ,InterruptNumber        ,1      ,04,00,00,00

[COMMON_NDIS.reg]
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
; HKR,NDI                ,NdiInstaller           ,0      ,"PRISMCFG.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"PRISM"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

 HKR,defaults,PSMode,0,1
 HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode,optional,0,1

[COMMON_NDIS.reg.ME]
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
; HKR,NDI                ,NdiInstaller           ,0      ,"PRISMCFG.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"PRISM"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

 HKR,defaults,PSMode,0,1
 HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode,optional,0,1

[COMMON_NDIS.reg.NT]
; HKR,                   ,EnumPropPages32        ,0      ,"PRISMCFG.cpl,NetPropPageProvider"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

 HKR,defaults,PSMode,0,1
 HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode\enum,3,,"Auto Enable"
 HKR,NDI\params\PSMode,optional,0,1

[COMMON.reg]
 HKR,                   ,PRISMIOC               ,0      ,"1"
 HKR,                   ,SilentInstall          ,0      ,"1"
;Uncomment the line above to install without user interface prompts

 HKR,defaults,ListenInterval,0,3
 HKR,NDI\params\ListenInterval,,0,3
 HKR,Ndi\params\ListenInterval,default,0,3
 HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
 HKR,NDI\params\ListenInterval,type,,int
 HKR,NDI\params\ListenInterval,flag,1,30,00,00,00
 HKR,NDI\params\ListenInterval,min,0,0
 HKR,NDI\params\ListenInterval,max,0,77
 HKR,NDI\params\ListenInterval,step,0,1
 HKR,NDI\params\ListenInterval,optional,0,1

 HKR,defaults,RTSThresh,0,2432
 HKR,NDI\params\RTSThresh,,0,2432
 HKR,Ndi\params\RTSThresh,default,0,2432
 HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
 HKR,NDI\params\RTSThresh,type,0,int
 HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
 HKR,NDI\params\RTSThresh,min,0,0
 HKR,NDI\params\RTSThresh,max,0,2432
 HKR,NDI\params\RTSThresh,step,0,64
 HKR,NDI\params\RTSThresh,optional,0,1

 HKR,defaults,FragThresh,0,2432
 HKR,NDI\params\FragThresh,,0,2432
 HKR,Ndi\params\FragThresh,default,0,2432
 HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
 HKR,NDI\params\FragThresh,type,0,int
 HKR,NDI\params\FragThresh,flag,1,20,00,00,00
 HKR,NDI\params\FragThresh,min,0,256
 HKR,NDI\params\FragThresh,max,0,2432
 HKR,NDI\params\FragThresh,step,0,128
 HKR,NDI\params\FragThresh,optional,0,1

 HKR,defaults,PreambleMode,0,1
 HKR,NDI\params\PreambleMode,,0,1
 HKR,Ndi\params\PreambleMode,default,0,1
 HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
 HKR,NDI\params\PreambleMode,type,,enum
 HKR,NDI\params\PreambleMode,flag,1,30,00,00,00
 HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
 HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
 HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
 HKR,NDI\params\PreambleMode,optional,0,1

 HKR,defaults,AuthentAlg,0,65535
 HKR,NDI\params\AuthentAlg,,0,65535
 HKR,NDI\params\AuthentAlg,default,0,65535
 HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
 HKR,NDI\params\AuthentAlg,type,,enum
 HKR,NDI\params\AuthentAlg,flag,1,30,00,00,00
 HKR,NDI\params\AuthentAlg\enum,1,,"WECA Compliant (always use Open)"
 HKR,NDI\params\AuthentAlg\enum,2,,"Must use Shared with WEP"
 HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
 HKR,NDI\params\AuthentAlg,optional,0,1

; HKR,defaults,AdhocDemoMode,0,0
; HKR,NDI\params\AdhocDemoMode,,0,0
; HKR,Ndi\params\AdhocDemoMode,default,0,0
; HKR,NDI\params\AdhocDemoMode,ParamDesc,,%ADHOC_DEMO_STR%
; HKR,NDI\params\AdhocDemoMode,type,,enum
; HKR,NDI\params\AdhocDemoMode,flag,1,30,00,00,00
; HKR,NDI\params\AdhocDemoMode\enum,0,,"Disable"
; HKR,NDI\params\AdhocDemoMode\enum,1,,"Enable"
; HKR,NDI\params\AdhocDemoMode,optional,0,1

;###############################################################################
[DestinationDirs]
;CopyFiles Section      = Destination Directory ID -- see layout.inf
;-----------------        ------------------------
 DefaultDestDir         = 11 ; Win9x=%windir%\system Win2k=%windir%\system32
 PRISM_DRIVER.copy      = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.ME   = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.NT   = 12 ; Win2k=%windir%\system32\drivers

[PRISM_NDI.copy]
 PRISMR16.dll           ; Win9x NDI
 PRISMCFG.dll           ; Win9x NDI

[PRISM_NDI.copy.ME]
 PRISMR16.dll           ; Win9x NDI
 PRISMCFG.dll           ; Win9x NDI

[PRISM_COINSTALL.copy.NT]
 PRISMRES.dll
 PRISMIOC.dll

[PRISM_DRIVER.copy]
 PRISMNDS.sys
 PRISMIOC.vxd           ; Win9x Ioctl interface

[PRISM_DRIVER.copy.ME]
 PRISMNDS.sys
 PRISMIOC.vxd           ; Win9x Ioctl interface

[PRISM_DRIVER.copy.NT]
 PRISMNDS.sys

[PRISM_APPLET.copy]
 PRISMRES.dll
 PRISMIOC.dll

[PRISM_APPLET.copy.ME]
 PRISMRES.dll
 PRISMIOC.dll

[PRISM_APPLET.copy.NT]

[SourceDisksNames]
;Source Disk ID         = Disk Name
;--------------           ---------
 1                      = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]      ; Win9x
;File Name              = Source Disk ID
;---------                --------------
 PRISMR16.dll           = 1
 PRISMCFG.dll           = 1
 PRISMIOC.vxd           = 1
 PRISMRES.dll           = 1
 PRISMIOC.dll           = 1
 PRISMNDS.sys           = 1

[SourceDisksFiles.ME]   ; WinMe
 PRISMR16.dll           = 1
 PRISMCFG.dll           = 1
 PRISMIOC.vxd           = 1
 PRISMRES.dll           = 1
 PRISMIOC.dll           = 1
 PRISMNDS.sys           = 1

[SourceDisksFiles.X86]  ; Win2k/Xp
 PRISMRES.dll           = 1
 PRISMIOC.dll           = 1
 PRISMNDS.sys           = 1

;###############################################################################
[Strings]
;String ID              = String Text
;---------                -----------
 VER_VENDOR_STR         = "I-O DATA"
 VER_VENDOR_NAME_STR    = "I-O DATA DEVICE,INC."

 PRISM_PCMCIA1_STR      = "I-O DATA WN-B11/PCMH Ethernet Adapter"
 PRISM_PCMCIA2_STR      = "I-O DATA WN-B11/PCM Ethernet Adapter"

 PRISM1_SERVICE_DISPLAY = "I-O DATA WN-B11/PCMH Ethernet Adapter Driver"
 PRISM2_SERVICE_DISPLAY = "I-O DATA WN-B11/PCM Ethernet Adapter Driver"
 INSTALL_DISK_STR       = "I-O DATA WN-B11/PCMx Support Software"

; ADHOC_DEMO_STR         = "Adhoc Demo Mode"
 SHORT_PREAM_STR        = "Preamble Mode"
 RTSTHRESH_STR          = "RTS Threshold"
 FRAGTHRESH_STR         = "Fragmentation Threshold"
 AUTHENT_TYPE_STR       = "Authentication Algorithm"
 LISTENINTERVAL_STR     = "Listen Interval"
 POWER_SAVE_STR         = "Power Save Mode"
 POWER_LEVEL_STR        = "Power Save Level"

