;; NETRTS5.INF (NT 5.0 & Win98 combined inf for NDIS5 driver)
;;
;; TP-Link TF-5239 Cardbus Fast Ethernet Network Interface Cards.
;;
;; Copyright 1996-1999, TP-Link Corporation
;;
;; .this release is primarily for motherboard OEM for WHQL test.

[version]
Signature   = "$Chicago$"
Compatible  = 1
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Realtek%                                 ;;
CatalogFile = netrts5.cat                               ;; for WHQL certified
DriverVer   = 08/04/2000,5.378.0804.2000

[Manufacturer]
%Realtek%   = Realtek

[ControlFlags]
ExcludeFromSelect     = PCI\VEN_10EC&DEV_8139

[Realtek]
%RTL8139.DeviceDesc%  = RTL8139.ndi, PCI\VEN_10EC&DEV_8139



;;****************************************************************************
;; Windows 9x
;;****************************************************************************
[rtl8139.ndi]
DriverVer       = 5/23/2000,376
AddReg          = rtl8139.id.reg, RTL8139.common.reg, RTL8139.win.reg, RTL8139.oncbs.reg
CopyFiles       = RTL8139.CopyFiles98
;DeviceID        = "PCI\VEN_10EC&DEV_8139"
;LogConfig       = DefaultConfig


;;****************************************************************************
;; NT 5.0
;;****************************************************************************
[RTL8139.ndi.NT]
AddReg          = RTL8139.common.reg, RTL8139.reg, RTL8139.oncbs.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTL8139.CopyFiles

[RTL8139.ndi.NT.Services]
AddService = rtl8139, 2, rtsnt.Service, RTL8139.EventLog



[RTL8139.CopyFiles]
RTL8139.sys,,,2

[RTL8139.CopyFiles98]
RTL8139.sys,,,2

;;----------------------------------------------------------------------------
;; RTL8139 Parameters
;;----------------------------------------------------------------------------
;;***************************************************************************
;; Windows 9x parameters
;;***************************************************************************
[rtl8139.id.reg]
HKR, Ndi,       DeviceID,       0,      "PCI\VEN_10EC&DEV_8139"

HKR, Ndi\Install,                       ,       0,      rtsnt.install
HKR, NDI\Params\DuplexMode,             flag,   1,      30, 00, 00, 00
HKR, Ndi\Params\EarlyTxThreshold,       flag,   1,      20, 00, 00, 00
HKR, NDI\Params\NetworkAddress,         flag,   1,      30, 00, 00, 00
HKR, NDI\Params\WakeUpFrame,            flag,   1,      30, 00, 00, 00

[RTL8139.win.reg]
;; key,subkey,valuname,type,value
HKR, ,  DriverDesc,     0,      "TP-Link TF-5239 Cardbus Fast Ethernet NIC"
HKR, ,  DevLoader,      0,      *ndis
HKR, ,  DeviceVxDs,     0,      rtl8139.sys
HKR, ,  EnumPropPages,  0,      netdi.dll,      EnumPropPages

;;params
HKR, ,  MediaType,      0,      1
HKR, ,  AdapterType,    0,      5
HKR, ,  BusType,        0,      5

;; NDIS Info
HKR, NDIS,              MajorNdisVersion,       1,      03
HKR, NDIS,              MinorNdisVersion,       1,      0a
HKR, NDIS,              LogDriverName,          0,      "TF-5239"

;; Interfaces
HKR, Ndi\Interfaces,    DefLower,               ,       "ethernet"
HKR, Ndi\Interfaces,    LowerRange,             ,       "ethernet"
HKR, Ndi\Interfaces,    DefUpper,               ,       "ndis3"
HKR, Ndi\Interfaces,    UpperRange,             ,       "ndis3"

;; Install sections
HKR, Ndi\Install,       ndis3,                  0,      "rtl139.ndis5"

;;****************************************************************************
;; RTL8139 common parameters
;;****************************************************************************
[RTL8139.oncbs.reg]
HKR,,ChipOnCardbus,,"0"

[RTL8139.common.reg]
HKR, Ndi\params\DuplexMode,      ParamDesc, 0, %DuplexMode%
HKR, Ndi\params\DuplexMode,      type,      0, "enum"
HKR, Ndi\params\DuplexMode,      default,   0, "1"
HKR, Ndi\params\DuplexMode\enum, 1,         0, %dmAutoMode%
HKR, Ndi\params\DuplexMode\enum, 2,         0, %dm10HalfMode%
HKR, Ndi\params\DuplexMode\enum, 3,         0, %dm10FullMode%
HKR, Ndi\params\DuplexMode\enum, 4,         0, %dm100HalfMode%
HKR, Ndi\params\DuplexMode\enum, 5,         0, %dm100FullMode%

HKR,Ndi\Params\EarlyTxThreshold, ParamDesc, 0, %EarlyTxThreshold%
HKR,Ndi\Params\EarlyTxThreshold, Type,      0, "int"
HKR,Ndi\Params\EarlyTxThreshold, Default,   0, "38"
HKR,Ndi\Params\EarlyTxThreshold, Min,       0, "0"
HKR,Ndi\Params\EarlyTxThreshold, Max,       0, "63"
HKR,Ndi\Params\EarlyTxThreshold, Step,      0, "1"
HKR,Ndi\Params\EarlyTxThreshold, Base,      0, "10"

HKR,Ndi\params\NetworkAddress,   ParamDesc, 0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,   type,      0, "edit"
HKR,Ndi\params\NetworkAddress,   default,   0, "000000000000"
HKR,Ndi\params\NetworkAddress,   LimitText, 0, "12"
HKR,Ndi\params\NetworkAddress,   UpperCase, 0, "1"
HKR,Ndi\params\NetworkAddress,   Optional,  0, "1"

;HKR,NDI\Params\TxMaxDMABurst,flag,1,30,00,00,00
;HKR,Ndi\params\TxMaxDMABurst,ParamDesc,0,"Transmit DMA burst size"
;HKR,Ndi\params\TxMaxDMABurst,type,0,enum
;HKR,Ndi\params\TxMaxDMABurst,default,0,6
;HKR,Ndi\params\TxMaxDMABurst\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,7,0,"7:2048 bytes"

;HKR,NDI\Params\RxMaxDMABurst,flag,1,30,00,00,00
;HKR,Ndi\params\RxMaxDMABurst,ParamDesc,0,"Receive DMA burst size"
;HKR,Ndi\params\RxMaxDMABurst,type,0,enum
;HKR,Ndi\params\RxMaxDMABurst,default,0,6
;HKR,Ndi\params\RxMaxDMABurst\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,7,0,"7:unlimitted"

;HKR,NDI\Params\EarlyRxThreshold,flag,1,30,00,00,00
;HKR,Ndi\params\EarlyRxThreshold,ParamDesc,0,"Receive FIFO threshold"
;HKR,Ndi\params\EarlyRxThreshold,type,0,enum
;HKR,Ndi\params\EarlyRxThreshold,default,0,2
;HKR,Ndi\params\EarlyRxThreshold\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,7,0,"7:No threshold"

;HKR,NDI\Params\TxInterFrameGap,flag,1,30,00,00,00
;HKR,Ndi\params\TxInterFrameGap,ParamDesc,0,"Tx IFG(10M/100M)"
;HKR,Ndi\params\TxInterFrameGap,type,0,enum
;HKR,Ndi\params\TxInterFrameGap,default,0,3
;HKR,Ndi\params\TxInterFrameGap\enum,0,0,"8.4us/840ns"
;HKR,Ndi\params\TxInterFrameGap\enum,1,0,"8.8us/880ns"
;HKR,Ndi\params\TxInterFrameGap\enum,2,0,"9.2us/920ns"
;HKR,Ndi\params\TxInterFrameGap\enum,3,0,"9.6us/960ns"

HKR, Ndi\params\WakeUpFrame,       ParamDesc,  0, "WakeUp Frame"
HKR, Ndi\params\WakeUpFrame,       default,    0, "0"
HKR, Ndi\params\WakeUpFrame,       type,       0, "enum"
HKR, Ndi\params\WakeUpFrame\enum,  "0",        0, "Enable"
HKR, Ndi\params\WakeUpFrame\enum,  "1",        0, "Disable"

HKR, Ndi\params\PME,               ParamDesc,  0, "APM Mode WakeUp"
HKR, Ndi\params\PME,               default,    0, "1"
HKR, Ndi\params\PME,               type,       0, "enum"
HKR, Ndi\params\PME\enum,          "0",        0, "Enable"
HKR, Ndi\params\PME\enum,          "1",        0, "Disable"

HKR, Ndi\params\EnableLDPS,        ParamDesc,  0, "Link Down Power Saving"
HKR, Ndi\params\EnableLDPS,        default,    0, "0"
HKR, Ndi\params\EnableLDPS,        type,       0, "enum"
HKR, Ndi\params\EnableLDPS\enum,   "0",        0, "Disable"
HKR, Ndi\params\EnableLDPS\enum,   "1",        0, "Enable"


;;****************************************************************************
;; NT 5.0 parameters
;;****************************************************************************
[RTL8139.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "TF-5239"

[rtsnt.Service]
DisplayName     = %RTL8139.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\RTL8139.SYS
LoadOrderGroup  = NDIS

[RTL8139.EventLog]
Addreg = RTL8139.AddEventLog.reg

[RTL8139.AddEventLog.reg]
HKR,    ,   EventMessageFile,   0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR,    ,   TypesSupported,     0x00010001, 7

;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
RTL8139.CopyFiles           = 12
RTL8139.CopyFiles98         = 11
DefaultDestDir              = 11        ; LDID_SYS

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
rtl8139.sys  = 1
;netrts5.inf  = 1
netrts5.cat  = 1

;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
;Msft                      = "Microsoft"
Realtek                   = "TP-Link"

;;Source disk name
DISKNAME = " TP-Link TF-5239 Cardbus Fast Ethernet NIC Driver Disk "

NetworkAddress            = "Network Address"
EarlyTxThreshold          = "Early Tx Threshold"
DuplexMode                = "Link Speed/Duplex Mode"
dmAutoMode                = "Auto Mode"
dm10HalfMode              = "10 Half Mode"
dm10FullMode              = "10 Full Mode"
dm100HalfMode             = "100 Half Mode"
dm100FullMode             = "100 Full Mode"

RTL8139.DeviceDesc        = "TP-Link TF-5239 Cardbus Fast Ethernet NIC"
RTL8139.Service.DispName  = "TP-Link TF-5239 Cardbus Fast Ethernet NIC NT Driver"

;
