
          DigitalChina DCN-530TX Fast Ethernet Adapter
               NetWare Server Driver Installation

  Contents:
  ---------

  (A) Driver Installation for NetWare Server 3.1x, 4.x, 5.x
  (B) Parameters Description for DCNODI.LAN

(A) Driver Installation for NetWare Server 3.1x, 4.x, 5.x
================================================================
   A.1 Driver Installation for NetWare Server 3.12

   1. Insert Driver Disk in your PC's floppy drive(A: or B:).
   2. Change to the NetWare Server directory
      for example:

        CD C:\SERVER.312

   3. Copy the following files from Driver Disk to the NetWare
      Server directory.

      X:\NETWARE\SERVER\3.12\NBI31X.NLM
      X:\NETWARE\SERVER\3.12\MSM31X.NLM
      X:\NETWARE\SERVER\ETHERTSM.NLM
      X:\NETWARE\SERVER\DCNODI.LAN

      Notice: X: means the floppy drive containing the driver,
              such as: A:, or B: etc.

   4. Sample AUTOEXEC.NCF for NetWare Server 3.12

             AUTOEXEC.NCF
             ============
                LOAD C:NBI31X
                LOAD C:MSM31X
                LOAD C:ETHERTSM
                LOAD C:DCNODI FRAME=ETHERNET_802.2 NAME=E_8022
                LOAD C:DCNODI FRAME=ETHERNET_802.3 NAME=E_8023
                LOAD C:DCNODI FRAME=ETHERNET_II NAME=E_II
                LOAD C:DCNODI FRAME=ETHERNET_SNAP NAME=E_SNAP
                BIND IPX E_8022 NET=10
                BIND IPX E_8023 NET=20
                BIND IPX E_II   NET=30
                BIND IPX E_SNAP NET=40

   A.2 Driver Installation for NetWare Server 4.X

   1. Copy the following files from the Driver Diskette to the
      NetWare Server directory.

      X:\NETWARE\SERVER\4.X\MSM.NLM
      X:\NETWARE\SERVER\ETHERTSM.NLM

      Notice: X: means the floppy drive containing the driver,
              such as: A:, or B: etc.

   2. Change to NetWare Server directory
      for example:
      
            CD C:\NWSERVER

   3. Load the NetWare Server System by typing SERVER,
      then press <Enter>.
      
   4. When the Server prompt appears, load the NetWare Server
      Installation Utility.  That is,

      :LOAD INSTALL

   5. Select "Driver options" from the "Installtion Options"
      menu, then press <Enter>.

   6. Select "Configure network drivers" from the "Driver
      Options" menu, then press <Enter>.
      
   7. Select "Select a driver" from the "Additional Driver
      Actions" menu, then press <Enter>.

   8. Press <Ins> to install a unlisted driver, then press <F3>
      to specify a different path.

   9. Insert Driver Diskette in your PC's floppy drive and
      specify the path X:\NETWARE\SERVER.

      Notice: X: means the floppy drive containing the driver,
              such as: A:, or B: etc.

  10. Select "DigitalChina DCN-530TX Fast Ethernet Adapter" from
      the "Select a driver to install:" menu, then press <Enter>.

  11. If necessary, select "Select/Modify driver parameters and
      protocols" from the "Board DCNODI_1(Driver DCNODI)
      Actions" menu, then press <Enter> to set up the driver
      parameters.
      
      Notice: Please refer to content (B) for detail. 

      Otherwise, select "Save parameters and load driver",
      then press <Enter>.

   12. Follow instructions to complete driver installation.

   13. Sample AUTOEXEC.NCF for NetWare Server 4.X

             AUTOEXEC.NCF (one board)
             ========================
              LOAD C:DCNODI FRAME=ETHERNET_802.2 NAME=E_8022
              LOAD C:DCNODI FRAME=ETHERNET_802.3 NAME=E_8023
              LOAD C:DCNODI FRAME=ETHERNET_II NAME=E_II
              LOAD C:DCNODI FRAME=ETHERNET_SNAP NAME=E_SNAP
              BIND IPX E_8022 NET=10
              BIND IPX E_8023 NET=20
              BIND IPX E_II   NET=30
              BIND IPX E_SNAP NET=40

             AUTOEXEC.NCF (two boards)
             =========================
              LOAD C:DCNODI PCI_SLOT=3 FRAME=ETHERNET_802.2 NAME=E_8022_1
              LOAD C:DCNODI PCI_SLOT=3 FRAME=ETHERNET_802.3 NAME=E_8023_1
              LOAD C:DCNODI PCI_SLOT=3 FRAME=ETHERNET_II NAME=E_II_1
              LOAD C:DCNODI PCI_SLOT=3 FRAME=ETHERNET_SNAP NAME=E_SNAP_1
              LOAD C:DCNODI PCI_SLOT=4 FRAME=ETHERNET_802.2 NAME=E_8022_2
              LOAD C:DCNODI PCI_SLOT=4 FRAME=ETHERNET_802.3 NAME=E_8023_2
              LOAD C:DCNODI PCI_SLOT=4 FRAME=ETHERNET_II NAME=E_II_2
              LOAD C:DCNODI PCI_SLOT=4 FRAME=ETHERNET_SNAP NAME=E_SNAP_2
              BIND IPX E_8022_1 NET=10
              BIND IPX E_8023_1 NET=20
              BIND IPX E_II_1   NET=30
              BIND IPX E_SNAP_1 NET=40
              BIND IPX E_8022_2 NET=50
              BIND IPX E_8023_2 NET=60
              BIND IPX E_II_2   NET=70
              BIND IPX E_SNAP_2 NET=80


   A.3 Driver Installation for NetWare Server 5.X

   1. Change to NetWare Server directory.
      for example:
      
            CD C:\NWSERVER
            
   2. Load the NetWare Server System by typing "SERVER",
      then press <Enter>.
   3. When the Server prompt appears, load the NetWare Server
      Installation Utility.  That is,

            :LOAD NWCONFIG

   4. Select "Driver options" from the "Installtion Options"
      menu, then press <Enter>.
   5. Select "Configure network drivers" from the "Driver
      Options" menu, then press <Enter>.
   6. Select "Select a driver" from the "Additional Driver
      Actions" menu, then press <Enter>.
   7. Press <Ins> to install a unlisted driver, then press
      <F3> to specify a different path.
   8. Insert the Driver Diskette in your PC's floppy drive and
      specify the path X:\NETWARE\SERVER.

      Notice: X: means the floppy drive containing the driver,
              such as: A:, or B: etc.
      
   9. Select "DigitalChina DCN-530TX Fast Ethernet Adapter" from
      the "Select a driver to install:" menu, and press <Enter>.
  10. If necessary, select "Select/Modify driver parameters and
      protocols" from the "Board DCNODI_1 (Driver DCNODI) 
      Actions" menu, then press <Enter> to set up the driver
      parameters.
      
      Notice: Please refer to content (B) for detail. 
            
      Otherwise, select "Save parameters and load driver", then
      press <Enter>.

  11. Follow instructions to complete driver installation.

  12. Sample AUTOEXEC.NCF for NetWare Server 5.X

             AUTOEXEC.NCF (one board)
             ========================
              LOAD C:DCNODI FRAME=ETHERNET_802.2 NAME=E_8022
              LOAD C:DCNODI FRAME=ETHERNET_802.3 NAME=E_8023
              LOAD C:DCNODI FRAME=ETHERNET_II NAME=E_II
              LOAD C:DCNODI FRAME=ETHERNET_SNAP NAME=E_SNAP
              BIND IPX E_8022 NET=10
              BIND IPX E_8023 NET=20
              BIND IPX E_II   NET=30
              BIND IPX E_SNAP NET=40

             AUTOEXEC.NCF (two boards)
             =========================
              LOAD C:DCNODI PCI_SLOT=3 FRAME=ETHERNET_802.2 NAME=E_8022_1
              LOAD C:DCNODI PCI_SLOT=3 FRAME=ETHERNET_802.3 NAME=E_8023_1
              LOAD C:DCNODI PCI_SLOT=3 FRAME=ETHERNET_II NAME=E_II_1
              LOAD C:DCNODI PCI_SLOT=3 FRAME=ETHERNET_SNAP NAME=E_SNAP_1
              LOAD C:DCNODI PCI_SLOT=4 FRAME=ETHERNET_802.2 NAME=E_8022_2
              LOAD C:DCNODI PCI_SLOT=4 FRAME=ETHERNET_802.3 NAME=E_8023_2
              LOAD C:DCNODI PCI_SLOT=4 FRAME=ETHERNET_II NAME=E_II_2
              LOAD C:DCNODI PCI_SLOT=4 FRAME=ETHERNET_SNAP NAME=E_SNAP_2
              BIND IPX E_8022_1 NET=10
              BIND IPX E_8023_1 NET=20
              BIND IPX E_II_1   NET=30
              BIND IPX E_SNAP_1 NET=40
              BIND IPX E_8022_2 NET=50
              BIND IPX E_8023_2 NET=60
              BIND IPX E_II_2   NET=70
              BIND IPX E_SNAP_2 NET=80


(B) Parameters Description for DCNODI.LAN
================================================================
  The following parameters are used in DCNODI.LAN.

    1. SLOT   : specifies which adapter is enabled when multiple
                DCN-530TX adapters are found in your computer.
                The SLOT keyword is an index value corresponding
                to PCI BIOS.  The mapping from SLOT to the
                physical PCI slot is different from one computer
                to another.

                E.g.: LOAD DCNODI SLOT=3 FRAME=ETHERNET_802.2

    2. FRAME  : specifies which frame type is used by the driver.
                Accepted values are Ethernet_802.2,
                Ethernet_802.3, Ethernet_II and Ethernet_SNAP.
                Multiple frame types can be enabled by loading
                the same driver with different FRAME types.

                E.g.: LOAD DCNODI FRAME=ETHERNET_802.2
                      LOAD DCNODI FRAME=ETHERNET_802.3
                      LOAD DCNODI FRAME=ETHERNET_II
                      LOAD DCNODI FRAME=ETHERNET_SNAP

    3. NODE   : Uses a different address to replace the node
                address burned in EEPROM.

                E.g.: LOAD DCNODI NODE=00030FFFFFFF

    4. Medium : Specifies which medium type is used by the
                driver. Accepted vaules are AUTO,10-HD,10-FD,
                100-HD, 100-FD.

                E.g.: LOAD DCNODI FRAME=ETHERNET_802.2 Medium=100-FD
