;; Version 3.100.46.5 for U.S. Robotics Wireless MAXg PC Card and PCI Adapter.
;; USRMAXG.inf support 2000/XP
;;
;; Copyright 1998-2004, Broadcom Corporation.
;; All Rights Reserved.
;;
;; This is UNPUBLISHED PROPRIETARY SOURCE CODE of Broadcom Corporation;
;; the contents of this file may not be disclosed to third parties, copied or
;; duplicated in any form, in whole or in part, without the prior written
;; permission of Broadcom Corporation.
;; 3.100.46.1 Last Modified by USR -TS on 01/14/2005 4:32 PM based on bcmwl5.inf v3.100.46.0 
;; 3.100.46.2 Commented out "USA" to be displayed only "Default" by USR-TS 01/21/05 3:33 PM
;; 3.100.46.3 Removed (tm) from all IBSS by USR-TS 01/21/05 4:43 PM
;; 3.100.46.4 Removed BCM430B/A/M and BCM43pc section and change %REG_SZ% to "REG_SC" USR-TS 02/07/05 4:35 PM.
;; 3.100.46.5 Removed branding string section USR -TS 02/09/05 10:29 AM

[version]
	Signature	= "$Windows NT$"		; Combined Win9x/Win2k inf
	Class=Net
	ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
	Provider	= %V_BCM%
	Compatible	= 1
DriverVer=02/09/2005, 3.100.46.5
	CatalogFile=USRMAXG.CAT

[Manufacturer]
	%V_BCM% = BROADCOM,NTx86.5.1

[ControlFlags] 
	ExcludeFromSelect = *

[BROADCOM.ntx86.5.1]
	%BCM430G_DeviceDesc% = BCM43XG, PCI\VEN_14E4&DEV_4318&SUBSYS_011916EC&REV_02
	%BCM430PCI_DeviceDesc% = BCM43XG, PCI\VEN_14E4&DEV_4318&SUBSYS_011A16EC&REV_02
[BROADCOM]

	%BCM430G_DeviceDesc% = BCM43XG, PCI\VEN_14E4&DEV_4318&SUBSYS_011916EC&REV_02
	%BCM430PCI_DeviceDesc% = BCM43XG, PCI\VEN_14E4&DEV_4318&SUBSYS_011A16EC&REV_02

;-----------------------------------------------------------------
; Win9x specific
;


[BCM43XG]
	AddReg		= BCM43XX.win.reg, BCM43XX.win.brcm.reg, common.reg, g.options.reg, bg.options.reg
	DelReg          = common.delreg, rate.delreg
	CopyFiles	= BCM43XX.sys.files
DriverVer=02/09/2005, 3.100.46.5


[BCM43XX.win.reg]
	HKR,	Ndi,	DeviceID,		,	"PCI\VEN_14E4&DEV_4307"
	; Ndis Info
	HKR,	,		EnumPropPages,		0,	"netdi.dll,EnumPropPages"
	HKR,	NDIS,	MajorNdisVersion,	1,	03
	HKR,	NDIS,	MinorNdisVersion,	1,	0A
	HKR,	NDIS,	LogDriverName,		,	"BCM43XX"
	HKR,	NDIS,	MajorDriverVersion,	1,	1
	HKR,	NDIS,	MinorDriverVersion,	1,	0
	;Install sections
	HKR,	Ndi\Install,	,		,	"BCM43XX.ndi.install"
	; Interfaces
	HKR,	Ndi\Interfaces,	DefUpper,	0,	"ndis3"
	HKR,	Ndi\Interfaces,	DefLower,	0,	"ethernet"
	HKR,	Ndi\Interfaces,	UpperRange,	0,	"ndis3"
	HKR,	Ndi\Interfaces,	LowerRange,	0,	"ethernet"

[BCM43XX.win.brcm.reg]
	HKR,	Ndi,	HelpText,		,	%BCM43XX_HELP%

[BCM43XX.ndi.install]
	AddReg		= BCM43XX.ndi.reg

[BCM43XX.ndi.reg]
	HKR,	,	DevLoader,		0,	"*ndis"
	HKR,	,	DeviceVxDs,		0,	"BCMWL5.SYS"

; Flag = 2 is COPYFLG_NOSKIP (2)
; Flag = 33 is COPYFLG_WARN_IF_SKIP (1) | COPYFLG_NO_VERSION_DIALOG (32)
[BCM43XX.sys.files]
	BCMWL5.SYS,,,2

;-----------------------------------------------------------------
; Win2k specific
;


[BCM43XG.NT]
	Characteristics	= 0x84	; NCF_PHYSICAL | NCF_HAS_UI
	BusType		= 5			; PCI bus
	AddReg		= BCM43XX.reg, BCM43XX.brcm.reg, common.reg, g.options.reg, bg.options.reg
	DelReg          = common.delreg, rate.delreg
	CopyFiles	= BCM43XX.files.NT
DriverVer=02/09/2005, 3.100.46.5

[BCM43XG.NT.Services]
	AddService = BCM43XX, 2, BCM43XX.Service, common.EventLog


[BCM43XX.reg]
	; Ndis Info
	; Interfaces
	HKR,	Ndi\Interfaces,	UpperRange,	,	"ndis5"
	HKR,	Ndi\Interfaces,	LowerRange,	,	"ethernet"

[BCM43XX.brcm.reg]
	HKR,	Ndi,	HelpText,		,	%BCM43XX_HELP%
	HKR,	Ndi,	Service,		0,	"BCM43XX"

[BCM43XX.Service]
	DisplayName	= %BCM43XX_Service_DispName%
	ServiceType	= 1			; %SERVICE_KERNEL_DRIVER%
	StartType	= 3			; %SERVICE_DEMAND_START%
	ErrorControl	= 1			; %SERVICE_ERROR_NORMAL%
	ServiceBinary	= %12%\bcmwl5.sys
	LoadOrderGroup	= NDIS

[common.EventLog]
	AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
	HKR,	,	EventMessageFile,	0x00020000,	"%%SystemRoot%%\System32\netevent.dll"
	HKR,	,	TypesSupported,		0x00010001,	7

[BCM43XX.files.NT]
	BCMWL5.SYS,,,2

;-----------------------------------------------------------------
; Both Win9x & Win2k
;

[common.delreg]
	HKR, Ndi\params\RoamPref
        HKR, Ndi\params\AssocPref
	HKR, Ndi\params\Locale
	HKR,,Locale

[rate.delreg]
	HKR, Ndi\params\Rate
	HKR, Ndi\params\RateA

[common.reg]
	HKR, ,"EnableSoftAP", 0, "0"
	HKR, ,"EnableAutoConnect", 0, "0"
	HKR,	Ndi\params\Country, ParamDesc,	0,	%Location%
	HKR,	Ndi\params\Country, type,		0,	"enum"
;;	HKR,	Ndi\params\Country\enum, "AF",	0,	%Afghanistan%
;;	HKR,	Ndi\params\Country\enum, "AL",	0,	%Albania%
;;	HKR,	Ndi\params\Country\enum, "DZ",	0,	%Algeria%
;;	HKR,	Ndi\params\Country\enum, "AS",	0,	%AmericanSamoa%
;;	HKR,	Ndi\params\Country\enum, "AD",	0,	%Andorra%
;;	HKR,	Ndi\params\Country\enum, "AO",	0,	%Angola%
;;	HKR,	Ndi\params\Country\enum, "AI",	0,	%Anguilla%
;;	HKR,	Ndi\params\Country\enum, "AQ",	0,	%Antarctica%
;	HKR,	Ndi\params\Country\enum, "AG",	0,	%AntiguaandBarbuda%
;	HKR,	Ndi\params\Country\enum, "AR",	0,	%Argentina%
;;	HKR,	Ndi\params\Country\enum, "AM",	0,	%Armenia%
;	HKR,	Ndi\params\Country\enum, "AW",	0,	%Aruba%
;	HKR,	Ndi\params\Country\enum, "AU",	0,	%Australia%
;	HKR,	Ndi\params\Country\enum, "AT",	0,	%Austria%
;;	HKR,	Ndi\params\Country\enum, "AZ",	0,	%Azerbaijan%
;	HKR,	Ndi\params\Country\enum, "BS",	0,	%BahamasThe%
;	HKR,	Ndi\params\Country\enum, "BH",	0,	%Bahrain%
;	HKR,	Ndi\params\Country\enum, "BD",	0,	%Bangladesh%
;	HKR,	Ndi\params\Country\enum, "BB",	0,	%Barbados%
;	HKR,	Ndi\params\Country\enum, "BY",	0,	%Belarus%
;	HKR,	Ndi\params\Country\enum, "BE",	0,	%Belgium%
;;	HKR,	Ndi\params\Country\enum, "BZ",	0,	%Belize%
;;	HKR,	Ndi\params\Country\enum, "BJ",	0,	%Benin%
;	HKR,	Ndi\params\Country\enum, "BM",	0,	%Bermuda%
;;	HKR,	Ndi\params\Country\enum, "BT",	0,	%Bhutan%
;	HKR,	Ndi\params\Country\enum, "BO",	0,	%Bolivia%
;	HKR,	Ndi\params\Country\enum, "BA",	0,	%BosniaandHerzegovina%
;;	HKR,	Ndi\params\Country\enum, "BW",	0,	%Botswana%
;;	HKR,	Ndi\params\Country\enum, "BV",	0,	%BouvetIsland%
;	HKR,	Ndi\params\Country\enum, "BR",	0,	%Brazil%
;;	HKR,	Ndi\params\Country\enum, "IO",	0,	%BritishIndianOceanTerritory%
;	HKR,	Ndi\params\Country\enum, "BN",	0,	%Brunei%
;	HKR,	Ndi\params\Country\enum, "BG",	0,	%Bulgaria%
;;	HKR,	Ndi\params\Country\enum, "BF",	0,	%BurkinaFaso%
;;	HKR,	Ndi\params\Country\enum, "BI",	0,	%Burundi%
;;	HKR,	Ndi\params\Country\enum, "KH",	0,	%Cambodia%
;;	HKR,	Ndi\params\Country\enum, "CM",	0,	%Cameroon%
;	HKR,	Ndi\params\Country\enum, "CA",	0,	%Canada%
;;	HKR,	Ndi\params\Country\enum, "CV",	0,	%CapeVerde%
;	HKR,	Ndi\params\Country\enum, "KY",	0,	%CaymanIslands%
;;	HKR,	Ndi\params\Country\enum, "CF",	0,	%CentralAfricanRepublic%
;;	HKR,	Ndi\params\Country\enum, "TD",	0,	%Chad%
;	HKR,	Ndi\params\Country\enum, "CL",	0,	%Chile%
;	HKR,	Ndi\params\Country\enum, "CN",	0,	%China%
;;	HKR,	Ndi\params\Country\enum, "CX",	0,	%ChristmasIsland%
;;	HKR,	Ndi\params\Country\enum, "CC",	0,	%CocosKeelingIslands%
;	HKR,	Ndi\params\Country\enum, "CO",	0,	%Colombia%
;;	HKR,	Ndi\params\Country\enum, "KM",	0,	%Comoros%
;;	HKR,	Ndi\params\Country\enum, "CD",	0,	%CongoDRC%
;;	HKR,	Ndi\params\Country\enum, "CG",	0,	%Congo%
;;	HKR,	Ndi\params\Country\enum, "CK",	0,	%CookIslands%
;	HKR,	Ndi\params\Country\enum, "CR",	0,	%CostaRica%
;;	HKR,	Ndi\params\Country\enum, "CI",	0,	%CotedIvoire%
;	HKR,	Ndi\params\Country\enum, "HR",	0,	%Croatia%
;;	HKR,	Ndi\params\Country\enum, "CU",	0,	%Cuba%
;	HKR,	Ndi\params\Country\enum, "CY",	0,	%Cyprus%
;	HKR,	Ndi\params\Country\enum, "CZ",	0,	%CzechRepublic%
;	HKR,	Ndi\params\Country\enum, "DK",	0,	%Denmark%
;;	HKR,	Ndi\params\Country\enum, "DJ",	0,	%Djibouti%
;;	HKR,	Ndi\params\Country\enum, "DM",	0,	%Dominica%
;	HKR,	Ndi\params\Country\enum, "DO",	0,	%DominicanRepublic%
;;	HKR,	Ndi\params\Country\enum, "TL",	0,	%EastTimor%
;	HKR,	Ndi\params\Country\enum, "EC",	0,	%Ecuador%
;	HKR,	Ndi\params\Country\enum, "EG",	0,	%Egypt%
;	HKR,	Ndi\params\Country\enum, "SV",	0,	%ElSalvador%
;;	HKR,	Ndi\params\Country\enum, "GQ",	0,	%EquatorialGuinea%
;;	HKR,	Ndi\params\Country\enum, "ER",	0,	%Eritrea%
;	HKR,	Ndi\params\Country\enum, "EE",	0,	%Estonia%
;;	HKR,	Ndi\params\Country\enum, "ET",	0,	%Ethiopia%
;;	HKR,	Ndi\params\Country\enum, "FK",	0,	%FalklandIslandsIslasMalvinas%
;;	HKR,	Ndi\params\Country\enum, "FO",	0,	%FaroeIslands%
;;	HKR,	Ndi\params\Country\enum, "FJ",	0,	%FijiIslands%
;	HKR,	Ndi\params\Country\enum, "FI",	0,	%Finland%
;	HKR,	Ndi\params\Country\enum, "FR",	0,	%France%
;;	HKR,	Ndi\params\Country\enum, "GF",	0,	%FrenchGuiana%
;;	HKR,	Ndi\params\Country\enum, "PF",	0,	%FrenchPolynesia%
;;	HKR,	Ndi\params\Country\enum, "TF",	0,	%FrenchSouthernandAntarcticLands%
;;	HKR,	Ndi\params\Country\enum, "GA",	0,	%Gabon%
;;	HKR,	Ndi\params\Country\enum, "GM",	0,	%Gambia%
;;	HKR,	Ndi\params\Country\enum, "GE",	0,	%Georgia%
;	HKR,	Ndi\params\Country\enum, "DE",	0,	%Germany%
;;	HKR,	Ndi\params\Country\enum, "GH",	0,	%Ghana%
;;	HKR,	Ndi\params\Country\enum, "GI",	0,	%Gibraltar%
;	HKR,	Ndi\params\Country\enum, "GR",	0,	%Greece%
;;	HKR,	Ndi\params\Country\enum, "GL",	0,	%Greenland%
;;	HKR,	Ndi\params\Country\enum, "GD",	0,	%Grenada%
;;	HKR,	Ndi\params\Country\enum, "GP",	0,	%Guadeloupe%
;	HKR,	Ndi\params\Country\enum, "GU",	0,	%Guam%
;	HKR,	Ndi\params\Country\enum, "GT",	0,	%Guatemala%
;;	HKR,	Ndi\params\Country\enum, "GW",	0,	%GuineaBissau%
;;	HKR,	Ndi\params\Country\enum, "GN",	0,	%Guinea%
;;	HKR,	Ndi\params\Country\enum, "GY",	0,	%Guyana%
;	HKR,	Ndi\params\Country\enum, "HT",	0,	%Haiti%
;;	HKR,	Ndi\params\Country\enum, "HM",	0,	%HeardIslandandMcDonaldIslands%
;	HKR,	Ndi\params\Country\enum, "HN",	0,	%Honduras%
;	HKR,	Ndi\params\Country\enum, "HK",	0,	%HongKongSAR%
;	HKR,	Ndi\params\Country\enum, "HU",	0,	%Hungary%
;	HKR,	Ndi\params\Country\enum, "IS",	0,	%Iceland%
;	HKR,	Ndi\params\Country\enum, "IN",	0,	%India%
;	HKR,	Ndi\params\Country\enum, "ID",	0,	%Indonesia%
;;	HKR,	Ndi\params\Country\enum, "IR",	0,	%Iran%
;;	HKR,	Ndi\params\Country\enum, "IQ",	0,	%Iraq%
;	HKR,	Ndi\params\Country\enum, "IE",	0,	%Ireland%
;	HKR,	Ndi\params\Country\enum, "IL",	0,	%Israel%
;	HKR,	Ndi\params\Country\enum, "IT",	0,	%Italy%
;;	HKR,	Ndi\params\Country\enum, "JM",	0,	%Jamaica%
;	HKR,	Ndi\params\Country\enum, "JP",	0,	%Japan%
;	HKR,	Ndi\params\Country\enum, "JO",	0,	%Jordan%
;;	HKR,	Ndi\params\Country\enum, "KZ",	0,	%Kazakhstan%
;;	HKR,	Ndi\params\Country\enum, "KE",	0,	%Kenya%
;;	HKR,	Ndi\params\Country\enum, "KI",	0,	%Kiribati%
;	HKR,	Ndi\params\Country\enum, "KR",	0,	%Korea%
;;	HKR,	Ndi\params\Country\enum, "KW",	0,	%Kuwait%
;;	HKR,	Ndi\params\Country\enum, "KG",	0,	%Kyrgyzstan%
;;	HKR,	Ndi\params\Country\enum, "LA",	0,	%Laos%
;	HKR,	Ndi\params\Country\enum, "LV",	0,	%Latvia%
;;	HKR,	Ndi\params\Country\enum, "LB",	0,	%Lebanon%
;;	HKR,	Ndi\params\Country\enum, "LS",	0,	%Lesotho%
;;	HKR,	Ndi\params\Country\enum, "LR",	0,	%Liberia%
;;	HKR,	Ndi\params\Country\enum, "LY",	0,	%Libya%
;	HKR,	Ndi\params\Country\enum, "LI",	0,	%Liechtenstein%
;	HKR,	Ndi\params\Country\enum, "LT",	0,	%Lithuania%
;	HKR,	Ndi\params\Country\enum, "LU",	0,	%Luxembourg%
;	HKR,	Ndi\params\Country\enum, "MO",	0,	%MacauSAR%
;;	HKR,	Ndi\params\Country\enum, "MK",	0,	%MacedoniaFormerYugoslavRepublicof%
;;	HKR,	Ndi\params\Country\enum, "MG",	0,	%Madagascar%
;;	HKR,	Ndi\params\Country\enum, "MW",	0,	%Malawi%
;	HKR,	Ndi\params\Country\enum, "MY",	0,	%Malaysia%
;;	HKR,	Ndi\params\Country\enum, "MV",	0,	%Maldives%
;;	HKR,	Ndi\params\Country\enum, "ML",	0,	%Mali%
;	HKR,	Ndi\params\Country\enum, "MT",	0,	%Malta%
;;	HKR,	Ndi\params\Country\enum, "MH",	0,	%MarshallIslands%
;;	HKR,	Ndi\params\Country\enum, "MQ",	0,	%Martinique%
;;	HKR,	Ndi\params\Country\enum, "MR",	0,	%Mauritania%
;;	HKR,	Ndi\params\Country\enum, "MU",	0,	%Mauritius%
;;	HKR,	Ndi\params\Country\enum, "YT",	0,	%Mayotte%
;	HKR,	Ndi\params\Country\enum, "MX",	0,	%Mexico%
;;	HKR,	Ndi\params\Country\enum, "FM",	0,	%Micronesia%
;;	HKR,	Ndi\params\Country\enum, "MD",	0,	%Moldova%
;	HKR,	Ndi\params\Country\enum, "MC",	0,	%Monaco%
;;	HKR,	Ndi\params\Country\enum, "MN",	0,	%Mongolia%
;;	HKR,	Ndi\params\Country\enum, "MS",	0,	%Montserrat%
;	HKR,	Ndi\params\Country\enum, "MA",	0,	%Morocco%
;;	HKR,	Ndi\params\Country\enum, "MZ",	0,	%Mozambique%
;;	HKR,	Ndi\params\Country\enum, "MM",	0,	%Myanmar%
;;	HKR,	Ndi\params\Country\enum, "NA",	0,	%Namibia%
;;	HKR,	Ndi\params\Country\enum, "NR",	0,	%Nauru%
;;	HKR,	Ndi\params\Country\enum, "NP",	0,	%Nepal%
;	HKR,	Ndi\params\Country\enum, "AN",	0,	%NetherlandsAntilles%
;	HKR,	Ndi\params\Country\enum, "NL",	0,	%NetherlandsThe%
;;	HKR,	Ndi\params\Country\enum, "NC",	0,	%NewCaledonia%
;	HKR,	Ndi\params\Country\enum, "NZ",	0,	%NewZealand%
;	HKR,	Ndi\params\Country\enum, "NI",	0,	%Nicaragua%
;;	HKR,	Ndi\params\Country\enum, "NE",	0,	%Niger%
;	HKR,	Ndi\params\Country\enum, "NG",	0,	%Nigeria%
;;	HKR,	Ndi\params\Country\enum, "NU",	0,	%Niue%
;;	HKR,	Ndi\params\Country\enum, "NF",	0,	%NorfolkIsland%
;;	HKR,	Ndi\params\Country\enum, "KP",	0,	%NorthKorea%
;;	HKR,	Ndi\params\Country\enum, "MP",	0,	%NorthernMarianaIslands%
;	HKR,	Ndi\params\Country\enum, "NO",	0,	%Norway%
;;	HKR,	Ndi\params\Country\enum, "OM",	0,	%Oman%
;	HKR,	Ndi\params\Country\enum, "PK",	0,	%Pakistan%
;;	HKR,	Ndi\params\Country\enum, "PW",	0,	%Palau%
;;	HKR,	Ndi\params\Country\enum, "PS",	0,	%PalestinianAuthority%
;	HKR,	Ndi\params\Country\enum, "PA",	0,	%Panama%
;;	HKR,	Ndi\params\Country\enum, "PG",	0,	%PapuaNewGuinea%
;	HKR,	Ndi\params\Country\enum, "PY",	0,	%Paraguay%
;	HKR,	Ndi\params\Country\enum, "PE",	0,	%Peru%
;	HKR,	Ndi\params\Country\enum, "PH",	0,	%Philippines%
;;	HKR,	Ndi\params\Country\enum, "PN",	0,	%Pitcairn%
;	HKR,	Ndi\params\Country\enum, "PL",	0,	%Poland%
;	HKR,	Ndi\params\Country\enum, "PT",	0,	%Portugal%
;;	HKR,	Ndi\params\Country\enum, "PR",	0,	%PuertoRico%
;;	HKR,	Ndi\params\Country\enum, "QA",	0,	%Qatar%
;;	HKR,	Ndi\params\Country\enum, "RE",	0,	%Reunion%
;	HKR,	Ndi\params\Country\enum, "RO",	0,	%Romania%
;	HKR,	Ndi\params\Country\enum, "RU",	0,	%Russia%
;;	HKR,	Ndi\params\Country\enum, "RW",	0,	%Rwanda%
;;	HKR,	Ndi\params\Country\enum, "WS",	0,	%Samoa%
;;	HKR,	Ndi\params\Country\enum, "SM",	0,	%SanMarino%
;;	HKR,	Ndi\params\Country\enum, "ST",	0,	%SaoTomeandPrincipe%
;	HKR,	Ndi\params\Country\enum, "SA",	0,	%SaudiArabia%
;;	HKR,	Ndi\params\Country\enum, "SN",	0,	%Senegal%
;;	HKR,	Ndi\params\Country\enum, "SC",	0,	%Seychelles%
;;	HKR,	Ndi\params\Country\enum, "SL",	0,	%SierraLeone%
;	HKR,	Ndi\params\Country\enum, "SG",	0,	%Singapore%
;	HKR,	Ndi\params\Country\enum, "SK",	0,	%Slovakia%
;	HKR,	Ndi\params\Country\enum, "SI",	0,	%Slovenia%
;;	HKR,	Ndi\params\Country\enum, "SB",	0,	%SolomonIslands%
;;	HKR,	Ndi\params\Country\enum, "SO",	0,	%Somalia%
;	HKR,	Ndi\params\Country\enum, "ZA",	0,	%SouthAfrica%
;;	HKR,	Ndi\params\Country\enum, "GS",	0,	%SouthGeorgiaandtheSouthSandwichIslands%
;	HKR,	Ndi\params\Country\enum, "ES",	0,	%Spain%
;	HKR,	Ndi\params\Country\enum, "LK",	0,	%SriLanka%
;;	HKR,	Ndi\params\Country\enum, "SH",	0,	%StHelena%
;;	HKR,	Ndi\params\Country\enum, "KN",	0,	%StKittsandNevis%
;;	HKR,	Ndi\params\Country\enum, "LC",	0,	%StLucia%
;;	HKR,	Ndi\params\Country\enum, "PM",	0,	%StPierreandMiquelon%
;;	HKR,	Ndi\params\Country\enum, "VC",	0,	%StVincentandtheGrenadines%
;;	HKR,	Ndi\params\Country\enum, "SD",	0,	%Sudan%
;;	HKR,	Ndi\params\Country\enum, "SR",	0,	%Suriname%
;;	HKR,	Ndi\params\Country\enum, "SJ",	0,	%SvalbardandJanMayen%
;;	HKR,	Ndi\params\Country\enum, "SZ",	0,	%Swaziland%
;	HKR,	Ndi\params\Country\enum, "SE",	0,	%Sweden%
;	HKR,	Ndi\params\Country\enum, "CH",	0,	%Switzerland%
;;	HKR,	Ndi\params\Country\enum, "SY",	0,	%Syria%
;	HKR,	Ndi\params\Country\enum, "TW",	0,	%Taiwan%
;;	HKR,	Ndi\params\Country\enum, "TJ",	0,	%Tajikistan%
;	HKR,	Ndi\params\Country\enum, "TZ",	0,	%Tanzania%
;	HKR,	Ndi\params\Country\enum, "TH",	0,	%Thailand%
;;	HKR,	Ndi\params\Country\enum, "TG",	0,	%Togo%
;;	HKR,	Ndi\params\Country\enum, "TK",	0,	%Tokelau%
;;	HKR,	Ndi\params\Country\enum, "TO",	0,	%Tonga%
;;	HKR,	Ndi\params\Country\enum, "TT",	0,	%TrinidadandTobago%
;	HKR,	Ndi\params\Country\enum, "TN",	0,	%Tunisia%
;	HKR,	Ndi\params\Country\enum, "TR",	0,	%Turkey%
;;	HKR,	Ndi\params\Country\enum, "TM",	0,	%Turkmenistan%
;;	HKR,	Ndi\params\Country\enum, "TC",	0,	%TurksandCaicosIslands%
;;	HKR,	Ndi\params\Country\enum, "TV",	0,	%Tuvalu%
;;	HKR,	Ndi\params\Country\enum, "UG",	0,	%Uganda%
;	HKR,	Ndi\params\Country\enum, "UA",	0,	%Ukraine%
;	HKR,	Ndi\params\Country\enum, "AE",	0,	%UnitedArabEmirates%
;	HKR,	Ndi\params\Country\enum, "GB",	0,	%UnitedKingdom%
;	HKR,	Ndi\params\Country\enum, "UM",	0,	%UnitedStatesMinorOutlyingIslands%
;	HKR,	Ndi\params\Country\enum, "US",	0,	%UnitedStates%
;	HKR,	Ndi\params\Country\enum, "UY",	0,	%Uruguay%
;;	HKR,	Ndi\params\Country\enum, "UZ",	0,	%Uzbekistan%
;;	HKR,	Ndi\params\Country\enum, "VU",	0,	%Vanuatu%
;;	HKR,	Ndi\params\Country\enum, "VA",	0,	%VaticanCity%
;	HKR,	Ndi\params\Country\enum, "VE",	0,	%Venezuela%
;	HKR,	Ndi\params\Country\enum, "VN",	0,	%VietNam%
;;	HKR,	Ndi\params\Country\enum, "VG",	0,	%VirginIslandsBritish%
;;	HKR,	Ndi\params\Country\enum, "VI",	0,	%VirginIslands%
;;	HKR,	Ndi\params\Country\enum, "WF",	0,	%WallisandFutuna%
;;	HKR,	Ndi\params\Country\enum, "EH",	0,	%WesternSahara%
;;	HKR,	Ndi\params\Country\enum, "YE",	0,	%Yemen%
;	HKR,	Ndi\params\Country\enum, "YU",	0,	%Yugoslavia%
;;	HKR,	Ndi\params\Country\enum, "ZM",	0,	%Zambia%
;;	HKR,	Ndi\params\Country\enum, "ZW",	0,	%Zimbabwe%
	HKR,	Ndi\params\Country\enum, "",	0,	%Default%
	HKR,	Ndi\params\Country,	default,, 	""

	HKR,	Ndi\params\RoamDelta, ParamDesc,	0,	%RoamingTendency%
	HKR,	Ndi\params\RoamDelta, type,		0,	"enum"
	HKR,	Ndi\params\RoamDelta\enum, "0",	        0,	%Aggressive%
	HKR,	Ndi\params\RoamDelta\enum, "1",         0,	%Moderate%
	HKR,	Ndi\params\RoamDelta\enum, "2",         0,	%Conservative%
	HKR,	Ndi\params\RoamDelta,default,,"1"

	HKR,	Ndi\params\RadioState, ParamDesc,	0,	%RadioEnableDisable%
	HKR,	Ndi\params\RadioState, type,		0,	"enum"
	HKR,	Ndi\params\RadioState\enum, "1",		0,	%Disabled%
	HKR,	Ndi\params\RadioState\enum, "0",		0,	%Enabled%
	HKR,    Ndi\params\RadioState,default,,"0"	

	HKR,	Ndi\params\MPC, ParamDesc,	        0,	%MiminumPowerConsumption%
	HKR,	Ndi\params\MPC, type,		        0,	"enum"
	HKR,	Ndi\params\MPC\enum, "0",		0,	%Disabled%
	HKR,	Ndi\params\MPC\enum, "1",		0,	%Enabled%
	HKR,    Ndi\params\MPC,default,,"1"

	HKR,	Ndi\params\PowerSaveMode, ParamDesc,	0,	%PowerSaveMode%
	HKR,	Ndi\params\PowerSaveMode, type,		0,	"enum"
	HKR,	Ndi\params\PowerSaveMode\enum, "0",		0,	%Disabled%
	HKR,	Ndi\params\PowerSaveMode\enum, "1",		0,	%Enabled%
	HKR,	Ndi\params\PowerSaveMode\enum, "2",		0,	%Fast%
	HKR,    Ndi\params\PowerSaveMode,default,,"0"	

	HKR,	Ndi\params\frag, ParamDesc,	0,	%FragmentationThreshold%
	HKR,	Ndi\params\frag,type,0,"dword"
	HKR,	Ndi\params\frag,min,,"256"
	HKR,	Ndi\params\frag,max,,"2346"
	HKR,	Ndi\params\frag,default,,"2346"

	HKR,	Ndi\params\rts, ParamDesc,	0,	%RTSThreshold%
	HKR,	Ndi\params\rts,type,0,"dword"
	HKR,	Ndi\params\rts,min,,"0"
	HKR,	Ndi\params\rts,max,,"2347"
	HKR,	Ndi\params\rts,default,,"2347"

	HKR,	Ndi\params\NetworkAddress, ParamDesc,	0, %LocallyAdministeredMACAddress%
	HKR,	Ndi\params\NetworkAddress, type,	0, "edit"
	HKR,	Ndi\params\NetworkAddress, LimitText,	0, "12"
	HKR,	Ndi\params\NetworkAddress, UpperCase,  0, "1"
	HKR,	Ndi\params\NetworkAddress, default,	0, ""
	HKR,	Ndi\params\NetworkAddress, optional,	0, "1"

	HKR,	Ndi\params\PwrOut, ParamDesc,	0,	%PowerOutput%
	HKR,	Ndi\params\PwrOut, type,		0,	"enum"
	HKR,	Ndi\params\PwrOut\enum, "100",	0,	"100%"
	HKR,	Ndi\params\PwrOut\enum, "75",	0,	"75%"
	HKR,	Ndi\params\PwrOut\enum, "50",	0,	"50%"
	HKR,	Ndi\params\PwrOut\enum, "25",	0,	"25%"
	HKR,	Ndi\params\PwrOut,default,,"100"

	HKR,	Ndi\params\FrameBursting, ParamDesc,	0,	%XPress_Technology%
	HKR,	Ndi\params\FrameBursting, type,		0,	"enum"
	HKR,	Ndi\params\FrameBursting\enum, "0",		0,	%Disabled%
	HKR,	Ndi\params\FrameBursting\enum, "1",		0,	%Enabled%
	HKR,    Ndi\params\FrameBursting,default,,"1"	

	HKR,	Ndi\params\BTCoexist, ParamDesc,	0,	%BlueToothCollaboration%
	HKR,	Ndi\params\BTCoexist, type,		0,	"enum"
	HKR,	Ndi\params\BTCoexist\enum, "1",	0,	%Enable%
	HKR,	Ndi\params\BTCoexist\enum, "0",	0,	%Disable%
	HKR,	Ndi\params\BTCoexist,default,,"0"

	HKR,,"WEP",0,	""
	HKR,,"NetworkType",	0,	"-1"
	HKR,,"SSID",	0,	""

	HKR,,"gpio0",	0,	"-1"
	HKR,,"gpio1",	0,	"-1"
	HKR,,"gpio2",	0,	"-1"
	HKR,,"gpio3",	0,	"-1"

	HKR,,"scan_channel_time",	0,"-1"
	HKR,,"scan_unassoc_time",	0,"-1"
	HKR,,"scan_home_time",		0,"-1"
	HKR,,"scan_passes",		0,"-1"

	HKR,,"BadFramePreempt",		0,"0"

	HKR,,"Interference_Mode",	0,"3"

	HKR,,"ccx_rm",			0,"1"
	HKR,,"ccx_rm_limit",		0,"300"

	HKR,	Ndi\params\antdiv, ParamDesc,	0,	%AntennaDiversity%
	HKR,	Ndi\params\antdiv, type,	0,	"enum"
	HKR,	Ndi\params\antdiv\enum, "-1",	0,	%Auto%
	HKR,	Ndi\params\antdiv,default,,"-1"

	HKR,	Ndi\params\WME, ParamDesc,	0,	%WME%
	HKR,	Ndi\params\WME, type,		0,	"enum"
	HKR,	Ndi\params\WME\enum, "1",	0,	%Enabled%
	HKR,	Ndi\params\WME\enum, "0",	0,	%Disabled%
	HKR,	Ndi\params\WME,default,,"0"

	HKLM,	Software\Broadcom\802.11, PerUserPN, 0x00010001, 0
	HKLM,	Software\Broadcom\802.11, DisallowPNChanges, 0x00010001, 0

	HKR, 	Ndi\params\WZCCoexist, ParamDesc,0,	%WZC_Managed_Ethernet%
	HKR, 	Ndi\params\WZCCoexist, type,     0, 	"enum"
	HKR, 	Ndi\params\WZCCoexist\enum, "0", 0,	%Disabled%
	HKR,	Ndi\params\WZCCoexist\enum, "1", 0,	%Enabled%
	HKR,    Ndi\params\WZCCoexist,default,,"0"

	HKR,	Ndi\params\IBSSLink, ParamDesc,	0,	%IBSS_Link_Indication%
	HKR,	Ndi\params\IBSSLink, type,	0,	"enum"
	HKR,	Ndi\params\IBSSLink\enum, "0",	0,	%Legacy%
	HKR,	Ndi\params\IBSSLink\enum, "1",	0,	%Default%
	HKR,	Ndi\params\IBSSLink,default,,"1"

[b.options.reg]
	HKR,	Ndi\params\PLCPHeader, ParamDesc,	0,	%PLCPHeader%
	HKR,	Ndi\params\PLCPHeader, type,		0,	"enum"
	HKR,	Ndi\params\PLCPHeader\enum, "-1",	0,	%Long%
	HKR,	Ndi\params\PLCPHeader\enum, "0",	0,	%AutoShortLong%
	HKR,	Ndi\params\PLCPHeader,default,,"0"

	HKR,	Ndi\params\Rate, ParamDesc,	0,	%Rate%
	HKR,	Ndi\params\Rate, type,		0,	"enum"
	HKR,	Ndi\params\Rate\enum, "0",	0,	%Usebestrate%
	HKR,	Ndi\params\Rate\enum, "2",	0,	" 1"
	HKR,	Ndi\params\Rate\enum, "4",	0,	" 2"
	HKR,	Ndi\params\Rate\enum, "11",	0,	" 5.5"
	HKR,	Ndi\params\Rate\enum, "22",	0,	"11"
	HKR,	Ndi\params\Rate,default,,"0"

[g.options.reg]
	HKR,	Ndi\params\RoamTrigger, ParamDesc,	0,	%RoamingDecision%
	HKR,	Ndi\params\RoamTrigger, type,		0,	"enum"
	HKR,	Ndi\params\RoamTrigger\enum, "-60",	0,	%OptimizeBandwidth%
	HKR,	Ndi\params\RoamTrigger\enum, "-70",	0,	%Default%
	HKR,	Ndi\params\RoamTrigger\enum, "-80",	0,	%OptimizeDistance%
	HKR,	Ndi\params\RoamTrigger,default,,"-70"

	HKR,	Ndi\params\PLCPHeader, ParamDesc,	0,	%BSSPLCPHeader%
	HKR,	Ndi\params\PLCPHeader, type,		0,	"enum"
	HKR,	Ndi\params\PLCPHeader\enum, "-1",	0,	%Long%
	HKR,	Ndi\params\PLCPHeader\enum, "0",	0,	%AutoShortLong%
	HKR,	Ndi\params\PLCPHeader,default,,"0"

	HKR,    Ndi\params\IBSSGMode, ParamDesc,	0,      %IBSS54gtmMode%
	HKR,    Ndi\params\IBSSGMode, type,         0,      "enum"
	HKR,    Ndi\params\IBSSGMode\enum, "0",     0,      %80211bOnly%
	HKR,    Ndi\params\IBSSGMode\enum, "1",     0,      %54gLRS%
	HKR,    Ndi\params\IBSSGMode\enum, "2",     0,      %54gAuto%
	HKR,    Ndi\params\IBSSGMode\enum, "4",     0,      %54gPerformance%
	HKR,    Ndi\params\IBSSGMode,default,,"2"

	HKR,    Ndi\params\IBSSGProtection, ParamDesc,	0,      %IBSS54gtmProtectionMode%
	HKR,    Ndi\params\IBSSGProtection, type,       0,      "enum"
	HKR,    Ndi\params\IBSSGProtection\enum, "0",   0,      %Disabled%
	HKR,    Ndi\params\IBSSGProtection\enum, "2",   0,      %Auto%
	HKR,    Ndi\params\IBSSGProtection,default,,"2"

	HKR,	Ndi\params\Rate, ParamDesc,	0,	%Rate%
	HKR,	Ndi\params\Rate, type,		0,	"enum"
	HKR,	Ndi\params\Rate\enum, "0",	0,	%Usebestrate%
	HKR,	Ndi\params\Rate\enum, "2",	0,	" 1"
	HKR,	Ndi\params\Rate\enum, "4",	0,	" 2"
	HKR,	Ndi\params\Rate\enum, "11",	0,	" 5.5"
	HKR,	Ndi\params\Rate\enum, "12",	0,	" 6"
	HKR,	Ndi\params\Rate\enum, "18",	0,	" 9"
	HKR,	Ndi\params\Rate\enum, "22",	0,	"11"
	HKR,	Ndi\params\Rate\enum, "24",	0,	"12"
	HKR,	Ndi\params\Rate\enum, "36",	0,	"18"
	HKR,	Ndi\params\Rate\enum, "48",	0,	"24"
	HKR,	Ndi\params\Rate\enum, "72",	0,	"36"
	HKR,	Ndi\params\Rate\enum, "96",	0,	"48"
	HKR,	Ndi\params\Rate\enum, "108",	0,	"54"
	HKR,	Ndi\params\Rate,default,,"0"

	HKR,    Ndi\params\Afterburner, ParamDesc,	0,      %Afterburner%
	HKR,    Ndi\params\Afterburner, type,       0,      "enum"
	HKR,    Ndi\params\Afterburner\enum, "0",   0,      %Disabled%
	HKR,    Ndi\params\Afterburner\enum, "1",   0,      %Enabled%
	HKR,    Ndi\params\Afterburner,default,,"1"

; options common to both b and g
[bg.options.reg]
	HKR,	Ndi\params\Channel, ParamDesc, 0, %IBSSChannelNumber%
	HKR,	Ndi\params\Channel, default,   0, "11"
	HKR,	Ndi\params\Channel, min,       0, "1"
	HKR,	Ndi\params\Channel, max,       0, "14"
	HKR,	Ndi\params\Channel, step,      0, "1"
	HKR,	Ndi\params\Channel, base,      0, "10"
	HKR,	Ndi\params\Channel, type,      0, "int"

	HKR,	Ndi\params\ApCompatMode, ParamDesc,	0,	%ApCompatibilityMode%
	HKR,	Ndi\params\ApCompatMode, type,		0,	"enum"
	HKR,	Ndi\params\ApCompatMode\enum, "1",	0,	%BroaderCompat%
	HKR,	Ndi\params\ApCompatMode\enum, "0",	0,	%HigherPerf%
	HKR,	Ndi\params\ApCompatMode,default,,"0"


[a.options.reg]
	HKR,    Ndi\params\Afterburner, ParamDesc,	0,      %Afterburner%
	HKR,    Ndi\params\Afterburner, type,       0,      "enum"
	HKR,    Ndi\params\Afterburner\enum, "0",   0,      %Disabled%
	HKR,    Ndi\params\Afterburner\enum, "1",   0,      %Enabled%
	HKR,    Ndi\params\Afterburner,default,,"1"

	HKR,	Ndi\params\RateA, ParamDesc,	0,	%Rate_802_11a%
	HKR,	Ndi\params\RateA, type,		0,	"enum"
	HKR,	Ndi\params\RateA\enum, "0",	0,	%Usebestrate%
	HKR,	Ndi\params\RateA\enum, "12",	0,	" 6"
	HKR,	Ndi\params\RateA\enum, "18",	0,	" 9"
	HKR,	Ndi\params\RateA\enum, "24",	0,	"12"
	HKR,	Ndi\params\RateA\enum, "36",	0,	"18"
	HKR,	Ndi\params\RateA\enum, "48",	0,	"24"
	HKR,	Ndi\params\RateA\enum, "72",	0,	"36"
	HKR,	Ndi\params\RateA\enum, "96",	0,	"48"
	HKR,	Ndi\params\RateA\enum, "108",0,	"54"
	HKR,	Ndi\params\RateA,default,,"0"

	; USA Low Band
	HKR,	Ndi\params\Channel, ParamDesc, 0, %IBSSChannelNumber%
	HKR,	Ndi\params\Channel, type,      0, "enum"
	HKR,	Ndi\params\Channel\enum, "36",   0, " 36"
	HKR,	Ndi\params\Channel\enum, "40",   0, " 40"
	HKR,	Ndi\params\Channel\enum, "44",   0, " 44"
	HKR,	Ndi\params\Channel\enum, "48",   0, " 48"
	HKR,	Ndi\params\Channel\enum, "52",   0, " 52"
	HKR,	Ndi\params\Channel\enum, "56",   0, " 56"
	HKR,	Ndi\params\Channel\enum, "60",   0, " 60"
	HKR,	Ndi\params\Channel\enum, "64",   0, " 64"
	; Europe
	HKR,	Ndi\params\Channel\enum, "100",   0, "100"
	HKR,	Ndi\params\Channel\enum, "104",   0, "104"
	HKR,	Ndi\params\Channel\enum, "108",   0, "108"
	HKR,	Ndi\params\Channel\enum, "112",   0, "112"
	HKR,	Ndi\params\Channel\enum, "116",   0, "116"
	HKR,	Ndi\params\Channel\enum, "120",   0, "120"

	HKR,	Ndi\params\Channel\enum, "124",   0, "124"
	HKR,	Ndi\params\Channel\enum, "128",   0, "128"
	HKR,	Ndi\params\Channel\enum, "132",   0, "132"
	HKR,	Ndi\params\Channel\enum, "136",   0, "136"
	HKR,	Ndi\params\Channel\enum, "140",   0, "140"

; 	Additional channels supported only on SPROM map version 2
;	HKR,	Ndi\params\Channel\enum, "149",   0, "149"
;	HKR,	Ndi\params\Channel\enum, "153",   0, "153"
;	HKR,	Ndi\params\Channel\enum, "157",   0, "157"
;	HKR,	Ndi\params\Channel\enum, "161",   0, "161"
;	HKR,	Ndi\params\Channel\enum, "165",   0, "165"

	HKR,	Ndi\params\Channel, default,   0, "36"

[bag.options.reg]
	HKR,    Ndi\params\Afterburner, ParamDesc,	0,      %Afterburner%
	HKR,    Ndi\params\Afterburner, type,       0,      "enum"
	HKR,    Ndi\params\Afterburner\enum, "0",   0,      %Disabled%
	HKR,    Ndi\params\Afterburner\enum, "1",   0,      %Enabled%
	HKR,    Ndi\params\Afterburner,default,,"1"

	HKR, 	Ndi\params\11HNetworks, ParamDesc, 0, 	"802.11h"
	HKR, 	Ndi\params\11HNetworks, type, 		0, "enum"
	HKR, 	Ndi\params\11HNetworks\enum, "0", 	0, %Disabled%
	HKR, 	Ndi\params\11HNetworks\enum, "1", 	0, %Loose%
	HKR, 	Ndi\params\11HNetworks\enum, "2", 	0, %Strict%
	HKR, 	Ndi\params\11HNetworks,default,,"0" 

	HKR,	Ndi\params\RoamTrigger, ParamDesc,	0,	%RoamingDecision%
	HKR,	Ndi\params\RoamTrigger, type,		0,	"enum"
	HKR,	Ndi\params\RoamTrigger\enum, "-60",	0,	%OptimizeBandwidth%
	HKR,	Ndi\params\RoamTrigger\enum, "-70",	0,	%Default%
	HKR,	Ndi\params\RoamTrigger\enum, "-80",	0,	%OptimizeDistance%
	HKR,	Ndi\params\RoamTrigger,default,,"-70"

	HKR,	Ndi\params\PLCPHeader, ParamDesc,	0,	%BSSPLCPHeader%
	HKR,	Ndi\params\PLCPHeader, type,		0,	"enum"
	HKR,	Ndi\params\PLCPHeader\enum, "-1",	0,	%Long%
	HKR,	Ndi\params\PLCPHeader\enum, "0",	0,	%AutoShortLong%
	HKR,	Ndi\params\PLCPHeader,default,,"0"

	HKR,	Ndi\params\band, ParamDesc,	0,	%DisableBands%
	HKR,	Ndi\params\band, type,		0,	"enum"
	HKR,	Ndi\params\band\enum, "0",	0,	%None%
	HKR,	Ndi\params\band\enum, "1",	0,	%Disable80211gb%
	HKR,	Ndi\params\band\enum, "2",	0,	%Disable80211a%
	HKR,	Ndi\params\band,default,,"0"

	HKR,	Ndi\params\BandPref, ParamDesc,	0,	%BandPreference%
	HKR,	Ndi\params\BandPref, type,		0,	"enum"
	HKR,	Ndi\params\BandPref\enum, "0",	0,	%None%
	HKR,	Ndi\params\BandPref\enum, "1",	0,	%Prefer80211a%
	HKR,	Ndi\params\BandPref\enum, "2",	0,	%Prefer80211gb%
	HKR,	Ndi\params\BandPref,default,,"0"
        
	HKR,	Ndi\params\AssocRoamPref, ParamDesc,	0,	%AssociationRoamPreference%
	HKR,	Ndi\params\AssocRoamPref, type,		0,	"enum"
	HKR,	Ndi\params\AssocRoamPref\enum, "0",	0,	%Disabled%
	HKR,	Ndi\params\AssocRoamPref\enum, "1",	0,	%Enabled%
	HKR,	Ndi\params\AssocRoamPref,default,,"0"

	HKR,    Ndi\params\IBSSGMode, ParamDesc,	0,      %IBSS54gtmMode%
	HKR,    Ndi\params\IBSSGMode, type,         0,      "enum"
	HKR,    Ndi\params\IBSSGMode\enum, "0",     0,      %80211bOnly%
	HKR,    Ndi\params\IBSSGMode\enum, "1",     0,      %54gLRS%
	HKR,    Ndi\params\IBSSGMode\enum, "2",     0,      %54gAuto%
	HKR,    Ndi\params\IBSSGMode\enum, "4",     0,      %54gPerformance%
	HKR,	Ndi\params\IBSSGMode,default,,"2"
	;default from bcmwl5[ei].inf

	HKR,    Ndi\params\IBSSGProtection, ParamDesc,	0,      %IBSS54gtmProtectionMode%
	HKR,    Ndi\params\IBSSGProtection, type,       0,      "enum"
	HKR,    Ndi\params\IBSSGProtection\enum, "0",   0,      %Disabled%
	HKR,    Ndi\params\IBSSGProtection\enum, "2",   0,      %Auto%
	HKR,    Ndi\params\IBSSGProtection,default,,"2"


	HKR,	Ndi\params\RateA, ParamDesc,	0,	%Rate_802_11a%
	HKR,	Ndi\params\RateA, type,		0,	"enum"
	HKR,	Ndi\params\RateA\enum, "0",	0,	%Usebestrate%
	HKR,	Ndi\params\RateA\enum, "12",	0,	" 6"
	HKR,	Ndi\params\RateA\enum, "18",	0,	" 9"
	HKR,	Ndi\params\RateA\enum, "24",	0,	"12"
	HKR,	Ndi\params\RateA\enum, "36",	0,	"18"
	HKR,	Ndi\params\RateA\enum, "48",	0,	"24"
	HKR,	Ndi\params\RateA\enum, "72",	0,	"36"
	HKR,	Ndi\params\RateA\enum, "96",	0,	"48"
	HKR,	Ndi\params\RateA\enum, "108",	0,	"54"
	HKR,	Ndi\params\RateA,default,,"0"


	HKR,	Ndi\params\Rate, ParamDesc,	0,	%Rate_802_11bg%
	HKR,	Ndi\params\Rate, type,		0,	"enum"
	HKR,	Ndi\params\Rate\enum, "0",	0,	%Usebestrate%
	HKR,	Ndi\params\Rate\enum, "2",	0,	" 1"
	HKR,	Ndi\params\Rate\enum, "4",	0,	" 2"
	HKR,	Ndi\params\Rate\enum, "11",	0,	" 5.5"
	HKR,	Ndi\params\Rate\enum, "12",	0,	" 6"
	HKR,	Ndi\params\Rate\enum, "18",	0,	" 9"
	HKR,	Ndi\params\Rate\enum, "22",	0,	"11"
	HKR,	Ndi\params\Rate\enum, "24",	0,	"12"
	HKR,	Ndi\params\Rate\enum, "36",	0,	"18"
	HKR,	Ndi\params\Rate\enum, "48",	0,	"24"
	HKR,	Ndi\params\Rate\enum, "72",	0,	"36"
	HKR,	Ndi\params\Rate\enum, "96",	0,	"48"
	HKR,	Ndi\params\Rate\enum, "108",	0,	"54"
	HKR,	Ndi\params\Rate,default,,"0"

	HKR,	Ndi\params\Channel, ParamDesc, 0, %IBSSChannelNumber%
	HKR,	Ndi\params\Channel, type,      0, "enum"
	HKR,	Ndi\params\Channel\enum, "1",   0, "  1"
	HKR,	Ndi\params\Channel\enum, "2",   0, "  2"
	HKR,	Ndi\params\Channel\enum, "3",   0, "  3"
	HKR,	Ndi\params\Channel\enum, "4",   0, "  4"
	HKR,	Ndi\params\Channel\enum, "5",   0, "  5"
	HKR,	Ndi\params\Channel\enum, "6",   0, "  6"
	HKR,	Ndi\params\Channel\enum, "7",   0, "  7"
	HKR,	Ndi\params\Channel\enum, "8",   0, "  8"
	HKR,	Ndi\params\Channel\enum, "9",   0, "  9"
	HKR,	Ndi\params\Channel\enum, "10",   0, " 10"
	HKR,	Ndi\params\Channel\enum, "11",   0, " 11"
	HKR,	Ndi\params\Channel\enum, "12",   0, " 12"
	HKR,	Ndi\params\Channel\enum, "13",   0, " 13"
	HKR,	Ndi\params\Channel\enum, "14",   0, " 14"
	; USA Low Band
	HKR,	Ndi\params\Channel\enum, "36",   0, " 36"
	HKR,	Ndi\params\Channel\enum, "40",   0, " 40"
	HKR,	Ndi\params\Channel\enum, "44",   0, " 44"
	HKR,	Ndi\params\Channel\enum, "48",   0, " 48"
	HKR,	Ndi\params\Channel\enum, "52",   0, " 52"
	HKR,	Ndi\params\Channel\enum, "56",   0, " 56"
	HKR,	Ndi\params\Channel\enum, "60",   0, " 60"
	HKR,	Ndi\params\Channel\enum, "64",   0, " 64"
	; Europe
	HKR,	Ndi\params\Channel\enum, "100",   0, "100"
	HKR,	Ndi\params\Channel\enum, "104",   0, "104"
	HKR,	Ndi\params\Channel\enum, "108",   0, "108"
	HKR,	Ndi\params\Channel\enum, "112",   0, "112"
	HKR,	Ndi\params\Channel\enum, "116",   0, "116"
	HKR,	Ndi\params\Channel\enum, "120",   0, "120"
	HKR,	Ndi\params\Channel\enum, "124",   0, "124"
	HKR,	Ndi\params\Channel\enum, "128",   0, "128"
	HKR,	Ndi\params\Channel\enum, "132",   0, "132"
	HKR,	Ndi\params\Channel\enum, "136",   0, "136"
	HKR,	Ndi\params\Channel\enum, "140",   0, "140"

	HKR,	Ndi\params\Channel, default,   0, "11"

	HKR,	Ndi\params\ApCompatMode, ParamDesc,	0,	%ApCompatibilityMode%
	HKR,	Ndi\params\ApCompatMode, type,		0,	"enum"
	HKR,	Ndi\params\ApCompatMode\enum, "1",	0,	%BroaderCompat%
	HKR,	Ndi\params\ApCompatMode\enum, "0",	0,	%HigherPerf%
	HKR,	Ndi\params\ApCompatMode,default,,"0"


[DestinationDirs]
	DefaultDestDir=11
	BCM43XX.sys.files=11
	BCM43XX.files.NT = 12

[SourceDisksNames]
	1=%BCM43XX_DiskName%,,

[SourceDisksFiles]
	BCMWL5.SYS=1

[strings]
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="United States"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - Performance"
80211bOnly="802.11b Only"
AntennaDiversity="Antenna Diversity"
Auto="Auto"
AutoShortLong="Auto (Short/Long)"
BSSPLCPHeader="BSS PLCP Header"
BlueToothCollaboration="Bluetooth Collaboration"
Default="Default"
Disable="Disable"
Disable80211a="Disable 802.11a"
Disable80211gb="Disable 802.11g/b"
DisableBands="Disable Bands"
Disabled="Disabled"
Enable="Enable"
Enabled="Enabled"
FragmentationThreshold="Fragmentation Threshold"
IBSS54gtmMode="IBSS 54g Mode"
IBSS54gtmProtectionMode="IBSS 54g Protection Mode"
IBSSChannelNumber="IBSS Channel Number"
LocallyAdministeredMACAddress="Locally Administered MAC Address"
Long="Long"
None="None"
OptimizeBandwidth="Optimize Bandwidth"
OptimizeDistance="Optimize Distance"
PLCPHeader="PLCP Header"
PowerOutput="Power Output"
PowerSaveMode="Power Save Mode"
Prefer80211a="Prefer 802.11a"
Prefer80211gb="Prefer 802.11g/b"
RTSThreshold="RTS Threshold"
RadioEnableDisable="Radio Enable/Disable"
Rate="Rate"
RoamingDecision="Roaming Decision"
Usebestrate="Use best rate"
XPress_Technology="54g+ (XPress)"
Location="Location"
Strict="Strict"
Loose="Loose"
Fast="Fast"
MiminumPowerConsumption="Minimum Power Consumption"
AssociationRoamPreference="Association Roam Preference"
BandPreference="Band Preference"
RoamingTendency="Roam Tendency"
Aggressive="Aggressive"
Moderate="Moderate"
Conservative="Conservative"
ApCompatibilityMode="AP Compatibility Mode"
BroaderCompat="Broader Compatibility"
HigherPerf="Higher Performance"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Rate (802.11a)"
Rate_802_11bg="Rate (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS Link Indication"


[strings.2c01] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="الولايات المتحدة"
54gAuto="54g - تلقائي"
54gLRS="54g - LRS"
54gPerformance="54g - الأداء"
80211bOnly="802.11b فقط"
AntennaDiversity="تنوع الهوائي"
Auto="تلقائي"
AutoShortLong="تلقائي (قصير/طويل)"
BSSPLCPHeader="رأس BSS PLCP"
BlueToothCollaboration="Bluetooth Collaboration"
Default="افتراضي"
Disable="تعطيل"
Disable80211a="تعطيل 802.11a"
Disable80211gb="تعطيل 802.11g/b"
DisableBands="تعطيل نطاقات"
Disabled="مُعطًَل"
Enable="تمكين"
Enabled="مُمكًَن"
FragmentationThreshold="حد التجزئة"
IBSS54gtmMode="وضع IBSS 54g"
IBSS54gtmProtectionMode="وضع حماية IBSS 54g"
IBSSChannelNumber="رقم قناة IBSS"
LocallyAdministeredMACAddress="عنوان MAC مُدار محلياً"
Long="طويل"
None="بلا"
OptimizeBandwidth="تحسين عرض النطاق الترددي"
OptimizeDistance="تحسين المسافة"
PLCPHeader="رأس PLCP"
PowerOutput="خرج الطاقة"
PowerSaveMode="وضع حفظ الطاقة"
Prefer80211a="تفضيل 802.11a"
Prefer80211gb="تفضيل 802.11g/b"
RTSThreshold="حد RTS"
RadioEnableDisable="تعطيل/تمكين الراديو"
Rate="المعدل"
RoamingDecision="تحديد التجوال"
Usebestrate="استخدام أفضل معدل"
XPress_Technology="54g+ (XPress)تكنولوجيا تم تطويرها بواسطة"
Location="الموقع"
Strict="مقيدة"
Loose="واسعة"
Fast="سريعة"
MiminumPowerConsumption="الحد الأدنى من استهلاك الطاقة"
AssociationRoamPreference="تفضيلات تجوال الاقتران"
BandPreference="تفضيلات الموجة"
RoamingTendency="توجه التجوال"
Aggressive="شديد"
Moderate="معتدل"
Conservative="محافظ"
ApCompatibilityMode="وضع توافق AP"
BroaderCompat="توافق أكثر"
HigherPerf="أداء أعلى"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="المعدل (802.11a)"
Rate_802_11bg="المعدل (802.11b/g)"
WZC_Managed_Ethernet="Ethernet مُدار بـ WZC"
Legacy="توارث"
IBSS_Link_Indication="مؤشر ارتباط IBSS"

[strings.0401] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="الولايات المتحدة"
54gAuto="54g - تلقائي"
54gLRS="54g - LRS"
54gPerformance="54g - الأداء"
80211bOnly="802.11b فقط"
AntennaDiversity="تنوع الهوائي"
Auto="تلقائي"
AutoShortLong="تلقائي (قصير/طويل)"
BSSPLCPHeader="رأس BSS PLCP"
BlueToothCollaboration="Bluetooth Collaboration"
Default="افتراضي"
Disable="تعطيل"
Disable80211a="تعطيل 802.11a"
Disable80211gb="تعطيل 802.11g/b"
DisableBands="تعطيل نطاقات"
Disabled="مُعطًَل"
Enable="تمكين"
Enabled="مُمكًَن"
FragmentationThreshold="حد التجزئة"
IBSS54gtmMode="وضع IBSS 54g"
IBSS54gtmProtectionMode="وضع حماية IBSS 54g"
IBSSChannelNumber="رقم قناة IBSS"
LocallyAdministeredMACAddress="عنوان MAC مُدار محلياً"
Long="طويل"
None="بلا"
OptimizeBandwidth="تحسين عرض النطاق الترددي"
OptimizeDistance="تحسين المسافة"
PLCPHeader="رأس PLCP"
PowerOutput="خرج الطاقة"
PowerSaveMode="وضع حفظ الطاقة"
Prefer80211a="تفضيل 802.11a"
Prefer80211gb="تفضيل 802.11g/b"
RTSThreshold="حد RTS"
RadioEnableDisable="تعطيل/تمكين الراديو"
Rate="المعدل"
RoamingDecision="تحديد التجوال"
Usebestrate="استخدام أفضل معدل"
XPress_Technology="54g+ (XPress) تكنولوجيا تم تطويرها بواسطة"
Location="الموقع"
Strict="مقيدة"
Loose="واسعة"
Fast="سريعة"
MiminumPowerConsumption="الحد الأدنى من استهلاك الطاقة"
AssociationRoamPreference="تفضيلات تجوال الاقتران"
BandPreference="تفضيلات الموجة"
RoamingTendency="توجه التجوال"
Aggressive="شديد"
Moderate="معتدل"
Conservative="محافظ"
ApCompatibilityMode="وضع توافق AP"
BroaderCompat="توافق أكثر"
HigherPerf="أداء أعلى"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="المعدل (802.11a)"
Rate_802_11bg="المعدل (802.11b/g)"
WZC_Managed_Ethernet="Ethernet مُدار بـ WZC"
Legacy="توارث"
IBSS_Link_Indication="مؤشر ارتباط IBSS"

[strings.3801] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="الولايات المتحدة"
54gAuto="54g - تلقائي"
54gLRS="54g - LRS"
54gPerformance="54g - الأداء"
80211bOnly="802.11b فقط"
AntennaDiversity="تنوع الهوائي"
Auto="تلقائي"
AutoShortLong="تلقائي (قصير/طويل)"
BSSPLCPHeader="رأس BSS PLCP"
BlueToothCollaboration="Bluetooth Collaboration"
Default="افتراضي"
Disable="تعطيل"
Disable80211a="تعطيل 802.11a"
Disable80211gb="تعطيل 802.11g/b"
DisableBands="تعطيل نطاقات"
Disabled="مُعطًَل"
Enable="تمكين"
Enabled="مُمكًَن"
FragmentationThreshold="حد التجزئة"
IBSS54gtmMode="وضع IBSS 54g"
IBSS54gtmProtectionMode="وضع حماية IBSS 54g"
IBSSChannelNumber="رقم قناة IBSS"
LocallyAdministeredMACAddress="عنوان MAC مُدار محلياً"
Long="طويل"
None="بلا"
OptimizeBandwidth="تحسين عرض النطاق الترددي"
OptimizeDistance="تحسين المسافة"
PLCPHeader="رأس PLCP"
PowerOutput="خرج الطاقة"
PowerSaveMode="وضع حفظ الطاقة"
Prefer80211a="تفضيل 802.11a"
Prefer80211gb="تفضيل 802.11g/b"
RTSThreshold="حد RTS"
RadioEnableDisable="تعطيل/تمكين الراديو"
Rate="المعدل"
RoamingDecision="تحديد التجوال"
Usebestrate="استخدام أفضل معدل"
XPress_Technology="54g+ (XPress) تكنولوجيا تم تطويرها بواسطة"
Location="الموقع"
Strict="مقيدة"
Loose="واسعة"
Fast="سريعة"
MiminumPowerConsumption="الحد الأدنى من استهلاك الطاقة"
AssociationRoamPreference="تفضيلات تجوال الاقتران"
BandPreference="تفضيلات الموجة"
RoamingTendency="توجه التجوال"
Aggressive="شديد"
Moderate="معتدل"
Conservative="محافظ"
ApCompatibilityMode="وضع توافق AP"
BroaderCompat="توافق أكثر"
HigherPerf="أداء أعلى"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="المعدل (802.11a)"
Rate_802_11bg="المعدل (802.11b/g)"
WZC_Managed_Ethernet="Ethernet مُدار بـ WZC"
Legacy="توارث"
IBSS_Link_Indication="مؤشر ارتباط IBSS"

[strings.0402] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Съединени щати"
54gAuto="54g - Авто"
54gLRS="54g - LRS"
54gPerformance="54g - Производителност"
80211bOnly="Само 802.11b"
AntennaDiversity="Антенно разнообразие"
Auto="Авто"
AutoShortLong="Aвто (дълго/късо)"
BSSPLCPHeader="BSS PLCP заглавка"
BlueToothCollaboration="Съвместимост с Bluetooth"
Default="По подразбиране"
Disable="Дезактивирай"
Disable80211a="Дезактивирай 802.11a"
Disable80211gb="Дезактивирай 802.11g/b"
DisableBands="Дезактивирай диапазоните"
Disabled="Дезактивиран"
Enable="Активирай"
Enabled="Активиран"
FragmentationThreshold="Праг на фрагментиране"
IBSS54gtmMode="IBSS 54g режим"
IBSS54gtmProtectionMode="IBSS 54g защитен режим"
IBSSChannelNumber="Номер на канал IBSS"
LocallyAdministeredMACAddress="Локално администриран MAC адрес"
Long="Дълъг"
None="Няма"
OptimizeBandwidth="Оптимизирай честотната лента"
OptimizeDistance="Оптимизирай разстоянието"
PLCPHeader="PLCP заглавка"
PowerOutput="Мощност на изхода"
PowerSaveMode="Режим на икономия на енергия"
Prefer80211a="Предпочитай 802.11a"
Prefer80211gb="Предпочитай 802.11g/b"
RTSThreshold="RTS праг"
RadioEnableDisable="Активиране/дезактивиране на радиомодем"
Rate="Скорост"
RoamingDecision="Решение за  роуминг"
Usebestrate="Използвай най-добрата скорост"
XPress_Technology="54g+ (XPress)"
Location="Местоположение"
Strict="Стриктно"
Loose="Нестриктно"
Fast="Бързо"
MiminumPowerConsumption="Минимално потребление на енергия"
AssociationRoamPreference="Предпочитание за роуминг при асоцииране"
BandPreference="Предпочитание на лента"
RoamingTendency="Тенденция при роуминг"
Aggressive="Агресивна"
Moderate="Умерена"
Conservative="Консервативна"
ApCompatibilityMode="Режим на AP съвместимост"
BroaderCompat="По-широка съвместимост"
HigherPerf="По-високи показатели"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Скорост (802.11a)"
Rate_802_11bg="Скорост (802.11b/g)"
WZC_Managed_Ethernet="Ethernet, управлявана от WZC"
Legacy="Стар стандарт"
IBSS_Link_Indication="Индикация за IBSS връзка"

[strings.0804] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="美国"
54gAuto="54g - 自动"
54gLRS="54g - LRS"
54gPerformance="54g - 性能"
80211bOnly="仅 802.11b"
AntennaDiversity="天线分集"
Auto="自动"
AutoShortLong="自动（短/长）"
BSSPLCPHeader="BSS PLCP 报头"
BlueToothCollaboration="蓝牙技术协作"
Default="默认"
Disable="禁用"
Disable80211a="禁用 802.11a"
Disable80211gb="禁用 802.11g/b"
DisableBands="禁用波段"
Disabled="禁用"
Enable="启用"
Enabled="启用"
FragmentationThreshold="分段阈值"
IBSS54gtmMode="IBSS 54g 模式"
IBSS54gtmProtectionMode="IBSS 54g 保护模式"
IBSSChannelNumber="IBSS 频道号"
LocallyAdministeredMACAddress="本地管理的 MAC 地址"
Long="长格式"
None="无"
OptimizeBandwidth="优化带宽"
OptimizeDistance="优化距离"
PLCPHeader="PLCP 报头"
PowerOutput="功率输出"
PowerSaveMode="节能模式"
Prefer80211a="首选 802.11a"
Prefer80211gb="首选 802.11g/b"
RTSThreshold="RTS 阀值"
RadioEnableDisable="启用/禁用无线电"
Rate="速率"
RoamingDecision="漫游决定"
Usebestrate="使用最佳传输率"
XPress_Technology="54g+ (XPress)"
Location="位置"
Strict="严格"
Loose="松弛"
Fast="快速"
MiminumPowerConsumption="最低功耗"
AssociationRoamPreference="关联漫游首选项"
BandPreference="波段首选项"
RoamingTendency="漫游趋势"
Aggressive="主动型"
Moderate="中等"
Conservative="保守型"
ApCompatibilityMode="AP 兼容性模式"
BroaderCompat="更广泛的兼容性"
HigherPerf="更高的性能"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="速率 (802.11a)"
Rate_802_11bg="速率 (802.11b/g)"
WZC_Managed_Ethernet="WZC 管理的以太网"
Legacy="Legacy"
IBSS_Link_Indication="IBSS（独立基本服务集）链路指示"

[strings.1004] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="美国"
54gAuto="54g - 自动"
54gLRS="54g - LRS"
54gPerformance="54g - 性能"
80211bOnly="仅 802.11b"
AntennaDiversity="天线分集"
Auto="自动"
AutoShortLong="自动（短/长）"
BSSPLCPHeader="BSS PLCP 报头"
BlueToothCollaboration="蓝牙技术协作"
Default="默认"
Disable="禁用"
Disable80211a="禁用 802.11a"
Disable80211gb="禁用 802.11g/b"
DisableBands="禁用波段"
Disabled="禁用"
Enable="启用"
Enabled="启用"
FragmentationThreshold="分段阈值"
IBSS54gtmMode="IBSS 54g 模式"
IBSS54gtmProtectionMode="IBSS 54g 保护模式"
IBSSChannelNumber="IBSS 频道号"
LocallyAdministeredMACAddress="本地管理的 MAC 地址"
Long="长格式"
None="无"
OptimizeBandwidth="优化带宽"
OptimizeDistance="优化距离"
PLCPHeader="PLCP 报头"
PowerOutput="功率输出"
PowerSaveMode="节能模式"
Prefer80211a="首选 802.11a"
Prefer80211gb="首选 802.11g/b"
RTSThreshold="RTS 阀值"
RadioEnableDisable="启用/禁用无线电"
Rate="速率"
RoamingDecision="漫游决定"
Usebestrate="使用最佳传输率"
XPress_Technology="54g+ (XPress)"
Location="位置"
Strict="严格"
Loose="松弛"
Fast="快速"
MiminumPowerConsumption="最低功耗"
AssociationRoamPreference="关联漫游首选项"
BandPreference="波段首选项"
RoamingTendency="漫游趋势"
Aggressive="主动型"
Moderate="中等"
Conservative="保守型"
ApCompatibilityMode="AP 兼容性模式"
BroaderCompat="更广泛的兼容性"
HigherPerf="更高的性能"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="速率 (802.11a)"
Rate_802_11bg="速率 (802.11b/g)"
WZC_Managed_Ethernet="WZC 管理的以太网"
Legacy="Legacy"
IBSS_Link_Indication="IBSS（独立基本服务集）链路指示"

[strings.0c04] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="美國"
54gAuto="54g - 自動"
54gLRS="54g - LRS"
54gPerformance="54g - 效能"
80211bOnly="僅 802.11b"
AntennaDiversity="天線散佈"
Auto="自動"
AutoShortLong="自動 (短/長)"
BSSPLCPHeader="BSS PLCP 標頭"
BlueToothCollaboration="藍芽技術合作"
Default="預設值"
Disable="停用"
Disable80211a="停用 802.11a"
Disable80211gb="停用 802.11g/b"
DisableBands="停用頻寬"
Disabled="已停用"
Enable="啟用"
Enabled="已啟用"
FragmentationThreshold="分散臨界值"
IBSS54gtmMode="IBSS 54g 模式"
IBSS54gtmProtectionMode="IBSS 54g 保護模式"
IBSSChannelNumber="IBSS 頻道號碼"
LocallyAdministeredMACAddress="本機管理 MAC 位址"
Long="長"
None="無"
OptimizeBandwidth="最佳化頻寬"
OptimizeDistance="最佳化距離"
PLCPHeader="PLCP 標頭"
PowerOutput="功率輸出"
PowerSaveMode="省電模式"
Prefer80211a="慣用 802.11a"
Prefer80211gb="慣用 802.11g/b"
RTSThreshold="RTS 臨界值"
RadioEnableDisable="啟用/停用無線功能"
Rate="速率"
RoamingDecision="漫遊決定"
Usebestrate="使用最佳速率"
XPress_Technology="54g+ (XPress)"
Location="位置"
Strict="嚴格"
Loose="寬鬆"
Fast="快速"
MiminumPowerConsumption="最低耗電量"
AssociationRoamPreference="漫遊關聯喜好設定"
BandPreference="頻寬喜好設定"
RoamingTendency="漫遊傾向"
Aggressive="積極"
Moderate="中等"
Conservative="傳統"
ApCompatibilityMode="AP 相容性模式"
BroaderCompat="高相容性"
HigherPerf="高效能"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="速率 (802.11a)"
Rate_802_11bg="速率 (802.11b/g)"
WZC_Managed_Ethernet="以 WZC 管理的 Ethernet"
Legacy="傳統"
IBSS_Link_Indication="IBSS 連結指示"

[strings.0404] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="802.11網路介面卡安裝盤"
UnitedStates="美國"
54gAuto="54g - 自動"
54gLRS="54g - LRS"
54gPerformance="54g - 效能"
80211bOnly="僅 802.11b"
AntennaDiversity="天線散佈"
Auto="自動"
AutoShortLong="自動 (短/長)"
BSSPLCPHeader="BSS PLCP 標頭"
BlueToothCollaboration="藍芽技術合作"
Default="預設值"
Disable="停用"
Disable80211a="停用 802.11a"
Disable80211gb="停用 802.11g/b"
DisableBands="停用頻寬"
Disabled="已停用"
Enable="啟用"
Enabled="已啟用"
FragmentationThreshold="分散臨界值"
IBSS54gtmMode="IBSS 54g 模式"
IBSS54gtmProtectionMode="IBSS 54g 保護模式"
IBSSChannelNumber="IBSS 頻道號碼"
LocallyAdministeredMACAddress="本機管理 MAC 位址"
Long="長"
None="無"
OptimizeBandwidth="最佳化頻寬"
OptimizeDistance="最佳化距離"
PLCPHeader="PLCP 標頭"
PowerOutput="功率輸出"
PowerSaveMode="省電模式"
Prefer80211a="慣用 802.11a"
Prefer80211gb="慣用 802.11g/b"
RTSThreshold="RTS 臨界值"
RadioEnableDisable="啟用/停用無線功能"
Rate="速率"
RoamingDecision="漫遊決定"
Usebestrate="使用最佳速率"
XPress_Technology="54g+ (XPress)"
Location="位置"
Strict="嚴格"
Loose="寬鬆"
Fast="快速"
MiminumPowerConsumption="最低耗電量"
AssociationRoamPreference="漫遊關聯喜好設定"
BandPreference="頻寬喜好設定"
RoamingTendency="漫遊傾向"
Aggressive="積極"
Moderate="中等"
Conservative="傳統"
ApCompatibilityMode="AP 相容性模式"
BroaderCompat="高相容性"
HigherPerf="高效能"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="速率 (802.11a)"
Rate_802_11bg="速率 (802.11b/g)"
WZC_Managed_Ethernet="以 WZC 管理的 Ethernet"
Legacy="傳統"
IBSS_Link_Indication="IBSS 連結指示"

[strings.041a] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Sjedinjene Države Djevičansko otočje"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - Izvedba"
80211bOnly="802.11b Samo"
AntennaDiversity="Višestruki antenski prijenos"
Auto="Automatski"
AutoShortLong="Auto (kratki/dugi)"
BSSPLCPHeader="BSS PLCP Zaglavlje"
BlueToothCollaboration="Bluetooth Suradnja"
Default="Zadano"
Disable="Onemogući"
Disable80211a="Onemogući 802.11a"
Disable80211gb="Onemogući 802.11g/b"
DisableBands="Onemogući frekvencijske pojaseve"
Disabled="Onemogućeno"
Enable="Omogući"
Enabled="Omogućeno"
FragmentationThreshold="Prag fragmentacije"
IBSS54gtmMode="IBSS 54g način rada"
IBSS54gtmProtectionMode="IBSS 54g način zaštite"
IBSSChannelNumber="IBSS broj kanala"
LocallyAdministeredMACAddress="Lokalno administrirana MAC adresa"
Long="Dugo"
None="Ništa"
OptimizeBandwidth="Optimiziraj širinu frekvencijskog pojasa"
OptimizeDistance="Optimiziraj udaljenost"
PLCPHeader="PLCP Zaglavlje"
PowerOutput="Izlazna snaga"
PowerSaveMode="Način rada s uštedom energije"
Prefer80211a="Povlastica 802.11a"
Prefer80211gb="Povlastica 802.11g/b"
RTSThreshold="RTS prag"
RadioEnableDisable="Omogući/onemogući radio"
Rate="Brzina"
RoamingDecision="Odluka o roamingu"
Usebestrate="Upotrijebi najbolju brzinu"
XPress_Technology="54g+ (XPress)"
Location="Lokacija"
Strict="Striktno"
Loose="Opušteno"
Fast="Brzo"
MiminumPowerConsumption="Minimalna potrošnja energije"
AssociationRoamPreference="Preferirano pridruživanje u roamingu"
BandPreference="Preferirani frekvencijski pojas"
RoamingTendency="Tendencija u roamingu"
Aggressive="Agresivno"
Moderate="Umjereno"
Conservative="Konzervativno"
ApCompatibilityMode="Kompatibilnost pristupne točke"
BroaderCompat="Šira kompatibilnost"
HigherPerf="Viša izvedba"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Brzina (802.11a)"
Rate_802_11bg="Brzina (802.11b/g)"
WZC_Managed_Ethernet="Upravljanje Ethernetom putem bežične nulte konfiguracije (WZC)"
Legacy="Nasljeđe"
IBSS_Link_Indication="Oznaka IBSS veze"

[strings.0405] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Spojené státy"
54gAuto="Protokol 54g - automaticky"
54gLRS="54g - LRS"
54gPerformance="Protokol 54g - výkonnost"
80211bOnly="Pouze protokol 802.11b"
AntennaDiversity="Anténa pro vícenásobný příjem"
Auto="Automatický"
AutoShortLong="Automatický (krátký/dlouhý)"
BSSPLCPHeader="Hlavička BSS PLCP"
BlueToothCollaboration="Součinnost zařízení Bluetooth"
Default="Výchozí"
Disable="Zakázat"
Disable80211a="Zakázat protokol 802.11a"
Disable80211gb="Zakázat protokol 802.11g/b"
DisableBands="Zakázat pásma"
Disabled="Zakázáno"
Enable="Povolit"
Enabled="Povoleno"
FragmentationThreshold="Mezní hodnota fragmentace"
IBSS54gtmMode="Režim protokolu IBSS 54g"
IBSS54gtmProtectionMode="Ochranný režim protokolu IBSS 54g"
IBSSChannelNumber="Číslo kanálu IBSS"
LocallyAdministeredMACAddress="Místně spravovaná adresa MAC"
Long="Dlouhé"
None="Žádný"
OptimizeBandwidth="Optimalizovat šířku pásma"
OptimizeDistance="Optimalizovat vzdálenost"
PLCPHeader="Záhlaví PLCP"
PowerOutput="Výstupní výkon"
PowerSaveMode="Režim úspory energie"
Prefer80211a="Upřednostnit protokol 802.11a"
Prefer80211gb="Upřednostnit protokol 802.11g/b"
RTSThreshold="Mezní hodnota RTS"
RadioEnableDisable="Zapnout nebo vypnout rádio"
Rate="Rychlost"
RoamingDecision="Možnost cestování (roaming)"
Usebestrate="Použít nejvhodnější rychlost"
XPress_Technology="54g+ (XPress)"
Location="Umístění"
Strict="Přesný"
Loose="Volný"
Fast="Rychlý"
MiminumPowerConsumption="Minimální spotřeba energie"
AssociationRoamPreference="Preference přiřazování u roamingu"
BandPreference="Preference pásma"
RoamingTendency="Tendence roamingu"
Aggressive="Agresivní"
Moderate="Mírně"
Conservative="Omezené"
ApCompatibilityMode="Režim kompatibility AP"
BroaderCompat="Širší kompatibilita"
HigherPerf="Vyšší výkon"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Rychlost (802.11a)"
Rate_802_11bg="Rychlost (802.11b/g)"
WZC_Managed_Ethernet="Ethernet řízený automatickou konfigurací bezdrátových zařízení"
Legacy="Starší verze"
IBSS_Link_Indication="Indikace spojení IBSS"

[strings.0406] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="USA"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - Ydeevne"
80211bOnly="Kun 802.11b"
AntennaDiversity="Antennevariation"
Auto="Automatisk"
AutoShortLong="Auto (Kort/Lang)"
BSSPLCPHeader="BSS PLCP-hoved"
BlueToothCollaboration="Bluetooth-samarbejde"
Default="Standard"
Disable="Deaktiver"
Disable80211a="Deaktiver 802.11a"
Disable80211gb="Deaktiver 802.11g/b"
DisableBands="Deaktiver bånd"
Disabled="Deaktiveret"
Enable="Aktiver"
Enabled="Aktiveret"
FragmentationThreshold="Fragmenteringstærskel"
IBSS54gtmMode="IBSS 54g Tilstand"
IBSS54gtmProtectionMode="IBSS 54g Beskyttelsestilstand"
IBSSChannelNumber="IBSS-kanalnummer"
LocallyAdministeredMACAddress="Lokalt administreret MAC-adresse"
Long="Lang"
None="Ingen"
OptimizeBandwidth="Optimer båndbredde"
OptimizeDistance="Optimer distance"
PLCPHeader="PLCP-hoved"
PowerOutput="Strømforbrug"
PowerSaveMode="Strømbesparelsestilstand"
Prefer80211a="Foretræk 802.11a"
Prefer80211gb="Foretræk 802.11g/b"
RTSThreshold="RTS-grænseværdi"
RadioEnableDisable="Aktiver/deaktiver radio"
Rate="Hastighed"
RoamingDecision="Roaming-valg"
Usebestrate="Brug bedste hastighed"
XPress_Technology="54g+ (XPress)"
Location="Placering"
Strict="Restriktiv"
Loose="Ikke-restriktiv"
Fast="Hurtig"
MiminumPowerConsumption="Minimalt strømforbrug"
AssociationRoamPreference="Indstillinger for tilknytning via roaming"
BandPreference="Foretrukket bånd"
RoamingTendency="Roaming-tendens"
Aggressive="Aggressiv"
Moderate="Moderat"
Conservative="Forsigtig"
ApCompatibilityMode="AP-kompatibilitetsmodus"
BroaderCompat="Bredere kompatibilitet"
HigherPerf="Højere ydeevne"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Hastighed (802.11a)"
Rate_802_11bg="Hastighed (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS-forbindelsesstatus"

[strings.0813] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Verenigde Staten"
54gAuto="54g - automatisch"
54gLRS="54g - LRS"
54gPerformance="54g - prestaties"
80211bOnly="Alleen 802.11b"
AntennaDiversity="Antennediversiteit"
Auto="Autom."
AutoShortLong="Autom. (kort/lang)"
BSSPLCPHeader="BSS-PLCP-koptekst"
BlueToothCollaboration="Samenwerking met Bluetooth"
Default="Standaard"
Disable="Uitschakelen"
Disable80211a="802.11a uitschakelen"
Disable80211gb="802.11g/b uitschakelen"
DisableBands="Frequentiebanden uitschakelen"
Disabled="Uitgeschakeld"
Enable="Inschakelen"
Enabled="Ingeschakeld"
FragmentationThreshold="Fragmentatiedrempel"
IBSS54gtmMode="IBSS 54g-modus"
IBSS54gtmProtectionMode="IBSS 54g-beveiligingsmodus"
IBSSChannelNumber="IBSS-kanaalnummer"
LocallyAdministeredMACAddress="Lokaal beheerd MAC-adres"
Long="Lang"
None="Geen"
OptimizeBandwidth="Bandbreedte optimaliseren"
OptimizeDistance="Afstand optimaliseren"
PLCPHeader="PLCP-koptekst"
PowerOutput="Vermogen"
PowerSaveMode="Energiespaarstand"
Prefer80211a="Voorkeur voor 802.11a"
Prefer80211gb="Voorkeur voor 802.11g/b"
RTSThreshold="RTS-drempel"
RadioEnableDisable="Radio inschakelen/uitschakelen"
Rate="Snelheid"
RoamingDecision="Roaming-beslissing"
Usebestrate="Beste snelheid gebruiken"
XPress_Technology="54g+ (XPress)"
Location="Locatie"
Strict="Streng"
Loose="Los"
Fast="Snel"
MiminumPowerConsumption="Minimaal energieverbruik"
AssociationRoamPreference="Roaming-voorkeur koppelen"
BandPreference="Voorkeur frequentieband"
RoamingTendency="Roaming-tendentie"
Aggressive="Agressief"
Moderate="Gemiddeld"
Conservative="Niet agressief"
ApCompatibilityMode="AP-compatibiliteitsmodus"
BroaderCompat="Hogere compatibiliteit"
HigherPerf="Betere prestaties"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Snelheid (802.11a)"
Rate_802_11bg="Snelheid (802.11b/g)"
WZC_Managed_Ethernet="Ethernet met WZC"
Legacy="Oude apparaten"
IBSS_Link_Indication="Indicatie voor IBSS-koppeling"

[strings.0413] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Verenigde Staten"
54gAuto="54g - automatisch"
54gLRS="54g - LRS"
54gPerformance="54g - prestaties"
80211bOnly="Alleen 802.11b"
AntennaDiversity="Antennediversiteit"
Auto="Autom."
AutoShortLong="Autom. (kort/lang)"
BSSPLCPHeader="BSS-PLCP-koptekst"
BlueToothCollaboration="Samenwerking met Bluetooth"
Default="Standaard"
Disable="Uitschakelen"
Disable80211a="802.11a uitschakelen"
Disable80211gb="802.11g/b uitschakelen"
DisableBands="Frequentiebanden uitschakelen"
Disabled="Uitgeschakeld"
Enable="Inschakelen"
Enabled="Ingeschakeld"
FragmentationThreshold="Fragmentatiedrempel"
IBSS54gtmMode="IBSS 54g-modus"
IBSS54gtmProtectionMode="IBSS 54g-beveiligingsmodus"
IBSSChannelNumber="IBSS-kanaalnummer"
LocallyAdministeredMACAddress="Lokaal beheerd MAC-adres"
Long="Lang"
None="Geen"
OptimizeBandwidth="Bandbreedte optimaliseren"
OptimizeDistance="Afstand optimaliseren"
PLCPHeader="PLCP-koptekst"
PowerOutput="Vermogen"
PowerSaveMode="Energiespaarstand"
Prefer80211a="Voorkeur voor 802.11a"
Prefer80211gb="Voorkeur voor 802.11g/b"
RTSThreshold="RTS-drempel"
RadioEnableDisable="Radio inschakelen/uitschakelen"
Rate="Snelheid"
RoamingDecision="Roaming-beslissing"
Usebestrate="Beste snelheid gebruiken"
XPress_Technology="54g+ (XPress)"
Location="Locatie"
Strict="Streng"
Loose="Los"
Fast="Snel"
MiminumPowerConsumption="Minimaal energieverbruik"
AssociationRoamPreference="Roaming-voorkeur koppelen"
BandPreference="Voorkeur frequentieband"
RoamingTendency="Roaming-tendentie"
Aggressive="Agressief"
Moderate="Gemiddeld"
Conservative="Niet agressief"
ApCompatibilityMode="AP-compatibiliteitsmodus"
BroaderCompat="Hogere compatibiliteit"
HigherPerf="Betere prestaties"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Snelheid (802.11a)"
Rate_802_11bg="Snelheid (802.11b/g)"
WZC_Managed_Ethernet="Ethernet met WZC"
Legacy="Oude apparaten"
IBSS_Link_Indication="Indicatie voor IBSS-koppeling"

[strings.0c09] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="United States"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - Performance"
80211bOnly="802.11b Only"
AntennaDiversity="Antenna Diversity"
Auto="Auto"
AutoShortLong="Auto (Short/Long)"
BSSPLCPHeader="BSS PLCP Header"
BlueToothCollaboration="Bluetooth Collaboration"
Default="Default"
Disable="Disable"
Disable80211a="Disable 802.11a"
Disable80211gb="Disable 802.11g/b"
DisableBands="Disable Bands"
Disabled="Disabled"
Enable="Enable"
Enabled="Enabled"
FragmentationThreshold="Fragmentation Threshold"
IBSS54gtmMode="IBSS 54g Mode"
IBSS54gtmProtectionMode="IBSS 54g Protection Mode"
IBSSChannelNumber="IBSS Channel Number"
LocallyAdministeredMACAddress="Locally Administered MAC Address"
Long="Long"
None="None"
OptimizeBandwidth="Optimize Bandwidth"
OptimizeDistance="Optimize Distance"
PLCPHeader="PLCP Header"
PowerOutput="Power Output"
PowerSaveMode="Power Save Mode"
Prefer80211a="Prefer 802.11a"
Prefer80211gb="Prefer 802.11g/b"
RTSThreshold="RTS Threshold"
RadioEnableDisable="Radio Enable/Disable"
Rate="Rate"
RoamingDecision="Roaming Decision"
Usebestrate="Use best rate"
XPress_Technology="54g+ (XPress)"
Location="Location"
Strict="Strict"
Loose="Loose"
Fast="Fast"
MiminumPowerConsumption="Minimum Power Consumption"
AssociationRoamPreference="Association Roam Preference"
BandPreference="Band Preference"
RoamingTendency="Roam Tendency"
Aggressive="Aggressive"
Moderate="Moderate"
Conservative="Conservative"
ApCompatibilityMode="AP Compatibility Mode"
BroaderCompat="Broader Compatibility"
HigherPerf="Higher Performance"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Rate (802.11a)"
Rate_802_11bg="Rate (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS Link Indication"

[strings.1009] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="United States"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - Performance"
80211bOnly="802.11b Only"
AntennaDiversity="Antenna Diversity"
Auto="Auto"
AutoShortLong="Auto (Short/Long)"
BSSPLCPHeader="BSS PLCP Header"
BlueToothCollaboration="Bluetooth Collaboration"
Default="Default"
Disable="Disable"
Disable80211a="Disable 802.11a"
Disable80211gb="Disable 802.11g/b"
DisableBands="Disable Bands"
Disabled="Disabled"
Enable="Enable"
Enabled="Enabled"
FragmentationThreshold="Fragmentation Threshold"
IBSS54gtmMode="IBSS 54g Mode"
IBSS54gtmProtectionMode="IBSS 54g Protection Mode"
IBSSChannelNumber="IBSS Channel Number"
LocallyAdministeredMACAddress="Locally Administered MAC Address"
Long="Long"
None="None"
OptimizeBandwidth="Optimize Bandwidth"
OptimizeDistance="Optimize Distance"
PLCPHeader="PLCP Header"
PowerOutput="Power Output"
PowerSaveMode="Power Save Mode"
Prefer80211a="Prefer 802.11a"
Prefer80211gb="Prefer 802.11g/b"
RTSThreshold="RTS Threshold"
RadioEnableDisable="Radio Enable/Disable"
Rate="Rate"
RoamingDecision="Roaming Decision"
Usebestrate="Use best rate"
XPress_Technology="54g+ (XPress)"
Location="Location"
Strict="Strict"
Loose="Loose"
Fast="Fast"
MiminumPowerConsumption="Minimum Power Consumption"
AssociationRoamPreference="Association Roam Preference"
BandPreference="Band Preference"
RoamingTendency="Roam Tendency"
Aggressive="Aggressive"
Moderate="Moderate"
Conservative="Conservative"
ApCompatibilityMode="AP Compatibility Mode"
BroaderCompat="Broader Compatibility"
HigherPerf="Higher Performance"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Rate (802.11a)"
Rate_802_11bg="Rate (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS Link Indication"

[strings.040f] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="United States"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - Performance"
80211bOnly="802.11b Only"
AntennaDiversity="Antenna Diversity"
Auto="Auto"
AutoShortLong="Auto (Short/Long)"
BSSPLCPHeader="BSS PLCP Header"
BlueToothCollaboration="Bluetooth Collaboration"
Default="Default"
Disable="Disable"
Disable80211a="Disable 802.11a"
Disable80211gb="Disable 802.11g/b"
DisableBands="Disable Bands"
Disabled="Disabled"
Enable="Enable"
Enabled="Enabled"
FragmentationThreshold="Fragmentation Threshold"
IBSS54gtmMode="IBSS 54g Mode"
IBSS54gtmProtectionMode="IBSS 54g Protection Mode"
IBSSChannelNumber="IBSS Channel Number"
LocallyAdministeredMACAddress="Locally Administered MAC Address"
Long="Long"
None="None"
OptimizeBandwidth="Optimize Bandwidth"
OptimizeDistance="Optimize Distance"
PLCPHeader="PLCP Header"
PowerOutput="Power Output"
PowerSaveMode="Power Save Mode"
Prefer80211a="Prefer 802.11a"
Prefer80211gb="Prefer 802.11g/b"
RTSThreshold="RTS Threshold"
RadioEnableDisable="Radio Enable/Disable"
Rate="Rate"
RoamingDecision="Roaming Decision"
Usebestrate="Use best rate"
XPress_Technology="54g+ (XPress)"
Location="Location"
Strict="Strict"
Loose="Loose"
Fast="Fast"
MiminumPowerConsumption="Minimum Power Consumption"
AssociationRoamPreference="Association Roam Preference"
BandPreference="Band Preference"
RoamingTendency="Roam Tendency"
Aggressive="Aggressive"
Moderate="Moderate"
Conservative="Conservative"
ApCompatibilityMode="AP Compatibility Mode"
BroaderCompat="Broader Compatibility"
HigherPerf="Higher Performance"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Rate (802.11a)"
Rate_802_11bg="Rate (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS Link Indication"

[strings.0421] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="United States"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - Performance"
80211bOnly="802.11b Only"
AntennaDiversity="Antenna Diversity"
Auto="Auto"
AutoShortLong="Auto (Short/Long)"
BSSPLCPHeader="BSS PLCP Header"
BlueToothCollaboration="Bluetooth Collaboration"
Default="Default"
Disable="Disable"
Disable80211a="Disable 802.11a"
Disable80211gb="Disable 802.11g/b"
DisableBands="Disable Bands"
Disabled="Disabled"
Enable="Enable"
Enabled="Enabled"
FragmentationThreshold="Fragmentation Threshold"
IBSS54gtmMode="IBSS 54g Mode"
IBSS54gtmProtectionMode="IBSS 54g Protection Mode"
IBSSChannelNumber="IBSS Channel Number"
LocallyAdministeredMACAddress="Locally Administered MAC Address"
Long="Long"
None="None"
OptimizeBandwidth="Optimize Bandwidth"
OptimizeDistance="Optimize Distance"
PLCPHeader="PLCP Header"
PowerOutput="Power Output"
PowerSaveMode="Power Save Mode"
Prefer80211a="Prefer 802.11a"
Prefer80211gb="Prefer 802.11g/b"
RTSThreshold="RTS Threshold"
RadioEnableDisable="Radio Enable/Disable"
Rate="Rate"
RoamingDecision="Roaming Decision"
Usebestrate="Use best rate"
XPress_Technology="54g+ (XPress)"
Location="Location"
Strict="Strict"
Loose="Loose"
Fast="Fast"
MiminumPowerConsumption="Minimum Power Consumption"
AssociationRoamPreference="Association Roam Preference"
BandPreference="Band Preference"
RoamingTendency="Roam Tendency"
Aggressive="Aggressive"
Moderate="Moderate"
Conservative="Conservative"
ApCompatibilityMode="AP Compatibility Mode"
BroaderCompat="Broader Compatibility"
HigherPerf="Higher Performance"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Rate (802.11a)"
Rate_802_11bg="Rate (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS Link Indication"

[strings.1809] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="United States"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - Performance"
80211bOnly="802.11b Only"
AntennaDiversity="Antenna Diversity"
Auto="Auto"
AutoShortLong="Auto (Short/Long)"
BSSPLCPHeader="BSS PLCP Header"
BlueToothCollaboration="Bluetooth Collaboration"
Default="Default"
Disable="Disable"
Disable80211a="Disable 802.11a"
Disable80211gb="Disable 802.11g/b"
DisableBands="Disable Bands"
Disabled="Disabled"
Enable="Enable"
Enabled="Enabled"
FragmentationThreshold="Fragmentation Threshold"
IBSS54gtmMode="IBSS 54g Mode"
IBSS54gtmProtectionMode="IBSS 54g Protection Mode"
IBSSChannelNumber="IBSS Channel Number"
LocallyAdministeredMACAddress="Locally Administered MAC Address"
Long="Long"
None="None"
OptimizeBandwidth="Optimize Bandwidth"
OptimizeDistance="Optimize Distance"
PLCPHeader="PLCP Header"
PowerOutput="Power Output"
PowerSaveMode="Power Save Mode"
Prefer80211a="Prefer 802.11a"
Prefer80211gb="Prefer 802.11g/b"
RTSThreshold="RTS Threshold"
RadioEnableDisable="Radio Enable/Disable"
Rate="Rate"
RoamingDecision="Roaming Decision"
Usebestrate="Use best rate"
XPress_Technology="54g+ (XPress)"
Location="Location"
Strict="Strict"
Loose="Loose"
Fast="Fast"
MiminumPowerConsumption="Minimum Power Consumption"
AssociationRoamPreference="Association Roam Preference"
BandPreference="Band Preference"
RoamingTendency="Roam Tendency"
Aggressive="Aggressive"
Moderate="Moderate"
Conservative="Conservative"
ApCompatibilityMode="AP Compatibility Mode"
BroaderCompat="Broader Compatibility"
HigherPerf="Higher Performance"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Rate (802.11a)"
Rate_802_11bg="Rate (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS Link Indication"

[strings.043e] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="United States"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - Performance"
80211bOnly="802.11b Only"
AntennaDiversity="Antenna Diversity"
Auto="Auto"
AutoShortLong="Auto (Short/Long)"
BSSPLCPHeader="BSS PLCP Header"
BlueToothCollaboration="Bluetooth Collaboration"
Default="Default"
Disable="Disable"
Disable80211a="Disable 802.11a"
Disable80211gb="Disable 802.11g/b"
DisableBands="Disable Bands"
Disabled="Disabled"
Enable="Enable"
Enabled="Enabled"
FragmentationThreshold="Fragmentation Threshold"
IBSS54gtmMode="IBSS 54g Mode"
IBSS54gtmProtectionMode="IBSS 54g Protection Mode"
IBSSChannelNumber="IBSS Channel Number"
LocallyAdministeredMACAddress="Locally Administered MAC Address"
Long="Long"
None="None"
OptimizeBandwidth="Optimize Bandwidth"
OptimizeDistance="Optimize Distance"
PLCPHeader="PLCP Header"
PowerOutput="Power Output"
PowerSaveMode="Power Save Mode"
Prefer80211a="Prefer 802.11a"
Prefer80211gb="Prefer 802.11g/b"
RTSThreshold="RTS Threshold"
RadioEnableDisable="Radio Enable/Disable"
Rate="Rate"
RoamingDecision="Roaming Decision"
Usebestrate="Use best rate"
XPress_Technology="54g+ (XPress)"
Location="Location"
Strict="Strict"
Loose="Loose"
Fast="Fast"
MiminumPowerConsumption="Minimum Power Consumption"
AssociationRoamPreference="Association Roam Preference"
BandPreference="Band Preference"
RoamingTendency="Roam Tendency"
Aggressive="Aggressive"
Moderate="Moderate"
Conservative="Conservative"
ApCompatibilityMode="AP Compatibility Mode"
BroaderCompat="Broader Compatibility"
HigherPerf="Higher Performance"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Rate (802.11a)"
Rate_802_11bg="Rate (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS Link Indication"

[strings.1409] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="United States"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - Performance"
80211bOnly="802.11b Only"
AntennaDiversity="Antenna Diversity"
Auto="Auto"
AutoShortLong="Auto (Short/Long)"
BSSPLCPHeader="BSS PLCP Header"
BlueToothCollaboration="Bluetooth Collaboration"
Default="Default"
Disable="Disable"
Disable80211a="Disable 802.11a"
Disable80211gb="Disable 802.11g/b"
DisableBands="Disable Bands"
Disabled="Disabled"
Enable="Enable"
Enabled="Enabled"
FragmentationThreshold="Fragmentation Threshold"
IBSS54gtmMode="IBSS 54g Mode"
IBSS54gtmProtectionMode="IBSS 54g Protection Mode"
IBSSChannelNumber="IBSS Channel Number"
LocallyAdministeredMACAddress="Locally Administered MAC Address"
Long="Long"
None="None"
OptimizeBandwidth="Optimize Bandwidth"
OptimizeDistance="Optimize Distance"
PLCPHeader="PLCP Header"
PowerOutput="Power Output"
PowerSaveMode="Power Save Mode"
Prefer80211a="Prefer 802.11a"
Prefer80211gb="Prefer 802.11g/b"
RTSThreshold="RTS Threshold"
RadioEnableDisable="Radio Enable/Disable"
Rate="Rate"
RoamingDecision="Roaming Decision"
Usebestrate="Use best rate"
XPress_Technology="54g+ (XPress)"
Location="Location"
Strict="Strict"
Loose="Loose"
Fast="Fast"
MiminumPowerConsumption="Minimum Power Consumption"
AssociationRoamPreference="Association Roam Preference"
BandPreference="Band Preference"
RoamingTendency="Roam Tendency"
Aggressive="Aggressive"
Moderate="Moderate"
Conservative="Conservative"
ApCompatibilityMode="AP Compatibility Mode"
BroaderCompat="Broader Compatibility"
HigherPerf="Higher Performance"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Rate (802.11a)"
Rate_802_11bg="Rate (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS Link Indication"

[strings.3409] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="United States"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - Performance"
80211bOnly="802.11b Only"
AntennaDiversity="Antenna Diversity"
Auto="Auto"
AutoShortLong="Auto (Short/Long)"
BSSPLCPHeader="BSS PLCP Header"
BlueToothCollaboration="Bluetooth Collaboration"
Default="Default"
Disable="Disable"
Disable80211a="Disable 802.11a"
Disable80211gb="Disable 802.11g/b"
DisableBands="Disable Bands"
Disabled="Disabled"
Enable="Enable"
Enabled="Enabled"
FragmentationThreshold="Fragmentation Threshold"
IBSS54gtmMode="IBSS 54g Mode"
IBSS54gtmProtectionMode="IBSS 54g Protection Mode"
IBSSChannelNumber="IBSS Channel Number"
LocallyAdministeredMACAddress="Locally Administered MAC Address"
Long="Long"
None="None"
OptimizeBandwidth="Optimize Bandwidth"
OptimizeDistance="Optimize Distance"
PLCPHeader="PLCP Header"
PowerOutput="Power Output"
PowerSaveMode="Power Save Mode"
Prefer80211a="Prefer 802.11a"
Prefer80211gb="Prefer 802.11g/b"
RTSThreshold="RTS Threshold"
RadioEnableDisable="Radio Enable/Disable"
Rate="Rate"
RoamingDecision="Roaming Decision"
Usebestrate="Use best rate"
XPress_Technology="54g+ (XPress)"
Location="Location"
Strict="Strict"
Loose="Loose"
Fast="Fast"
MiminumPowerConsumption="Minimum Power Consumption"
AssociationRoamPreference="Association Roam Preference"
BandPreference="Band Preference"
RoamingTendency="Roam Tendency"
Aggressive="Aggressive"
Moderate="Moderate"
Conservative="Conservative"
ApCompatibilityMode="AP Compatibility Mode"
BroaderCompat="Broader Compatibility"
HigherPerf="Higher Performance"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Rate (802.11a)"
Rate_802_11bg="Rate (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS Link Indication"

[strings.1c09] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="United States"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - Performance"
80211bOnly="802.11b Only"
AntennaDiversity="Antenna Diversity"
Auto="Auto"
AutoShortLong="Auto (Short/Long)"
BSSPLCPHeader="BSS PLCP Header"
BlueToothCollaboration="Bluetooth Collaboration"
Default="Default"
Disable="Disable"
Disable80211a="Disable 802.11a"
Disable80211gb="Disable 802.11g/b"
DisableBands="Disable Bands"
Disabled="Disabled"
Enable="Enable"
Enabled="Enabled"
FragmentationThreshold="Fragmentation Threshold"
IBSS54gtmMode="IBSS 54g Mode"
IBSS54gtmProtectionMode="IBSS 54g Protection Mode"
IBSSChannelNumber="IBSS Channel Number"
LocallyAdministeredMACAddress="Locally Administered MAC Address"
Long="Long"
None="None"
OptimizeBandwidth="Optimize Bandwidth"
OptimizeDistance="Optimize Distance"
PLCPHeader="PLCP Header"
PowerOutput="Power Output"
PowerSaveMode="Power Save Mode"
Prefer80211a="Prefer 802.11a"
Prefer80211gb="Prefer 802.11g/b"
RTSThreshold="RTS Threshold"
RadioEnableDisable="Radio Enable/Disable"
Rate="Rate"
RoamingDecision="Roaming Decision"
Usebestrate="Use best rate"
XPress_Technology="54g+ (XPress)"
Location="Location"
Strict="Strict"
Loose="Loose"
Fast="Fast"
MiminumPowerConsumption="Minimum Power Consumption"
AssociationRoamPreference="Association Roam Preference"
BandPreference="Band Preference"
RoamingTendency="Roam Tendency"
Aggressive="Aggressive"
Moderate="Moderate"
Conservative="Conservative"
ApCompatibilityMode="AP Compatibility Mode"
BroaderCompat="Broader Compatibility"
HigherPerf="Higher Performance"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Rate (802.11a)"
Rate_802_11bg="Rate (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS Link Indication"

[strings.0809] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="United States"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - Performance"
80211bOnly="802.11b Only"
AntennaDiversity="Antenna Diversity"
Auto="Auto"
AutoShortLong="Auto (Short/Long)"
BSSPLCPHeader="BSS PLCP Header"
BlueToothCollaboration="Bluetooth Collaboration"
Default="Default"
Disable="Disable"
Disable80211a="Disable 802.11a"
Disable80211gb="Disable 802.11g/b"
DisableBands="Disable Bands"
Disabled="Disabled"
Enable="Enable"
Enabled="Enabled"
FragmentationThreshold="Fragmentation Threshold"
IBSS54gtmMode="IBSS 54g Mode"
IBSS54gtmProtectionMode="IBSS 54g Protection Mode"
IBSSChannelNumber="IBSS Channel Number"
LocallyAdministeredMACAddress="Locally Administered MAC Address"
Long="Long"
None="None"
OptimizeBandwidth="Optimize Bandwidth"
OptimizeDistance="Optimize Distance"
PLCPHeader="PLCP Header"
PowerOutput="Power Output"
PowerSaveMode="Power Save Mode"
Prefer80211a="Prefer 802.11a"
Prefer80211gb="Prefer 802.11g/b"
RTSThreshold="RTS Threshold"
RadioEnableDisable="Radio Enable/Disable"
Rate="Rate"
RoamingDecision="Roaming Decision"
Usebestrate="Use best rate"
XPress_Technology="54g+ (XPress)"
Location="Location"
Strict="Strict"
Loose="Loose"
Fast="Fast"
MiminumPowerConsumption="Minimum Power Consumption"
AssociationRoamPreference="Association Roam Preference"
BandPreference="Band Preference"
RoamingTendency="Roam Tendency"
Aggressive="Aggressive"
Moderate="Moderate"
Conservative="Conservative"
ApCompatibilityMode="AP Compatibility Mode"
BroaderCompat="Broader Compatibility"
HigherPerf="Higher Performance"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Rate (802.11a)"
Rate_802_11bg="Rate (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS Link Indication"

[strings.0409] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="United States"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - Performance"
80211bOnly="802.11b Only"
AntennaDiversity="Antenna Diversity"
Auto="Auto"
AutoShortLong="Auto (Short/Long)"
BSSPLCPHeader="BSS PLCP Header"
BlueToothCollaboration="Bluetooth Collaboration"
Default="Default"
Disable="Disable"
Disable80211a="Disable 802.11a"
Disable80211gb="Disable 802.11g/b"
DisableBands="Disable Bands"
Disabled="Disabled"
Enable="Enable"
Enabled="Enabled"
FragmentationThreshold="Fragmentation Threshold"
IBSS54gtmMode="IBSS 54g Mode"
IBSS54gtmProtectionMode="IBSS 54g Protection Mode"
IBSSChannelNumber="IBSS Channel Number"
LocallyAdministeredMACAddress="Locally Administered MAC Address"
Long="Long"
None="None"
OptimizeBandwidth="Optimize Bandwidth"
OptimizeDistance="Optimize Distance"
PLCPHeader="PLCP Header"
PowerOutput="Power Output"
PowerSaveMode="Power Save Mode"
Prefer80211a="Prefer 802.11a"
Prefer80211gb="Prefer 802.11g/b"
RTSThreshold="RTS Threshold"
RadioEnableDisable="Radio Enable/Disable"
Rate="Rate"
RoamingDecision="Roaming Decision"
Usebestrate="Use best rate"
XPress_Technology="54g+ (XPress)"
Location="Location"
Strict="Strict"
Loose="Loose"
Fast="Fast"
MiminumPowerConsumption="Minimum Power Consumption"
AssociationRoamPreference="Association Roam Preference"
BandPreference="Band Preference"
RoamingTendency="Roam Tendency"
Aggressive="Aggressive"
Moderate="Moderate"
Conservative="Conservative"
ApCompatibilityMode="AP Compatibility Mode"
BroaderCompat="Broader Compatibility"
HigherPerf="Higher Performance"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Rate (802.11a)"
Rate_802_11bg="Rate (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS Link Indication"

[strings.0425] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Ameerika Ühendriigid"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - kiirus"
80211bOnly="Ainult 802.11b"
AntennaDiversity="Antenni erisus"
Auto="Automaatne"
AutoShortLong="Automaatne (lühike/pikk)"
BSSPLCPHeader="BSS PLCP päis"
BlueToothCollaboration="Bluetoothi koostöö"
Default="Vaikimisi"
Disable="Blokeeri"
Disable80211a="Blokeeri 802.11a"
Disable80211gb="Blokeeri 802.11g/b"
DisableBands="Blokeeri sagedusribad"
Disabled="Blokeeritud"
Enable="Luba"
Enabled="Lubatud"
FragmentationThreshold="Fragmentatsioonilävi"
IBSS54gtmMode="IBSS 54g režiim"
IBSS54gtmProtectionMode="IBSS 54g kaitserežiim"
IBSSChannelNumber="IBSS-kanalinumber"
LocallyAdministeredMACAddress="Kohaliku administreerimisega MAC-aadress"
Long="Pikk"
None="Pole"
OptimizeBandwidth="Optimeeri ribalaius"
OptimizeDistance="Optimeeri kaugus"
PLCPHeader="PLCP päis"
PowerOutput="Võimsusväljund"
PowerSaveMode="Energiasäästurežiim"
Prefer80211a="Eelista 802.11a"
Prefer80211gb="Eelista 802.11g/b"
RTSThreshold="RTS-lävi"
RadioEnableDisable="Lülita raadio sisse/välja"
Rate="Kiirus"
RoamingDecision="Rändeotsus"
Usebestrate="Kasuta parimat kiirust"
XPress_Technology="54g+ (XPress)"
Location="Asukoht"
Strict="Range"
Loose="Vaba"
Fast="Kiire"
MiminumPowerConsumption="Minimaalne energiakulu"
AssociationRoamPreference="Seose rändamiseelistus"
BandPreference="Eelistatud sagedusala"
RoamingTendency="Rändamine"
Aggressive="Jõuline"
Moderate="Mõõdukas"
Conservative="Konservatiivne"
ApCompatibilityMode="AP ühilduvuse režiim"
BroaderCompat="Ulatuslikum ühilduvus"
HigherPerf="Parem jõudlus"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Kiirus (802.11a)"
Rate_802_11bg="Kiirus (802.11b/g)"
WZC_Managed_Ethernet="WZC hallatav Ethernet"
Legacy="Pärand"
IBSS_Link_Indication="IBSS liini näidik"

[strings.040b] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="USA"
54gAuto="54 g - Auto"
54gLRS="54 g - LRS"
54gPerformance="54g - Suorituskyky"
80211bOnly="Vain 802.11b"
AntennaDiversity="Erotusantenni"
Auto="Automaattinen"
AutoShortLong="Auto (lyhyt/pitkä)"
BSSPLCPHeader="BSS PLCP -otsikko"
BlueToothCollaboration="Bluetooth-yhteistyö"
Default="Oletusarvo"
Disable="Poista käytöstä"
Disable80211a="Poista 802.11a käytöstä"
Disable80211gb="Poista 802.11g/b käytöstä"
DisableBands="Poista taajuusalue käytöstä"
Disabled="Poista käytöstä"
Enable="Ota käyttöön"
Enabled="Otettu käyttöön"
FragmentationThreshold="Fragmentoitumiskynnys"
IBSS54gtmMode="IBSS 54g -tila"
IBSS54gtmProtectionMode="IBSS 54g -suojaustila"
IBSSChannelNumber="IBSS-kanavan numero"
LocallyAdministeredMACAddress="Paikallisesti hallittu MAC-osoite"
Long="Pitkä"
None="Ei yhtään"
OptimizeBandwidth="Optimoi taajuusalue"
OptimizeDistance="Optimoi välimatka"
PLCPHeader="PLCP-otsikko"
PowerOutput="Antoteho"
PowerSaveMode="Virransäästötila"
Prefer80211a="Aseta 802.11a etusijalle"
Prefer80211gb="Aseta 802.11g/b etusijalle"
RTSThreshold="RTS-kynnys"
RadioEnableDisable="Radio käyttöön / pois käytöstä"
Rate="Nopeus"
RoamingDecision="Verkkovierailupäätös"
Usebestrate="Käytä parasta tasoa"
XPress_Technology="54g+ (XPress)"
Location="Sijainti"
Strict="Tarkka"
Loose="Löyhä"
Fast="Nopea"
MiminumPowerConsumption="Vähimmäisvirrankulutus"
AssociationRoamPreference="Verkkovierailuyhteyssuositus"
BandPreference="Kaistasuositus"
RoamingTendency="Verkkovierailutapa"
Aggressive="Rohkea"
Moderate="Maltillinen"
Conservative="Varovainen"
ApCompatibilityMode="AP-yhteensopivuustila"
BroaderCompat="Kattava yhteensopivuus"
HigherPerf="Parempi suorituskyky"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Nopeus (802.11a)"
Rate_802_11bg="Nopeus (802.11b/g)"
WZC_Managed_Ethernet="WZC (Windows Zero Configuration) -ohjattu Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="Ilmoitus IBSS-linkistä"

[strings.0c0c] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="États-Unis d'Amérique"
54gAuto="Auto - 54g"
54gLRS="LRS - 54g"
54gPerformance="Performance - 54g"
80211bOnly="802.11b uniquement"
AntennaDiversity="Diversité d'antenne"
Auto="Automatique"
AutoShortLong="Auto (court/long)"
BSSPLCPHeader="En-tête PLCP BSS"
BlueToothCollaboration="Collaboration Bluetooth"
Default="Défaut"
Disable="Désactiver"
Disable80211a="Désactiver 802.11a"
Disable80211gb="Désactiver 802.11g/b"
DisableBands="Désactiver bandes"
Disabled="Désactivé(e/s)"
Enable="Activer"
Enabled="Activé(e/s)"
FragmentationThreshold="Seuil de fragmentation"
IBSS54gtmMode="Mode IBSS 54g"
IBSS54gtmProtectionMode="Mode Protection IBSS 54g"
IBSSChannelNumber="N° canal IBSS"
LocallyAdministeredMACAddress="Adresse MAC administrée localement"
Long="Long"
None="Aucun"
OptimizeBandwidth="Optimiser largeur de bande"
OptimizeDistance="Optimiser distance"
PLCPHeader="En-tête PLCP"
PowerOutput="Puissance sortie"
PowerSaveMode="Mode Gestion énergie"
Prefer80211a="802.11a préféré"
Prefer80211gb="802.11g/b préféré"
RTSThreshold="Seuil RTS"
RadioEnableDisable="Activer/désactiver radio"
Rate="Débit"
RoamingDecision="Option Itinérance"
Usebestrate="Utiliser meilleur taux"
XPress_Technology="54g+ (XPress)"
Location="Emplacement"
Strict="Strict"
Loose="Relâché"
Fast="Rapide"
MiminumPowerConsumption="Consommation électrique minimale"
AssociationRoamPreference="Préférence d'itinérance d'association"
BandPreference="Préférence de bande"
RoamingTendency="Tendance d'itinérance"
Aggressive="Agressif"
Moderate="Modéré"
Conservative="Conservateur"
ApCompatibilityMode="Mode de compatibilité AP"
BroaderCompat="Compatibilité plus large"
HigherPerf="Performances plus élevées"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Débit (802.11a)"
Rate_802_11bg="Débit (802.11b/g)"
WZC_Managed_Ethernet="Ethernet géré par WZC"
Legacy="Hérité"
IBSS_Link_Indication="Indication de liaison IBSS"

[strings.040c] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="États-Unis d'Amérique"
54gAuto="Auto - 54g"
54gLRS="LRS - 54g"
54gPerformance="Performance - 54g"
80211bOnly="802.11b uniquement"
AntennaDiversity="Diversité d'antenne"
Auto="Automatique"
AutoShortLong="Auto (court/long)"
BSSPLCPHeader="En-tête PLCP BSS"
BlueToothCollaboration="Collaboration Bluetooth"
Default="Défaut"
Disable="Désactiver"
Disable80211a="Désactiver 802.11a"
Disable80211gb="Désactiver 802.11g/b"
DisableBands="Désactiver bandes"
Disabled="Désactivé(e/s)"
Enable="Activer"
Enabled="Activé(e/s)"
FragmentationThreshold="Seuil de fragmentation"
IBSS54gtmMode="Mode IBSS 54g"
IBSS54gtmProtectionMode="Mode Protection IBSS 54g"
IBSSChannelNumber="N° canal IBSS"
LocallyAdministeredMACAddress="Adresse MAC administrée localement"
Long="Long"
None="Aucun"
OptimizeBandwidth="Optimiser largeur de bande"
OptimizeDistance="Optimiser distance"
PLCPHeader="En-tête PLCP"
PowerOutput="Puissance sortie"
PowerSaveMode="Mode Gestion énergie"
Prefer80211a="802.11a préféré"
Prefer80211gb="802.11g/b préféré"
RTSThreshold="Seuil RTS"
RadioEnableDisable="Activer/désactiver radio"
Rate="Débit"
RoamingDecision="Option Itinérance"
Usebestrate="Utiliser meilleur taux"
XPress_Technology="54g+ (XPress)"
Location="Emplacement"
Strict="Strict"
Loose="Relâché"
Fast="Rapide"
MiminumPowerConsumption="Consommation électrique minimale"
AssociationRoamPreference="Préférence d'itinérance d'association"
BandPreference="Préférence de bande"
RoamingTendency="Tendance d'itinérance"
Aggressive="Agressif"
Moderate="Modéré"
Conservative="Conservateur"
ApCompatibilityMode="Mode de compatibilité AP"
BroaderCompat="Compatibilité plus large"
HigherPerf="Performances plus élevées"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Débit (802.11a)"
Rate_802_11bg="Débit (802.11b/g)"
WZC_Managed_Ethernet="Ethernet géré par WZC"
Legacy="Hérité"
IBSS_Link_Indication="Indication de liaison IBSS"

[strings.180c] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="États-Unis d'Amérique"
54gAuto="Auto - 54g"
54gLRS="LRS - 54g"
54gPerformance="Performance - 54g"
80211bOnly="802.11b uniquement"
AntennaDiversity="Diversité d'antenne"
Auto="Automatique"
AutoShortLong="Auto (court/long)"
BSSPLCPHeader="En-tête PLCP BSS"
BlueToothCollaboration="Collaboration Bluetooth"
Default="Défaut"
Disable="Désactiver"
Disable80211a="Désactiver 802.11a"
Disable80211gb="Désactiver 802.11g/b"
DisableBands="Désactiver bandes"
Disabled="Désactivé(e/s)"
Enable="Activer"
Enabled="Activé(e/s)"
FragmentationThreshold="Seuil de fragmentation"
IBSS54gtmMode="Mode IBSS 54g"
IBSS54gtmProtectionMode="Mode Protection IBSS 54g"
IBSSChannelNumber="N° canal IBSS"
LocallyAdministeredMACAddress="Adresse MAC administrée localement"
Long="Long"
None="Aucun"
OptimizeBandwidth="Optimiser largeur de bande"
OptimizeDistance="Optimiser distance"
PLCPHeader="En-tête PLCP"
PowerOutput="Puissance sortie"
PowerSaveMode="Mode Gestion énergie"
Prefer80211a="802.11a préféré"
Prefer80211gb="802.11g/b préféré"
RTSThreshold="Seuil RTS"
RadioEnableDisable="Activer/désactiver radio"
Rate="Débit"
RoamingDecision="Option Itinérance"
Usebestrate="Utiliser meilleur taux"
XPress_Technology="54g+ (XPress)"
Location="Emplacement"
Strict="Strict"
Loose="Relâché"
Fast="Rapide"
MiminumPowerConsumption="Consommation électrique minimale"
AssociationRoamPreference="Préférence d'itinérance d'association"
BandPreference="Préférence de bande"
RoamingTendency="Tendance d'itinérance"
Aggressive="Agressif"
Moderate="Modéré"
Conservative="Conservateur"
ApCompatibilityMode="Mode de compatibilité AP"
BroaderCompat="Compatibilité plus large"
HigherPerf="Performances plus élevées"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Débit (802.11a)"
Rate_802_11bg="Débit (802.11b/g)"
WZC_Managed_Ethernet="Ethernet géré par WZC"
Legacy="Hérité"
IBSS_Link_Indication="Indication de liaison IBSS"

[strings.100c] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="États-Unis d'Amérique"
54gAuto="Auto - 54g"
54gLRS="LRS - 54g"
54gPerformance="Performance - 54g"
80211bOnly="802.11b uniquement"
AntennaDiversity="Diversité d'antenne"
Auto="Automatique"
AutoShortLong="Auto (court/long)"
BSSPLCPHeader="En-tête PLCP BSS"
BlueToothCollaboration="Collaboration Bluetooth"
Default="Défaut"
Disable="Désactiver"
Disable80211a="Désactiver 802.11a"
Disable80211gb="Désactiver 802.11g/b"
DisableBands="Désactiver bandes"
Disabled="Désactivé(e/s)"
Enable="Activer"
Enabled="Activé(e/s)"
FragmentationThreshold="Seuil de fragmentation"
IBSS54gtmMode="Mode IBSS 54g"
IBSS54gtmProtectionMode="Mode Protection IBSS 54g"
IBSSChannelNumber="N° canal IBSS"
LocallyAdministeredMACAddress="Adresse MAC administrée localement"
Long="Long"
None="Aucun"
OptimizeBandwidth="Optimiser largeur de bande"
OptimizeDistance="Optimiser distance"
PLCPHeader="En-tête PLCP"
PowerOutput="Puissance sortie"
PowerSaveMode="Mode Gestion énergie"
Prefer80211a="802.11a préféré"
Prefer80211gb="802.11g/b préféré"
RTSThreshold="Seuil RTS"
RadioEnableDisable="Activer/désactiver radio"
Rate="Débit"
RoamingDecision="Option Itinérance"
Usebestrate="Utiliser meilleur taux"
XPress_Technology="54g+ (XPress)"
Location="Emplacement"
Strict="Strict"
Loose="Relâché"
Fast="Rapide"
MiminumPowerConsumption="Consommation électrique minimale"
AssociationRoamPreference="Préférence d'itinérance d'association"
BandPreference="Préférence de bande"
RoamingTendency="Tendance d'itinérance"
Aggressive="Agressif"
Moderate="Modéré"
Conservative="Conservateur"
ApCompatibilityMode="Mode de compatibilité AP"
BroaderCompat="Compatibilité plus large"
HigherPerf="Performances plus élevées"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Débit (802.11a)"
Rate_802_11bg="Débit (802.11b/g)"
WZC_Managed_Ethernet="Ethernet géré par WZC"
Legacy="Hérité"
IBSS_Link_Indication="Indication de liaison IBSS"

[strings.0c07] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Vereinigte Staaten von Amerika"
54gAuto="54g Auto"
54gLRS="54g LRS"
54gPerformance="54g Performance"
80211bOnly="Nur 802.11b"
AntennaDiversity="Antennendiversität"
Auto="Automatisch"
AutoShortLong="Auto (Kurz/Lang)"
BSSPLCPHeader="BSS-PLCP-Header"
BlueToothCollaboration="Bluetooth-Kompatibilität"
Default="Standard"
Disable="Deaktivieren"
Disable80211a="802.11a deaktivieren"
Disable80211gb="802.11g/b deaktivieren"
DisableBands="Frequenzbereiche deaktivieren"
Disabled="Deaktiviert"
Enable="Aktivieren"
Enabled="Aktiviert"
FragmentationThreshold="Fragmentierungsschwelle"
IBSS54gtmMode="IBSS-54g(tm)-Modus"
IBSS54gtmProtectionMode="IBSS-54g(tm)-Schutzmodus"
IBSSChannelNumber="IBSS-Kanalnummer"
LocallyAdministeredMACAddress="Lokal verwaltete MAC-Adresse"
Long="Lang"
None="Keine"
OptimizeBandwidth="Bandbreite optimieren"
OptimizeDistance="Entfernung optimieren"
PLCPHeader="PLCP-Header"
PowerOutput="Ausgangsleistung"
PowerSaveMode="Stromsparmodus"
Prefer80211a="802.11a bevorzugt"
Prefer80211gb="802.11g/b bevorzugt"
RTSThreshold="RTS-Schwelle"
RadioEnableDisable="Funkgerät aktiviert/deaktiviert"
Rate="Geschwindigkeit"
RoamingDecision="Roamingentscheidung"
Usebestrate="Beste Geschwindigkeit verwenden"
XPress_Technology="54g+ (XPress)"
Location="Standort"
Strict="Streng"
Loose="Lose"
Fast="Schnell"
MiminumPowerConsumption="Mindeststromverbrauch"
AssociationRoamPreference="Bevorzugte Roaming-Zuordnung"
BandPreference="Bevorzugtes Band"
RoamingTendency="Roaming-Tendenz"
Aggressive="Hoch"
Moderate="Mittel"
Conservative="Traditionell"
ApCompatibilityMode="Modus ""AP-Kompatibilität"""
BroaderCompat="Größere Kompatibilität"
HigherPerf="Höhere Leistung"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Geschwindigkeit (802.11a)"
Rate_802_11bg="Geschwindigkeit (802.11b/g)"
WZC_Managed_Ethernet="WZC verwaltetes Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS-Verbindungsindikator"

[strings.0407] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Vereinigte Staaten von Amerika"
54gAuto="54g Auto"
54gLRS="54g LRS"
54gPerformance="54g Performance"
80211bOnly="Nur 802.11b"
AntennaDiversity="Antennendiversität"
Auto="Automatisch"
AutoShortLong="Auto (Kurz/Lang)"
BSSPLCPHeader="BSS-PLCP-Header"
BlueToothCollaboration="Bluetooth-Kompatibilität"
Default="Standard"
Disable="Deaktivieren"
Disable80211a="802.11a deaktivieren"
Disable80211gb="802.11g/b deaktivieren"
DisableBands="Frequenzbereiche deaktivieren"
Disabled="Deaktiviert"
Enable="Aktivieren"
Enabled="Aktiviert"
FragmentationThreshold="Fragmentierungsschwelle"
IBSS54gtmMode="IBSS-54g(tm)-Modus"
IBSS54gtmProtectionMode="IBSS-54g(tm)-Schutzmodus"
IBSSChannelNumber="IBSS-Kanalnummer"
LocallyAdministeredMACAddress="Lokal verwaltete MAC-Adresse"
Long="Lang"
None="Keine"
OptimizeBandwidth="Bandbreite optimieren"
OptimizeDistance="Entfernung optimieren"
PLCPHeader="PLCP-Header"
PowerOutput="Ausgangsleistung"
PowerSaveMode="Stromsparmodus"
Prefer80211a="802.11a bevorzugt"
Prefer80211gb="802.11g/b bevorzugt"
RTSThreshold="RTS-Schwelle"
RadioEnableDisable="Funkgerät aktiviert/deaktiviert"
Rate="Geschwindigkeit"
RoamingDecision="Roamingentscheidung"
Usebestrate="Beste Geschwindigkeit verwenden"
XPress_Technology="54g+ (XPress)"
Location="Standort"
Strict="Streng"
Loose="Lose"
Fast="Schnell"
MiminumPowerConsumption="Mindeststromverbrauch"
AssociationRoamPreference="Bevorzugte Roaming-Zuordnung"
BandPreference="Bevorzugtes Band"
RoamingTendency="Roaming-Tendenz"
Aggressive="Hoch"
Moderate="Mittel"
Conservative="Traditionell"
ApCompatibilityMode="Modus ""AP-Kompatibilität"""
BroaderCompat="Größere Kompatibilität"
HigherPerf="Höhere Leistung"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Geschwindigkeit (802.11a)"
Rate_802_11bg="Geschwindigkeit (802.11b/g)"
WZC_Managed_Ethernet="WZC verwaltetes Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS-Verbindungsindikator"

[strings.1407] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Vereinigte Staaten von Amerika"
54gAuto="54g Auto"
54gLRS="54g LRS"
54gPerformance="54g Performance"
80211bOnly="Nur 802.11b"
AntennaDiversity="Antennendiversität"
Auto="Automatisch"
AutoShortLong="Auto (Kurz/Lang)"
BSSPLCPHeader="BSS-PLCP-Header"
BlueToothCollaboration="Bluetooth-Kompatibilität"
Default="Standard"
Disable="Deaktivieren"
Disable80211a="802.11a deaktivieren"
Disable80211gb="802.11g/b deaktivieren"
DisableBands="Frequenzbereiche deaktivieren"
Disabled="Deaktiviert"
Enable="Aktivieren"
Enabled="Aktiviert"
FragmentationThreshold="Fragmentierungsschwelle"
IBSS54gtmMode="IBSS-54g(tm)-Modus"
IBSS54gtmProtectionMode="IBSS-54g(tm)-Schutzmodus"
IBSSChannelNumber="IBSS-Kanalnummer"
LocallyAdministeredMACAddress="Lokal verwaltete MAC-Adresse"
Long="Lang"
None="Keine"
OptimizeBandwidth="Bandbreite optimieren"
OptimizeDistance="Entfernung optimieren"
PLCPHeader="PLCP-Header"
PowerOutput="Ausgangsleistung"
PowerSaveMode="Stromsparmodus"
Prefer80211a="802.11a bevorzugt"
Prefer80211gb="802.11g/b bevorzugt"
RTSThreshold="RTS-Schwelle"
RadioEnableDisable="Funkgerät aktiviert/deaktiviert"
Rate="Geschwindigkeit"
RoamingDecision="Roamingentscheidung"
Usebestrate="Beste Geschwindigkeit verwenden"
XPress_Technology="54g+ (XPress)"
Location="Standort"
Strict="Streng"
Loose="Lose"
Fast="Schnell"
MiminumPowerConsumption="Mindeststromverbrauch"
AssociationRoamPreference="Bevorzugte Roaming-Zuordnung"
BandPreference="Bevorzugtes Band"
RoamingTendency="Roaming-Tendenz"
Aggressive="Hoch"
Moderate="Mittel"
Conservative="Traditionell"
ApCompatibilityMode="Modus ""AP-Kompatibilität"""
BroaderCompat="Größere Kompatibilität"
HigherPerf="Höhere Leistung"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Geschwindigkeit (802.11a)"
Rate_802_11bg="Geschwindigkeit (802.11b/g)"
WZC_Managed_Ethernet="WZC verwaltetes Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS-Verbindungsindikator"

[strings.1007] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Vereinigte Staaten von Amerika"
54gAuto="54g Auto"
54gLRS="54g LRS"
54gPerformance="54g Performance"
80211bOnly="Nur 802.11b"
AntennaDiversity="Antennendiversität"
Auto="Automatisch"
AutoShortLong="Auto (Kurz/Lang)"
BSSPLCPHeader="BSS-PLCP-Header"
BlueToothCollaboration="Bluetooth-Kompatibilität"
Default="Standard"
Disable="Deaktivieren"
Disable80211a="802.11a deaktivieren"
Disable80211gb="802.11g/b deaktivieren"
DisableBands="Frequenzbereiche deaktivieren"
Disabled="Deaktiviert"
Enable="Aktivieren"
Enabled="Aktiviert"
FragmentationThreshold="Fragmentierungsschwelle"
IBSS54gtmMode="IBSS-54g(tm)-Modus"
IBSS54gtmProtectionMode="IBSS-54g(tm)-Schutzmodus"
IBSSChannelNumber="IBSS-Kanalnummer"
LocallyAdministeredMACAddress="Lokal verwaltete MAC-Adresse"
Long="Lang"
None="Keine"
OptimizeBandwidth="Bandbreite optimieren"
OptimizeDistance="Entfernung optimieren"
PLCPHeader="PLCP-Header"
PowerOutput="Ausgangsleistung"
PowerSaveMode="Stromsparmodus"
Prefer80211a="802.11a bevorzugt"
Prefer80211gb="802.11g/b bevorzugt"
RTSThreshold="RTS-Schwelle"
RadioEnableDisable="Funkgerät aktiviert/deaktiviert"
Rate="Geschwindigkeit"
RoamingDecision="Roamingentscheidung"
Usebestrate="Beste Geschwindigkeit verwenden"
XPress_Technology="54g+ (XPress)"
Location="Standort"
Strict="Streng"
Loose="Lose"
Fast="Schnell"
MiminumPowerConsumption="Mindeststromverbrauch"
AssociationRoamPreference="Bevorzugte Roaming-Zuordnung"
BandPreference="Bevorzugtes Band"
RoamingTendency="Roaming-Tendenz"
Aggressive="Hoch"
Moderate="Mittel"
Conservative="Traditionell"
ApCompatibilityMode="Modus ""AP-Kompatibilität"""
BroaderCompat="Größere Kompatibilität"
HigherPerf="Höhere Leistung"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Geschwindigkeit (802.11a)"
Rate_802_11bg="Geschwindigkeit (802.11b/g)"
WZC_Managed_Ethernet="WZC verwaltetes Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS-Verbindungsindikator"

[strings.0807] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Vereinigte Staaten von Amerika"
54gAuto="54g Auto"
54gLRS="54g LRS"
54gPerformance="54g Performance"
80211bOnly="Nur 802.11b"
AntennaDiversity="Antennendiversität"
Auto="Automatisch"
AutoShortLong="Auto (Kurz/Lang)"
BSSPLCPHeader="BSS-PLCP-Header"
BlueToothCollaboration="Bluetooth-Kompatibilität"
Default="Standard"
Disable="Deaktivieren"
Disable80211a="802.11a deaktivieren"
Disable80211gb="802.11g/b deaktivieren"
DisableBands="Frequenzbereiche deaktivieren"
Disabled="Deaktiviert"
Enable="Aktivieren"
Enabled="Aktiviert"
FragmentationThreshold="Fragmentierungsschwelle"
IBSS54gtmMode="IBSS-54g(tm)-Modus"
IBSS54gtmProtectionMode="IBSS-54g(tm)-Schutzmodus"
IBSSChannelNumber="IBSS-Kanalnummer"
LocallyAdministeredMACAddress="Lokal verwaltete MAC-Adresse"
Long="Lang"
None="Keine"
OptimizeBandwidth="Bandbreite optimieren"
OptimizeDistance="Entfernung optimieren"
PLCPHeader="PLCP-Header"
PowerOutput="Ausgangsleistung"
PowerSaveMode="Stromsparmodus"
Prefer80211a="802.11a bevorzugt"
Prefer80211gb="802.11g/b bevorzugt"
RTSThreshold="RTS-Schwelle"
RadioEnableDisable="Funkgerät aktiviert/deaktiviert"
Rate="Geschwindigkeit"
RoamingDecision="Roamingentscheidung"
Usebestrate="Beste Geschwindigkeit verwenden"
XPress_Technology="54g+ (XPress)"
Location="Standort"
Strict="Streng"
Loose="Lose"
Fast="Schnell"
MiminumPowerConsumption="Mindeststromverbrauch"
AssociationRoamPreference="Bevorzugte Roaming-Zuordnung"
BandPreference="Bevorzugtes Band"
RoamingTendency="Roaming-Tendenz"
Aggressive="Hoch"
Moderate="Mittel"
Conservative="Traditionell"
ApCompatibilityMode="Modus ""AP-Kompatibilität"""
BroaderCompat="Größere Kompatibilität"
HigherPerf="Höhere Leistung"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Geschwindigkeit (802.11a)"
Rate_802_11bg="Geschwindigkeit (802.11b/g)"
WZC_Managed_Ethernet="WZC verwaltetes Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS-Verbindungsindikator"

[strings.0408] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Ηνωμένες Πολιτείες"
54gAuto="54g - Αυτόματο"
54gLRS="54g - LRS"
54gPerformance="54g - Επιδόσεις"
80211bOnly="802.11b μόνο"
AntennaDiversity="Διαφορισμός κεραίας"
Auto="Αυτόματα"
AutoShortLong="Αυτόματα (Βραχέα/Μακρά)"
BSSPLCPHeader="Κεφαλίδα BSS PLCP"
BlueToothCollaboration="Συμβατότητα με Bluetooth"
Default="Προεπιλογή"
Disable="Απενεργοποίηση"
Disable80211a="Απενεργοποίηση 802.11a"
Disable80211gb="Απενεργοποίηση 802.11g/b"
DisableBands="Απενεργοποίηση ζωνών"
Disabled="Απενεργοποιημένο"
Enable="Ενεργοποίηση"
Enabled="Ενεργοποιημένο"
FragmentationThreshold="Όριο κατακερματισμού"
IBSS54gtmMode="Λειτουργία IBSS 54g"
IBSS54gtmProtectionMode="Λειτουργία προστασίας IBSS 54g"
IBSSChannelNumber="Αριθμός καναλιού IBSS"
LocallyAdministeredMACAddress="Τοπικά διαχειριζόμενη διεύθυνση MAC"
Long="Μεγάλου μήκους"
None="Κανένα"
OptimizeBandwidth="Βελτιστοποίηση εύρους συχνοτήτων"
OptimizeDistance="Βελτιστοποίηση απόστασης"
PLCPHeader="Κεφαλίδα PLCP"
PowerOutput="Ισχύς Εξόδου"
PowerSaveMode="Κατάσταση εξοικονόμηση ενέργειας"
Prefer80211a="Προτιμώ το 802.11a"
Prefer80211gb="Προτιμώ το 802.11g/b"
RTSThreshold="Όριο RTS"
RadioEnableDisable="Ενεργοποίηση / Απενεργοποίηση ραδιοεπικοινωνίας"
Rate="Ταχύτητα"
RoamingDecision="Απόφαση για την περιαγωγή"
Usebestrate="Χρήση καλύτερης ταχύτητας"
XPress_Technology="54g+ (XPress)"
Location="Τοποθεσία"
Strict="Βασική"
Loose="Χαλαρή"
Fast="Γρήγορη"
MiminumPowerConsumption="Ελάχιστη κατανάλωση ενέργειας"
AssociationRoamPreference="Προτίμηση περιαγωγής συνδεδεμένου σημείου πρόσβασης"
BandPreference="Προτίμηση ζώνης"
RoamingTendency="Επίπεδο εκτίμησης προορισμού περιαγωγής"
Aggressive="Υψηλό"
Moderate="Μέτριο"
Conservative="Χαμηλό"
ApCompatibilityMode="Λειτουργία συμβατότητας AP"
BroaderCompat="Διευρυμένη συμβατότητα"
HigherPerf="Υψηλότερη απόδοση"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Ταχύτητα (802.11a)"
Rate_802_11bg="Ταχύτητα (802.11b/g)"
WZC_Managed_Ethernet="Διαχείριση Ethernet από WZC"
Legacy="Προηγούμενες εκδόσεις"
IBSS_Link_Indication="Ένδειξη σύνδεσης IBSS"

[strings.040d] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="ארצות הברית"
54gAuto="54g - אוטומטי"
54gLRS="54g - LRS"
54gPerformance="54g - ביצועים"
80211bOnly="802.11b בלבד"
AntennaDiversity="ריבוי אנטנות"
Auto="אוטומטי"
AutoShortLong="אוטומטי (קצר/ארוך)"
BSSPLCPHeader="כותרת BSS PLCP"
BlueToothCollaboration="שיתוף פעולה בטכנולוגיית Bluetooth"
Default="ברירת מחדל"
Disable="בטל"
Disable80211a="בטל 802.11a"
Disable80211gb="בטל 802.11g/b"
DisableBands="בטל רצועות"
Disabled="לא זמין"
Enable="אפשר / הפעל"
Enabled="מאופשר / מופעל"
FragmentationThreshold="סף פיצול"
IBSS54gtmMode="מצב IBSS 54g"
IBSS54gtmProtectionMode="מצב הגנת IBSS 54g"
IBSSChannelNumber="מספר ערוץ IBSS"
LocallyAdministeredMACAddress="כתובת MAC בניהול מקומי"
Long="ארוכה"
None="ללא"
OptimizeBandwidth="בצע מיטוב של רוחב פס"
OptimizeDistance="בצע מיטוב של מרחק"
PLCPHeader="כותרת PLCP"
PowerOutput="תפוקת חשמל"
PowerSaveMode="מצב חיסכון בחשמל"
Prefer80211a="העדף 802.11a"
Prefer80211gb="העדף 802.11g/b"
RTSThreshold="סף RTS"
RadioEnableDisable="הפעלת/ביטול רדיו"
Rate="קצב"
RoamingDecision="החלטת נדידה"
Usebestrate="השתמש בקצב הטוב ביותר"
XPress_Technology="54g+ (XPress)"
Location="מיקום"
Strict="מחמיר"
Loose="לא מחמיר"
Fast="מהיר"
MiminumPowerConsumption="צריכת חשמל מינימלית"
AssociationRoamPreference="העדפת נדידה משויכת"
BandPreference="העדפת פס"
RoamingTendency="מגמת נדידה"
Aggressive="אגרסיבי"
Moderate="מתון"
Conservative="שמרני"
ApCompatibilityMode="מצב תואם AP"
BroaderCompat="תאימות מקיפה"
HigherPerf="ביצועים גבוהים יותר"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="קצב (802.11a)"
Rate_802_11bg="קצב (802.11b/g)"
WZC_Managed_Ethernet="Ethernet מנוהל WZC"
Legacy="דור קודם"
IBSS_Link_Indication="ציון קישור IBSS"

[strings.040e] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Egyesült Államok"
54gAuto="54g - automatikus"
54gLRS="54g - LRS"
54gPerformance="54g - teljesítmény"
80211bOnly="Csak 802.11b"
AntennaDiversity="Antenna diverzitás"
Auto="Automatikus"
AutoShortLong="Automatikus (short - rövid/long - hosszú)"
BSSPLCPHeader="BSS PLCP fejléc"
BlueToothCollaboration="Bluetooth támogatás"
Default="Alapértelmezett"
Disable="Tiltás"
Disable80211a="802.11a tiltása"
Disable80211gb="802.11g/b tiltása"
DisableBands="Sávok tiltása"
Disabled="Letiltva"
Enable="Engedélyezés"
Enabled="Engedélyezve"
FragmentationThreshold="Tördelési küszöb"
IBSS54gtmMode="IBSS 54g mód"
IBSS54gtmProtectionMode="IBSS 54g védett mód"
IBSSChannelNumber="IBSS csatorna szám"
LocallyAdministeredMACAddress="Helyileg kezelt MAC-cím"
Long="Long (hosszú)"
None="Nincs"
OptimizeBandwidth="Sávszélesség optimális beállítása"
OptimizeDistance="Távolság optimális beállítása"
PLCPHeader="PLCP fejléc"
PowerOutput="Leadott teljesítmény"
PowerSaveMode="Energiatakarékos üzemmód"
Prefer80211a="802.11a előválasztása"
Prefer80211gb="802.11g/b előválasztása"
RTSThreshold="RTS küszöb"
RadioEnableDisable="Rádió engedélyezése/tiltása"
Rate="Sebesség"
RoamingDecision="Roaming döntés"
Usebestrate="Legjobb sebesség alkalmazása"
XPress_Technology="54g+ (XPress)"
Location="Hely"
Strict="Szigorú"
Loose="Laza"
Fast="Gyors"
MiminumPowerConsumption="Legkisebb teljesítményfelvétel"
AssociationRoamPreference="Roaming előválasztása"
BandPreference="Sáv előválasztása"
RoamingTendency="Várható roaming aktivitás"
Aggressive="Élénk"
Moderate="Mérsékelt"
Conservative="Eseti"
ApCompatibilityMode="AP-kompatibilitási mód"
BroaderCompat="Nagyobb kompatibilitás"
HigherPerf="Jobb teljesítmény"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Sebesség (802.11a)"
Rate_802_11bg="Sebesség (802.11b/g)"
WZC_Managed_Ethernet="Konfigurációmentes vezeték nélküli hálózati szolgáltatással (WZC) menedzselt Ethernet"
Legacy="Korábbi verzió"
IBSS_Link_Indication="IBSS hivatkozás jelzése"

[strings.0410] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Stati Uniti"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - Prestazioni"
80211bOnly="Solo 802.11b"
AntennaDiversity="Diversità di antenna"
Auto="Automatico"
AutoShortLong="Auto (corto/lungo)"
BSSPLCPHeader="Intestazione PLCP BSS"
BlueToothCollaboration="Collaborazione Bluetooth"
Default="Impostazione predefinita"
Disable="Disabilita"
Disable80211a="Disabilita 802.11a"
Disable80211gb="Disabilita 802.11g/b"
DisableBands="Disabilita bande"
Disabled="Disabilitato"
Enable="Abilita"
Enabled="Abilitato"
FragmentationThreshold="Soglia frammentazione"
IBSS54gtmMode="Modalità IBSS 54g"
IBSS54gtmProtectionMode="Modalità protezione IBSS 54g"
IBSSChannelNumber="Numero canale IBSS"
LocallyAdministeredMACAddress="Indirizzo MAC gestito localmente"
Long="Lungo"
None="Nessuno"
OptimizeBandwidth="Ottimizza larghezza di banda"
OptimizeDistance="Ottimizza distanza"
PLCPHeader="Intestazione PLCP"
PowerOutput="Potenza di uscita"
PowerSaveMode="Modalità risparmio energia"
Prefer80211a="Preferire 802.11a"
Prefer80211gb="Preferire 802.11g/b"
RTSThreshold="Soglia RTS"
RadioEnableDisable="Attiva/Disattiva radio"
Rate="Velocità"
RoamingDecision="Decisione Roaming"
Usebestrate="Utilizza la velocità migliore"
XPress_Technology="54g+ (XPress)"
Location="Percorso"
Strict="Stretto"
Loose="Sciolto"
Fast="Veloce"
MiminumPowerConsumption="Consumo energetico minimo"
AssociationRoamPreference="Preferenze di associazione roaming"
BandPreference="Preferenza di banda"
RoamingTendency="Tendenza di roaming"
Aggressive="Aggressiva"
Moderate="Moderata"
Conservative="Conservatrice"
ApCompatibilityMode="Modalità compatibilità AP"
BroaderCompat="Compatibilità estesa"
HigherPerf="Prestazioni superiori"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Velocità (802.11a)"
Rate_802_11bg="Velocità (802.11b/g)"
WZC_Managed_Ethernet="Gestione Ethernet tramite WZC"
Legacy="Legacy"
IBSS_Link_Indication="Indicazione collegamento IBSS"

[strings.0810] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Stati Uniti"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - Prestazioni"
80211bOnly="Solo 802.11b"
AntennaDiversity="Diversità di antenna"
Auto="Automatico"
AutoShortLong="Auto (corto/lungo)"
BSSPLCPHeader="Intestazione PLCP BSS"
BlueToothCollaboration="Collaborazione Bluetooth"
Default="Impostazione predefinita"
Disable="Disabilita"
Disable80211a="Disabilita 802.11a"
Disable80211gb="Disabilita 802.11g/b"
DisableBands="Disabilita bande"
Disabled="Disabilitato"
Enable="Abilita"
Enabled="Abilitato"
FragmentationThreshold="Soglia frammentazione"
IBSS54gtmMode="Modalità IBSS 54g"
IBSS54gtmProtectionMode="Modalità protezione IBSS 54g"
IBSSChannelNumber="Numero canale IBSS"
LocallyAdministeredMACAddress="Indirizzo MAC gestito localmente"
Long="Lungo"
None="Nessuno"
OptimizeBandwidth="Ottimizza larghezza di banda"
OptimizeDistance="Ottimizza distanza"
PLCPHeader="Intestazione PLCP"
PowerOutput="Potenza di uscita"
PowerSaveMode="Modalità risparmio energia"
Prefer80211a="Preferire 802.11a"
Prefer80211gb="Preferire 802.11g/b"
RTSThreshold="Soglia RTS"
RadioEnableDisable="Attiva/Disattiva radio"
Rate="Velocità"
RoamingDecision="Decisione Roaming"
Usebestrate="Utilizza la velocità migliore"
XPress_Technology="54g+ (XPress)"
Location="Percorso"
Strict="Stretto"
Loose="Sciolto"
Fast="Veloce"
MiminumPowerConsumption="Consumo energetico minimo"
AssociationRoamPreference="Preferenze di associazione roaming"
BandPreference="Preferenza di banda"
RoamingTendency="Tendenza di roaming"
Aggressive="Aggressiva"
Moderate="Moderata"
Conservative="Conservatrice"
ApCompatibilityMode="Modalità compatibilità AP"
BroaderCompat="Compatibilità estesa"
HigherPerf="Prestazioni superiori"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Velocità (802.11a)"
Rate_802_11bg="Velocità (802.11b/g)"
WZC_Managed_Ethernet="Gestione Ethernet tramite WZC"
Legacy="Legacy"
IBSS_Link_Indication="Indicazione collegamento IBSS"

[strings.0411] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="米国"
54gAuto="54g 自動"
54gLRS="54g - LRS"
54gPerformance="54g パフォーマンス"
80211bOnly="802.11b のみ"
AntennaDiversity="アンテナ ダイバーシティ"
Auto="自動"
AutoShortLong="自動 (ショート/ロング)"
BSSPLCPHeader="BSS PLCP ヘッダー"
BlueToothCollaboration="Bluetooth コラボレーション"
Default="既定"
Disable="無効にする"
Disable80211a="802.11a を無効にする"
Disable80211gb="802.11g/b を無効にする"
DisableBands="バンドを無効にする"
Disabled="無効"
Enable="有効にする"
Enabled="有効"
FragmentationThreshold="断片化しきい値"
IBSS54gtmMode="IBSS 54g モード"
IBSS54gtmProtectionMode="IBSS 54g 保護モード"
IBSSChannelNumber="IBSS チャンネル番号"
LocallyAdministeredMACAddress="ローカルで管理されている MAC アドレス"
Long="ロング"
None="なし"
OptimizeBandwidth="帯域幅を最適化する"
OptimizeDistance="距離を最適化する"
PLCPHeader="PLCP ヘッダー"
PowerOutput="出力電力"
PowerSaveMode="省電力モード"
Prefer80211a="802.11a を選択"
Prefer80211gb="802.11g/b を選択"
RTSThreshold="RTS しきい値"
RadioEnableDisable="ラジオ有効/無効"
Rate="レート"
RoamingDecision="ローミング判断"
Usebestrate="最適速度を使用"
XPress_Technology="54g+ (XPress)"
Location="場所"
Strict="厳密"
Loose="非厳密"
Fast="高速"
MiminumPowerConsumption="最小電力消費量"
AssociationRoamPreference="ローミングの関連付け設定"
BandPreference="バンド設定"
RoamingTendency="ローミング傾向"
Aggressive="強"
Moderate="中"
Conservative="弱"
ApCompatibilityMode="AP 互換モード"
BroaderCompat="Broader 互換"
HigherPerf="高パフォーマンス"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="レート (802.11a)"
Rate_802_11bg="レート (802.11b/g)"
WZC_Managed_Ethernet="WZC によるイーサネットの管理"
Legacy="レガシ"
IBSS_Link_Indication="独立基本サービスセット (IBSS) リンク確認"

[strings.0412] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="미국"
54gAuto="54g - 성능"
54gLRS="54g - LRS"
54gPerformance="802.11b 상태"
80211bOnly="연결 기본 설정"
AntennaDiversity="자동(숏/롱)"
Auto="BSS 모드"
AutoShortLong="BSS PLCP 헤더"
BSSPLCPHeader="802.11a 사용 안 함"
BlueToothCollaboration="802.11g/b 사용 안 함"
Default="사용"
Disable="사용 안 함"
Disable80211a="802.11a 사용 안 함"
Disable80211gb="802.11g/b 사용 안 함"
DisableBands="밴드 사용 안 함"
Disabled="사용 안 됨"
Enable="사용"
Enabled="사용됨"
FragmentationThreshold="분할 임계값"
IBSS54gtmMode="IBSS 54g 모드"
IBSS54gtmProtectionMode="IBSS 54g 보호 모드"
IBSSChannelNumber="IBSS 채널 번호"
LocallyAdministeredMACAddress="로컬로 관리되는 MAC 주소"
Long="롱"
None="없음"
OptimizeBandwidth="대역폭 최적화"
OptimizeDistance="거리 최적화"
PLCPHeader="PLCP 헤더"
PowerOutput="출력"
PowerSaveMode="절전 모드"
Prefer80211a="802.11a 선택"
Prefer80211gb="802.11g/b 선택"
RTSThreshold="RTS 임계값"
RadioEnableDisable="라디오 사용/사용 안 함"
Rate="속도"
RoamingDecision="로밍 결정"
Usebestrate="최상의 속도 사용"
XPress_Technology="54g+ (XPress)"
Location="위치"
Strict="엄격"
Loose="느슨"
Fast="고속"
MiminumPowerConsumption="최소 전력 소모량"
AssociationRoamPreference="연결 로밍 기본 설정"
BandPreference="밴드 기본 설정"
RoamingTendency="로밍 설정"
Aggressive="강"
Moderate="중"
Conservative="약"
ApCompatibilityMode="AP 호환성 모드"
BroaderCompat="호환성 확장"
HigherPerf="성능 강화"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="속도 (802.11a)"
Rate_802_11bg="속도 (802.11b/g)"
WZC_Managed_Ethernet="WZC 관리 Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS 연결 표시"

[strings.0426] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Amerikas Savienotās Valstis"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - veiktspēja"
80211bOnly="Tikai 802.11b"
AntennaDiversity="Antenas nevienādība"
Auto="Automātiski"
AutoShortLong="Auto (īss/Garš)"
BSSPLCPHeader="BSS PLCP virsraksti"
BlueToothCollaboration="Bluetooth sadarbība"
Default="Standarta"
Disable="Izslēgts"
Disable80211a="Izslēgts 802.11a"
Disable80211gb="Izslēgts 802.11g/b"
DisableBands="Izslēgtas frekvenču joslas"
Disabled="Izslēgts"
Enable="Ieslēgts"
Enabled="Ieslēgts"
FragmentationThreshold="Fragmentācijas slieksnis"
IBSS54gtmMode="IBSS 54g režīms"
IBSS54gtmProtectionMode="IBSS 54g aizsardzības režīms"
IBSSChannelNumber="IBSS kanāla numurs"
LocallyAdministeredMACAddress="Lokāli administrēta MAC adrese"
Long="Garš"
None="Nav"
OptimizeBandwidth="Optimizēt joslas platumu"
OptimizeDistance="Optimizēt distanci"
PLCPHeader="PLCP virsraksti"
PowerOutput="Barošanas izeja"
PowerSaveMode="Barošanas ekonomiskais režīms"
Prefer80211a="Izvirzītais 802.11a"
Prefer80211gb="Izvirzītais 802.11g/b"
RTSThreshold="RTS slieksnis"
RadioEnableDisable="Radio ieslēgts/izslēgts"
Rate="Ātrums"
RoamingDecision="Viesabonēšana"
Usebestrate="Izmantot labāko ātrumu"
XPress_Technology="54g+ (XPress)"
Location="Atrašanās vieta"
Strict="Noteikts"
Loose="Nenoteikts"
Fast="Ātrs"
MiminumPowerConsumption="Minimālais strāvas patēriņš"
AssociationRoamPreference="Asociatīvās Panoramēšanas izvēle"
BandPreference="Joslas izvēle"
RoamingTendency="Panoramēšanas tendence"
Aggressive="Agresīva"
Moderate="Vidēja"
Conservative="Konservatīva"
ApCompatibilityMode="AP saderības režīms"
BroaderCompat="Plašāka saderība"
HigherPerf="Lielāka veiktspēja"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Ātrums (802.11a)"
Rate_802_11bg="Ātrums (802.11b/g)"
WZC_Managed_Ethernet="Ethernet tīkls ar WZC vadību "
Legacy="Mantojums"
IBSS_Link_Indication="IBBSS saites indikācija"

[strings.0427] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Jungtinės Amerikos Valstijos"
54gAuto="54g - Automatinis"
54gLRS="54g - LRS"
54gPerformance="54g - Našumas"
80211bOnly="Tik 802.11b"
AntennaDiversity="Antenų pasirinkimas"
Auto="Automatinis"
AutoShortLong="Automatinis (trumpas/ilgas)"
BSSPLCPHeader="BSS PLCP antraštė"
BlueToothCollaboration="Darbas su Bluetooth"
Default="Numatytasis"
Disable="Išjungti"
Disable80211a="Išjungti 802.11a"
Disable80211gb="Išjungti 802.11g/b"
DisableBands="Išjungti dažnių juostas"
Disabled="Išjungtas"
Enable="Įjungtas"
Enabled="Įjungtas"
FragmentationThreshold="Fragmentacijos kritinė riba"
IBSS54gtmMode="IBSS 54g režimas"
IBSS54gtmProtectionMode="IBSS 54g apsaugos režimas"
IBSSChannelNumber="IBSS kanalo numeris"
LocallyAdministeredMACAddress="Vietoje tvarkomas MAC adresas"
Long="Ilgas"
None="Nėra"
OptimizeBandwidth="Optimizuoti dažnių juostą"
OptimizeDistance="Optimizuoti atstumą"
PLCPHeader="PLCP antraštė"
PowerOutput="Maitinimo išvestis"
PowerSaveMode="Energijos taupymo režimas"
Prefer80211a="Nuostata 802.11a"
Prefer80211gb="Nuostata 802.11g/b"
RTSThreshold="RTS kritinė riba"
RadioEnableDisable="Įjungti/Išjungti radiją"
Rate="Dažnis"
RoamingDecision="Tarptinklinio ryšio sprendimas"
Usebestrate="Naudoti geriausią dažnį"
XPress_Technology="54g+ (XPress)"
Location="Vieta"
Strict="Griežtas"
Loose="Nepririštas"
Fast="Greitas"
MiminumPowerConsumption="Minimalus sunaudojamos el. energijos kiekis"
AssociationRoamPreference="Pageidaujamas tarptinklinis susiejimas"
BandPreference="Pageidaujama dažnių juosta"
RoamingTendency="Tarptinklinio ryšio ypatumai"
Aggressive="Atkaklus"
Moderate="Nuosaikus"
Conservative="Konservatyvus"
ApCompatibilityMode="AP suderinamumo režimas"
BroaderCompat="Išplėtimo priemonės suderinamumas"
HigherPerf="Efektyvus veikimas"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Dažnis (802.11a)"
Rate_802_11bg="Dažnis (802.11b/g)"
WZC_Managed_Ethernet="WZC valdomas Ethernet tinklas"
Legacy="Senesnė įranga"
IBSS_Link_Indication="IBSS (nepriklausomo pagrindinių paslaugų rinkinio) saito rodymas"

[strings.0414] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="USA"
54gAuto="54g - automatisk"
54gLRS="54g – LRS"
54gPerformance="54g - ytelse"
80211bOnly="Bare 802.11b"
AntennaDiversity="Antennevariasjon"
Auto="Automatisk"
AutoShortLong="Auto (kort/lang)"
BSSPLCPHeader="BSS PLCP-hode"
BlueToothCollaboration="Bluetooth-samarbeid"
Default="Standard"
Disable="Deaktiver"
Disable80211a="Deaktiver 802.11a"
Disable80211gb="Deaktiver 802.11g/b"
DisableBands="Deaktiver bånd"
Disabled="Deaktivert"
Enable="Aktiver"
Enabled="Aktivert"
FragmentationThreshold="Fragmenteringsterskel"
IBSS54gtmMode="IBSS 54g-modus"
IBSS54gtmProtectionMode="IBSS 54g-beskyttelsesmodus"
IBSSChannelNumber="IBSS-kanalnummer"
LocallyAdministeredMACAddress="Lokalt administrert MAC-adresse"
Long="Lang"
None="Ingen"
OptimizeBandwidth="Optimaliser båndbredde"
OptimizeDistance="Optimaliser avstand"
PLCPHeader="PLCP-hode"
PowerOutput="Utgangseffekt, strøm"
PowerSaveMode="Strømsparingsmodus"
Prefer80211a="Bruk 802.11a"
Prefer80211gb="Bruk 802.11g/b"
RTSThreshold="RTS-terskel"
RadioEnableDisable="Aktiver/deaktiver radio"
Rate="Hastighet"
RoamingDecision="Roaming-avgjørelse"
Usebestrate="Bruk høyeste hastighet"
XPress_Technology="54g+ (XPress)"
Location="Plassering"
Strict="Streng"
Loose="Mindre streng"
Fast="Rask"
MiminumPowerConsumption="Minimum energiforbruk"
AssociationRoamPreference="Roaming-innstilling for tilknytning"
BandPreference="Båndinnstilling"
RoamingTendency="Roaming-tendens"
Aggressive="Aggressiv"
Moderate="Moderat"
Conservative="Konservativ"
ApCompatibilityMode="AP-kompatibilitetsmodus"
BroaderCompat="Større kompatibilitet"
HigherPerf="Høyere ytelse"
WME="WME (Wi-Fi Multimedia Extensions)"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Hastighet (802.11a)"
Rate_802_11bg="Hastighet (802.11b/g)"
WZC_Managed_Ethernet="WZC-styrt Ethernet (Wireless Zero Configuration)"
Legacy="Tidligere"
IBSS_Link_Indication="IBSS-kobling"

[strings.0415] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Stany Zjednoczone"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="Program 54g - działanie"
80211bOnly="tylko 802.11b"
AntennaDiversity="Zróżnicowanie anten"
Auto="Automatycznie"
AutoShortLong="Auto (krótkie/długie)"
BSSPLCPHeader="Nagłówek BSS PLCP"
BlueToothCollaboration="Współpraca z Bluetooth"
Default="Ustawienie domyślne"
Disable="Wyłącz"
Disable80211a="Wyłącz 802.11a"
Disable80211gb="Wyłącz 802.11g/b"
DisableBands="Wyłącz pasma"
Disabled="Wyłączone"
Enable="Włącz"
Enabled="Włączone"
FragmentationThreshold="Próg fragmentacji"
IBSS54gtmMode="Tryb IBSS 54g"
IBSS54gtmProtectionMode="Tryb zabezpieczenia IBSS 54g"
IBSSChannelNumber="Numer kanału IBSS"
LocallyAdministeredMACAddress="Adres MAC administrowany lokalnie"
Long="Długi"
None="Brak"
OptimizeBandwidth="Ustaw optymalną szerokość pasma"
OptimizeDistance="Ustaw optymalną odległość"
PLCPHeader="Nagłówek PLCP"
PowerOutput="Napięcie wyjściowe"
PowerSaveMode="Tryb oszczędzania energii"
Prefer80211a="Preferuj 802.11a"
Prefer80211gb="Preferuj 802.11g/b"
RTSThreshold="Próg RTS"
RadioEnableDisable="Radio wł./wył."
Rate="Prędkość"
RoamingDecision="Wybór roamingu"
Usebestrate="Wybierz najlepszą prędkość"
XPress_Technology="54g+ (XPress)"
Location="Lokalizacja"
Strict="Dokładnie"
Loose="W przybliżeniu"
Fast="Szybki"
MiminumPowerConsumption="Minimalny pobór mocy"
AssociationRoamPreference="Preferencje roamingu - ustawienia"
BandPreference="Preferencje pasma"
RoamingTendency="Tendencje roamingu"
Aggressive="Agresywna"
Moderate="Umiarkowana"
Conservative="Konserwatywna"
ApCompatibilityMode="Tryb kompatybilności AP"
BroaderCompat="Większa kompatybilność"
HigherPerf="Wyższa wydajność"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Prędkość (802.11a)"
Rate_802_11bg="Prędkość (802.11b/g)"
WZC_Managed_Ethernet="Ethernet zarządzany WZC"
Legacy="Tryb Legacy"
IBSS_Link_Indication="Wskaźnik połączenia IBSS"

[strings.0416] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Estados Unidos"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - Desempenho"
80211bOnly="Apenas 802.11b"
AntennaDiversity="Diversidade da antena"
Auto="Automático"
AutoShortLong="Auto (Curto/Longo)"
BSSPLCPHeader="Cabeçalho PLCP de BSS"
BlueToothCollaboration="Colaboração Bluetooth"
Default="Predefinição"
Disable="Desactivar"
Disable80211a="Desactivar 802.11a"
Disable80211gb="Desactivar 802.11g/b"
DisableBands="Desactivar bandas"
Disabled="Desactivado"
Enable="Activar"
Enabled="Activado"
FragmentationThreshold="Limiar de fragmentação"
IBSS54gtmMode="Modo IBSS 54g"
IBSS54gtmProtectionMode="Modo de protecção IBSS 54g"
IBSSChannelNumber="Número do Canal IBSS"
LocallyAdministeredMACAddress="Endereço MAC administrado localmente"
Long="Longo"
None="Nenhum"
OptimizeBandwidth="Optimizar largura de banda"
OptimizeDistance="Optimizar distância"
PLCPHeader="Cabeçalho PLCP"
PowerOutput="Potência de saída"
PowerSaveMode="Modo economia de energia"
Prefer80211a="Preferir 802.11a"
Prefer80211gb="Preferir 802.11g/b"
RTSThreshold="Limiar de RTS"
RadioEnableDisable="Activar/desactivar Rádio"
Rate="Taxa"
RoamingDecision="Decisão de roaming"
Usebestrate="Utilizar a melhor taxa"
XPress_Technology="54g+ (XPress)"
Location="Local"
Strict="Preciso"
Loose="Lato"
Fast="Rápido"
MiminumPowerConsumption="Consumo mínimo de energia"
AssociationRoamPreference="Preferência de associação móvel"
BandPreference="Preferência de banda"
RoamingTendency="Tendência para mobilidade"
Aggressive="Agressivo"
Moderate="Moderado"
Conservative="Conservadora"
ApCompatibilityMode="Modo de compatibilidade AP"
BroaderCompat="Compatibilidade alargada"
HigherPerf="Elevando rendimento"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Taxa (802.11a)"
Rate_802_11bg="Taxa (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="Indicação de ligação IBSS"

[strings.0816] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Estados Unidos"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - Desempenho"
80211bOnly="Apenas 802.11b"
AntennaDiversity="Diversidade da antena"
Auto="Automático"
AutoShortLong="Auto (Curto/Longo)"
BSSPLCPHeader="Cabeçalho PLCP de BSS"
BlueToothCollaboration="Colaboração Bluetooth"
Default="Predefinição"
Disable="Desactivar"
Disable80211a="Desactivar 802.11a"
Disable80211gb="Desactivar 802.11g/b"
DisableBands="Desactivar bandas"
Disabled="Desactivado"
Enable="Activar"
Enabled="Activado"
FragmentationThreshold="Limiar de fragmentação"
IBSS54gtmMode="Modo IBSS 54g"
IBSS54gtmProtectionMode="Modo de protecção IBSS 54g"
IBSSChannelNumber="Número do Canal IBSS"
LocallyAdministeredMACAddress="Endereço MAC administrado localmente"
Long="Longo"
None="Nenhum"
OptimizeBandwidth="Optimizar largura de banda"
OptimizeDistance="Optimizar distância"
PLCPHeader="Cabeçalho PLCP"
PowerOutput="Potência de saída"
PowerSaveMode="Modo economia de energia"
Prefer80211a="Preferir 802.11a"
Prefer80211gb="Preferir 802.11g/b"
RTSThreshold="Limiar de RTS"
RadioEnableDisable="Activar/desactivar Rádio"
Rate="Taxa"
RoamingDecision="Decisão de roaming"
Usebestrate="Utilizar a melhor taxa"
XPress_Technology="54g+ (XPress)"
Location="Local"
Strict="Preciso"
Loose="Lato"
Fast="Rápido"
MiminumPowerConsumption="Consumo mínimo de energia"
AssociationRoamPreference="Preferência de associação móvel"
BandPreference="Preferência de banda"
RoamingTendency="Tendência para mobilidade"
Aggressive="Agressivo"
Moderate="Moderado"
Conservative="Conservadora"
ApCompatibilityMode="Modo de compatibilidade AP"
BroaderCompat="Compatibilidade alargada"
HigherPerf="Elevando rendimento"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Taxa (802.11a)"
Rate_802_11bg="Taxa (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="Indicação de ligação IBSS"

[strings.0419] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="США"
54gAuto="54g - Автомат."
54gLRS="54g - LRS"
54gPerformance="54g - Производительность"
80211bOnly="Только 802.11b"
AntennaDiversity="Разнесение антенн"
Auto="Автомат."
AutoShortLong="Автомат. выбор (короткий/длинный)"
BSSPLCPHeader="Заголовок BSS в протоколе PLCP"
BlueToothCollaboration="Взаимодействие с Bluetooth"
Default="По умолчанию"
Disable="Отключить"
Disable80211a="Отключить 802.11a"
Disable80211gb="Отключить 802.11g/b"
DisableBands="Отключить диапазоны"
Disabled="Отключено"
Enable="Разрешить"
Enabled="Разрешено"
FragmentationThreshold="Порог фрагментации пакетов"
IBSS54gtmMode="Режим IBSS 54g"
IBSS54gtmProtectionMode="Режим защиты IBSS 54g"
IBSSChannelNumber="Номер канала IBSS"
LocallyAdministeredMACAddress="Локально управляемый MAC-адрес"
Long="Длинный"
None="Нет"
OptimizeBandwidth="Оптимизировать полосу пропускания"
OptimizeDistance="Оптимизировать расстояние"
PLCPHeader="Заголовок PLCP"
PowerOutput="Выходная мощность"
PowerSaveMode="Режим экономии электроэнергии"
Prefer80211a="Предпочтительно 802.11a"
Prefer80211gb="Предпочтительно 802.11g/b"
RTSThreshold="Порог RTS"
RadioEnableDisable="Радио включено/отключено"
Rate="Скорость"
RoamingDecision="Решение по роумингу"
Usebestrate="Работать с оптимальной скоростью"
XPress_Technology="54g+ (XPress)"
Location="Местонахождение"
Strict="Точный"
Loose="Приблизительный"
Fast="Быстрый"
MiminumPowerConsumption="Минимальное потребление электроэнергии"
AssociationRoamPreference="Предпочтение совместного роуминга"
BandPreference="Предпочтение полосы частот"
RoamingTendency="Тенденции роуминга"
Aggressive="Агрессивный"
Moderate="Умеренный"
Conservative="Сдержанный"
ApCompatibilityMode="Режим совместимости AP"
BroaderCompat="Более широкая совместимость"
HigherPerf="Более высокая производительность"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Скорость (802.11a)"
Rate_802_11bg="Скорость (802.11b/g)"
WZC_Managed_Ethernet="Ethernet под управлением WZC"
Legacy="Устаревший"
IBSS_Link_Indication="Индикация соединения IBSS"

[strings.041b] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Spojené štáty americké"
54gAuto="Nastavenie 54g - automaticky"
54gLRS="Nastavenie LRS 54g"
54gPerformance="Nastavenie 54g - výkon"
80211bOnly="Len sieť 802.11b"
AntennaDiversity="Anténa pre viacnásobný príjem"
Auto="Automaticky"
AutoShortLong="Automaticky (krátke/dlhé)"
BSSPLCPHeader="Hlavička BSS PLCP"
BlueToothCollaboration="Spolupráca so systémom Bluetooth"
Default="Predvolené"
Disable="Vypnúť"
Disable80211a="Vypnúť sieť 802.11a"
Disable80211gb="Vypnúť sieť 802.11g/b"
DisableBands="Vypnúť pásma"
Disabled="Vypnuté"
Enable="Zapnúť"
Enabled="Zapnuté"
FragmentationThreshold="Hraničná hodnota fragmentácie"
IBSS54gtmMode="Režim IBSS 54g"
IBSS54gtmProtectionMode="Režim ochrany IBSS 54g"
IBSSChannelNumber="Číslo kanála IBSS"
LocallyAdministeredMACAddress="Lokálne spravovaná adresa MAC"
Long="Dlhý"
None="Žiadny"
OptimizeBandwidth="Optimalizovať šírku pásma"
OptimizeDistance="Optimalizovať vzdialenosť"
PLCPHeader="Hlavička PLCP"
PowerOutput="Výstupný výkon"
PowerSaveMode="Režim na úsporu energie"
Prefer80211a="Preferovať sieť 802.11a"
Prefer80211gb="Preferovať sieť 802.11g/b"
RTSThreshold="Hraničná hodnota RTS"
RadioEnableDisable="Zapnúť a vypnúť rádio"
Rate="Rýchlosť"
RoamingDecision="Rozhodnutie o roamingu"
Usebestrate="Použiť najlepšiu rýchlosť"
XPress_Technology="54g+ (XPress)"
Location="Umiestnenie"
Strict="Presné"
Loose="Voľné"
Fast="Rýchle"
MiminumPowerConsumption="Minimálna spotreba energie"
AssociationRoamPreference="Priradená preferencia roamingu"
BandPreference="Preferencia pásma"
RoamingTendency="Tendencia roamingu"
Aggressive="Agresívna"
Moderate="Mierna"
Conservative="Konzervatívna"
ApCompatibilityMode="Režim kompatibility prístupového bodu"
BroaderCompat="Širšia kompatibilita"
HigherPerf="Vyšší výkon"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Rýchlosť (802.11a)"
Rate_802_11bg="Rýchlosť (802.11b/g)"
WZC_Managed_Ethernet="WZC riadený Ethernet"
Legacy="Dedičstvo"
IBSS_Link_Indication="Indikácia prepojenia IBSS"

[strings.0424] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Združene države"
54gAuto="54g - Samodejno"
54gLRS="54g - LRS"
54gPerformance="54g - Učinkovitost"
80211bOnly="Samo 802.11b"
AntennaDiversity="Prilagodljivost antene"
Auto="Samodejno"
AutoShortLong="Samodejno (Kratko/Dolgo)"
BSSPLCPHeader="BSS PLCP glava"
BlueToothCollaboration="Bluetooth sodelovanje"
Default="Privzeto"
Disable="Onemogoči"
Disable80211a="Onemogoči 802.11a"
Disable80211gb="Onemogoči 802.11g/b"
DisableBands="Onemogoči pasove"
Disabled="Onemogočeno"
Enable="Omogoči"
Enabled="Omogočeno"
FragmentationThreshold="Prag fragmentacije"
IBSS54gtmMode="Način IBSS 54g"
IBSS54gtmProtectionMode="Način zaščite IBSS 54g"
IBSSChannelNumber="IBSS številka kanala"
LocallyAdministeredMACAddress="Lokalno upravljan MAC naslov"
Long="Dolgo"
None="Brez"
OptimizeBandwidth="Optimiraj pasovno širino"
OptimizeDistance="Optimiraj razdaljo"
PLCPHeader="Glava PLCP"
PowerOutput="Izhodna moč"
PowerSaveMode="Način varčevanja z energijo"
Prefer80211a="Prednostno 802.11a"
Prefer80211gb="Prednostno 802.11g/b"
RTSThreshold="Prag RTS"
RadioEnableDisable="Radio omogoči/onemogoči"
Rate="Hitrost"
RoamingDecision="Odločitev o sledenju"
Usebestrate="Uporabi najboljšo hitrost"
XPress_Technology="54g+ (XPress)"
Location="Mesto"
Strict="Dosledno"
Loose="Ohlapno"
Fast="Hitro"
MiminumPowerConsumption="Minimalna poraba energije"
AssociationRoamPreference="Prednost sledenja združevanja"
BandPreference="Prednostni pas"
RoamingTendency="Tendenca sledenja"
Aggressive="Agresivno"
Moderate="Zmerno"
Conservative="Konzervativno"
ApCompatibilityMode="Način združljivosti AP"
BroaderCompat="Širša združljivost"
HigherPerf="Višja učinkovitost"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Hitrost (802.11a)"
Rate_802_11bg="Hitrost (802.11b/g)"
WZC_Managed_Ethernet="Upravljani ethernet WZC"
Legacy="Legacy"
IBSS_Link_Indication="Označba za povezavo IBSS"

[strings.2c0a] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Estados Unidos"
54gAuto="54g - Automático"
54gLRS="54 g - LRS"
54gPerformance="54g - Rendimiento"
80211bOnly="Sólo 802.11b"
AntennaDiversity="Diversidad de antena"
Auto="Automático"
AutoShortLong="Automático (corto/largo)"
BSSPLCPHeader="Encabezamiento BSS PLCP"
BlueToothCollaboration="Colaboración Bluetooth"
Default="Predeterminado"
Disable="Deshabilitar"
Disable80211a="Deshabilitar 802.11a"
Disable80211gb="Deshabilitar 802.11g/b"
DisableBands="Deshabilitar bandas"
Disabled="Deshabilitado"
Enable="Habilitar"
Enabled="Habilitado"
FragmentationThreshold="Umbral de fragmentación"
IBSS54gtmMode="Modo 54g(tm) IBSS"
IBSS54gtmProtectionMode="Modo de protección 54g(tm) IBSS"
IBSSChannelNumber="Número de canal IBSS"
LocallyAdministeredMACAddress="Dirección MAC administrada de manera local"
Long="Largo"
None="Ninguno"
OptimizeBandwidth="Optimizar ancho de banda"
OptimizeDistance="Optimizar distancia"
PLCPHeader="Encabezamiento PLCP"
PowerOutput="Salida de energía"
PowerSaveMode="Modo para ahorrar energía"
Prefer80211a="Preferir 802.11a"
Prefer80211gb="Preferir 802.11g/b"
RTSThreshold="Umbral RTS"
RadioEnableDisable="Habilitar/Deshabilitar radio"
Rate="Tasa"
RoamingDecision="Decisión de movilidad"
Usebestrate="Usar la mejor tasa"
XPress_Technology="54g+ (XPress)"
Location="Ubicación"
Strict="Estricto"
Loose="Flexible"
Fast="Rápido"
MiminumPowerConsumption="Consumo mínimo de energía"
AssociationRoamPreference="Preferencia de movilidad de asociación"
BandPreference="Preferencia de banda"
RoamingTendency="Tendencia de movilidad"
Aggressive="Agresiva"
Moderate="Moderada"
Conservative="Conservadora"
ApCompatibilityMode="Modo de compatibilidad AP"
BroaderCompat="Compatibilidad amplia"
HigherPerf="Alto rendimiento"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Tasa (802.11a)"
Rate_802_11bg="Tasa (802.11b/g)"
WZC_Managed_Ethernet="Ethernet administrada por WZC"
Legacy="Legacy"
IBSS_Link_Indication="Indicación de enlace IBSS"

[strings.400a] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Estados Unidos"
54gAuto="54g - Automático"
54gLRS="54 g - LRS"
54gPerformance="54g - Rendimiento"
80211bOnly="Sólo 802.11b"
AntennaDiversity="Diversidad de antena"
Auto="Automático"
AutoShortLong="Automático (corto/largo)"
BSSPLCPHeader="Encabezamiento BSS PLCP"
BlueToothCollaboration="Colaboración Bluetooth"
Default="Predeterminado"
Disable="Deshabilitar"
Disable80211a="Deshabilitar 802.11a"
Disable80211gb="Deshabilitar 802.11g/b"
DisableBands="Deshabilitar bandas"
Disabled="Deshabilitado"
Enable="Habilitar"
Enabled="Habilitado"
FragmentationThreshold="Umbral de fragmentación"
IBSS54gtmMode="Modo 54g(tm) IBSS"
IBSS54gtmProtectionMode="Modo de protección 54g(tm) IBSS"
IBSSChannelNumber="Número de canal IBSS"
LocallyAdministeredMACAddress="Dirección MAC administrada de manera local"
Long="Largo"
None="Ninguno"
OptimizeBandwidth="Optimizar ancho de banda"
OptimizeDistance="Optimizar distancia"
PLCPHeader="Encabezamiento PLCP"
PowerOutput="Salida de energía"
PowerSaveMode="Modo para ahorrar energía"
Prefer80211a="Preferir 802.11a"
Prefer80211gb="Preferir 802.11g/b"
RTSThreshold="Umbral RTS"
RadioEnableDisable="Habilitar/Deshabilitar radio"
Rate="Tasa"
RoamingDecision="Decisión de movilidad"
Usebestrate="Usar la mejor tasa"
XPress_Technology="54g+ (XPress)"
Location="Ubicación"
Strict="Estricto"
Loose="Flexible"
Fast="Rápido"
MiminumPowerConsumption="Consumo mínimo de energía"
AssociationRoamPreference="Preferencia de movilidad de asociación"
BandPreference="Preferencia de banda"
RoamingTendency="Tendencia de movilidad"
Aggressive="Agresiva"
Moderate="Moderada"
Conservative="Conservadora"
ApCompatibilityMode="Modo de compatibilidad AP"
BroaderCompat="Compatibilidad amplia"
HigherPerf="Alto rendimiento"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Tasa (802.11a)"
Rate_802_11bg="Tasa (802.11b/g)"
WZC_Managed_Ethernet="Ethernet administrada por WZC"
Legacy="Legacy"
IBSS_Link_Indication="Indicación de enlace IBSS"

[strings.340a] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Estados Unidos"
54gAuto="54g - Automático"
54gLRS="54 g - LRS"
54gPerformance="54g - Rendimiento"
80211bOnly="Sólo 802.11b"
AntennaDiversity="Diversidad de antena"
Auto="Automático"
AutoShortLong="Automático (corto/largo)"
BSSPLCPHeader="Encabezamiento BSS PLCP"
BlueToothCollaboration="Colaboración Bluetooth"
Default="Predeterminado"
Disable="Deshabilitar"
Disable80211a="Deshabilitar 802.11a"
Disable80211gb="Deshabilitar 802.11g/b"
DisableBands="Deshabilitar bandas"
Disabled="Deshabilitado"
Enable="Habilitar"
Enabled="Habilitado"
FragmentationThreshold="Umbral de fragmentación"
IBSS54gtmMode="Modo 54g(tm) IBSS"
IBSS54gtmProtectionMode="Modo de protección 54g(tm) IBSS"
IBSSChannelNumber="Número de canal IBSS"
LocallyAdministeredMACAddress="Dirección MAC administrada de manera local"
Long="Largo"
None="Ninguno"
OptimizeBandwidth="Optimizar ancho de banda"
OptimizeDistance="Optimizar distancia"
PLCPHeader="Encabezamiento PLCP"
PowerOutput="Salida de energía"
PowerSaveMode="Modo para ahorrar energía"
Prefer80211a="Preferir 802.11a"
Prefer80211gb="Preferir 802.11g/b"
RTSThreshold="Umbral RTS"
RadioEnableDisable="Habilitar/Deshabilitar radio"
Rate="Tasa"
RoamingDecision="Decisión de movilidad"
Usebestrate="Usar la mejor tasa"
XPress_Technology="54g+ (XPress)"
Location="Ubicación"
Strict="Estricto"
Loose="Flexible"
Fast="Rápido"
MiminumPowerConsumption="Consumo mínimo de energía"
AssociationRoamPreference="Preferencia de movilidad de asociación"
BandPreference="Preferencia de banda"
RoamingTendency="Tendencia de movilidad"
Aggressive="Agresiva"
Moderate="Moderada"
Conservative="Conservadora"
ApCompatibilityMode="Modo de compatibilidad AP"
BroaderCompat="Compatibilidad amplia"
HigherPerf="Alto rendimiento"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Tasa (802.11a)"
Rate_802_11bg="Tasa (802.11b/g)"
WZC_Managed_Ethernet="Ethernet administrada por WZC"
Legacy="Legacy"
IBSS_Link_Indication="Indicación de enlace IBSS"

[strings.240a] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Estados Unidos"
54gAuto="54g - Automático"
54gLRS="54 g - LRS"
54gPerformance="54g - Rendimiento"
80211bOnly="Sólo 802.11b"
AntennaDiversity="Diversidad de antena"
Auto="Automático"
AutoShortLong="Automático (corto/largo)"
BSSPLCPHeader="Encabezamiento BSS PLCP"
BlueToothCollaboration="Colaboración Bluetooth"
Default="Predeterminado"
Disable="Deshabilitar"
Disable80211a="Deshabilitar 802.11a"
Disable80211gb="Deshabilitar 802.11g/b"
DisableBands="Deshabilitar bandas"
Disabled="Deshabilitado"
Enable="Habilitar"
Enabled="Habilitado"
FragmentationThreshold="Umbral de fragmentación"
IBSS54gtmMode="Modo 54g(tm) IBSS"
IBSS54gtmProtectionMode="Modo de protección 54g(tm) IBSS"
IBSSChannelNumber="Número de canal IBSS"
LocallyAdministeredMACAddress="Dirección MAC administrada de manera local"
Long="Largo"
None="Ninguno"
OptimizeBandwidth="Optimizar ancho de banda"
OptimizeDistance="Optimizar distancia"
PLCPHeader="Encabezamiento PLCP"
PowerOutput="Salida de energía"
PowerSaveMode="Modo para ahorrar energía"
Prefer80211a="Preferir 802.11a"
Prefer80211gb="Preferir 802.11g/b"
RTSThreshold="Umbral RTS"
RadioEnableDisable="Habilitar/Deshabilitar radio"
Rate="Tasa"
RoamingDecision="Decisión de movilidad"
Usebestrate="Usar la mejor tasa"
XPress_Technology="54g+ (XPress)"
Location="Ubicación"
Strict="Estricto"
Loose="Flexible"
Fast="Rápido"
MiminumPowerConsumption="Consumo mínimo de energía"
AssociationRoamPreference="Preferencia de movilidad de asociación"
BandPreference="Preferencia de banda"
RoamingTendency="Tendencia de movilidad"
Aggressive="Agresiva"
Moderate="Moderada"
Conservative="Conservadora"
ApCompatibilityMode="Modo de compatibilidad AP"
BroaderCompat="Compatibilidad amplia"
HigherPerf="Alto rendimiento"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Tasa (802.11a)"
Rate_802_11bg="Tasa (802.11b/g)"
WZC_Managed_Ethernet="Ethernet administrada por WZC"
Legacy="Legacy"
IBSS_Link_Indication="Indicación de enlace IBSS"

[strings.300a] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Estados Unidos"
54gAuto="54g - Automático"
54gLRS="54 g - LRS"
54gPerformance="54g - Rendimiento"
80211bOnly="Sólo 802.11b"
AntennaDiversity="Diversidad de antena"
Auto="Automático"
AutoShortLong="Automático (corto/largo)"
BSSPLCPHeader="Encabezamiento BSS PLCP"
BlueToothCollaboration="Colaboración Bluetooth"
Default="Predeterminado"
Disable="Deshabilitar"
Disable80211a="Deshabilitar 802.11a"
Disable80211gb="Deshabilitar 802.11g/b"
DisableBands="Deshabilitar bandas"
Disabled="Deshabilitado"
Enable="Habilitar"
Enabled="Habilitado"
FragmentationThreshold="Umbral de fragmentación"
IBSS54gtmMode="Modo 54g(tm) IBSS"
IBSS54gtmProtectionMode="Modo de protección 54g(tm) IBSS"
IBSSChannelNumber="Número de canal IBSS"
LocallyAdministeredMACAddress="Dirección MAC administrada de manera local"
Long="Largo"
None="Ninguno"
OptimizeBandwidth="Optimizar ancho de banda"
OptimizeDistance="Optimizar distancia"
PLCPHeader="Encabezamiento PLCP"
PowerOutput="Salida de energía"
PowerSaveMode="Modo para ahorrar energía"
Prefer80211a="Preferir 802.11a"
Prefer80211gb="Preferir 802.11g/b"
RTSThreshold="Umbral RTS"
RadioEnableDisable="Habilitar/Deshabilitar radio"
Rate="Tasa"
RoamingDecision="Decisión de movilidad"
Usebestrate="Usar la mejor tasa"
XPress_Technology="54g+ (XPress)"
Location="Ubicación"
Strict="Estricto"
Loose="Flexible"
Fast="Rápido"
MiminumPowerConsumption="Consumo mínimo de energía"
AssociationRoamPreference="Preferencia de movilidad de asociación"
BandPreference="Preferencia de banda"
RoamingTendency="Tendencia de movilidad"
Aggressive="Agresiva"
Moderate="Moderada"
Conservative="Conservadora"
ApCompatibilityMode="Modo de compatibilidad AP"
BroaderCompat="Compatibilidad amplia"
HigherPerf="Alto rendimiento"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Tasa (802.11a)"
Rate_802_11bg="Tasa (802.11b/g)"
WZC_Managed_Ethernet="Ethernet administrada por WZC"
Legacy="Legacy"
IBSS_Link_Indication="Indicación de enlace IBSS"

[strings.080a] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Estados Unidos"
54gAuto="54g - Automático"
54gLRS="54 g - LRS"
54gPerformance="54g - Rendimiento"
80211bOnly="Sólo 802.11b"
AntennaDiversity="Diversidad de antena"
Auto="Automático"
AutoShortLong="Automático (corto/largo)"
BSSPLCPHeader="Encabezamiento BSS PLCP"
BlueToothCollaboration="Colaboración Bluetooth"
Default="Predeterminado"
Disable="Deshabilitar"
Disable80211a="Deshabilitar 802.11a"
Disable80211gb="Deshabilitar 802.11g/b"
DisableBands="Deshabilitar bandas"
Disabled="Deshabilitado"
Enable="Habilitar"
Enabled="Habilitado"
FragmentationThreshold="Umbral de fragmentación"
IBSS54gtmMode="Modo 54g(tm) IBSS"
IBSS54gtmProtectionMode="Modo de protección 54g(tm) IBSS"
IBSSChannelNumber="Número de canal IBSS"
LocallyAdministeredMACAddress="Dirección MAC administrada de manera local"
Long="Largo"
None="Ninguno"
OptimizeBandwidth="Optimizar ancho de banda"
OptimizeDistance="Optimizar distancia"
PLCPHeader="Encabezamiento PLCP"
PowerOutput="Salida de energía"
PowerSaveMode="Modo para ahorrar energía"
Prefer80211a="Preferir 802.11a"
Prefer80211gb="Preferir 802.11g/b"
RTSThreshold="Umbral RTS"
RadioEnableDisable="Habilitar/Deshabilitar radio"
Rate="Tasa"
RoamingDecision="Decisión de movilidad"
Usebestrate="Usar la mejor tasa"
XPress_Technology="54g+ (XPress)"
Location="Ubicación"
Strict="Estricto"
Loose="Flexible"
Fast="Rápido"
MiminumPowerConsumption="Consumo mínimo de energía"
AssociationRoamPreference="Preferencia de movilidad de asociación"
BandPreference="Preferencia de banda"
RoamingTendency="Tendencia de movilidad"
Aggressive="Agresiva"
Moderate="Moderada"
Conservative="Conservadora"
ApCompatibilityMode="Modo de compatibilidad AP"
BroaderCompat="Compatibilidad amplia"
HigherPerf="Alto rendimiento"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Tasa (802.11a)"
Rate_802_11bg="Tasa (802.11b/g)"
WZC_Managed_Ethernet="Ethernet administrada por WZC"
Legacy="Legacy"
IBSS_Link_Indication="Indicación de enlace IBSS"

[strings.180a] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Estados Unidos"
54gAuto="54g - Automático"
54gLRS="54 g - LRS"
54gPerformance="54g - Rendimiento"
80211bOnly="Sólo 802.11b"
AntennaDiversity="Diversidad de antena"
Auto="Automático"
AutoShortLong="Automático (corto/largo)"
BSSPLCPHeader="Encabezamiento BSS PLCP"
BlueToothCollaboration="Colaboración Bluetooth"
Default="Predeterminado"
Disable="Deshabilitar"
Disable80211a="Deshabilitar 802.11a"
Disable80211gb="Deshabilitar 802.11g/b"
DisableBands="Deshabilitar bandas"
Disabled="Deshabilitado"
Enable="Habilitar"
Enabled="Habilitado"
FragmentationThreshold="Umbral de fragmentación"
IBSS54gtmMode="Modo 54g(tm) IBSS"
IBSS54gtmProtectionMode="Modo de protección 54g(tm) IBSS"
IBSSChannelNumber="Número de canal IBSS"
LocallyAdministeredMACAddress="Dirección MAC administrada de manera local"
Long="Largo"
None="Ninguno"
OptimizeBandwidth="Optimizar ancho de banda"
OptimizeDistance="Optimizar distancia"
PLCPHeader="Encabezamiento PLCP"
PowerOutput="Salida de energía"
PowerSaveMode="Modo para ahorrar energía"
Prefer80211a="Preferir 802.11a"
Prefer80211gb="Preferir 802.11g/b"
RTSThreshold="Umbral RTS"
RadioEnableDisable="Habilitar/Deshabilitar radio"
Rate="Tasa"
RoamingDecision="Decisión de movilidad"
Usebestrate="Usar la mejor tasa"
XPress_Technology="54g+ (XPress)"
Location="Ubicación"
Strict="Estricto"
Loose="Flexible"
Fast="Rápido"
MiminumPowerConsumption="Consumo mínimo de energía"
AssociationRoamPreference="Preferencia de movilidad de asociación"
BandPreference="Preferencia de banda"
RoamingTendency="Tendencia de movilidad"
Aggressive="Agresiva"
Moderate="Moderada"
Conservative="Conservadora"
ApCompatibilityMode="Modo de compatibilidad AP"
BroaderCompat="Compatibilidad amplia"
HigherPerf="Alto rendimiento"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Tasa (802.11a)"
Rate_802_11bg="Tasa (802.11b/g)"
WZC_Managed_Ethernet="Ethernet administrada por WZC"
Legacy="Legacy"
IBSS_Link_Indication="Indicación de enlace IBSS"

[strings.280a] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Estados Unidos"
54gAuto="54g - Automático"
54gLRS="54 g - LRS"
54gPerformance="54g - Rendimiento"
80211bOnly="Sólo 802.11b"
AntennaDiversity="Diversidad de antena"
Auto="Automático"
AutoShortLong="Automático (corto/largo)"
BSSPLCPHeader="Encabezamiento BSS PLCP"
BlueToothCollaboration="Colaboración Bluetooth"
Default="Predeterminado"
Disable="Deshabilitar"
Disable80211a="Deshabilitar 802.11a"
Disable80211gb="Deshabilitar 802.11g/b"
DisableBands="Deshabilitar bandas"
Disabled="Deshabilitado"
Enable="Habilitar"
Enabled="Habilitado"
FragmentationThreshold="Umbral de fragmentación"
IBSS54gtmMode="Modo 54g(tm) IBSS"
IBSS54gtmProtectionMode="Modo de protección 54g(tm) IBSS"
IBSSChannelNumber="Número de canal IBSS"
LocallyAdministeredMACAddress="Dirección MAC administrada de manera local"
Long="Largo"
None="Ninguno"
OptimizeBandwidth="Optimizar ancho de banda"
OptimizeDistance="Optimizar distancia"
PLCPHeader="Encabezamiento PLCP"
PowerOutput="Salida de energía"
PowerSaveMode="Modo para ahorrar energía"
Prefer80211a="Preferir 802.11a"
Prefer80211gb="Preferir 802.11g/b"
RTSThreshold="Umbral RTS"
RadioEnableDisable="Habilitar/Deshabilitar radio"
Rate="Tasa"
RoamingDecision="Decisión de movilidad"
Usebestrate="Usar la mejor tasa"
XPress_Technology="54g+ (XPress)"
Location="Ubicación"
Strict="Estricto"
Loose="Flexible"
Fast="Rápido"
MiminumPowerConsumption="Consumo mínimo de energía"
AssociationRoamPreference="Preferencia de movilidad de asociación"
BandPreference="Preferencia de banda"
RoamingTendency="Tendencia de movilidad"
Aggressive="Agresiva"
Moderate="Moderada"
Conservative="Conservadora"
ApCompatibilityMode="Modo de compatibilidad AP"
BroaderCompat="Compatibilidad amplia"
HigherPerf="Alto rendimiento"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Tasa (802.11a)"
Rate_802_11bg="Tasa (802.11b/g)"
WZC_Managed_Ethernet="Ethernet administrada por WZC"
Legacy="Legacy"
IBSS_Link_Indication="Indicación de enlace IBSS"

[strings.0c0a] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Estados Unidos"
54gAuto="54g - Automático"
54gLRS="54 g - LRS"
54gPerformance="54g - Rendimiento"
80211bOnly="Sólo 802.11b"
AntennaDiversity="Diversidad de antena"
Auto="Automático"
AutoShortLong="Automático (corto/largo)"
BSSPLCPHeader="Encabezamiento BSS PLCP"
BlueToothCollaboration="Colaboración Bluetooth"
Default="Predeterminado"
Disable="Deshabilitar"
Disable80211a="Deshabilitar 802.11a"
Disable80211gb="Deshabilitar 802.11g/b"
DisableBands="Deshabilitar bandas"
Disabled="Deshabilitado"
Enable="Habilitar"
Enabled="Habilitado"
FragmentationThreshold="Umbral de fragmentación"
IBSS54gtmMode="Modo 54g(tm) IBSS"
IBSS54gtmProtectionMode="Modo de protección 54g(tm) IBSS"
IBSSChannelNumber="Número de canal IBSS"
LocallyAdministeredMACAddress="Dirección MAC administrada de manera local"
Long="Largo"
None="Ninguno"
OptimizeBandwidth="Optimizar ancho de banda"
OptimizeDistance="Optimizar distancia"
PLCPHeader="Encabezamiento PLCP"
PowerOutput="Salida de energía"
PowerSaveMode="Modo para ahorrar energía"
Prefer80211a="Preferir 802.11a"
Prefer80211gb="Preferir 802.11g/b"
RTSThreshold="Umbral RTS"
RadioEnableDisable="Habilitar/Deshabilitar radio"
Rate="Tasa"
RoamingDecision="Decisión de movilidad"
Usebestrate="Usar la mejor tasa"
XPress_Technology="54g+ (XPress)"
Location="Ubicación"
Strict="Estricto"
Loose="Flexible"
Fast="Rápido"
MiminumPowerConsumption="Consumo mínimo de energía"
AssociationRoamPreference="Preferencia de movilidad de asociación"
BandPreference="Preferencia de banda"
RoamingTendency="Tendencia de movilidad"
Aggressive="Agresiva"
Moderate="Moderada"
Conservative="Conservadora"
ApCompatibilityMode="Modo de compatibilidad AP"
BroaderCompat="Compatibilidad amplia"
HigherPerf="Alto rendimiento"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Tasa (802.11a)"
Rate_802_11bg="Tasa (802.11b/g)"
WZC_Managed_Ethernet="Ethernet administrada por WZC"
Legacy="Legacy"
IBSS_Link_Indication="Indicación de enlace IBSS"

[strings.380a] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Estados Unidos"
54gAuto="54g - Automático"
54gLRS="54 g - LRS"
54gPerformance="54g - Rendimiento"
80211bOnly="Sólo 802.11b"
AntennaDiversity="Diversidad de antena"
Auto="Automático"
AutoShortLong="Automático (corto/largo)"
BSSPLCPHeader="Encabezamiento BSS PLCP"
BlueToothCollaboration="Colaboración Bluetooth"
Default="Predeterminado"
Disable="Deshabilitar"
Disable80211a="Deshabilitar 802.11a"
Disable80211gb="Deshabilitar 802.11g/b"
DisableBands="Deshabilitar bandas"
Disabled="Deshabilitado"
Enable="Habilitar"
Enabled="Habilitado"
FragmentationThreshold="Umbral de fragmentación"
IBSS54gtmMode="Modo 54g(tm) IBSS"
IBSS54gtmProtectionMode="Modo de protección 54g(tm) IBSS"
IBSSChannelNumber="Número de canal IBSS"
LocallyAdministeredMACAddress="Dirección MAC administrada de manera local"
Long="Largo"
None="Ninguno"
OptimizeBandwidth="Optimizar ancho de banda"
OptimizeDistance="Optimizar distancia"
PLCPHeader="Encabezamiento PLCP"
PowerOutput="Salida de energía"
PowerSaveMode="Modo para ahorrar energía"
Prefer80211a="Preferir 802.11a"
Prefer80211gb="Preferir 802.11g/b"
RTSThreshold="Umbral RTS"
RadioEnableDisable="Habilitar/Deshabilitar radio"
Rate="Tasa"
RoamingDecision="Decisión de movilidad"
Usebestrate="Usar la mejor tasa"
XPress_Technology="54g+ (XPress)"
Location="Ubicación"
Strict="Estricto"
Loose="Flexible"
Fast="Rápido"
MiminumPowerConsumption="Consumo mínimo de energía"
AssociationRoamPreference="Preferencia de movilidad de asociación"
BandPreference="Preferencia de banda"
RoamingTendency="Tendencia de movilidad"
Aggressive="Agresiva"
Moderate="Moderada"
Conservative="Conservadora"
ApCompatibilityMode="Modo de compatibilidad AP"
BroaderCompat="Compatibilidad amplia"
HigherPerf="Alto rendimiento"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Tasa (802.11a)"
Rate_802_11bg="Tasa (802.11b/g)"
WZC_Managed_Ethernet="Ethernet administrada por WZC"
Legacy="Legacy"
IBSS_Link_Indication="Indicación de enlace IBSS"

[strings.200a] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="Estados Unidos"
54gAuto="54g - Automático"
54gLRS="54 g - LRS"
54gPerformance="54g - Rendimiento"
80211bOnly="Sólo 802.11b"
AntennaDiversity="Diversidad de antena"
Auto="Automático"
AutoShortLong="Automático (corto/largo)"
BSSPLCPHeader="Encabezamiento BSS PLCP"
BlueToothCollaboration="Colaboración Bluetooth"
Default="Predeterminado"
Disable="Deshabilitar"
Disable80211a="Deshabilitar 802.11a"
Disable80211gb="Deshabilitar 802.11g/b"
DisableBands="Deshabilitar bandas"
Disabled="Deshabilitado"
Enable="Habilitar"
Enabled="Habilitado"
FragmentationThreshold="Umbral de fragmentación"
IBSS54gtmMode="Modo 54g(tm) IBSS"
IBSS54gtmProtectionMode="Modo de protección 54g(tm) IBSS"
IBSSChannelNumber="Número de canal IBSS"
LocallyAdministeredMACAddress="Dirección MAC administrada de manera local"
Long="Largo"
None="Ninguno"
OptimizeBandwidth="Optimizar ancho de banda"
OptimizeDistance="Optimizar distancia"
PLCPHeader="Encabezamiento PLCP"
PowerOutput="Salida de energía"
PowerSaveMode="Modo para ahorrar energía"
Prefer80211a="Preferir 802.11a"
Prefer80211gb="Preferir 802.11g/b"
RTSThreshold="Umbral RTS"
RadioEnableDisable="Habilitar/Deshabilitar radio"
Rate="Tasa"
RoamingDecision="Decisión de movilidad"
Usebestrate="Usar la mejor tasa"
XPress_Technology="54g+ (XPress)"
Location="Ubicación"
Strict="Estricto"
Loose="Flexible"
Fast="Rápido"
MiminumPowerConsumption="Consumo mínimo de energía"
AssociationRoamPreference="Preferencia de movilidad de asociación"
BandPreference="Preferencia de banda"
RoamingTendency="Tendencia de movilidad"
Aggressive="Agresiva"
Moderate="Moderada"
Conservative="Conservadora"
ApCompatibilityMode="Modo de compatibilidad AP"
BroaderCompat="Compatibilidad amplia"
HigherPerf="Alto rendimiento"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Tasa (802.11a)"
Rate_802_11bg="Tasa (802.11b/g)"
WZC_Managed_Ethernet="Ethernet administrada por WZC"
Legacy="Legacy"
IBSS_Link_Indication="Indicación de enlace IBSS"

[strings.041d] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="USA"
54gAuto="54g - Auto"
54gLRS="54g - LRS"
54gPerformance="54g - Prestanda"
80211bOnly="Endast 802.11b"
AntennaDiversity="Antenndiversitet"
Auto="Automatisk"
AutoShortLong="Auto (kort/lång)"
BSSPLCPHeader="BSS PLCP-huvud"
BlueToothCollaboration="Bluetooth-samarbete"
Default="Standardvärde"
Disable="Avaktivera"
Disable80211a="Avaktivera 802.11a"
Disable80211gb="Avaktivera 802.11g/b"
DisableBands="Avaktivera band"
Disabled="Avaktivera"
Enable="Aktivera"
Enabled="Aktiverad"
FragmentationThreshold="Fragmentationsgräns"
IBSS54gtmMode="IBSS 54g-läge"
IBSS54gtmProtectionMode="IBSS 54g-skyddsläge"
IBSSChannelNumber="IBSS-kanal"
LocallyAdministeredMACAddress="Lokalt tilldelad MAC-adress"
Long="Lång"
None="Ingen"
OptimizeBandwidth="Optimera bandbredd"
OptimizeDistance="Optimera avstånd"
PLCPHeader="PLCP-huvud"
PowerOutput="Uteffekt"
PowerSaveMode="Strömsparläge"
Prefer80211a="Föredra 802.11a"
Prefer80211gb="Föredra 802.11g/b"
RTSThreshold="RTS-gräns"
RadioEnableDisable="Aktivera/avaktivera radio"
Rate="Hastighet"
RoamingDecision="Roamingbeslut"
Usebestrate="Använd högsta hastighet"
XPress_Technology="54g+ (XPress)"
Location="Plats"
Strict="Absolut"
Loose="Lös"
Fast="Snabb"
MiminumPowerConsumption="Minsta strömförbrukning"
AssociationRoamPreference="Associationsroaminginställning"
BandPreference="Bandinställning"
RoamingTendency="Roamingbenägenhet"
Aggressive="Hög"
Moderate="Medelhög"
Conservative="Låg"
ApCompatibilityMode="AP-kompatibilitetsläge"
BroaderCompat="Bredare kompatibilitet"
HigherPerf="Högre prestanda"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Hastighet (802.11a)"
Rate_802_11bg="Hastighet (802.11b/g)"
WZC_Managed_Ethernet="WZC-hanterat Ethernet"
Legacy="Tidigare versioner"
IBSS_Link_Indication="IBSS-länkangivelse"

[strings.041e] 
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="สหรัฐอเมริกา"
54gAuto="54g - อัตโนมัติ"
54gLRS="54g - LRS"
54gPerformance="แบบ 54g"
80211bOnly="802.11b เท่านั้น"
AntennaDiversity="สายอากาศแบบต่างๆ"
Auto="อัตโนมัติ"
AutoShortLong="อัตโนมัติ (สั้น/ยาว)"
BSSPLCPHeader="BSS PLCP ส่วนหน้า"
BlueToothCollaboration="การใช้งานร่วมกับบลูทูธ"
Default="ค่าเริ่มต้น"
Disable="ปิดการใช้งาน"
Disable80211a="ปิดการใช้งานของ 802.11a"
Disable80211gb="ปิดการใช้งานของ 802.11g/b"
DisableBands="ปิดการใช้งานคลื่นความถี่"
Disabled="ปิดการใช้งาน"
Enable="เปิดการใช้งาน"
Enabled="เปิดการใช้งานอยู่"
FragmentationThreshold="การแบ่งแยกช่องสัญญาณ"
IBSS54gtmMode="แบบ IBSS 54g"
IBSS54gtmProtectionMode="แบบ IBSS 54g พร้อมการป้องกัน"
IBSSChannelNumber="หมายเลขของช่องสัญญาณ IBSS"
LocallyAdministeredMACAddress="ตำแหน่ง MAC ที่ได้รับการควบคุมในระบบ"
Long="ยาว"
None="ไม่มี"
OptimizeBandwidth="การปรับช่วงกว้างของสัญญาณให้ได้ผลดีที่สุด"
OptimizeDistance="การปรับช่วงระยะห่างของสัญญาณให้ได้ผลดีที่สุด"
PLCPHeader="PLCP ส่วนหน้า"
PowerOutput="เอาต์พุตพลังงาน"
PowerSaveMode="แบบประหยัดพลังงาน"
Prefer80211a="น่าจะเลือก 802.11a"
Prefer80211gb="น่าจะเลือก 802.11g/b"
RTSThreshold="ค่าที่ตั้งไว้ของ RTS"
RadioEnableDisable="คลื่นวิทยุ เปิด/ปิดการใช้งาน"
Rate="อัตรา"
RoamingDecision="ตัดสินใจเลือก โรมมิ่ง"
Usebestrate="เลือกใช้ อัตราที่ดีที่สุด"
XPress_Technology="54g+ (XPress)"
Location="ตำแหน่งที่ตั้ง"
Strict="โดยเฉพาะ"
Loose="ไม่รีบ"
Fast="รวดเร็ว"
MiminumPowerConsumption="พลังงานไฟฟ้าที่ใช้ต่ำสุด"
AssociationRoamPreference="การตั้งค่าโรมมิ่งการเชื่อมต่อ"
BandPreference="การตั้งค่าย่านความถี่"
RoamingTendency="แนวโน้มของโรมมิ่ง"
Aggressive="เชิงรุก"
Moderate="ปานกลาง"
Conservative="แบบเก่า"
ApCompatibilityMode="โหมดที่ใช้ร่วมกับ AP ได้"
BroaderCompat="ใช้ร่วมกันได้อย่างหลากหลาย"
HigherPerf="ประสิทธิภาพสูงขึ้น"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="อัตรา (802.11a)"
Rate_802_11bg="อัตรา (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="แบบเก่า"
IBSS_Link_Indication="การแสดงการเชื่อมต่อ IBSS"

[strings.041f]
V_BCM="U.S. Robotics Corporation"
BCM430G_DeviceDesc="U.S. Robotics Wireless MAXg PC Card"
BCM430PCI_DeviceDesc="U.S. Robotics Wireless MAXg PCI Adapter"
BCM43XX_HELP="U.S. Robotics Wireless MAXg Adapter provides wireless local area networking."
BCM43XX_Service_DispName="U.S. Robotics Wireless MAXg Adapter"
BCM43XX_DiskName="U.S. Robotics Wireless MAXg Network Adapter Install Disk"
UnitedStates="A.B.D."
54gAuto="54g - Otomatik"
54gLRS="54g LRS"
54gPerformance="54g - Performans"
80211bOnly="Sadece 802.11b"
AntennaDiversity="Anten Çeşitliliği"
Auto="Otomatik"
AutoShortLong="Otomatik (Kısa/Uzun)"
BSSPLCPHeader="BSS PLCP Üstbilgisi"
BlueToothCollaboration="Bluetooth ile Birlikte Çalışma"
Default="Varsayılan"
Disable="Devre dışı"
Disable80211a="802.11a'yı devre dışı bırak"
Disable80211gb="802.11g/b'yi devre dışı bırak"
DisableBands="Bantları Devre Dışı Bırak"
Disabled="Devre Dışı"
Enable="Etkinleştir"
Enabled="Etkin"
FragmentationThreshold="Parçalanma Eşik Değeri"
IBSS54gtmMode="IBSS 54g Modu"
IBSS54gtmProtectionMode="IBSS 54g Koruma Modu"
IBSSChannelNumber="IBSS Kanal Numarası"
LocallyAdministeredMACAddress="Yerel Olarak Yönetilen MAC Adresi"
Long="Uzun"
None="Yok"
OptimizeBandwidth="Bant genişliğini en iyi duruma getir"
OptimizeDistance="Uzaklığı en iyi duruma getir"
PLCPHeader="PLCP Üstbilgisi"
PowerOutput="Güç Çıkışı"
PowerSaveMode="Güç Tasarruf Modu"
Prefer80211a="802.11a'yı tercih et"
Prefer80211gb="802.11g/b'yi tercih et"
RTSThreshold="RTS Eşik Değeri"
RadioEnableDisable="Sinyal Etkin/Devre Dışı"
Rate="Hız"
RoamingDecision="Dolaşım Kararı"
Usebestrate="En iyi hızı kullan"
XPress_Technology="54g+ (XPress)"
Location="Konum"
Strict="Sıkı"
Loose="Gevşek"
Fast="Hızlı"
MiminumPowerConsumption="Minimum Güç Tüketimi"
AssociationRoamPreference="İlişkili Dolaşım Tercihi"
BandPreference="Bant Tercihi"
RoamingTendency="Dolaşma Eğilimi"
Aggressive="Etkin"
Moderate="Orta"
Conservative="Tutucu"
ApCompatibilityMode="AP Uyumluluk Modu"
BroaderCompat="Daha Fazla Uyumluluk"
HigherPerf="Daha Yüksek Performans"
WME="WME"
Afterburner="MAXg (125 Mbps)"
Rate_802_11a="Hız (802.11a)"
Rate_802_11bg="Hız (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="Eski"
IBSS_Link_Indication="IBSS Bağlantı Göstergesi"
