;=============================================================================
; NetANI.INF
;
; Windows 2k/XP installation file for 
; Airgo Networks True MIMO (tm) Wireless LAN NICs
;
; Copyright 2004-2005, Airgo Networks, Inc. All rights reserved.
;
;=============================================================================


; ----------------------------------------------------------------------------
;
; Signature:
;   There are three possible values for the Signature entry: 
;
;   $Windows 95$ 
;   If the INF file is for use only on Windows 95/98, $Windows 95$ is the 
;   correct signature. An INF file that has a $Windows 95$ signature will not
;    run on Windows 2000.
;
;   $Windows NT$ 
;   If the INF file is for use only on Windows 2000, $Windows NT$ is the 
;   correct signature. An INF file that has a $Windows NT$ signature will 
;   not run on Windows 95/98.
;   
;   $Chicago$
;   If the INF file will be used on both Windows 95/98 and Windows 2000, 
;   $Chicago$ is the correct signature. A network INF file that has a 
;   $Chicago$ signature must also have the following line in the Version 
;   section:
; 
;   Compatible=1
; 
;   A network INF file that has a $Chicago$ signature will not run on Windows
;   2000 unless the Compatible entry in the Version section is set to 1.
;
; ----------------------------------------------------------------------------
[version]
Signature   = "$Chicago$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %AirgoNet%
Compatible  = 1
DriverVer   = 06/30/2005, 1.5.0.147
MillenniumPreferred = .ME
CatalogFile = AniNet.cat

; ----------------------------------------------------------------------------
[SourceDisksNames]
1= %Disk_1%,,,

[SourceDisksFiles]
WniHdd51.sys  = 1
WniHdd50.sys  = 1
wni6000.bin   = 1

; ----------------------------------------------------------------------------
;
; This defines the destination directories for all files copied via this INF.
;
;    11 is the system directory
;         %windir%\system on win9x systems
;         %windir%\system32 on winNT/2k/XP systems
;
;    12 is the drivers directory
;         %windir%\system32\drivers on winNT/2k/XP systems
;
; ----------------------------------------------------------------------------
[DestinationDirs]
DefaultDestDir                = 11  
;
Airgo_Driver.Copyfiles        = 12
Airgo_Driver.NT.5.1.Copyfiles = 12

; ----------------------------------------------------------------------------
[Manufacturer]
%Airgo%  = Airgo,NT.5.1

[ControlFlags]
ExcludeFromSelect = PCI\VEN_17CB&DEV_0001&SUBSYS_000117CB

[Airgo]
;
; Display Name         DDInstall Section   hardware id
; ------------		   -----------------   -----------

%Airgo.DeviceDesc% = Airgo.ndi, PCI\VEN_17CB&DEV_0001&SUBSYS_000117CB

[Airgo.NT.5.1]

%Airgo.DeviceDesc% = Airgo.ndi.NT.5.1, PCI\VEN_17CB&DEV_0001&SUBSYS_000117CB

; ----------------------------------------------------------------------------
;
; This is the network install section for Windows 2000/XP
;
; Characteristics:
; 
;    0x01 = NCF_VIRTUAL	
;           Specifies that the component is a virtual adapter.
;
;    0x02 = NCF_SOFTWARE_ENUMERATED 
;           Specifies that the component is a software-enumerated adapter.
;
;    0x04 = NCF_PHYSICAL 
;           Specifies that the component is a physical adapter.
;
;    0x08 = NCF_HIDDEN 
;           Specifies that the component should not be shown in any user 
;           interface
;
;    0x10 = NCF_NO_SERVICE 
;           Specifies that the component does not have an associated service 
;           (device driver).
;
;    0x20 = NCF_NOT_USER_REMOVEABLE
;           Specifies that the component cannot be removed by the user (for
;           example, through the Control Panel or Device Manager).
;
;    0x40 = NCF_MULTIPORT_INSTANCED_ADAPTER
;           Specifies that the component has multiple ports, each of which is 
;           installed as a separate device. Each port has its own hw-id 
;           (component ID) and can be individually installed. This is 
;           applicable only to EISA adapters
;
;    0x80 = NCV_HAS_UI 
;           Specifies that the component supports a user interface (for 
;           example,the Advanced Page or a custom properties sheet).
; 
;    0x400 = NCF_FILTER 
;            Specifies that the component is a filter
;
; 
; BusType:
; 
;   5 = PCI
;   8 = PCMCIA
;
; ----------------------------------------------------------------------------

; Windows 2000 specific sections ---------------------------------

[Airgo.ndi.NT]
Characteristics = 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = Airgo.NT.reg, AdvancedParms, StaticParms
CopyFiles       = Airgo_Driver.CopyFiles

[Airgo.ndi.NT.Services]
AddService      = Airgo, 2, Airgo.Service, Airgo.EventLog

[Airgo.Service]
DisplayName     = %Airgo.Service.DispName%
ServiceType     = 1 ; %SERVICE_KERNEL_DRIVER%
StartType       = 3 ; %SERVICE_DEMAND_START%
ErrorControl    = 1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\WniHdd50.sys
LoadOrderGroup  = NDIS


[Airgo.EventLog]
AddReg = Airgo.AddEventLog.reg

[Airgo.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll, %%SystemRoot%%\System32\drivers\WniHdd50.sys"
HKR, , TypesSupported,   0x00010001, 7

; Windows XP specific sections -----------------------------------

[Airgo.ndi.NT.5.1]
Characteristics = 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = Airgo.NT.reg, AdvancedParms, StaticParms
CopyFiles       = Airgo_Driver.NT.5.1.CopyFiles

[Airgo.ndi.NT.5.1.Services]
AddService      = Airgo, 2, Airgo.NT.5.1.Service, Airgo.EventLog


[Airgo.NT.5.1.Service]
DisplayName     = %Airgo.Service.DispName%
ServiceType     = 1 ; %SERVICE_KERNEL_DRIVER%
StartType       = 3 ; %SERVICE_DEMAND_START%
ErrorControl    = 1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\WniHdd51.sys
LoadOrderGroup  = NDIS

[Airgo.EventLog]
AddReg = Airgo.NT.5.1.AddEventLog.reg

[Airgo.NT.5.1.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll, %%SystemRoot%%\System32\drivers\WniHdd51.sys"
HKR, , TypesSupported,   0x00010001, 7

; Windows 2000 and Windows XP common sections --------------------

[Airgo.NT.reg]
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, DefUpper,   0, "ndis5"
HKR, Ndi\Interfaces, DefLower,   0, "ethernet"
HKR, Ndi,            Service,    0, %Airgo.Service.Name%
; HKR, ,EnumPropPages32, ,"NicProp.dll,NicPropPageProvider"


; ============================================================================
; Copyfiles sections...
; ============================================================================

[Airgo_Driver.Copyfiles]
WniHdd50.sys,,,2
wni6000.bin,,,2

[Airgo_Driver.NT.5.1.CopyFiles]
WniHdd51.sys,,,2
wni6000.bin,,,2

; ============================================================================
; Parameters on the 'Advanced' Property page
; ============================================================================
[AdvancedParms]	  

; ----------------------------------------------------------------------------
; HardwareFileName
; ----------------------------------------------------------------------------
HKR,,HardwareFileName,,"wni6000.bin"
; HKR,NDI\params\HardwareFileName, ParamDesc, 0, "HardwareFileName"
; HKR,NDI\params\HardwareFileName, type,      0, "edit"
; HKR,NDI\params\HardwareFileName, default,   0, "wni6000.bin"

; ----------------------------------------------------------------------------
; Monitor buffer size
; ----------------------------------------------------------------------------
HKR,,MonBufSize,,"2600"
; HKR,NDI\params\MonBufSize, ParamDesc, 0, "Monitor Buffer Size"
; HKR,NDI\params\MonBufSize, type,      0, "int"
; HKR,NDI\params\MonBufSize, default,   0, "2600"
; HKR,NDI\params\MonBufSize, min,       0, "128"
; HKR,NDI\params\MonBufSize, max,       0, "4096"

; ----------------------------------------------------------------------------
; Monitor buffer count
; ----------------------------------------------------------------------------
HKR,,MonBufCount,,"12"
; HKR,NDI\params\MonBufCount, ParamDesc, 0, "Monitor Buffer Count"
; HKR,NDI\params\MonBufCount, type,      0, "int"
; HKR,NDI\params\MonBufCount, default,   0, "12"
; HKR,NDI\params\MonBufCount, min,       0, "4"
; HKR,NDI\params\MonBufCount, max,       0, "1024"

; ----------------------------------------------------------------------------
; Mailbox message buffer size
; ----------------------------------------------------------------------------
HKR,,MBMsgBufSize,,"4096"
; HKR,NDI\params\MBMsgBufSize, ParamDesc, 0, "MB Msg Buffer Size"
; HKR,NDI\params\MBMsgBufSize, type,      0, "int"
; HKR,NDI\params\MBMsgBufSize, default,   0, "4096"
; HKR,NDI\params\MBMsgBufSize, min,       0, "4096"
; HKR,NDI\params\MBMsgBufSize, max,       0, "4096"

; ----------------------------------------------------------------------------
; Mailbox message buffer count
; ----------------------------------------------------------------------------
HKR,,MBMsgBufCount,,"6"
; HKR,NDI\params\MBMsgBufCount, ParamDesc, 0, "MB Msg Buffer Count"
; HKR,NDI\params\MBMsgBufCount, type,      0, "int"
; HKR,NDI\params\MBMsgBufCount, default,   0, "6"
; HKR,NDI\params\MBMsgBufCount, min,       0, "4"
; HKR,NDI\params\MBMsgBufCount, max,       0, "1024"

; ----------------------------------------------------------------------------
; Receive buffer count
; ----------------------------------------------------------------------------
HKR,,RxBufferCount,,"100"
;HKR,NDI\params\RxBufferCount, ParamDesc, 0, "Rx Buffer Count"
;HKR,NDI\params\RxBufferCount, type,      0, "dword"
;HKR,NDI\params\RxBufferCount, default,   0, "100"
;HKR,NDI\params\RxBufferCount, min,       0, "10"
;HKR,NDI\params\RxBufferCount, max,       0, "100000"
;HKR,NDI\params\RxBufferCount, step,      0, "10"

; ----------------------------------------------------------------------------
; Receive buffer size
; ----------------------------------------------------------------------------
HKR,,RxBufferSize,,"256"
; HKR,NDI\params\RxBufferSize,       ParamDesc, 0, "Rx Buffer Size"
; HKR,NDI\params\RxBufferSize,       type,      0, "enum"
; HKR,NDI\params\RxBufferSize,       default,   0, "256"
; HKR,NDI\params\RxBufferSize\enum,  "256",     0, "256 bytes"
; HKR,NDI\params\RxBufferSize\enum,  "512",     0, "512 bytes"
; HKR,NDI\params\RxBufferSize\enum, "1024",     0, "1024 bytes"
; HKR,NDI\params\RxBufferSize\enum, "2048",     0, "2048 bytes"
; HKR,NDI\params\RxBufferSize\enum, "4096",     0, "4096 bytes"

; ----------------------------------------------------------------------------
; Transmit descriptor count
; ----------------------------------------------------------------------------
HKR,,TxDescCount,,"128"
; HKR,NDI\params\TxDescCount, ParamDesc, 0, "Tx Descriptor Count"
; HKR,NDI\params\TxDescCount, type,      0, "int"
; HKR,NDI\params\TxDescCount, default,   0, "128"
; HKR,NDI\params\TxDescCount, min,       0, "10"
; HKR,NDI\params\TxDescCount, max,       0, "4096"
; HKR,NDI\params\TxDescCount, step,      0, "1"

; ----------------------------------------------------------------------------
; Receive descriptor count
; ----------------------------------------------------------------------------
HKR,,RxDescCount,,"128"
; HKR,NDI\params\RxDescCount, ParamDesc, 0, "Rx Descriptor Count"
; HKR,NDI\params\RxDescCount, type,      0, "int"
; HKR,NDI\params\RxDescCount, default,   0, "128"
; HKR,NDI\params\RxDescCount, min,       0, "10"
; HKR,NDI\params\RxDescCount, max,       0, "4096"
; HKR,NDI\params\RxDescCount, step,      0, "1"


; ----------------------------------------------------------------------------
; Network Density
; ----------------------------------------------------------------------------
HKR,,gNwDensity,,"Auto"
;HKR,NDI\params\gNwDensity,       ParamDesc, 0, "Network Density"
;HKR,NDI\params\gNwDensity,       type,      0, "enum"
;HKR,NDI\params\gNwDensity,       default,   0, "Medium"
;HKR,NDI\params\gNwDensity\enum,  "Auto",    0, "Adaptive"


; ----------------------------------------------------------------------------
; Tx Power Level
; ----------------------------------------------------------------------------
HKR,,gTxPwrLevel,,"High"
HKR,NDI\params\gTxPwrLevel,       ParamDesc, 0, "Transmit Power"
HKR,NDI\params\gTxPwrLevel,       type,      0, "enum"
HKR,NDI\params\gTxPwrLevel,       default,   0, "High"
HKR,NDI\params\gTxPwrLevel\enum,  "High",    0, "High"
HKR,NDI\params\gTxPwrLevel\enum,  "Low",     0, "Low"


; ----------------------------------------------------------------------------
; Tx Antennas
; ----------------------------------------------------------------------------
HKR,,gNumTxAntenna,,"0"
;HKR,NDI\params\gNumTxAntenna, ParamDesc, 0, "Num Tx Antennas"
;HKR,NDI\params\gNumTxAntenna, type,      0, "int"
;HKR,NDI\params\gNumTxAntenna, default,   0, "0"
;HKR,NDI\params\gNumTxAntenna, min,       0, "0"
;HKR,NDI\params\gNumTxAntenna, max,       0, "2"
;HKR,NDI\params\gNumTxAntenna, step,      0, "1"

; ----------------------------------------------------------------------------
; Rx Antennas
; ----------------------------------------------------------------------------
HKR,,gNumRxAntenna,,"0"
;HKR,NDI\params\gNumRxAntenna, ParamDesc, 0, "Num Rx Antennas"
;HKR,NDI\params\gNumRxAntenna, type,      0, "int"
;HKR,NDI\params\gNumRxAntenna, default,   0, "0"
;HKR,NDI\params\gNumRxAntenna, min,       0, "0"
;HKR,NDI\params\gNumRxAntenna, max,       0, "3"
;HKR,NDI\params\gNumRxAntenna, step,      0, "1"

; ----------------------------------------------------------------------------
; AckTimeout11A
; ----------------------------------------------------------------------------
HKR,,gAckTimeout11A,,"25"
;HKR,NDI\params\gAckTimeout11A, ParamDesc, 0, "AckTimeout11A"
;HKR,NDI\params\gAckTimeout11A, type,      0, "int"
;HKR,NDI\params\gAckTimeout11A, default,   0, "25"
;HKR,NDI\params\gAckTimeout11A, min,       0, "0"
;HKR,NDI\params\gAckTimeout11A, max,       0, "100"
;HKR,NDI\params\gAckTimeout11A, step,      0, "1"

; ----------------------------------------------------------------------------
; AckTimeout11BG
; ----------------------------------------------------------------------------
HKR,,gAckTimeout11BG,,"30"
;HKR,NDI\params\gAckTimeout11BG, ParamDesc, 0, "AckTimeout11BG"
;HKR,NDI\params\gAckTimeout11BG, type,      0, "int"
;HKR,NDI\params\gAckTimeout11BG, default,   0, "30"
;HKR,NDI\params\gAckTimeout11BG, min,       0, "0"
;HKR,NDI\params\gAckTimeout11BG, max,       0, "100"
;HKR,NDI\params\gAckTimeout11BG, step,      0, "1"


; ----------------------------------------------------------------------------
; ShortRetryLimit
; ----------------------------------------------------------------------------
HKR,,gShortRetryLimit,,"0"
HKR,NDI\params\gShortRetryLimit, ParamDesc, 0, "ShortRetryLimit"
HKR,NDI\params\gShortRetryLimit, type,      0, "int"
HKR,NDI\params\gShortRetryLimit, default,   0, "0"
HKR,NDI\params\gShortRetryLimit, min,       0, "0"
HKR,NDI\params\gShortRetryLimit, max,       0, "255"
HKR,NDI\params\gShortRetryLimit, step,      0, "1"

; ----------------------------------------------------------------------------
; LongRetryLimit
; ----------------------------------------------------------------------------
HKR,,gLongRetryLimit,,"0"
HKR,NDI\params\gLongRetryLimit, ParamDesc, 0, "LongRetryLimit"
HKR,NDI\params\gLongRetryLimit, type,      0, "int"
HKR,NDI\params\gLongRetryLimit, default,   0, "0"
HKR,NDI\params\gLongRetryLimit, min,       0, "0"
HKR,NDI\params\gLongRetryLimit, max,       0, "255"
HKR,NDI\params\gLongRetryLimit, step,      0, "1"

; ----------------------------------------------------------------------------
; Fragmentation Threshold
; ----------------------------------------------------------------------------
HKR,,gFragmentationThreshold,,"2000"
HKR,NDI\params\gFragmentationThreshold, ParamDesc, 0, "Fragmentation Threshold"
HKR,NDI\params\gFragmentationThreshold, type,      0, "int"
HKR,NDI\params\gFragmentationThreshold, default,   0, "2000"
HKR,NDI\params\gFragmentationThreshold, min,       0, "256"
HKR,NDI\params\gFragmentationThreshold, max,       0, "2346"
HKR,NDI\params\gFragmentationThreshold, step,      0, "1"

; ----------------------------------------------------------------------------
; RTS Threshold
; ----------------------------------------------------------------------------
HKR,,gRTSThreshold,,"2347"
HKR,NDI\params\gRTSThreshold, ParamDesc, 0, "RTS Threshold"
HKR,NDI\params\gRTSThreshold, type,      0, "int"
HKR,NDI\params\gRTSThreshold, default,   0, "2347"
HKR,NDI\params\gRTSThreshold, min,       0, "0"
HKR,NDI\params\gRTSThreshold, max,       0, "2347"
HKR,NDI\params\gRTSThreshold, step,      0, "1"

; ----------------------------------------------------------------------------
; Max Ack Rate (11A)
; ----------------------------------------------------------------------------
HKR,,gMaxAckRate11A,,"5"
;HKR,NDI\params\gMaxAckRate11A, ParamDesc, 0, "Max Ack Rate (11A)"
;HKR,NDI\params\gMaxAckRate11A, type,      0, "int"
;HKR,NDI\params\gMaxAckRate11A, default,   0, "5"
;HKR,NDI\params\gMaxAckRate11A, min,       0, "1"
;HKR,NDI\params\gMaxAckRate11A, max,       0, "108"
;HKR,NDI\params\gMaxAckRate11A, step,      0, "1"

; ----------------------------------------------------------------------------
; Max Ack Rate (11B)
; ----------------------------------------------------------------------------
HKR,,gMaxAckRate11B,,"22"
;HKR,NDI\params\gMaxAckRate11B, ParamDesc, 0, "Max Ack Rate (11B)"
;HKR,NDI\params\gMaxAckRate11B, type,      0, "int"
;HKR,NDI\params\gMaxAckRate11B, default,   0, "22"
;HKR,NDI\params\gMaxAckRate11B, min,       0, "2"
;HKR,NDI\params\gMaxAckRate11B, max,       0, "22"
;HKR,NDI\params\gMaxAckRate11B, step,      0, "1"

; ----------------------------------------------------------------------------
; Calibration On / Off
; ----------------------------------------------------------------------------
HKR,,gCalibration,,"1"
;HKR,NDI\params\gCalibration,       ParamDesc, 0, "Calibration (on/off)"
;HKR,NDI\params\gCalibration,       type,      0, "enum"
;HKR,NDI\params\gCalibration,       default,   0, "1"
;HKR,NDI\params\gCalibration\enum,  "0",       0, "OFF"
;HKR,NDI\params\gCalibration\enum,  "1",       0, "ON"

; ----------------------------------------------------------------------------
; Calibration period
; ----------------------------------------------------------------------------
HKR,,gCalibrationPeriod,,"5"
;HKR,NDI\params\gCalibrationPeriod,       ParamDesc, 0, "Calibration period (minutes)"
;HKR,NDI\params\gCalibrationPeriod,       type,      0, "int"
;HKR,NDI\params\gCalibrationPeriod,       default,   0, "5"
;HKR,NDI\params\gCalibrationPeriod,       min,       0, "2"
;HKR,NDI\params\gCalibrationPeriod,       max,       0, "10"
;HKR,NDI\params\gCalibrationPeriod,       step,      0, "1"

; ----------------------------------------------------------------------------
; Background scan period
; ----------------------------------------------------------------------------
HKR,,gBgScanPeriod,,"5000"
HKR,NDI\params\gBgScanPeriod,       ParamDesc, 0, "Background Scan period (milliseconds)"
HKR,NDI\params\gBgScanPeriod,       type,      0, "dword"
HKR,NDI\params\gBgScanPeriod,       default,   0, "5000"
HKR,NDI\params\gBgScanPeriod,       min,       0, "0"
HKR,NDI\params\gBgScanPeriod,       max,       0, "180000"
HKR,NDI\params\gBgScanPeriod,       step,      0, "1"

; ----------------------------------------------------------------------------
; Background scan minimum channel time
; ----------------------------------------------------------------------------
HKR,,gBgScanMinChannelTime,,"20"
;HKR,NDI\params\gBgScanMinChannelTime,       ParamDesc, 0, "Background Min Channel Time (milliseconds)"
;HKR,NDI\params\gBgScanMinChannelTime,       type,      0, "dword"
;HKR,NDI\params\gBgScanMinChannelTime,       default,   0, "20"
;HKR,NDI\params\gBgScanMinChannelTime,       min,       0, "1"
;HKR,NDI\params\gBgScanMinChannelTime,       max,       0, "65535"
;HKR,NDI\params\gBgScanMinChannelTime,       step,      0, "1"

; ----------------------------------------------------------------------------
; Background scan maximum channel time
; ----------------------------------------------------------------------------
HKR,,gBgScanMaxChannelTime,,"40"
;HKR,NDI\params\gBgScanMaxChannelTime,       ParamDesc, 0, "Background Max Channel Time (milliseconds)"
;HKR,NDI\params\gBgScanMaxChannelTime,       type,      0, "dword"
;HKR,NDI\params\gBgScanMaxChannelTime,       default,   0, "40"
;HKR,NDI\params\gBgScanMaxChannelTime,       min,       0, "1"
;HKR,NDI\params\gBgScanMaxChannelTime,       max,       0, "65535"
;HKR,NDI\params\gBgScanMaxChannelTime,       step,      0, "1"


; ----------------------------------------------------------------------------
; CCA Mode
; ----------------------------------------------------------------------------
HKR,,gCCAMode,,"7"
;HKR,NDI\params\gCCAMode,       ParamDesc, 0, "CCA Mode"
;HKR,NDI\params\gCCAMode,       type,      0, "enum"
;HKR,NDI\params\gCCAMode,       default,   0, "7"
;HKR,NDI\params\gCCAMode\enum,  "0",       0, "None"
;HKR,NDI\params\gCCAMode\enum,  "1",	      0, "ED"
;HKR,NDI\params\gCCAMode\enum,  "2",       0, "CD"
;HKR,NDI\params\gCCAMode\enum,  "3",       0, "CD and CS"
;HKR,NDI\params\gCCAMode\enum,  "4",       0, "ED and CD"
;HKR,NDI\params\gCCAMode\enum,  "5",       0, "ED or CD"
;HKR,NDI\params\gCCAMode\enum,  "6",       0, "ED and CS and CD"
;HKR,NDI\params\gCCAMode\enum,  "7",       0, "ED or CS and CD"
								

; ----------------------------------------------------------------------------
; ED Threshold
; ----------------------------------------------------------------------------
HKR,,gEDThreshold,,"60"
;HKR,NDI\params\gEDThreshold,       ParamDesc,          0, "ED Threshold"
;HKR,NDI\params\gEDThreshold,       type,               0, "dword"
;HKR,NDI\params\gEDThreshold,       default,            0, "60"
;HKR,NDI\params\gEDThreshold,       min,                0, "0"
;HKR,NDI\params\gEDThreshold,       max,                0, "114"
;HKR,NDI\params\gEDThreshold,       step,               0, "1"

; ----------------------------------------------------------------------------
; ACK Policy
; ----------------------------------------------------------------------------
HKR,,gAckPolicy,,"0"
HKR,NDI\params\gAckPolicy,       ParamDesc, 0, "Ack Policy"
HKR,NDI\params\gAckPolicy,       type,      0, "enum"
HKR,NDI\params\gAckPolicy,       default,   0, "0"
HKR,NDI\params\gAckPolicy\enum,  "0",       0, "Immediate"
;HKR,NDI\params\gAckPolicy\enum,  "1",       0, "No Ack"
;HKR,NDI\params\gAckPolicy\enum,  "2",       0, "Automatic"
HKR,NDI\params\gAckPolicy\enum,  "3",       0, "Burst"

; ----------------------------------------------------------------------------
; 802.11 Mode
; ----------------------------------------------------------------------------
HKR,,gDot11Mode,,"0"
HKR,NDI\params\gDot11Mode,       ParamDesc, 0, "802.11 Mode"
HKR,NDI\params\gDot11Mode,       type,      0, "enum"
HKR,NDI\params\gDot11Mode,       default,   0, "0"
HKR,NDI\params\gDot11Mode\enum,  "0",       0, "All"
HKR,NDI\params\gDot11Mode\enum,  "1",	    0, "802.11a"
HKR,NDI\params\gDot11Mode\enum,  "2",       0, "802.11b"
HKR,NDI\params\gDot11Mode\enum,  "3",       0, "802.11g"

; ----------------------------------------------------------------------------
; Enhanced Rates
; ----------------------------------------------------------------------------
HKR,,gEnhancedRatesEnabled,,"1"
HKR,NDI\params\gEnhancedRatesEnabled,   	ParamDesc, 0, "Enhanced Rates"
HKR,NDI\params\gEnhancedRatesEnabled,       type,      0, "enum"
HKR,NDI\params\gEnhancedRatesEnabled,       default,   0, "1"
HKR,NDI\params\gEnhancedRatesEnabled\enum,  "0",       0, "Off"
HKR,NDI\params\gEnhancedRatesEnabled\enum,  "1",       0, "On"

; ----------------------------------------------------------------------------
; Power Save Mode
; ----------------------------------------------------------------------------
HKR,,gPowerUsage,,"5"
HKR,NDI\params\gPowerUsage,   				ParamDesc, 0, "Power Save Mode"
HKR,NDI\params\gPowerUsage,       			type,      0, "enum"
HKR,NDI\params\gPowerUsage,       			default,   0, "5"
HKR,NDI\params\gPowerUsage\enum,  			"1",       0, "Maximum"
HKR,NDI\params\gPowerUsage\enum,  			"5",       0, "Off"

; ----------------------------------------------------------------------------
; Generic CFG settings
; ----------------------------------------------------------------------------
HKR,,gCfg1Id,,"0"
;HKR,NDI\params\gCfg1Id,       ParamDesc,    0, "Generic Cfg 1 Id (decimal; 0 == N/A)"
;HKR,NDI\params\gCfg1Id,       type,         0, "dword"
;HKR,NDI\params\gCfg1Id,       default,      0, "0"

HKR,,gCfg1Value,,"0"
;HKR,NDI\params\gCfg1Value,    ParamDesc,    0, "Generic Cfg 1 Value (decimal)"
;HKR,NDI\params\gCfg1Value,    type,         0, "dword"
;HKR,NDI\params\gCfg1Value,    default,      0, "0"

HKR,,gCfg2Id,,"0"
;HKR,NDI\params\gCfg2Id,       ParamDesc,    0, "Generic Cfg 2 Id (decimal; 0 == N/A)"
;HKR,NDI\params\gCfg2Id,       type,         0, "dword"
;HKR,NDI\params\gCfg2Id,       default,      0, "0"

HKR,,gCfg2Value,,"0"
;HKR,NDI\params\gCfg2Value,    ParamDesc,    0, "Generic Cfg 2 Value (decimal)"
;HKR,NDI\params\gCfg2Value,    type,         0, "dword"
;HKR,NDI\params\gCfg2Value,    default,      0, "0"

HKR,,gCfg3Id,,"0"
;HKR,NDI\params\gCfg3Id,       ParamDesc,    0, "Generic Cfg 3 Id (decimal; 0 == N/A)"
;HKR,NDI\params\gCfg3Id,       type,         0, "dword"
;HKR,NDI\params\gCfg3Id,       default,      0, "0"

HKR,,gCfg3Value,,"0"
;HKR,NDI\params\gCfg3Value,    ParamDesc,    0, "Generic Cfg 3 Value (decimal)"
;HKR,NDI\params\gCfg3Value,    type,         0, "dword"
;HKR,NDI\params\gCfg3Value,    default,      0, "0"

HKR,,gCfg4Id,,"0"
;HKR,NDI\params\gCfg4Id,       ParamDesc,    0, "Generic Cfg 4 Id (decimal; 0 == N/A)"
;HKR,NDI\params\gCfg4Id,       type,         0, "dword"
;HKR,NDI\params\gCfg4Id,       default,      0, "0"

HKR,,gCfg4Value,,"0"
;HKR,NDI\params\gCfg4Value,    ParamDesc,    0, "Generic Cfg 4 Value (decimal)"
;HKR,NDI\params\gCfg4Value,    type,         0, "dword"
;HKR,NDI\params\gCfg4Value,    default,      0, "0"

HKR,,gCfg5Id,,"0"
;HKR,NDI\params\gCfg5Id,       ParamDesc,    0, "Generic Cfg 5 Id (decimal; 0 == N/A)"
;HKR,NDI\params\gCfg5Id,       type,         0, "dword"
;HKR,NDI\params\gCfg5Id,       default,      0, "0"

HKR,,gCfg5Value,,"0"
;HKR,NDI\params\gCfg5Value,    ParamDesc,    0, "Generic Cfg 5 Value (decimal)"
;HKR,NDI\params\gCfg5Value,    type,         0, "dword"
;HKR,NDI\params\gCfg5Value,    default,      0, "0"


; ----------------------------------------------------------------------------
; Short Slot Time Enabled
; ----------------------------------------------------------------------------
HKR,,gShortSlotTimeEnabled,,"1"
;HKR,NDI\params\gShortSlotTimeEnabled,       ParamDesc,          0, ".11g Short Slot Time"
;HKR,NDI\params\gShortSlotTimeEnabled,       type,               0, "dword"
;HKR,NDI\params\gShortSlotTimeEnabled,       default,            0, "1"
;HKR,NDI\params\gShortSlotTimeEnabled,       min,                0, "0"
;HKR,NDI\params\gShortSlotTimeEnabled,       max,                0, "1"
;HKR,NDI\params\gShortSlotTimeEnabled,       step,               0, "1"

; ----------------------------------------------------------------------------
; 11d Support Enabled
; ----------------------------------------------------------------------------
HKR,,g11dSupportEnabled,,"1"
HKR,NDI\params\g11dSupportEnabled,       ParamDesc, 0, "802.11d Support"
HKR,NDI\params\g11dSupportEnabled,       type,      0, "enum"
HKR,NDI\params\g11dSupportEnabled,       default,   0, "1"
HKR,NDI\params\g11dSupportEnabled\enum,  "0",       0, "Off"
HKR,NDI\params\g11dSupportEnabled\enum,  "1",       0, "On"

; ----------------------------------------------------------------------------
; 11h Support Enabled
; ----------------------------------------------------------------------------
HKR,,g11hSupportEnabled,,"1"
HKR,NDI\params\g11hSupportEnabled,       ParamDesc, 0, "802.11h Support"
HKR,NDI\params\g11hSupportEnabled,       type,      0, "enum"
HKR,NDI\params\g11hSupportEnabled,       default,   0, "1"
HKR,NDI\params\g11hSupportEnabled\enum,  "0",       0, "Off"
HKR,NDI\params\g11hSupportEnabled\enum,  "1",       0, "On"

; ----------------------------------------------------------------------------
; WMM Support
; ----------------------------------------------------------------------------
HKR,,gWMMSupportEnabled,,"0"
HKR,NDI\params\gWMMSupportEnabled,       ParamDesc, 0, "Wi-Fi Multimedia (WMM) Support"
HKR,NDI\params\gWMMSupportEnabled,       type,      0, "enum"
HKR,NDI\params\gWMMSupportEnabled,       default,   0, "1"
HKR,NDI\params\gWMMSupportEnabled\enum,  "0",       0, "Off"
HKR,NDI\params\gWMMSupportEnabled\enum,  "1",       0, "On"

; ----------------------------------------------------------------------------
; DSCP or 802.1P Support   -- ww 4-08-05
; ----------------------------------------------------------------------------
HKR,,gDscpOr8021p,,"0"
HKR,NDI\params\gDscpOr8021p,       ParamDesc, 0, "Priority: DSCP or 802.1P"
HKR,NDI\params\gDscpOr8021p,       type,      0, "enum"
HKR,NDI\params\gDscpOr8021p,       default,   0, "1"
HKR,NDI\params\gDscpOr8021p\enum,  "0",       0, "Off"
HKR,NDI\params\gDscpOr8021p\enum,  "1",       0, "802.1P"
HKR,NDI\params\gDscpOr8021p\enum,  "2",       0, "DSCP"

; ----------------------------------------------------------------------------
; 11e Support Enabled
; ----------------------------------------------------------------------------
HKR,,g11eSupportEnabled,,"1"
HKR,NDI\params\g11eSupportEnabled,       ParamDesc, 0, "802.11e Support"
HKR,NDI\params\g11eSupportEnabled,       type,      0, "enum"
HKR,NDI\params\g11eSupportEnabled,       default,   0, "1"
HKR,NDI\params\g11eSupportEnabled\enum,  "0",       0, "Off"
HKR,NDI\params\g11eSupportEnabled\enum,  "1",       0, "eDCA"

; ----------------------------------------------------------------------------
; Heartbeat Threshold (2.4 GHz)
; ----------------------------------------------------------------------------
HKR,,gHeartbeat24,,"10"
;HKR,NDI\params\gHeartbeat24,       ParamDesc,          0, "Heartbeat Thresh (2.4)"
;HKR,NDI\params\gHeartbeat24,       type,               0, "dword"
;HKR,NDI\params\gHeartbeat24,       default,            0, "10"
;HKR,NDI\params\gHeartbeat24,       min,                0, "1"
;HKR,NDI\params\gHeartbeat24,       max,                0, "50"
;HKR,NDI\params\gHeartbeat24,       step,               0, "1"

; ----------------------------------------------------------------------------
; Heartbeat Threshold (5.0 GHz)
; ----------------------------------------------------------------------------
HKR,,gHeartbeat50,,"6"
;HKR,NDI\params\gHeartbeat50,       ParamDesc,          0, "Heartbeat Thresh (5.0)"
;HKR,NDI\params\gHeartbeat50,       type,               0, "dword"
;HKR,NDI\params\gHeartbeat50,       default,            0, "6"
;HKR,NDI\params\gHeartbeat50,       min,                0, "1"
;HKR,NDI\params\gHeartbeat50,       max,                0, "50"
;HKR,NDI\params\gHeartbeat50,       step,               0, "1"


; ----------------------------------------------------------------------------
; Scan Results Aging Time
; ----------------------------------------------------------------------------
HKR,,gAgingTimerInBKScanUnits,,"3"
;HKR,NDI\params\gAgingTimerInBKScanUnits,       ParamDesc,          0, "Scan Results Age"
;HKR,NDI\params\gAgingTimerInBKScanUnits,       type,               0, "dword"
;HKR,NDI\params\gAgingTimerInBKScanUnits,       default,            0, "3"
;HKR,NDI\params\gAgingTimerInBKScanUnits,       min,                0, "2"
;HKR,NDI\params\gAgingTimerInBKScanUnits,       max,                0, "10"
;HKR,NDI\params\gAgingTimerInBKScanUnits,       step,               0, "1"


; ----------------------------------------------------------------------------
; Country Code override
; ----------------------------------------------------------------------------
HKR,,gCountryCode,,"AGN"
; HKR,NDI\params\gCountryCode,       ParamDesc, 0, "Country Override"
; HKR,NDI\params\gCountryCode,       type,      0, "enum"
; HKR,NDI\params\gCountryCode,       default,   0, "AGN"
; HKR,NDI\params\gCountryCode\enum,  "AGN",     0, "None"
; HKR,NDI\params\gCountryCode\enum,  "USI",     0, "United States"
; HKR,NDI\params\gCountryCode\enum,  "JPI",     0, "Japan"

; ----------------------------------------------------------------------------
; Fixed Rate setting
; ----------------------------------------------------------------------------
HKR,,gFixedRate,,"0"
HKR,NDI\params\gFixedRate,       ParamDesc, 0, "Transmit Rate"
HKR,NDI\params\gFixedRate,       type,      0, "enum"
HKR,NDI\params\gFixedRate,       default,   0, "0"
HKR,NDI\params\gFixedRate\enum,  "0",       0, "Adaptive"
HKR,NDI\params\gFixedRate\enum,  "1",       0, "  1.0 Mbps"
HKR,NDI\params\gFixedRate\enum,  "2",       0, "  2.0 Mbps"
HKR,NDI\params\gFixedRate\enum,  "4",       0, "  5.5 Mbps"
HKR,NDI\params\gFixedRate\enum,  "8",       0, "  6.0 Mbps"
HKR,NDI\params\gFixedRate\enum,  "16",      0, "  9.0 Mbps"
HKR,NDI\params\gFixedRate\enum,  "32",      0, " 11.0 Mbps"
HKR,NDI\params\gFixedRate\enum,  "64",      0, " 12.0 Mbps"
HKR,NDI\params\gFixedRate\enum,  "128",     0, " 18.0 Mbps"
HKR,NDI\params\gFixedRate\enum,  "256",     0, " 24.0 Mbps"
HKR,NDI\params\gFixedRate\enum,  "512",     0, " 36.0 Mbps"
HKR,NDI\params\gFixedRate\enum,  "1024",    0, " 48.0 Mbps"
HKR,NDI\params\gFixedRate\enum,  "2048",    0, " 54.0 Mbps"
HKR,NDI\params\gFixedRate\enum,  "4096",    0, " 72.0 Mbps"
HKR,NDI\params\gFixedRate\enum,  "8192",    0, " 96.0 Mbps"
HKR,NDI\params\gFixedRate\enum,  "16384",   0, "108.0 Mbps"


; ----------------------------------------------------------------------------
; ----------------------------------------------------------------------------
; Static parameters (these do not show on the property page)
; ----------------------------------------------------------------------------
; ----------------------------------------------------------------------------
[StaticParms]
; HardwareID
HKR, ,HardwareID, ,"WNI0000"

; ----------------------------------------------------------------------------
; Roaming Features
; ----------------------------------------------------------------------------
HKR,,RoamingFeatures,,"3"

; ----------------------------------------------------------------------------
; Roaming Feature:  Signal Degraded parameters
; ----------------------------------------------------------------------------
HKR,,RoamingSignalDegradedThresh,,"30"
HKR,,RoamingSignalDegradedBeaconsPerPeriod,,"10"
HKR,,RoamingSignalDegradedPeriods,,"10"
HKR,,RoamingSignalDegradedNewRssiThreshold,,"27"
HKR,,RoamingScanOnSignalDegradation,,"0"


; HKR, ,MBMsgBufSize,  0, "256"
; HKR, ,MBSMsgCount,   0,  "10"
; HKR, ,RxBufferCount, 0, "100"
; HKR, ,RxBufferSize,  0, "256"


;----------------------------------------------------------------------------
; Replaceable strings
;----------------------------------------------------------------------------
[Strings]
Airgo                    = "Airgo"
AirgoNet                 = "Airgo Networks, Inc."
Disk_1                   = "Driver Installation Disk"
Airgo.Service.DispName   = "Airgo Networks True MIMO (tm) Wireless Driver"
Airgo.Service.Name       = "Airgo"

Airgo.DeviceDesc = "Airgo Networks True MIMO (tm) Wireless Adapter" 
