;; NETDLKR5.INF (Win2K, WinXP & Win98 combined inf for NDIS5 driver)
;;
;;  D-Link DFE-530TX+ PCI Adapter
;;
;; Copyright 2001-2002, D-Link Corporation. All Rights Reserved.
;;
;; .this release is primarily for motherboard OEM for WHQL test.

[version]
Signature      = "$Chicago$"
Compatible     = 1
Class          = Net
ClassGUID      = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider       = %D-Link%                             ;;
CatalogFile    = NETDLKR5.CAT                               ;; for WHQL certified
CatalogFile.NT = NETDLKRN.CAT
DriverVer      = 08/23/2001,5.397.0823.2001

[Manufacturer]
%D-Link%   = D-Link

[ControlFlags]
;;ExcludeFromSelect     = PCI\VEN_1186&DEV_1300
;;ExcludeFromSelect     = PCI\VEN_1186&DEV_1300&SUBSYS_13011186                 
;;ExcludeFromSelect     = PCI\VEN_10EC&DEV_8139

[D-Link]
%DFE530.DeviceDesc%  = DFE530.ndi, PCI\VEN_1186&DEV_1300
%DFE530_A.DeviceDesc%  = DFE530_A.ndi, PCI\VEN_1186&DEV_1300&SUBSYS_13011186
%DFE530_A.DeviceDesc%  = DFE530_A.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_13011186

;;****************************************************************************
;; Windows 9x
;;****************************************************************************
[DFE530.ndi]
DriverVer       = 08/23/2001,397
AddReg          = DFE530.id.reg, DFE530.common.reg, DFE530.win.reg, DFE530.oncbs.reg
CopyFiles       = DFE530.CopyFiles98
;DeviceID        = "PCI\VEN_1186&DEV_1300"
;LogConfig       = DefaultConfig

[DFE530_A.ndi]
DriverVer       = 08/23/2001,397
AddReg          = DFE530.id.reg, DFE530.common.reg, DFE530.win.reg, DFE530.oncbs.reg
CopyFiles       = DFE530.CopyFiles98
;DeviceID        = "PCI\VEN_1186&DEV_1300&SUBSYS_13011186"
;LogConfig       = DefaultConfig

;;****************************************************************************
;; Win2K, WinXP
;;****************************************************************************
[DFE530.ndi.NT]
AddReg          = DFE530.common.reg, DFE530.reg, DFE530.oncbs.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = DFE530.CopyFiles

[DFE530.ndi.NT.Services]
AddService = DLKRTS, 2, rtsnt.Service, DFE530.EventLog

[DFE530_A.ndi.NT]
AddReg          = DFE530.common.reg, DFE530.reg, DFE530.oncbs.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = DFE530.CopyFiles

[DFE530_A.ndi.NT.Services]
AddService = DLKRTS, 2, rtsnt.Service, DFE530.EventLog

[DFE530.CopyFiles]
DLKRTS.SYS,,,2

[DFE530.CopyFiles98]
DLKRTS.SYS,,,2

;;----------------------------------------------------------------------------
;; DFE-530TX+ Parameters
;;----------------------------------------------------------------------------
;;***************************************************************************
;; Windows 9x parameters
;;***************************************************************************
[DFE530.id.reg]
HKR, Ndi,       DeviceID,       0,      "PCI\VEN_1186&DEV_1300"

HKR, Ndi\Install,                       ,       0,      rtsnt.install
HKR, NDI\Params\DuplexMode,             flag,   1,      30, 00, 00, 00
HKR, Ndi\Params\EarlyTxThreshold,       flag,   1,      20, 00, 00, 00
HKR, NDI\Params\NetworkAddress,         flag,   1,      30, 00, 00, 00
HKR, NDI\Params\WakeUpFrame,            flag,   1,      30, 00, 00, 00

[DFE530.win.reg]
;; key,subkey,valuname,type,value
HKR, ,  DriverDesc,     0,      "D-Link DFE-530TX+ PCI Adapter"
HKR, ,  DevLoader,      0,      *ndis
HKR, ,  DeviceVxDs,     0,      DLKRTS.SYS
HKR, ,  EnumPropPages,  0,      netdi.dll,      EnumPropPages

;;params
HKR, ,  MediaType,      0,      1
HKR, ,  AdapterType,    0,      5
HKR, ,  BusType,        0,      5

;; NDIS Info
HKR, NDIS,              MajorNdisVersion,       1,      03
HKR, NDIS,              MinorNdisVersion,       1,      0a
HKR, NDIS,              LogDriverName,          0,      "DLKRTS"

;; Interfaces
HKR, Ndi\Interfaces,    DefLower,               ,       "ethernet"
HKR, Ndi\Interfaces,    LowerRange,             ,       "ethernet"
HKR, Ndi\Interfaces,    DefUpper,               ,       "ndis3"
HKR, Ndi\Interfaces,    UpperRange,             ,       "ndis3"

;; Install sections
HKR, Ndi\Install,       ndis3,                  0,      "DFE530.ndis5"

;;****************************************************************************
;; DFE-530TX+ common parameters
;;****************************************************************************
[DFE530.oncbs.reg]
HKR,,ChipOnCardbus,,"0"

[DFE530.common.reg]
HKR, Ndi\params\DuplexMode,      ParamDesc, 0, %DuplexMode%
HKR, Ndi\params\DuplexMode,      type,      0, "enum"
HKR, Ndi\params\DuplexMode,      default,   0, "1"
HKR, Ndi\params\DuplexMode\enum, 1,         0, %dmAutoMode%
HKR, Ndi\params\DuplexMode\enum, 2,         0, %dm10HalfMode%
HKR, Ndi\params\DuplexMode\enum, 3,         0, %dm10FullMode%
HKR, Ndi\params\DuplexMode\enum, 4,         0, %dm100HalfMode%
HKR, Ndi\params\DuplexMode\enum, 5,         0, %dm100FullMode%

HKR,Ndi\Params\EarlyTxThreshold, ParamDesc, 0, %EarlyTxThreshold%
HKR,Ndi\Params\EarlyTxThreshold, Type,      0, "int"
HKR,Ndi\Params\EarlyTxThreshold, Default,   0, "15"
HKR,Ndi\Params\EarlyTxThreshold, Min,       0, "0"
HKR,Ndi\Params\EarlyTxThreshold, Max,       0, "63"
HKR,Ndi\Params\EarlyTxThreshold, Step,      0, "1"
HKR,Ndi\Params\EarlyTxThreshold, Base,      0, "10"

HKR,Ndi\params\NetworkAddress,   ParamDesc, 0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,   type,      0, "edit"
HKR,Ndi\params\NetworkAddress,   default,   0, "000000000000"
HKR,Ndi\params\NetworkAddress,   LimitText, 0, "12"
HKR,Ndi\params\NetworkAddress,   UpperCase, 0, "1"
HKR,Ndi\params\NetworkAddress,   Optional,  0, "1"

;HKR,NDI\Params\TxMaxDMABurst,flag,1,30,00,00,00
;HKR,Ndi\params\TxMaxDMABurst,ParamDesc,0,"Transmit DMA burst size"
;HKR,Ndi\params\TxMaxDMABurst,type,0,enum
;HKR,Ndi\params\TxMaxDMABurst,default,0,6
;HKR,Ndi\params\TxMaxDMABurst\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,7,0,"7:2048 bytes"

;HKR,NDI\Params\RxMaxDMABurst,flag,1,30,00,00,00
;HKR,Ndi\params\RxMaxDMABurst,ParamDesc,0,"Receive DMA burst size"
;HKR,Ndi\params\RxMaxDMABurst,type,0,enum
;HKR,Ndi\params\RxMaxDMABurst,default,0,6
;HKR,Ndi\params\RxMaxDMABurst\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,7,0,"7:unlimitted"

;HKR,NDI\Params\EarlyRxThreshold,flag,1,30,00,00,00
;HKR,Ndi\params\EarlyRxThreshold,ParamDesc,0,"Receive FIFO threshold"
;HKR,Ndi\params\EarlyRxThreshold,type,0,enum
;HKR,Ndi\params\EarlyRxThreshold,default,0,2
;HKR,Ndi\params\EarlyRxThreshold\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,7,0,"7:No threshold"

;HKR,NDI\Params\TxInterFrameGap,flag,1,30,00,00,00
;HKR,Ndi\params\TxInterFrameGap,ParamDesc,0,"Tx IFG(10M/100M)"
;HKR,Ndi\params\TxInterFrameGap,type,0,enum
;HKR,Ndi\params\TxInterFrameGap,default,0,3
;HKR,Ndi\params\TxInterFrameGap\enum,0,0,"8.4us/840ns"
;HKR,Ndi\params\TxInterFrameGap\enum,1,0,"8.8us/880ns"
;HKR,Ndi\params\TxInterFrameGap\enum,2,0,"9.2us/920ns"
;HKR,Ndi\params\TxInterFrameGap\enum,3,0,"9.6us/960ns"

;HKR, Ndi\params\WakeOnLan,         ParamDesc,  0, "Smart Power Saving"
;HKR, Ndi\params\WakeOnLan,         default,    0, "0"  
;HKR, Ndi\params\WakeOnLan,         type,       0, "enum"
;HKR, Ndi\params\WakeOnLan\enum,    "0",        0, "Disable"
;HKR, Ndi\params\WakeOnLan\enum,    "1",        0, "Enable (No WakeUp)"

HKR,Ndi\params\RxBufLen,	   ParamDesc,  0, "Receive Buffer Size"
HKR,Ndi\params\RxBufLen,	   type,       0, "enum"
HKR,Ndi\params\RxBufLen,	   default,    0, "3"
HKR,Ndi\params\RxBufLen\enum,	   "0",	       0, "8K bytes"
HKR,Ndi\params\RxBufLen\enum,	   "1",	       0, "16K bytes"
HKR,Ndi\params\RxBufLen\enum,	   "2",	       0, "32K bytes"
HKR,Ndi\params\RxBufLen\enum,	   "3",	       0, "64K bytes"

HKR, Ndi\params\LinkUp,            ParamDesc,  0, "WakeUp on Link Change"
HKR, Ndi\params\LinkUp,            default,    0, "0"
HKR, Ndi\params\LinkUp,            type,       0, "enum"
HKR, Ndi\params\LinkUp\enum,       "1",        0, "Enable"
HKR, Ndi\params\LinkUp\enum,       "0",        0, "Disable"

HKR, Ndi\params\WakeUpFrame,       ParamDesc,  0, "WakeUp on ARP/PING"
HKR, Ndi\params\WakeUpFrame,       default,    0, "0"
HKR, Ndi\params\WakeUpFrame,       type,       0, "enum"
HKR, Ndi\params\WakeUpFrame\enum,  "0",        0, "Enable"
HKR, Ndi\params\WakeUpFrame\enum,  "1",        0, "Disable"

HKR, Ndi\params\PME,               ParamDesc,  0, "WakeUp using APM Mode"
HKR, Ndi\params\PME,               default,    0, "1"
HKR, Ndi\params\PME,               type,       0, "enum"
HKR, Ndi\params\PME\enum,          "0",        0, "Enable"
HKR, Ndi\params\PME\enum,          "1",        0, "Disable"

HKR, Ndi\params\EnableLDPS,        ParamDesc,  0, "Link Down Power Saving"
HKR, Ndi\params\EnableLDPS,        default,    0, "0"
HKR, Ndi\params\EnableLDPS,        type,       0, "enum"
HKR, Ndi\params\EnableLDPS\enum,   "0",        0, "Disable"
HKR, Ndi\params\EnableLDPS\enum,   "1",        0, "Enable"


;;****************************************************************************
;; Win2K, WinXP parameters
;;****************************************************************************
[DFE530.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "DLKRTS"

[rtsnt.Service]
DisplayName     = %DFE530.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\DLKRTS.SYS
LoadOrderGroup  = NDIS

[DFE530.EventLog]
Addreg = DFE530.AddEventLog.reg

[DFE530.AddEventLog.reg]
HKR,    ,   EventMessageFile,   0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR,    ,   TypesSupported,     0x00010001, 7

;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
DFE530.CopyFiles           = 12
DFE530.CopyFiles98         = 11
DefaultDestDir              = 11        ; LDID_SYS

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
DLKRTS.SYS  = 1
DLKRTS.SYS  = 1              ;;Windows 2K,XP 
;NETDLKR5.INF  = 1
;NETDLKR5.INF  = 1             ;;Windows 2K,XP
;NETDLKR5.CAT  = 1
;NETDLKRN.CAT  = 1

;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
;Msft                      = "D-Link Corporation."
D-Link                   = "D-Link Corporation."

;;Source disk name
DISKNAME = "D-Link DFE-530TX+ PCI Adapter Driver Disk"

NetworkAddress            = "Network Address"
EarlyTxThreshold          = "Early Tx Threshold"
DuplexMode                = "Link Speed/Duplex Mode"
dmAutoMode                = "Auto Mode"
dm10HalfMode              = "10 Half Mode"
dm10FullMode              = "10 Full Mode"
dm100HalfMode             = "100 Half Mode"
dm100FullMode             = "100 Full Mode"

DFE530.DeviceDesc        = "D-Link DFE-530TX+ PCI Adapter"
DFE530.Service.DispName  = "D-Link DFE-530TX+ PCI Adapter"
DFE530_A.DeviceDesc      = "D-Link DFE-530TX+ PCI Adapter"
