;
; Sierra Wireless AirCard GPRS/EDGE NIC + Modem PC Card Setup File
; Copyright (c) 1993-2004 Sierra Wireless Inc.
; Manufacturer: Sierra Wireless Inc.
;****************************************************************************
;Ver 2.0.0.4
;Windows 98/Me/2K/XP
;Ndis5
;****************************************************************************


[Version]
Signature    = "$Chicago$"
Provider     = %SWI%
Class        = MultiFunction
ClassGUID    = {4d36e971-e325-11ce-bfc1-08002be10318}
DriverVer    = 05/05/2004,2.0.0.4
CatalogFile  = mfacgprs.cat

[Manufacturer]
%SWI% = SWIModels

[ControlFlags]
ExcludeFromSelect = PCMCIA\Sierra_Wireless-AC710/AC750-B00E
ExcludeFromSelect = PCMCIA\PC7000-GPRS_Network_Adapter-64AB
ExcludeFromSelect = PCMCIA\Sierra_Wireless-AC775-F092
ExcludeFromSelect = PCMCIA\PC7200-EDGE_Network_Adapter-F401

ExcludeFromSelect.nt = PCMCIA\Sierra_Wireless-AC710/AC750-B00E
ExcludeFromSelect.nt = PCMCIA\PC7000-GPRS_Network_Adapter-64AB
ExcludeFromSelect.nt = PCMCIA\Sierra_Wireless-AC775-F092
ExcludeFromSelect.nt = PCMCIA\PC7200-EDGE_Network_Adapter-F401

[SWIModels]
%SWI_Parent% = SWIACGPRS, PCMCIA\Sierra_Wireless-AC710/AC750-B00E
%SWI_775%    = SWIACEDGE, PCMCIA\Sierra_Wireless-AC775-F092
%PC7000%     = PC7000,    PCMCIA\PC7000-GPRS_Network_Adapter-64AB
%PC7200%     = PC7200,    PCMCIA\PC7200-EDGE_Network_Adapter-F401 


;****************************************************************************
;  Installation script for Windows 98
;****************************************************************************

[SWIACGPRS]
AddReg = SWIACGPRS.9x.reg, SWIACGPRS.Overrides.9x.reg
DriverVer = 05/05/2004,2.0.0.4

[SWIACGPRS.HW]
AddReg = SWIACGPRS.RegHW

[SWIACGPRS.RegHW]
HKR,Child0000,HardwareID,,MF\AirCardGPRS_DEV0 ;modem
HKR,Child0000,ResourceMap,1,00,02
HKR,Child0001,HardwareID,,MF\AirCardGPRS_DEV1 ;net
HKR,Child0001,ResourceMap,1,01,02,03,04


[SWIACEDGE]
AddReg = SWIACGPRS.9x.reg, SWIACGPRS.Overrides.9x.reg
DriverVer = 05/05/2004,2.0.0.4

[SWIACEDGE.HW]
AddReg = SWIACEDGE.RegHW

[SWIACEDGE.RegHW]
HKR,Child0000,HardwareID,,MF\AirCardEDGE_DEV0 ;modem
HKR,Child0000,ResourceMap,1,00,02
HKR,Child0001,HardwareID,,MF\AirCardEDGE_DEV1 ;net
HKR,Child0001,ResourceMap,1,01,02,03,04


[PC7000]
AddReg = SWIACGPRS.9x.reg, SWIACGPRS.Overrides.9x.reg
DriverVer = 05/05/2004,2.0.0.4

[PC7000.HW]
AddReg = SWIACEDGE.RegHW

[PC7000.RegHW]
HKR,Child0000,HardwareID,,MF\PC7000_DEV0 ;modem
HKR,Child0000,ResourceMap,1,00,02
HKR,Child0001,HardwareID,,MF\PC7000_DEV1 ;net
HKR,Child0001,ResourceMap,1,01,02,03,04


[PC7200]
AddReg = SWIACGPRS.9x.reg, SWIACGPRS.Overrides.9x.reg
DriverVer = 05/05/2004,2.0.0.4

[PC7200.HW]
AddReg = SWIACEDGE.RegHW

[PC7200.RegHW]
HKR,Child0000,HardwareID,,MF\PC7200_DEV0 ;modem
HKR,Child0000,ResourceMap,1,00,02
HKR,Child0001,HardwareID,,MF\PC7200_DEV1 ;net
HKR,Child0001,ResourceMap,1,01,02,03,04


[SWIACGPRS.9x.Reg]
HKR, , DevLoader,, *CONFIGMG
HKR, , Enumerator, , *CONFIGMG
HKR, , CMDrivFlags, 01, 03, 00, 00, 00

[SWIACGPRS.Overrides.9x.reg]
;****************************************************************************
; The override section is only needed if the CIS does NOT contain a proper
; Config_Table_Entry tuple describing the necessary I\O, IRQ, & memory
; resources.  We need it to allow us to open separate I/O windows for the COM
; port and the network adapter.
;****************************************************************************
; OVERRIDE for COM3 (3E8,4)
HKR,Override,0001,1, \
;
; CONFIGMG_VERSION
00,04,00,00, \
;
; PRIORITY
00,30,00,00, \
;
; I/O Resource Descriptor 0: COM port
;
24,00,00,00, \ ; Total length of I/O Resource Descriptor
02,00,00,00, \ ; ResType_IO = 0x00000002
01,00, \       ; IOD_Count;
0C,00, \       ; IOD_Type;         // IOType_Range = 0x000C
00,00, \       ; IOD_Alloc_Base;
00,00, \       ; IOD_Alloc_End;
00,00, \       ; IOD_DesFlags;
00, \          ; IOD_Alloc_Alias;
00, \          ; IOD_Alloc_Decode;
F8,FF, \       ; IOR_Align;        // Mask for base alignment
08,00, \       ; IOR_nPorts;       // Number of ports
E8,03, \       ; IOR_Min;          // Min port address
EF,03, \       ; IOR_Max;          // Max port address
00,00, \       ; IOR_RangeFlags;   // Flags
00, \          ; IOR_Alias;        // Alias offset
00, \          ; IOR_Decode;       // Address specified
64,00,00,00, \ ; PCCARD flags, 0x40 = 16-bit port
;
; I/O Resource Descriptor 1 : network port
;
24,00,00,00, \ ; Total length of I/O Resource Descriptor
02,00,00,00, \ ; ResType_IO = 0x00000002
01,00, \       ; IOD_Count;
0C,00, \       ; IOD_Type;         // IOType_Range = 0x000C
00,00, \       ; IOD_Alloc_Base;
00,00, \       ; IOD_Alloc_End;
00,00, \       ; IOD_DesFlags;
00, \          ; IOD_Alloc_Alias;
00, \          ; IOD_Alloc_Decode;
C0,FF, \       ; IOR_Align;        // Mask for base alignment
20,00, \       ; IOR_nPorts;       // Number of ports
00,01, \       ; IOR_Min;          // Min port address
FF,FF, \       ; IOR_Max;          // Max port address
00,00, \       ; IOR_RangeFlags;   // Flags
00, \          ; IOR_Alias;        // Alias offset
00, \          ; IOR_Decode;       // Address specified
64,00,00,00, \ ; PCCARD flags, 0x40 = 16-bit port
;
; IRQ Resource Descriptor
;
14,00,00,00, \ ; Total length of IRQ Resource Descriptor
04,00,00,00, \ ; ResType_IRQ = 0x00000004
00,00, \       ; IRQD_Flags;
00,00, \       ; IRQD_Alloc_Num;   // Allocated IRQ number
10,00, \       ; IRQD_Req_Mask;    // Mask of possible IRQs
00,00, \       ; IRQD_Reserved;
20,00,00,00, \ ; PCCARD flags, 0x20 = Level mode interrupts
;
; MEM Resource Descriptor 0
; 8K attribute memory window mapped to adapter address offset F000
;
34,00,00,00, \ ; Total length of Memory Resource Descriptor
01,00,00,00, \ ; ResType_Mem = 0x00000001
01,00, \       ; MD_Count;
14,00, \       ; MD_Type;          // MType_Range = 0x0014
00,00,00,00, \ ; MD_Alloc_Base;
00,00,00,00, \ ; MD_Alloc_End;
00,00, \       ; MD_Flags;
00,00, \       ; MD_Reserved;
00,F0,FF,FF, \ ; MR_Align;      // Mask for base alignment
00,20,00,00, \ ; MR_nBytes;     // Count of bytes
00,00,00,00, \ ; MR_Min;        // Min Address
FF,FF,FF,FF, \ ; MR_Max;        // Max Address
00,00, \       ; MR_Flags;      // Flags
00,00, \       ; MR_Reserved;
02,00,00,00, \  ; PC Card flags // 0x02 = attribute mem
;                               // 0x04 = 8-bit common mem (undocumented)
;                               // 0x08 = 16-bit common men
00,F0,00,00, \ ; Memory card address
;

;
; REQUEST_CONFIG_PKT Descriptor
; Same as PCMCIA Card Services RequestConfiguration argument structure.
; The Socket field in this structure does not need to be filled in.
;
19,00,00,00, \ ; Total length of REQUEST_CONFIG_PKT Descriptor
7C,89,00,00, \ ; (ResType_Ignored_Bit + PCCARD_DEVICE_ID) = 0x897C
00,00, \       ; Socket;
02,00, \       ; Attributes;
32, \          ; Vcc;
32, \          ; Vpp1
32, \          ; Vpp2
02, \          ; IntType;
00,07,00,00, \ ; ConfigBase;
00, \          ; Status;
00, \          ; Pin;
00, \          ; Copy;
5F, \          ; ConfigIndex;
73, \          ; Present;
;
; TERMINATOR
;
00,00,00,00
;
;
; OVERRIDE for COM2 (2F8,3)
;
HKR,Override,0002,1, \
;
; CONFIGMG_VERSION
;
00,04,00,00, \
;
; PRIORITY
;
00,30,00,00, \
;
; I/O Resource Descriptor 0: COM port
;
24,00,00,00, \ ; Total length of I/O Resource Descriptor
02,00,00,00, \ ; ResType_IO = 0x00000002
01,00, \       ; IOD_Count;
0C,00, \       ; IOD_Type;         // IOType_Range = 0x000C
00,00, \       ; IOD_Alloc_Base;
00,00, \       ; IOD_Alloc_End;
00,00, \       ; IOD_DesFlags;
00, \          ; IOD_Alloc_Alias;
00, \          ; IOD_Alloc_Decode;
F8,FF, \       ; IOR_Align;        // Mask for base alignment
08,00, \       ; IOR_nPorts;       // Number of ports
F8,02, \       ; IOR_Min;          // Min port address
FF,02, \       ; IOR_Max;          // Max port address
00,00, \       ; IOR_RangeFlags;   // Flags
00, \          ; IOR_Alias;        // Alias offset
00, \          ; IOR_Decode;       // Address specified
64,00,00,00, \ ; PCCARD flags, 0x40 = 16-bit port
;
; I/O Resource Descriptor 1 : network port
;
24,00,00,00, \ ; Total length of I/O Resource Descriptor
02,00,00,00, \ ; ResType_IO = 0x00000002
01,00, \       ; IOD_Count;
0C,00, \       ; IOD_Type;         // IOType_Range = 0x000C
00,00, \       ; IOD_Alloc_Base;
00,00, \       ; IOD_Alloc_End;
00,00, \       ; IOD_DesFlags;
00, \          ; IOD_Alloc_Alias;
00, \          ; IOD_Alloc_Decode;
C0,FF, \       ; IOR_Align;        // Mask for base alignment
20,00, \       ; IOR_nPorts;       // Number of ports
00,01, \       ; IOR_Min;          // Min port address
FF,FF, \       ; IOR_Max;          // Max port address
00,00, \       ; IOR_RangeFlags;   // Flags
00, \          ; IOR_Alias;        // Alias offset
00, \          ; IOR_Decode;       // Address specified
64,00,00,00, \ ; PCCARD flags, 0x40 = 16-bit port
;
; IRQ Resource Descriptor
;
14,00,00,00, \ ; Total length of IRQ Resource Descriptor
04,00,00,00, \ ; ResType_IRQ = 0x00000004
00,00, \       ; IRQD_Flags;
00,00, \       ; IRQD_Alloc_Num;   // Allocated IRQ number
08,00, \       ; IRQD_Req_Mask;    // Mask of possible IRQs
00,00, \       ; IRQD_Reserved;
20,00,00,00, \ ; PCCARD flags, 0x20 = Level mode interrupts
;
; MEM Resource Descriptor 0
; 8K attribute memory window mapped to adapter address offset F000
;
34,00,00,00, \ ; Total length of Memory Resource Descriptor
01,00,00,00, \ ; ResType_Mem = 0x00000001
01,00, \       ; MD_Count;
14,00, \       ; MD_Type;          // MType_Range = 0x0014
00,00,00,00, \ ; MD_Alloc_Base;
00,00,00,00, \ ; MD_Alloc_End;
00,00, \       ; MD_Flags;
00,00, \       ; MD_Reserved;
00,F0,FF,FF, \ ; MR_Align;      // Mask for base alignment
00,20,00,00, \ ; MR_nBytes;     // Count of bytes
00,00,00,00, \ ; MR_Min;        // Min Address
FF,FF,FF,FF, \ ; MR_Max;        // Max Address
00,00, \       ; MR_Flags;      // Flags
00,00, \       ; MR_Reserved;
02,00,00,00, \  ; PC Card flags // 0x02 = attribute mem
;                               // 0x04 = 8-bit common mem (undocumented)
;                               // 0x08 = 16-bit common men
00,F0,00,00, \ ; Memory card address
;
; REQUEST_CONFIG_PKT Descriptor
; Same as PCMCIA Card Services RequestConfiguration argument structure.
; The Socket field in this structure does not need to be filled in.
;
19,00,00,00, \ ; Total length of REQUEST_CONFIG_PKT Descriptor
7C,89,00,00, \ ; (ResType_Ignored_Bit + PCCARD_DEVICE_ID) = 0x897C
00,00, \       ; Socket;
02,00, \       ; Attributes;
32, \          ; Vcc;
00, \          ; Vpp1
00, \          ; Vpp2
02, \          ; IntType;
00,07,00,00, \ ; ConfigBase;
00, \          ; Status;
00, \          ; Pin;
00, \          ; Copy;
57, \          ; ConfigIndex;
73, \          ; Present;
;
; TERMINATOR
;
00,00,00,00
;
;
; OVERRIDE for COM1 (3F8,4)
;
HKR,Override,0003,1, \
;
; CONFIGMG_VERSION
;
00,04,00,00, \
;
; PRIORITY
;
00,30,00,00, \
;
; I/O Resource Descriptor 0: COM port
;
24,00,00,00, \ ; Total length of I/O Resource Descriptor
02,00,00,00, \ ; ResType_IO = 0x00000002
01,00, \       ; IOD_Count;
0C,00, \       ; IOD_Type;         // IOType_Range = 0x000C
00,00, \       ; IOD_Alloc_Base;
00,00, \       ; IOD_Alloc_End;
00,00, \       ; IOD_DesFlags;
00, \          ; IOD_Alloc_Alias;
00, \          ; IOD_Alloc_Decode;
F8,FF, \       ; IOR_Align;        // Mask for base alignment
08,00, \       ; IOR_nPorts;       // Number of ports
F8,03, \       ; IOR_Min;          // Min port address
FF,03, \       ; IOR_Max;          // Max port address
00,00, \       ; IOR_RangeFlags;   // Flags
00, \          ; IOR_Alias;        // Alias offset
00, \          ; IOR_Decode;       // Address specified
64,00,00,00, \ ; PCCARD flags, 0x40 = 16-bit port
;
; I/O Resource Descriptor 1 : network port
;
24,00,00,00, \ ; Total length of I/O Resource Descriptor
02,00,00,00, \ ; ResType_IO = 0x00000002
01,00, \       ; IOD_Count;
0C,00, \       ; IOD_Type;         // IOType_Range = 0x000C
00,00, \       ; IOD_Alloc_Base;
00,00, \       ; IOD_Alloc_End;
00,00, \       ; IOD_DesFlags;
00, \          ; IOD_Alloc_Alias;
00, \          ; IOD_Alloc_Decode;
C0,FF, \       ; IOR_Align;        // Mask for base alignment
20,00, \       ; IOR_nPorts;       // Number of ports
00,01, \       ; IOR_Min;          // Min port address
FF,FF, \       ; IOR_Max;          // Max port address
00,00, \       ; IOR_RangeFlags;   // Flags
00, \          ; IOR_Alias;        // Alias offset
00, \          ; IOR_Decode;       // Address specified
64,00,00,00, \ ; PCCARD flags, 0x40 = 16-bit port
;
; IRQ Resource Descriptor
;
14,00,00,00, \ ; Total length of IRQ Resource Descriptor
04,00,00,00, \ ; ResType_IRQ = 0x00000004
00,00, \       ; IRQD_Flags;
00,00, \       ; IRQD_Alloc_Num;   // Allocated IRQ number
10,00, \       ; IRQD_Req_Mask;    // Mask of possible IRQs
00,00, \       ; IRQD_Reserved;
20,00,00,00, \ ; PCCARD flags, 0x20 = Level mode interrupts
;
; MEM Resource Descriptor 0
; 8K attribute memory window mapped to adapter address offset F000
;
34,00,00,00, \ ; Total length of Memory Resource Descriptor
01,00,00,00, \ ; ResType_Mem = 0x00000001
01,00, \       ; MD_Count;
14,00, \       ; MD_Type;          // MType_Range = 0x0014
00,00,00,00, \ ; MD_Alloc_Base;
00,00,00,00, \ ; MD_Alloc_End;
00,00, \       ; MD_Flags;
00,00, \       ; MD_Reserved;
00,F0,FF,FF, \ ; MR_Align;      // Mask for base alignment
00,20,00,00, \ ; MR_nBytes;     // Count of bytes
00,00,00,00, \ ; MR_Min;        // Min Address
FF,FF,FF,FF, \ ; MR_Max;        // Max Address
00,00, \       ; MR_Flags;      // Flags
00,00, \       ; MR_Reserved;
02,00,00,00, \  ; PC Card flags // 0x02 = attribute mem
;                               // 0x04 = 8-bit common mem (undocumented)
;                               // 0x08 = 16-bit common men
00,F0,00,00, \ ; Memory card address
;
;
; REQUEST_CONFIG_PKT Descriptor
; Same as PCMCIA Card Services RequestConfiguration argument structure.
; The Socket field in this structure does not need to be filled in.
;
19,00,00,00, \ ; Total length of REQUEST_CONFIG_PKT Descriptor
7C,89,00,00, \ ; (ResType_Ignored_Bit + PCCARD_DEVICE_ID) = 0x897C
00,00, \       ; Socket;
02,00, \       ; Attributes;
32, \          ; Vcc;
00, \          ; Vpp1
00, \          ; Vpp2
02, \          ; IntType;
00,07,00,00, \ ; ConfigBase;
00, \          ; Status;
00, \          ; Pin;
00, \          ; Copy;
4F, \          ; ConfigIndex;
73, \          ; Present;
;
; TERMINATOR
;
00,00,00,00
;
;
; OVERRIDE for COM4 (2E8,xx)
;
HKR,Override,0004,1, \
;
; CONFIGMG_VERSION
;
00,04,00,00, \
;
; PRIORITY
;
00,30,00,00, \
;
; I/O Resource Descriptor 0: COM port
;
24,00,00,00, \ ; Total length of I/O Resource Descriptor
02,00,00,00, \ ; ResType_IO = 0x00000002
01,00, \       ; IOD_Count;
0C,00, \       ; IOD_Type;         // IOType_Range = 0x000C
00,00, \       ; IOD_Alloc_Base;
00,00, \       ; IOD_Alloc_End;
00,00, \       ; IOD_DesFlags;
00, \          ; IOD_Alloc_Alias;
00, \          ; IOD_Alloc_Decode;
F8,FF, \       ; IOR_Align;        // Mask for base alignment
08,00, \       ; IOR_nPorts;       // Number of ports
E8,02, \       ; IOR_Min;          // Min port address
EF,02, \       ; IOR_Max;          // Max port address
00,00, \       ; IOR_RangeFlags;   // Flags
00, \          ; IOR_Alias;        // Alias offset
00, \          ; IOR_Decode;       // Address specified
64,00,00,00, \ ; PCCARD flags, 0x40 = 16-bit port
;
; I/O Resource Descriptor 1 : network port
;
24,00,00,00, \ ; Total length of I/O Resource Descriptor
02,00,00,00, \ ; ResType_IO = 0x00000002
01,00, \       ; IOD_Count;
0C,00, \       ; IOD_Type;         // IOType_Range = 0x000C
00,00, \       ; IOD_Alloc_Base;
00,00, \       ; IOD_Alloc_End;
00,00, \       ; IOD_DesFlags;
00, \          ; IOD_Alloc_Alias;
00, \          ; IOD_Alloc_Decode;
C0,FF, \       ; IOR_Align;        // Mask for base alignment
20,00, \       ; IOR_nPorts;       // Number of ports
00,01, \       ; IOR_Min;          // Min port address
FF,FF, \       ; IOR_Max;          // Max port address
00,00, \       ; IOR_RangeFlags;   // Flags
00, \          ; IOR_Alias;        // Alias offset
00, \          ; IOR_Decode;       // Address specified
64,00,00,00, \ ; PCCARD flags, 0x40 = 16-bit port
;
; IRQ Resource Descriptor
;
14,00,00,00, \ ; Total length of IRQ Resource Descriptor
04,00,00,00, \ ; ResType_IRQ = 0x00000004
00,00, \       ; IRQD_Flags;
00,00, \       ; IRQD_Alloc_Num;   // Allocated IRQ number
ff,ff, \       ; IRQD_Req_Mask;    // Mask of possible IRQs
00,00, \       ; IRQD_Reserved;
20,00,00,00, \ ; PCCARD flags, 0x20 = Level mode interrupts
;
; MEM Resource Descriptor 0
; 8K attribute memory window mapped to adapter address offset F000
;
34,00,00,00, \ ; Total length of Memory Resource Descriptor
01,00,00,00, \ ; ResType_Mem = 0x00000001
01,00, \       ; MD_Count;
14,00, \       ; MD_Type;          // MType_Range = 0x0014
00,00,00,00, \ ; MD_Alloc_Base;
00,00,00,00, \ ; MD_Alloc_End;
00,00, \       ; MD_Flags;
00,00, \       ; MD_Reserved;
00,F0,FF,FF, \ ; MR_Align;      // Mask for base alignment
00,20,00,00, \ ; MR_nBytes;     // Count of bytes
00,00,00,00, \ ; MR_Min;        // Min Address
FF,FF,FF,FF, \ ; MR_Max;        // Max Address
00,00, \       ; MR_Flags;      // Flags
00,00, \       ; MR_Reserved;
02,00,00,00, \  ; PC Card flags // 0x02 = attribute mem
;                               // 0x04 = 8-bit common mem (undocumented)
;                               // 0x08 = 16-bit common men
00,F0,00,00, \ ; Memory card address
;
;
; REQUEST_CONFIG_PKT Descriptor
; Same as PCMCIA Card Services RequestConfiguration argument structure.
; The Socket field in this structure does not need to be filled in.
;
19,00,00,00, \ ; Total length of REQUEST_CONFIG_PKT Descriptor
7C,89,00,00, \ ; (ResType_Ignored_Bit + PCCARD_DEVICE_ID) = 0x897C
00,00, \       ; Socket;
02,00, \       ; Attributes;
32, \          ; Vcc;
32, \          ; Vpp1
32, \          ; Vpp2
02, \          ; IntType;
00,07,00,00, \ ; ConfigBase;
00, \          ; Status;
00, \          ; Pin;
00, \          ; Copy;
67, \          ; ConfigIndex;
73, \          ; Present;
;
; TERMINATOR
;
00,00,00,00
;
;
; OVERRIDE for COM3 (3E8,xx)
;
HKR,Override,0005,1, \
;
; CONFIGMG_VERSION
;
00,04,00,00, \
;
; PRIORITY
;
00,30,00,00, \
;
; I/O Resource Descriptor 0: COM port
;
24,00,00,00, \ ; Total length of I/O Resource Descriptor
02,00,00,00, \ ; ResType_IO = 0x00000002
01,00, \       ; IOD_Count;
0C,00, \       ; IOD_Type;         // IOType_Range = 0x000C
00,00, \       ; IOD_Alloc_Base;
00,00, \       ; IOD_Alloc_End;
00,00, \       ; IOD_DesFlags;
00, \          ; IOD_Alloc_Alias;
00, \          ; IOD_Alloc_Decode;
F8,FF, \       ; IOR_Align;        // Mask for base alignment
08,00, \       ; IOR_nPorts;       // Number of ports
E8,03, \       ; IOR_Min;          // Min port address
EF,03, \       ; IOR_Max;          // Max port address
00,00, \       ; IOR_RangeFlags;   // Flags
00, \          ; IOR_Alias;        // Alias offset
00, \          ; IOR_Decode;       // Address specified
64,00,00,00, \ ; PCCARD flags, 0x40 = 16-bit port
;
; I/O Resource Descriptor 1 : network port
;
24,00,00,00, \ ; Total length of I/O Resource Descriptor
02,00,00,00, \ ; ResType_IO = 0x00000002
01,00, \       ; IOD_Count;
0C,00, \       ; IOD_Type;         // IOType_Range = 0x000C
00,00, \       ; IOD_Alloc_Base;
00,00, \       ; IOD_Alloc_End;
00,00, \       ; IOD_DesFlags;
00, \          ; IOD_Alloc_Alias;
00, \          ; IOD_Alloc_Decode;
C0,FF, \       ; IOR_Align;        // Mask for base alignment
20,00, \       ; IOR_nPorts;       // Number of ports
00,01, \       ; IOR_Min;          // Min port address
FF,FF, \       ; IOR_Max;          // Max port address
00,00, \       ; IOR_RangeFlags;   // Flags
00, \          ; IOR_Alias;        // Alias offset
00, \          ; IOR_Decode;       // Address specified
64,00,00,00, \ ; PCCARD flags, 0x40 = 16-bit port
;
; IRQ Resource Descriptor
;
14,00,00,00, \ ; Total length of IRQ Resource Descriptor
04,00,00,00, \ ; ResType_IRQ = 0x00000004
00,00, \       ; IRQD_Flags;
00,00, \       ; IRQD_Alloc_Num;   // Allocated IRQ number
ff,ff, \       ; IRQD_Req_Mask;    // Mask of possible IRQs
00,00, \       ; IRQD_Reserved;
20,00,00,00, \ ; PCCARD flags, 0x20 = Level mode interrupts
;
; MEM Resource Descriptor 0
; 8K attribute memory window mapped to adapter address offset F000
;
34,00,00,00, \ ; Total length of Memory Resource Descriptor
01,00,00,00, \ ; ResType_Mem = 0x00000001
01,00, \       ; MD_Count;
14,00, \       ; MD_Type;          // MType_Range = 0x0014
00,00,00,00, \ ; MD_Alloc_Base;
00,00,00,00, \ ; MD_Alloc_End;
00,00, \       ; MD_Flags;
00,00, \       ; MD_Reserved;
00,F0,FF,FF, \ ; MR_Align;      // Mask for base alignment
00,20,00,00, \ ; MR_nBytes;     // Count of bytes
00,00,00,00, \ ; MR_Min;        // Min Address
FF,FF,FF,FF, \ ; MR_Max;        // Max Address
00,00, \       ; MR_Flags;      // Flags
00,00, \       ; MR_Reserved;
02,00,00,00, \  ; PC Card flags // 0x02 = attribute mem
;                               // 0x04 = 8-bit common mem (undocumented)
;                               // 0x08 = 16-bit common men
00,F0,00,00, \ ; Memory card address
;
;
; REQUEST_CONFIG_PKT Descriptor
; Same as PCMCIA Card Services RequestConfiguration argument structure.
; The Socket field in this structure does not need to be filled in.
;
19,00,00,00, \ ; Total length of REQUEST_CONFIG_PKT Descriptor
7C,89,00,00, \ ; (ResType_Ignored_Bit + PCCARD_DEVICE_ID) = 0x897C
00,00, \       ; Socket;
02,00, \       ; Attributes;
32, \          ; Vcc;
32, \          ; Vpp1
32, \          ; Vpp2
02, \          ; IntType;
00,07,00,00, \ ; ConfigBase;
00, \          ; Status;
00, \          ; Pin;
00, \          ; Copy;
5F, \          ; ConfigIndex;
73, \          ; Present;
;
; TERMINATOR
;
00,00,00,00
;
;
; OVERRIDE for COM2 (2F8,xx)
;
HKR,Override,0006,1, \
;
; CONFIGMG_VERSION
;
00,04,00,00, \
;
; PRIORITY
;
00,30,00,00, \
;
; I/O Resource Descriptor 0: COM port
;
24,00,00,00, \ ; Total length of I/O Resource Descriptor
02,00,00,00, \ ; ResType_IO = 0x00000002
01,00, \       ; IOD_Count;
0C,00, \       ; IOD_Type;         // IOType_Range = 0x000C
00,00, \       ; IOD_Alloc_Base;
00,00, \       ; IOD_Alloc_End;
00,00, \       ; IOD_DesFlags;
00, \          ; IOD_Alloc_Alias;
00, \          ; IOD_Alloc_Decode;
F8,FF, \       ; IOR_Align;        // Mask for base alignment
08,00, \       ; IOR_nPorts;       // Number of ports
F8,02, \       ; IOR_Min;          // Min port address
FF,02, \       ; IOR_Max;          // Max port address
00,00, \       ; IOR_RangeFlags;   // Flags
00, \          ; IOR_Alias;        // Alias offset
00, \          ; IOR_Decode;       // Address specified
64,00,00,00, \ ; PCCARD flags, 0x40 = 16-bit port
;
; I/O Resource Descriptor 1 : network port
;
24,00,00,00, \ ; Total length of I/O Resource Descriptor
02,00,00,00, \ ; ResType_IO = 0x00000002
01,00, \       ; IOD_Count;
0C,00, \       ; IOD_Type;         // IOType_Range = 0x000C
00,00, \       ; IOD_Alloc_Base;
00,00, \       ; IOD_Alloc_End;
00,00, \       ; IOD_DesFlags;
00, \          ; IOD_Alloc_Alias;
00, \          ; IOD_Alloc_Decode;
C0,FF, \       ; IOR_Align;        // Mask for base alignment
20,00, \       ; IOR_nPorts;       // Number of ports
00,01, \       ; IOR_Min;          // Min port address
FF,FF, \       ; IOR_Max;          // Max port address
00,00, \       ; IOR_RangeFlags;   // Flags
00, \          ; IOR_Alias;        // Alias offset
00, \          ; IOR_Decode;       // Address specified
64,00,00,00, \ ; PCCARD flags, 0x40 = 16-bit port
;
; IRQ Resource Descriptor
;
14,00,00,00, \ ; Total length of IRQ Resource Descriptor
04,00,00,00, \ ; ResType_IRQ = 0x00000004
00,00, \       ; IRQD_Flags;
00,00, \       ; IRQD_Alloc_Num;   // Allocated IRQ number
ff,ff, \       ; IRQD_Req_Mask;    // Mask of possible IRQs
00,00, \       ; IRQD_Reserved;
20,00,00,00, \ ; PCCARD flags, 0x20 = Level mode interrupts
;
; MEM Resource Descriptor 0
; 8K attribute memory window mapped to adapter address offset F000
;
34,00,00,00, \ ; Total length of Memory Resource Descriptor
01,00,00,00, \ ; ResType_Mem = 0x00000001
01,00, \       ; MD_Count;
14,00, \       ; MD_Type;          // MType_Range = 0x0014
00,00,00,00, \ ; MD_Alloc_Base;
00,00,00,00, \ ; MD_Alloc_End;
00,00, \       ; MD_Flags;
00,00, \       ; MD_Reserved;
00,F0,FF,FF, \ ; MR_Align;      // Mask for base alignment
00,20,00,00, \ ; MR_nBytes;     // Count of bytes
00,00,00,00, \ ; MR_Min;        // Min Address
FF,FF,FF,FF, \ ; MR_Max;        // Max Address
00,00, \       ; MR_Flags;      // Flags
00,00, \       ; MR_Reserved;
02,00,00,00, \  ; PC Card flags // 0x02 = attribute mem
;                               // 0x04 = 8-bit common mem (undocumented)
;                               // 0x08 = 16-bit common men
00,F0,00,00, \ ; Memory card address
;
;
; REQUEST_CONFIG_PKT Descriptor
; Same as PCMCIA Card Services RequestConfiguration argument structure.
; The Socket field in this structure does not need to be filled in.
;
19,00,00,00, \ ; Total length of REQUEST_CONFIG_PKT Descriptor
7C,89,00,00, \ ; (ResType_Ignored_Bit + PCCARD_DEVICE_ID) = 0x897C
00,00, \       ; Socket;
02,00, \       ; Attributes;
32, \          ; Vcc;
00, \          ; Vpp1
00, \          ; Vpp2
02, \          ; IntType;
00,07,00,00, \ ; ConfigBase;
00, \          ; Status;
00, \          ; Pin;
00, \          ; Copy;
57, \          ; ConfigIndex;
73, \          ; Present;
;
; TERMINATOR
;
00,00,00,00
;
;
; OVERRIDE for COM1 (3F8,xx)
;
HKR,Override,0007,1, \
;
; CONFIGMG_VERSION
;
00,04,00,00, \
;
; PRIORITY
;
00,30,00,00, \
;
; I/O Resource Descriptor 0: COM port
;
24,00,00,00, \ ; Total length of I/O Resource Descriptor
02,00,00,00, \ ; ResType_IO = 0x00000002
01,00, \       ; IOD_Count;
0C,00, \       ; IOD_Type;         // IOType_Range = 0x000C
00,00, \       ; IOD_Alloc_Base;
00,00, \       ; IOD_Alloc_End;
00,00, \       ; IOD_DesFlags;
00, \          ; IOD_Alloc_Alias;
00, \          ; IOD_Alloc_Decode;
F8,FF, \       ; IOR_Align;        // Mask for base alignment
08,00, \       ; IOR_nPorts;       // Number of ports
F8,03, \       ; IOR_Min;          // Min port address
FF,03, \       ; IOR_Max;          // Max port address
00,00, \       ; IOR_RangeFlags;   // Flags
00, \          ; IOR_Alias;        // Alias offset
00, \          ; IOR_Decode;       // Address specified
64,00,00,00, \ ; PCCARD flags, 0x40 = 16-bit port
;
; I/O Resource Descriptor 1 : network port
;
24,00,00,00, \ ; Total length of I/O Resource Descriptor
02,00,00,00, \ ; ResType_IO = 0x00000002
01,00, \       ; IOD_Count;
0C,00, \       ; IOD_Type;         // IOType_Range = 0x000C
00,00, \       ; IOD_Alloc_Base;
00,00, \       ; IOD_Alloc_End;
00,00, \       ; IOD_DesFlags;
00, \          ; IOD_Alloc_Alias;
00, \          ; IOD_Alloc_Decode;
C0,FF, \       ; IOR_Align;        // Mask for base alignment
20,00, \       ; IOR_nPorts;       // Number of ports
00,01, \       ; IOR_Min;          // Min port address
FF,FF, \       ; IOR_Max;          // Max port address
00,00, \       ; IOR_RangeFlags;   // Flags
00, \          ; IOR_Alias;        // Alias offset
00, \          ; IOR_Decode;       // Address specified
64,00,00,00, \ ; PCCARD flags, 0x40 = 16-bit port
;
; IRQ Resource Descriptor
;
14,00,00,00, \ ; Total length of IRQ Resource Descriptor
04,00,00,00, \ ; ResType_IRQ = 0x00000004
00,00, \       ; IRQD_Flags;
00,00, \       ; IRQD_Alloc_Num;   // Allocated IRQ number
ff,ff, \       ; IRQD_Req_Mask;    // Mask of possible IRQs
00,00, \       ; IRQD_Reserved;
20,00,00,00, \ ; PCCARD flags, 0x20 = Level mode interrupts
;
; MEM Resource Descriptor 0
; 8K attribute memory window mapped to adapter address offset F000
;
34,00,00,00, \ ; Total length of Memory Resource Descriptor
01,00,00,00, \ ; ResType_Mem = 0x00000001
01,00, \       ; MD_Count;
14,00, \       ; MD_Type;          // MType_Range = 0x0014
00,00,00,00, \ ; MD_Alloc_Base;
00,00,00,00, \ ; MD_Alloc_End;
00,00, \       ; MD_Flags;
00,00, \       ; MD_Reserved;
00,F0,FF,FF, \ ; MR_Align;      // Mask for base alignment
00,20,00,00, \ ; MR_nBytes;     // Count of bytes
00,00,00,00, \ ; MR_Min;        // Min Address
FF,FF,FF,FF, \ ; MR_Max;        // Max Address
00,00, \       ; MR_Flags;      // Flags
00,00, \       ; MR_Reserved;
02,00,00,00, \  ; PC Card flags // 0x02 = attribute mem
;                               // 0x04 = 8-bit common mem (undocumented)
;                               // 0x08 = 16-bit common men
00,F0,00,00, \ ; Memory card address
;
;
; REQUEST_CONFIG_PKT Descriptor
; Same as PCMCIA Card Services RequestConfiguration argument structure.
; The Socket field in this structure does not need to be filled in.
;
19,00,00,00, \ ; Total length of REQUEST_CONFIG_PKT Descriptor
7C,89,00,00, \ ; (ResType_Ignored_Bit + PCCARD_DEVICE_ID) = 0x897C
00,00, \       ; Socket;
02,00, \       ; Attributes;
32, \          ; Vcc;
00, \          ; Vpp1
00, \          ; Vpp2
02, \          ; IntType;
00,07,00,00, \ ; ConfigBase;
00, \          ; Status;
00, \          ; Pin;
00, \          ; Copy;
4F, \          ; ConfigIndex;
73, \          ; Present;
;
; TERMINATOR
;
00,00,00,00
;
;
; OVERRIDE for Any 1 (2020-203F,xx)
;
HKR,Override,008,1, \
;
; CONFIGMG_VERSION
;
00,04,00,00, \
;
; PRIORITY
;
00,30,00,00, \
;
; I/O Resource Descriptor 0: COM port
;
24,00,00,00, \ ; Total length of I/O Resource Descriptor
02,00,00,00, \ ; ResType_IO = 0x00000002
01,00, \       ; IOD_Count;
0C,00, \       ; IOD_Type;         // IOType_Range = 0x000C
00,00, \       ; IOD_Alloc_Base;
00,00, \       ; IOD_Alloc_End;
00,00, \       ; IOD_DesFlags;
00, \          ; IOD_Alloc_Alias;
00, \          ; IOD_Alloc_Decode;
F8,FF, \       ; IOR_Align;        // Mask for base alignment
08,00, \       ; IOR_nPorts;       // Number of ports
20,20, \       ; IOR_Min;          // Min port address
3F,20, \       ; IOR_Max;          // Max port address
00,00, \       ; IOR_RangeFlags;   // Flags
00, \          ; IOR_Alias;        // Alias offset
00, \          ; IOR_Decode;       // Address specified
64,00,00,00, \ ; PCCARD flags, 0x40 = 16-bit port
;
; I/O Resource Descriptor 1 : network port
;
24,00,00,00, \ ; Total length of I/O Resource Descriptor
02,00,00,00, \ ; ResType_IO = 0x00000002
01,00, \       ; IOD_Count;
0C,00, \       ; IOD_Type;         // IOType_Range = 0x000C
00,00, \       ; IOD_Alloc_Base;
00,00, \       ; IOD_Alloc_End;
00,00, \       ; IOD_DesFlags;
00, \          ; IOD_Alloc_Alias;
00, \          ; IOD_Alloc_Decode;
C0,FF, \       ; IOR_Align;        // Mask for base alignment
20,00, \       ; IOR_nPorts;       // Number of ports
00,01, \       ; IOR_Min;          // Min port address
FF,FF, \       ; IOR_Max;          // Max port address
00,00, \       ; IOR_RangeFlags;   // Flags
00, \          ; IOR_Alias;        // Alias offset
00, \          ; IOR_Decode;       // Address specified
64,00,00,00, \ ; PCCARD flags, 0x40 = 16-bit port
;
; IRQ Resource Descriptor
;
14,00,00,00, \ ; Total length of IRQ Resource Descriptor
04,00,00,00, \ ; ResType_IRQ = 0x00000004
00,00, \       ; IRQD_Flags;
00,00, \       ; IRQD_Alloc_Num;   // Allocated IRQ number
ff,ff, \       ; IRQD_Req_Mask;    // Mask of possible IRQs
00,00, \       ; IRQD_Reserved;
20,00,00,00, \ ; PCCARD flags, 0x20 = Level mode interrupts
;
; MEM Resource Descriptor 0
; 8K attribute memory window mapped to adapter address offset F000
;
34,00,00,00, \ ; Total length of Memory Resource Descriptor
01,00,00,00, \ ; ResType_Mem = 0x00000001
01,00, \       ; MD_Count;
14,00, \       ; MD_Type;          // MType_Range = 0x0014
00,00,00,00, \ ; MD_Alloc_Base;
00,00,00,00, \ ; MD_Alloc_End;
00,00, \       ; MD_Flags;
00,00, \       ; MD_Reserved;
00,F0,FF,FF, \ ; MR_Align;      // Mask for base alignment
00,20,00,00, \ ; MR_nBytes;     // Count of bytes
00,00,00,00, \ ; MR_Min;        // Min Address
FF,FF,FF,FF, \ ; MR_Max;        // Max Address
00,00, \       ; MR_Flags;      // Flags
00,00, \       ; MR_Reserved;
02,00,00,00, \  ; PC Card flags // 0x02 = attribute mem
;                               // 0x04 = 8-bit common mem (undocumented)
;                               // 0x08 = 16-bit common men
00,F0,00,00, \ ; Memory card address
;
;
; REQUEST_CONFIG_PKT Descriptor
; Same as PCMCIA Card Services RequestConfiguration argument structure.
; The Socket field in this structure does not need to be filled in.
;
19,00,00,00, \ ; Total length of REQUEST_CONFIG_PKT Descriptor
7C,89,00,00, \ ; (ResType_Ignored_Bit + PCCARD_DEVICE_ID) = 0x897C
00,00, \       ; Socket;
02,00, \       ; Attributes;
32, \          ; Vcc;
00, \          ; Vpp1
00, \          ; Vpp2
02, \          ; IntType;
00,07,00,00, \ ; ConfigBase;
00, \          ; Status;
00, \          ; Pin;
00, \          ; Copy;
4F, \          ; ConfigIndex;
73, \          ; Present;
;
; TERMINATOR
;
00,00,00,00
;
;
; OVERRIDE for Any 2 (4FE0-4FFF,xx)
;
HKR,Override,009,1, \
;
; CONFIGMG_VERSION
;
00,04,00,00, \
;
; PRIORITY
;
00,30,00,00, \
;
; I/O Resource Descriptor 0: COM port
;
24,00,00,00, \ ; Total length of I/O Resource Descriptor
02,00,00,00, \ ; ResType_IO = 0x00000002
01,00, \       ; IOD_Count;
0C,00, \       ; IOD_Type;         // IOType_Range = 0x000C
00,00, \       ; IOD_Alloc_Base;
00,00, \       ; IOD_Alloc_End;
00,00, \       ; IOD_DesFlags;
00, \          ; IOD_Alloc_Alias;
00, \          ; IOD_Alloc_Decode;
F8,FF, \       ; IOR_Align;        // Mask for base alignment
08,00, \       ; IOR_nPorts;       // Number of ports
E0,4F, \       ; IOR_Min;          // Min port address
FF,4F, \       ; IOR_Max;          // Max port address
00,00, \       ; IOR_RangeFlags;   // Flags
00, \          ; IOR_Alias;        // Alias offset
00, \          ; IOR_Decode;       // Address specified
64,00,00,00, \ ; PCCARD flags, 0x40 = 16-bit port
;
; I/O Resource Descriptor 1 : network port
;
24,00,00,00, \ ; Total length of I/O Resource Descriptor
02,00,00,00, \ ; ResType_IO = 0x00000002
01,00, \       ; IOD_Count;
0C,00, \       ; IOD_Type;         // IOType_Range = 0x000C
00,00, \       ; IOD_Alloc_Base;
00,00, \       ; IOD_Alloc_End;
00,00, \       ; IOD_DesFlags;
00, \          ; IOD_Alloc_Alias;
00, \          ; IOD_Alloc_Decode;
C0,FF, \       ; IOR_Align;        // Mask for base alignment
20,00, \       ; IOR_nPorts;       // Number of ports
00,01, \       ; IOR_Min;          // Min port address
FF,FF, \       ; IOR_Max;          // Max port address
00,00, \       ; IOR_RangeFlags;   // Flags
00, \          ; IOR_Alias;        // Alias offset
00, \          ; IOR_Decode;       // Address specified
64,00,00,00, \ ; PCCARD flags, 0x40 = 16-bit port
;
; IRQ Resource Descriptor
;
14,00,00,00, \ ; Total length of IRQ Resource Descriptor
04,00,00,00, \ ; ResType_IRQ = 0x00000004
00,00, \       ; IRQD_Flags;
00,00, \       ; IRQD_Alloc_Num;   // Allocated IRQ number
ff,ff, \       ; IRQD_Req_Mask;    // Mask of possible IRQs
00,00, \       ; IRQD_Reserved;
20,00,00,00, \ ; PCCARD flags, 0x20 = Level mode interrupts
;
; MEM Resource Descriptor 0
; 8K attribute memory window mapped to adapter address offset F000
;
34,00,00,00, \ ; Total length of Memory Resource Descriptor
01,00,00,00, \ ; ResType_Mem = 0x00000001
01,00, \       ; MD_Count;
14,00, \       ; MD_Type;          // MType_Range = 0x0014
00,00,00,00, \ ; MD_Alloc_Base;
00,00,00,00, \ ; MD_Alloc_End;
00,00, \       ; MD_Flags;
00,00, \       ; MD_Reserved;
00,F0,FF,FF, \ ; MR_Align;      // Mask for base alignment
00,20,00,00, \ ; MR_nBytes;     // Count of bytes
00,00,00,00, \ ; MR_Min;        // Min Address
FF,FF,FF,FF, \ ; MR_Max;        // Max Address
00,00, \       ; MR_Flags;      // Flags
00,00, \       ; MR_Reserved;
02,00,00,00, \  ; PC Card flags // 0x02 = attribute mem
;                               // 0x04 = 8-bit common mem (undocumented)
;                               // 0x08 = 16-bit common men
00,F0,00,00, \ ; Memory card address
;
;
; REQUEST_CONFIG_PKT Descriptor
; Same as PCMCIA Card Services RequestConfiguration argument structure.
; The Socket field in this structure does not need to be filled in.
;
19,00,00,00, \ ; Total length of REQUEST_CONFIG_PKT Descriptor
7C,89,00,00, \ ; (ResType_Ignored_Bit + PCCARD_DEVICE_ID) = 0x897C
00,00, \       ; Socket;
02,00, \       ; Attributes;
32, \          ; Vcc;
00, \          ; Vpp1
00, \          ; Vpp2
02, \          ; IntType;
00,07,00,00, \ ; ConfigBase;
00, \          ; Status;
00, \          ; Pin;
00, \          ; Copy;
4F, \          ; ConfigIndex;
73, \          ; Present;
;
; TERMINATOR
;
00,00,00,00

;****************************************************************************
;  Installation script for Windows 2000
;****************************************************************************

[SWIACGPRS.nt]
AddReg = SWIACGPRS.nt.AddReg

[SWIACGPRS.nt.AddReg]

[SWIACGPRS.nt.HW]
AddReg = SWIACGPRS.nt.RegHW

[SWIACGPRS.nt.RegHW]
HKR,Child0000,HardwareID,,MF\AircardGPRS_DEV0	; Modem
HKR,Child0000,ResourceMap,1,00,02
HKR,Child0001,HardwareID,,MF\AircardGPRS_DEV1	; net
HKR,Child0001,ResourceMap,1,01,02,03

[SWIACGPRS.nt.Services]
AddService = mf, 2, nt_Services

[nt_Services]
ServiceType    = 1                      ;SERVICE_KERNEL_DRIVER
StartType      = 3                      ;SERVICE_DEMAND_START
ErrorControl   = 1                      ;SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\mf.sys
LoadOrderGroup = System Bus Extender

[SWIACGPRS.nt.LogConfigOverride]
LogConfig = SWIACGPRS.nt.Override0
LogConfig = SWIACGPRS.nt.Override1
LogConfig = SWIACGPRS.nt.Override2
LogConfig = SWIACGPRS.nt.Override3
LogConfig = SWIACGPRS.nt.Override4
LogConfig = SWIACGPRS.nt.Override5
LogConfig = SWIACGPRS.nt.Override6
LogConfig = SWIACGPRS.nt.Override7

[SWIACGPRS.nt.Override0]    ;COM3
ConfigPriority=NORMAL
IOConfig=3e8-3ef
IOConfig=20@100-FFFF%FFC0
IRQConfig=3,4,5,7,9,10,11
PcCardConfig=5F(W)

[SWIACGPRS.nt.Override1]    ;COM2
ConfigPriority=NORMAL
IOConfig=2f8-2ff
IOConfig=20@100-FFFF%FFC0
IRQConfig=3,4,5,7,9,10,11
PcCardConfig=57(W)

[SWIACGPRS.nt.Override2]    ;COM4
ConfigPriority=NORMAL
IOConfig=2e8-2ef
IOConfig=20@100-FFFF%FFC0
IRQConfig=3,4,5,7,9,10,11
PcCardConfig=67(W)

[SWIACGPRS.nt.Override3]    ;COM1
ConfigPriority=NORMAL
IOConfig=3f8-3ff
IOConfig=20@100-FFFF%FFC0
IRQConfig=3,4,5,7,9,10,11
PcCardConfig=4F(W)

[SWIACGPRS.nt.Override4]    ; Any1
ConfigPriority=NORMAL
IOConfig=8@2020-203F%FFF8,8@20E0-20FF%FFF8,8@2F20-2F3F%FFF8,8@2FE0-2FFF%FFF8,8@4020-403F%FFF8,8@40E0-40FF%FFF8,8@4F20-4F3F%FFF8,8@4FE0-4FFF%FFF8
IOConfig=20@100-FFFF%FFC0
IRQConfig=3,4,5,7,9,10,11
PcCardConfig=6F(W)

[SWIACGPRS.nt.Override5]    ; Any2
ConfigPriority=NORMAL
IOConfig=8@6020-603F%FFF8,8@60E0-60FF%FFF8,8@6F20-6F3F%FFF8,8@6FE0-6FFF%FFF8,8@8020-803F%FFF8,8@80E0-80FF%FFF8,8@8F20-8F3F%FFF8,8@8FE0-8FFF%FFF8
IOConfig=20@100-FFFF%FFC0
IRQConfig=3,4,5,7,9,10,11
PcCardConfig=7F(W)

[SWIACGPRS.nt.Override6]    ; Any3
ConfigPriority=NORMAL
IOConfig=8@A020-A03F%FFF8,8@AFE0-AFFF%FFF8,8@B020-B03F%FFF8,8@BFE0-BFFF%FFF8,8@C020-C03F%FFF8,8@CFE0-CFFF%FFF8,8@D020-D03F%FFF8,8@DFE0-DFFF%FFF8
IOConfig=20@100-FFFF%FFC0
IRQConfig=3,4,5,7,9,10,11
PcCardConfig=47(W)

[SWIACGPRS.nt.Override7]    ; Any4
ConfigPriority=NORMAL
IOConfig=8@E020-E03F%FFF8,8@E0E0-E0FF%FFF8,8@EF20-EF3F%FFF8,8@EFE0-EFFF%FFF8,8@F020-F03F%FFF8,8@F0E0-F0FF%FFF8,8@FF20-FF3F%FFF8,8@FFE0-FFFF%FFF8
IOConfig=20@100-FFFF%FFC0
IRQConfig=3,4,5,7,9,10,11
PcCardConfig=77(W)

[SWIACEDGE.nt]
AddReg = SWIACEDGE.nt.AddReg

[SWIACEDGE.nt.AddReg]

[SWIACEDGE.nt.HW]
AddReg = SWIACEDGE.nt.RegHW

[SWIACEDGE.nt.RegHW]
HKR,Child0000,HardwareID,,MF\AirCardEDGE_DEV0	; Modem
HKR,Child0000,ResourceMap,1,00,02
HKR,Child0001,HardwareID,,MF\AirCardEDGE_DEV1	; net
HKR,Child0001,ResourceMap,1,01,02,03

[SWIACEDGE.nt.Services]
AddService = mf, 2, nt_Services

[SWIACEDGE.nt.LogConfigOverride]
LogConfig = SWIACGPRS.nt.Override0
LogConfig = SWIACGPRS.nt.Override1
LogConfig = SWIACGPRS.nt.Override2
LogConfig = SWIACGPRS.nt.Override3
LogConfig = SWIACGPRS.nt.Override4
LogConfig = SWIACGPRS.nt.Override5
LogConfig = SWIACGPRS.nt.Override6
LogConfig = SWIACGPRS.nt.Override7

[PC7000.nt]
AddReg = PC7000.nt.AddReg

[PC7000.nt.AddReg]

[PC7000.nt.HW]
AddReg = PC7000.nt.RegHW

[PC7000.nt.RegHW]
HKR,Child0000,HardwareID,,MF\PC7000_DEV0	; Modem
HKR,Child0000,ResourceMap,1,00,02
HKR,Child0001,HardwareID,,MF\PC7000_DEV1	; net
HKR,Child0001,ResourceMap,1,01,02,03

[PC7000.nt.Services]
AddService = mf, 2, nt_Services

[PC7000.nt.LogConfigOverride]
LogConfig = SWIACGPRS.nt.Override0
LogConfig = SWIACGPRS.nt.Override1
LogConfig = SWIACGPRS.nt.Override2
LogConfig = SWIACGPRS.nt.Override3
LogConfig = SWIACGPRS.nt.Override4
LogConfig = SWIACGPRS.nt.Override5
LogConfig = SWIACGPRS.nt.Override6
LogConfig = SWIACGPRS.nt.Override7

[PC7200.nt]
AddReg = PC7200.nt.AddReg

[PC7200.nt.AddReg]

[PC7200.nt.HW]
AddReg = PC7200.nt.RegHW

[PC7200.nt.RegHW]
HKR,Child0000,HardwareID,,MF\PC7200_DEV0	; Modem
HKR,Child0000,ResourceMap,1,00,02
HKR,Child0001,HardwareID,,MF\PC7200_DEV1	; net
HKR,Child0001,ResourceMap,1,01,02,03

[PC7200.nt.Services]
AddService = mf, 2, nt_Services

[PC7200.nt.LogConfigOverride]
LogConfig = SWIACGPRS.nt.Override0
LogConfig = SWIACGPRS.nt.Override1
LogConfig = SWIACGPRS.nt.Override2
LogConfig = SWIACGPRS.nt.Override3
LogConfig = SWIACGPRS.nt.Override4
LogConfig = SWIACGPRS.nt.Override5
LogConfig = SWIACGPRS.nt.Override6
LogConfig = SWIACGPRS.nt.Override7

[Strings]
SWI          =  "Sierra Wireless Inc"
SWI_Parent   =  "Sierra Wireless AirCard GPRS Adapter Parent"
SWI_775      =  "Sierra Wireless AirCard EDGE Adapter Parent"
PC7000       =  "PC7000 GPRS Adapter Parent"
PC7200       =  "PC7200 EDGE Adapter Parent"
