;; netrtwlanu.inf 
;;
;; Realtek Wireless 802.11b/g/n USB 2.0 Network Adapter
;;
;; Copyright (C) 2012 Realtek Semiconductor Corp.
;;
;; This release is primarily for WHQL test.
;;

;; FOR XP/Vista/Win7/Win8

[Version]
Signature	= "$Windows NT$"
Class		= Net
ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
Provider	= %Realtek%
CatalogFile.NT	= netrtwlanu.cat		;; for WHQL certified
DriverVer = 09/28/2012,1021.4.0928.2012

[Manufacturer]
%Realtek% = Realtek,NTx86
%PCI% = PCI,NTx86
%Sitecom% = Sitecom,NTx86
%EDIMAX% = EDIMAX,NTx86
%Abocom% = Abocom,NTx86
%Amigo% = Amigo,NTx86
%Hercules% = Hercules,NTx86
%DLink% = DLink,NTx86
%Belkin% = Belkin,NTx86
%Zyxel% = Zyxel,NTx86
%ATKK% = ATKK,NTx86
%TRENDnet% = TRENDnet,NTx86
%Feixun% = Feixun,NTx86
%NetweeN% = NetweeN,NTx86
%XAVI% = XAVI,NTx86
%Netgear% = Netgear,NTx86
%Oar_Inc% = Oar_Inc,NTx86
%ASUS% = ASUS,NTx86
%HAWKING% = HAWKING,NTx86
%Compare% = Compare,NTx86
%IO_DATA% = IO_DATA,NTx86
%Logitec% = Logitec,NTx86
%TPLINK% = TPLINK,NTx86
%Actiontec% = Actiontec,NTx86


[ControlFlags]
ExcludeFromSelect = *

[Realtek.NTx86]
;; For 8192C RTK common		================================================================
%RTL8188cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BFF&PID_8160								; RTK 88CU board for B/G/N      
%RTL8188cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8176								; RTK 88CU board for B/G/N
%RTL8188cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8176&REV_0200&SS
%RTL8188cu_G.DeviceDesc% 			= RTL8192cu_G.ndi, 		USB\VID_0BDA&PID_8177							; RTK 88CU board for B/G
%RTL8188cu_G.DeviceDesc% 			= RTL8192cu_G.ndi, 		USB\VID_0BDA&PID_8177&REV_0200&SS
%RTL8188ce_vau.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8170							; RTK 88CE_VAU board for B/G/N
%RTL8188ce_vau.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8170&REV_0200&SS
%RTL8188ce_vau_G.DeviceDesc% 		= RTL8192cu_G.ndi, 		USB\VID_0BDA&PID_817E						; RTK 88CE_VAU board for B/G
%RTL8188ce_vau_G.DeviceDesc% 		= RTL8192cu_G.ndi, 		USB\VID_0BDA&PID_817E&REV_0200&SS
%RTL8192ce_vau.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_817C							; RTK 92CE_VAU board for B/G/N
%RTL8192ce_vau.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_817C&REV_0200&SS
%RTL8188cu_slim_solo.DeviceDesc% 	= RTL8192cu.ndi, 		USB\VID_0BDA&PID_817A						; RTK slim_solo board for B/G/N
%RTL8188cu_slim_solo.DeviceDesc% 	= RTL8192cu.ndi, 		USB\VID_0BDA&PID_817A&REV_0200&SS
%RTL8188cu_slim_solo_lc.DeviceDesc% = RTL8192cu_wow.ndi, 	USB\VID_0BDA&PID_819A					; LC slim solo for BGN.
%RTL8188cu_slim_solo_lc.DeviceDesc% = RTL8192cu_wow.ndi, 	USB\VID_0BDA&PID_819A&REV_0200&SS
%RTL8188cu_slim_combo.DeviceDesc% 	= RTL8192cu.ndi, 		USB\VID_0BDA&PID_817B					; RTK slim_combo board for B/G/N
%RTL8188cu_slim_combo.DeviceDesc% 	= RTL8192cu.ndi, 		USB\VID_0BDA&PID_817B&REV_0200&SS
%RTL8188ru.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_817F								; RTK 88RU board for B/G/N
%RTL8188ru.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_817F&REV_0200&SS
%RTL8188ru.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_317F								; RTK 88RU board for B/G/N
%RTL8188ru.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_317F&REV_0200&SS
%RTL8188cus_vl.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_818A								; RTK 88RU board for B/G/N
%RTL8188cus_vl.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_818A&REV_0200&SS
%RTL8188cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_103C&PID_1629								; HP/Liteon board for B/G/N
%RTL8192cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8192
%RTL8192cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8178								; RTK 92CU board for B/G/N
%RTL8192cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8178&REV_0200&SS
%RTK_AZ88vau.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_13D3&PID_3358								; AZ 88CE_VAU for B/G/N
%RTK_AZ88vau.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_13D3&PID_3358&REV_0200&SS
%RTK_AZ88vau_G.DeviceDesc% 			= RTL8192cu_G.ndi, 		USB\VID_13D3&PID_3359							; AZ 88CE_VAU for B/G
%RTK_AZ88vau_G.DeviceDesc% 			= RTL8192cu_G.ndi, 		USB\VID_13D3&PID_3359&REV_0200&SS
%RTK_AZ88cus.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_13D3&PID_3357								; AZ 88CUS for B/G/N
%RTK_AZ88cus.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_13D3&PID_3357&REV_0200&SS
%RTL8188ctv.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_018A								; 8188CTV for BGN test only.

;; For 8192D RTK common		================================================================
%RTL8192du.DeviceDesc% 				= RTL8192du.ndi, 	USB\VID_0BDA&PID_8194
%RTL8192du.DeviceDesc%  			= RTL8192du.ndi, 	USB\VID_0BDA&PID_8111
%RTL8192du0.DeviceDesc% 			= RTL8192du0.ndi, 	USB\VID_0BDA&PID_8193&MI_00
%RTL8192du1.DeviceDesc% 			= RTL8192du1.ndi, 	USB\VID_0BDA&PID_8193&MI_01
%RTL8192du2.DeviceDesc% 			= RTL8192du0.ndi, 	USB\VID_0BDA&PID_0193&MI_00
%RTL8192du3.DeviceDesc% 			= RTL8192du1.ndi, 	USB\VID_0BDA&PID_0193&MI_01

;; For 8723 RTK common		================================================================
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_872B
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_8725&MI_02
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_0723&MI_02
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_0724&MI_02
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_0724&REV_0200&MI_02&SS
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_1724&MI_02
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_1724&REV_0200&MI_02&SS
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_A724

;; For 8188E RTK common		================================================================
%RTL8188eu.DeviceDesc%  			= RTL8188eu.ndi, 	USB\VID_0BDA&PID_8179
%RTL8188eu.DeviceDesc%  			= RTL8188eu.ndi, 	USB\VID_0BDA&PID_8179&REV_0200&SS
%RTL8188ee_vau.DeviceDesc%  		= RTL8188eu.ndi, 	USB\VID_0BDA&PID_A179
%RTL8188ee_vau.DeviceDesc%  		= RTL8188eu.ndi, 	USB\VID_0BDA&PID_A179&REV_0200&SS





[PCI.NTx86]
;; For 8192C PCI			================================================================
%PCI.DeviceDesc% 					= RTL8192cu.ndi, 	USB\VID_2019&PID_ED17
%PCI-2.DeviceDesc% 					= RTL8192cu.ndi, 	USB\VID_2019&PID_4902
%PCI_Abocom88cu.DeviceDesc% 		= RTL8192cu.ndi, 	USB\VID_2019&PID_AB2A
%PCI_Abocom92cu.DeviceDesc% 		= RTL8192cu.ndi, 	USB\VID_2019&PID_AB2B
%PCI_Vencer.DeviceDesc% 			= RTL8192cu.ndi, 	USB\VID_2019&PID_1201

;; For 8192D PCI			================================================================
%PCI_Abocom_du0.DeviceDesc% 		= RTL8192du0.ndi,	USB\VID_2019&PID_AB2C&MI_00
%PCI_Abocom_du1.DeviceDesc% 		= RTL8192du1.ndi,	USB\VID_2019&PID_AB2C&MI_01
%PCI_3_du0.DeviceDesc% 				= RTL8192du0.ndi,	USB\VID_2019&PID_4903&MI_00
%PCI_3_du1.DeviceDesc% 				= RTL8192du1.ndi,	USB\VID_2019&PID_4903&MI_01
%PCI_4_du0.DeviceDesc% 				= RTL8192du0.ndi,	USB\VID_2019&PID_4904&MI_00
%PCI_4_du1.DeviceDesc% 				= RTL8192du1.ndi,	USB\VID_2019&PID_4904&MI_01
%PCIWIDI_92DU.DeviceDesc% 			= RTL8192du.ndi, 	USB\VID_2019&PID_AB2D

[Sitecom.NTx86]
;; For 8192C SITECOM			================================================================
%Sitecom.DeviceDesc% 				= RTL8192cu.ndi, USB\VID_0DF6&PID_0052
%Sitecom_UN.DeviceDesc% 			= RTL8192cu.ndi, USB\VID_0DF6&PID_005C
%Sitecom_HG.DeviceDesc% 			= RTL8192cu.ndi, USB\VID_0DF6&PID_0061
%Sitecom_0070.DeviceDesc% 			= RTL8192cu.ndi, USB\VID_0DF6&PID_0070

[EDIMAX.NTx86]
;; For 8192C EDIMAX			================================================================
%EDIMAX.DeviceDesc% 			= RTL8192cu.ndi, 	USB\VID_7392&PID_7811
%EDIMAX300.DeviceDesc% 			= RTL8192cu.ndi, 	USB\VID_7392&PID_7822
;; For 8192D EDIMAX			================================================================
%EDIMAX5G.DeviceDesc% 			= RTL8192du_5G.ndi, 	USB\VID_0BDA&PID_E194

[Abocom.NTx86]
;; For 8192C ABOCOM			================================================================
%Abocom.DeviceDesc% 			= RTL8192cu.ndi, 	USB\VID_07B8&PID_8189
%Abocom92cu.DeviceDesc% 		= RTL8192cu.ndi, 	USB\VID_07B8&PID_8178

[Actiontec.NTx86]
;; For 8192D Actiontec			================================================================
%Actiontec.DeviceDesc% 			= RTL8192du.ndi, 	USB\VID_1668&PID_8102

;; For 8192D ABOCOM			================================================================
%Abocom_92DU0.DeviceDesc% 		= RTL8192du0.ndi, 	USB\VID_07B8&PID_8193&MI_00
%Abocom_92DU1.DeviceDesc% 		= RTL8192du1.ndi, 	USB\VID_07B8&PID_8193&MI_01

[Amigo.NTx86]
;; For 8192C AMIGO			================================================================
%Amigo.DeviceDesc% 				= RTL8192cu.ndi, 	USB\VID_0EB0&PID_9071

[Hercules.NTx86]
;; For 8192C HERCULES		================================================================
%Hercules.DeviceDesc% 			= RTL8192cu.ndi, 	USB\VID_06F8&PID_E033
%Hercules-E035.DeviceDesc% 		= RTL8192cu.ndi, 	USB\VID_06F8&PID_E035

[DLink.NTx86]
;; For 8192C DLINK			================================================================
%DLink-1.DeviceDesc% 			= RTL8192cu.ndi, 	USB\VID_2001&PID_330A
%DLink-2.DeviceDesc% 			= RTL8192cu.ndi, 	USB\VID_2001&PID_3309
%DLink-3.DeviceDesc% 			= RTL8192cu.ndi, 	USB\VID_2001&PID_3308
%DLink-4.DeviceDesc% 			= RTL8192cu.ndi, 	USB\VID_2001&PID_3307
%DLink-5.DeviceDesc% 			= RTL8192cu.ndi, 	USB\VID_2001&PID_330B

%DLink-DWA151.DeviceDesc% 		= RTL8192du.ndi, 	USB\VID_2001&PID_330C

[Belkin.NTx86]
;; For 8192C BELKIN			================================================================
%Belkin.DeviceDesc% 			= Belkin.ndi, 		USB\VID_050D&PID_1102
%Belkin-2.DeviceDesc% 			= Belkin.ndi, 		USB\VID_050D&PID_2102
%Belkin-3.DeviceDesc% 			= Belkin.ndi, 		USB\VID_050D&PID_2103
%Belkin-4.DeviceDesc% 			= Belkin.ndi, 		USB\VID_050D&PID_1004

;; For 8192D BELKIN			================================================================
%Belkin-N600DB.DeviceDesc% 		= BelkinN600.ndi, 	USB\VID_050D&PID_110A
%Belkin-N450DB.DeviceDesc% 		= BelkinN450.ndi, 	USB\VID_050D&PID_1105
%Belkin-N300DB.DeviceDesc% 		= BelkinN300.ndi, 	USB\VID_050D&PID_120A 

[Zyxel.NTx86]
;; For 8192C ZYXEL			================================================================
%Zyxel.DeviceDesc% 				= RTL8192cu.ndi, 	USB\VID_0586&PID_341F

[ATKK.NTx86]
;; For 8192C ATKK			================================================================
%ATKK.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_07AA&PID_0056

[TRENDnet.NTx86]
;; For 8192C TREDENT			================================================================
%TRENDnet.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_20F4&PID_648B
%TRENDnet_2.DeviceDesc% 		= RTL8192cu.ndi, 		USB\VID_20F4&PID_624D

;; For 8192D TREDENT			================================================================
%TRENDnet_3_du.DeviceDesc%		= RTL8192du.ndi, 		USB\VID_20F4&PID_664B

[Feixun.NTx86]
;; For 8192C FEXIUN			================================================================
%Feixun.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_4855&PID_0090				; Feixun 88CUS for B/G/N
%Feixun.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_4855&PID_0091				; Feixun 92CU for B/G/N

[NetweeN.NTx86]
;; For 8192C NETWEEN			================================================================
%NetweeN.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_4856&PID_0091			; Feixun 8188CUS for B/G/N

[XAVI.NTx86]
;; For 8192C XAVI			================================================================
%XAVI.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_04F2&PID_AFF7				; XAVI 88CUSlim solo for B/G/N
%XAVI.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_04F2&PID_AFF9				; XAVI 88CUSlim solo for B/G/N
%XAVI.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_04F2&PID_AFFA				; XAVI 88CUSlim solo for B/G/N
%XAVI88cusc.DeviceDesc% 		= RTL8192cu.ndi, 		USB\VID_04F2&PID_AFF8				; XAVI 88CUSlim combo for B/G/N
%XAVI88cusc.DeviceDesc% 		= RTL8192cu.ndi, 		USB\VID_04F2&PID_AFFB				; XAVI 88CUSlim combo for B/G/N
%XAVI88cusc.DeviceDesc% 		= RTL8192cu.ndi, 		USB\VID_04F2&PID_AFFC				; XAVI 88CUSlim combo for B/G/N

[Netgear.NTx86]
;; For 8192C NETGEAR			================================================================
;;%Netgear.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0846&PID_9041				; Netgear 88CUSfor B/G/N

[Oar_Inc.NTx86]
;; For 8192C OAR			================================================================
%Oar_Inc.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_2019&PID_AB2E

[ASUS.NTx86]
;; For 8192C ASUS			================================================================
%ASUS.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0B05&PID_17AB
%ASUS-2.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0B05&PID_17BA
%ASUS-17C0.DeviceDesc% = RTL8192cu.ndi, USB\VID_0B05&PID_17C0

[HAWKING.NTx86]
;; For 8192C HAWKING			================================================================
%Hawking-1.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0E66&PID_0019
%Hawking-2.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0E66&PID_0020

[Compare.NTx86]
;; For 8192C COMPARE			================================================================
%Compare-1.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_CDAB&PID_8010

[IO_DATA.NTx86]
;; For 8192C COMPARE			================================================================
%IO_DATA_094c.DeviceDesc% 		= RTL8192cu.ndi, USB\VID_04BB&PID_094C
%IO_DATA_0950.DeviceDesc% 		= RTL8192cu.ndi, USB\VID_04BB&PID_0950

[Logitec.NTx86]
;; For 8192D Logitec			================================================================
%Logitec.DeviceDesc%			= RTL8192du_5G.ndi, 	USB\VID_0789&PID_0019

[TPLINK.NTx86]
;; For 8192C COMPARE			================================================================
%TPLINK-0100.DeviceDesc% 		= RTL8192cu.ndi, USB\VID_2357&PID_0100

;;----------------------------------------------------------------------------
;; Realtek default installation
;;----------------------------------------------------------------------------
[RTL8192cu.ndi.NT]
AddReg				= NDIS_51.reg, UsbCommon.reg, RTLWLAN.reg, Ndis5UsbRxAgg.reg, RtlSsOff.reg, 11nWirelessMode.reg, TxByTimerOff.reg, Ndis5Set.reg, BandWidthSetting.reg
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles

[RTL8192cu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog




;;----------------------------------------------------------------------------
;; Realtek G mode sku installation
;;----------------------------------------------------------------------------
[RTL8192cu_G.ndi.NT]
AddReg				= NDIS_51.reg, UsbCommon.reg, Ndis5UsbRxAgg.reg, RtlSsOff.reg, RTLWLAN.reg, Ndis5Set.reg, 11gWirelessMode.reg, BandWidthSetting.reg
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles

[RTL8192cu_G.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog




;;----------------------------------------------------------------------------
;; Realtek N mode wake on wlan sku installation
;;----------------------------------------------------------------------------
[RTL8192cu_wow.ndi.NT]
AddReg				= NDIS_51.reg, UsbCommon.reg, Ndis5UsbRxAgg.reg, RtlSsOff.reg, RTLWLAN.reg, Ndis5Set.reg, 11nWirelessMode.reg, WoWModeOnn.reg,BandWidthSetting.reg
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles

[RTL8192cu_wow.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog




;;----------------------------------------------------------------------------
;; Intel customized installation
;;----------------------------------------------------------------------------

;;----------------------------------------------------------------------------
;; Belkin customized installation
;;----------------------------------------------------------------------------
[Belkin.ndi.NT]
AddReg				= NDIS_51.reg, UsbCommon.reg, Ndis5UsbRxAgg.reg, RtlSsOff.reg, RTLWLAN.reg, Ndis5Set.reg, Belkin.reg, BandWidthSetting.reg
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles

[Belkin.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog





;;----------------------------------------------------------------------------
;; Realtek 8192DU default installation
;;----------------------------------------------------------------------------
[RTL8192du.ndi.NT]
AddReg				= NDIS_51.reg, RTL8192du.common.reg, DUUsbRxAggrSettingOS51.reg, RTLWLAN.reg, Ndis5Set.reg, 2G40MHzAnd5G40MHz.reg
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles

[RTL8192du.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog

[RTL8192du0.ndi.NT]
AddReg				= NDIS_51.reg, RTL8192du.common.reg, DUUsbRxAggrSettingOS51.reg, RTLWLAN.reg, Ndis5Set.reg, 2G40MHzAnd5G40MHz.reg
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles

[RTL8192du0.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog

[RTL8192du1.ndi.NT]
AddReg				= NDIS_51.reg, RTL8192du.common.reg, DUUsbRxAggrSettingOS51.reg, RTLWLAN.reg, Ndis5Set.reg, ConcurrentMode.reg, 2G40MHzAnd5G40MHz.reg
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles

[RTL8192du1.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog




;;----------------------------------------------------------------------------
;; Belkin customized installation
;;----------------------------------------------------------------------------
[BelkinN600.ndi.NT]
AddReg			= NDIS_51.reg, RTL8192du.common.reg, DUUsbRxAggrSettingOS51.reg, RTLWLAN.reg, Ndis5Set.reg, 2G40MHzAnd5G40MHz.reg,BelkinCustomId.reg,Belkin.reg,BandSet.reg
Characteristics		= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles

[BelkinN600.ndi.NT.Services]
AddService		= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog




[BelkinN450.ndi.NT]
AddReg			= NDIS_51.reg, RTL8192du.common.reg, DUUsbRxAggrSettingOS51.reg, RTLWLAN.reg, Ndis5Set.reg, 2G20MHzAnd5G40MHz.reg,BelkinCustomId.reg,Belkin.reg,BandSet.reg
Characteristics		= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles

[BelkinN450.ndi.NT.Services]
AddService		= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog




[BelkinN300.ndi.NT]
AddReg				= NDIS_51.reg, RTL8192du.common.reg, DUUsbRxAggrSettingOS51.reg, RTLWLAN.reg, Ndis5Set.reg, 2G20MHzAnd5G20MHz.reg, BelkinCustomId.reg,Belkin.reg,BandSet.reg
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles

[BelkinN300.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog





;;----------------------------------------------------------------------------
;; 92DU only 5G customized installation
;;----------------------------------------------------------------------------
[RTL8192du_5G.ndi.NT]
AddReg				= NDIS_51.reg, RTL8192du.common.reg, DUUsbRxAggrSettingOS51.reg, RTLWLAN.reg, Ndis5Set.reg, 2G40MHzAnd5G40MHz.reg,BandOnly5G.reg
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles

[RTL8192du_5G.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog




;;----------------------------------------------------------------------------
;; Realtek 8723au default installation
;;----------------------------------------------------------------------------
[RTL8723au.ndi.NT]
AddReg				= NDIS_51.reg, RTL8723au.common.reg, Ndis5UsbRxAgg.reg, RtlSsOff.reg, RAAndIbssSet.reg, RTLWLAN.reg, Ndis5Set.reg, BandWidthSetting.reg
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles

[RTL8723au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog

             


;;----------------------------------------------------------------------------
;; Realtek 8188eu default installation
;;----------------------------------------------------------------------------
[RTL8188eu.ndi.NT]
AddReg				= NDIS_51.reg, UsbCommon.reg, RTLWLAN.reg, Ndis5UsbRxAgg.reg, RtlSsOff.reg, 11nWirelessMode.reg, TxByTimerOff.reg, Ndis5Set.reg, BandWidthSetting.reg
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles

[RTL8188eu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog








;;
;; OS relative registry.
;;
[NDIS_51.reg]
HKR, Ndi\Interfaces,	UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,	LowerRange, 0, "ethernet"
HKR, Ndi,				Service,    0, "RtlWlanu"
;;
;; OS relative service.
;;
[RtlWlanu.Service]
DisplayName    	= %RtlWlanu.DeviceDesc.DispName%
ServiceType    	= 1		; %SERVICE_KERNEL_DRIVER%
StartType      	= 3		; %SERRVICE_DEMAND_START%
ErrorControl   	= 1		; %SERRVICE_ERROR_NORMAL%
ServiceBinary  	= %12%\rtwlanu.sys
LoadOrderGroup 	= NDIS

;;
;; OS relative event log.
;;
[RtlWlanu.EventLog]
AddReg 			= RtlWlanu.AddEventLog.reg

[RtlWlanu.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported  , 0x00010001, 7

;*******************************************************************************
; USB common paramters
;*******************************************************************************
[UsbCommon.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

;; For GPIO detect setting.
HKR,,TimerGPIO,0,"0"
HKR,,GPIODelay,0,"2000"
HKR,,GPIOBack,0,"2000"

;; For PDN mode switch.
HKR,,PDNMode,0,"0"

;; For PDN mode switch.
HKR,,DongleSS,0,"1"

;; For Different selective suspend power save level. Now support 1 and 2. 2 is better.
HKR,,SSPwrLvl,0,"2"

;; For wake on WLAN mode enable.
;;HKR,,WoWLANMode,0,"0"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggBlockCount,0,"8"
HKR,,UsbRxAggBlockCount,0,"8"

HKR,defaults,UsbRxAggBlockTimeout,0,"6"
HKR,,UsbRxAggBlockTimeout,0,"6"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"6"
HKR,,UsbTxAggDescNum,0,"6"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation OS Relative
;-------------------------------------------------------------------------------
[Ndis5UsbRxAgg.reg]
HKR,defaults,UsbRxAggMode,0,"3"
HKR,,UsbRxAggMode,0,"3"
HKR,defaults,UsbRxAggPageCount,0,"72"
HKR,,UsbRxAggPageCount,0,"72"

[Ndis6UsbRxAgg.reg]
HKR,defaults,UsbRxAggMode,0,"2"
HKR,,UsbRxAggMode,0,"2"
HKR,defaults,UsbRxAggPageCount,0,"16"
HKR,,UsbRxAggPageCount,0,"16"

[Ndis5UsbRxAgg_Jaguar.reg]
HKR,defaults,UsbRxAggMode,0,"1"
HKR,,UsbRxAggMode,0,"1"
HKR,defaults,UsbRxAggPageCount,0,"72"
HKR,,UsbRxAggPageCount,0,"72"

[Ndis6UsbRxAgg_Jaguar.reg]
HKR,defaults,UsbRxAggMode,0,"1"
HKR,,UsbRxAggMode,0,"1"
HKR,defaults,UsbRxAggPageCount,0,"16"
HKR,,UsbRxAggPageCount,0,"16"

;-------------------------------------------------------------------------------
;	USB selective suspend.
;-------------------------------------------------------------------------------
[RtlSsOnn.reg]
HKR,,EnableUsbSS,0,"1"
[RtlSsOff.reg]
HKR,,EnableUsbSS,0,"0"

;-------------------------------------------------------------------------------
;	PnP pre-transition handling
;-------------------------------------------------------------------------------
[PnpPreTransOn.reg]
HKR,,PreTransPnP,0,"1"
[PnpPreTransOff.reg]
HKR,,PreTransPnP,0,"0"

;-------------------------------------------------------------------------------
;	TX path selection.
;-------------------------------------------------------------------------------
[TxByTimerOnn.reg]
HKR,,SendPacketByTimer,0,"1"
[TxByTimerOff.reg]
HKR,,SendPacketByTimer,0,"0"

;-------------------------------------------------------------------------------
; Intel Soft AP Mode Reg
;-------------------------------------------------------------------------------
[Intel.reg]
HKR,Ndi\params\ForcedBstDataRate,        ParamDesc,  0, "Broadcast/Multicast Data Rate"
HKR,Ndi\params\ForcedBstDataRate,        type,       0, "enum"
HKR,Ndi\params\ForcedBstDataRate,        default,    0, "0"
HKR,Ndi\params\ForcedBstDataRate\enum,   "0",        0, "Auto"
HKR,Ndi\params\ForcedBstDataRate\enum,   "2",        0, "1Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "4",        0, "2Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "11",      0, "5.5Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "22",     0, "11Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "12",      0, "6Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "18",     0, "9Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "24",     0, "12Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "36",     0, "18Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "48",     0, "24Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "72",     0, "36Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "96",     0, "48Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "108",     0, "54Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "128",     0, "MCS0"
HKR,Ndi\params\ForcedBstDataRate\enum,   "129",     0, "MCS1"
HKR,Ndi\params\ForcedBstDataRate\enum,   "130",     0, "MCS2"
HKR,Ndi\params\ForcedBstDataRate\enum,   "131",     0, "MCS3"
HKR,Ndi\params\ForcedBstDataRate\enum,   "132",     0, "MCS4"
HKR,Ndi\params\ForcedBstDataRate\enum,   "133",     0, "MCS5"
HKR,Ndi\params\ForcedBstDataRate\enum,   "134",     0, "MCS6"
HKR,Ndi\params\ForcedBstDataRate\enum,   "135",     0, "MCS7"
HKR,Ndi\params\ForcedBstDataRate\enum,   "136",     0, "MCS8"
HKR,Ndi\params\ForcedBstDataRate\enum,   "137",     0, "MCS9"
HKR,Ndi\params\ForcedBstDataRate\enum,   "138",     0, "MCS10"
HKR,Ndi\params\ForcedBstDataRate\enum,   "139",     0, "MCS11"
HKR,Ndi\params\ForcedBstDataRate\enum,   "140",     0, "MCS12"
HKR,Ndi\params\ForcedBstDataRate\enum,   "141",     0, "MCS13"
HKR,Ndi\params\ForcedBstDataRate\enum,   "142",     0, "MCS14"
HKR,Ndi\params\ForcedBstDataRate\enum,   "143",     0, "MCS15"

;*******************************************************************************
; RTL8192du common paramters
;*******************************************************************************
[RTL8192du.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

;; For Earlymode 1:Enable 0:Disable
HKR,,bEarlymodeEnable,,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

HKR,defaults,SupportTxPacketBufferColease,0,"0"
HKR,,SupportTxPacketBufferColease,0,"0"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggBlockCount,0,"18"
HKR,,UsbRxAggBlockCount,0,"18"

HKR,defaults,UsbRxAggBlockTimeout,0,"7"
HKR,,UsbRxAggBlockTimeout,0,"7"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"4"
HKR,,UsbTxAggDescNum,0,"4"

[DUUsbRxAggrSettingOS51.reg]
HKR,defaults,UsbRxAggMode,0,"2"
HKR,,UsbRxAggMode,0,"2"

HKR,defaults,UsbRxAggPageCount,0,"72"
HKR,,UsbRxAggPageCount,0,"72"

;*******************************************************************************
; RTL8723au common paramters
;*******************************************************************************
[RTL8723au.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

;; For GPIO detect setting.
HKR,,TimerGPIO,0,"0"
HKR,,GPIODelay,0,"1000"
HKR,,GPIOBack,0,"1000"

;; For PDN mode switch.
HKR,,PDNMode,0,"1"

;; For PDN mode switch.
HKR,,DongleSS,0,"1"

HKR,,bLowPowerEnable,0,"0"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggBlockCount,0,"8"
HKR,,UsbRxAggBlockCount,0,"8"

HKR,defaults,UsbRxAggBlockTimeout,0,"6"
HKR,,UsbRxAggBlockTimeout,0,"6"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"6"
HKR,,UsbTxAggDescNum,0,"6"


[RAAndIbssSet.reg]
HKR,defaults,WiFi11bIbss,0,"0"
HKR,,WiFi11bIbss,0,"0"

HKR,defaults,bRateAdaptive,0,"1"
HKR,,bRateAdaptive,0,"1"


;;----------------------------------------------------------------------------
;; Realtek WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTLWLAN.reg]
HKR,defaults,SSID,0,"ANY"
HKR,,SSID,0,"ANY"

HKR,defaults,Channel,0,"1"
HKR,,Channel,0,"1"

;; Antenna Diversity Type
HKR,Ndi\params\AntennaDivType, 	default, 	0, "1"
HKR,Ndi\params\AntennaDivType,	ParamDesc, 	0, "Antenna Diversity Type"
HKR,Ndi\params\AntennaDivType, 	type, 		0, "int"
HKR,Ndi\params\AntennaDivType, 	min, 		0, "1"
HKR,Ndi\params\AntennaDivType, 	max, 		0, "3"
HKR,Ndi\params\AntennaDivType, 	step, 		0, "1"

;;HKR,Ndi\params\NetworkType,			ParamDesc,  0, %NETWORK_TYPE_STR%
;;HKR,Ndi\params\NetworkType,			type,       0, "enum"
;;HKR,Ndi\params\NetworkType,			default,    0, "1"
;;HKR,Ndi\params\NetworkType\enum,		"0",        0, %AD_HOC_STR%
;;HKR,Ndi\params\NetworkType\enum,		"1",        0, %INFRASTRUCTURE_STR%
;;HKR,Ndi\params\NetworkType\enum,		"2",        0, %AUTO_SELECT%
;;HKR,defaults,NetworkType,0,"1"
;;HKR,,NetworkType,0,"1"

HKR,defaults,StaUapsd,0,"0"
HKR,,StaUapsd,0,"0"

; For B/G mode and B/G/N mode switch, we will use different wireless mode registry in later section
;HKR,Ndi\params\WirelessMode, 			ParamDesc, 	0, %WL_MODE_STR%
;HKR,Ndi\params\WirelessMode, 			type, 		0, "enum"
;HKR,Ndi\params\WirelessMode, 			default, 	0, "8"
;HKR,Ndi\params\WirelessMode\enum, 		"2", 		0, %IEEE_802_11B_STR%
;HKR,Ndi\params\WirelessMode\enum, 		"4", 		0, %IEEE_802_11BG_STR%
;HKR,Ndi\params\WirelessMode\enum, 		"8", 		0, %IEEE_802_11BGN_STR%
;HKR,defaults,WirelessMode, 0, "8"
;HKR,,WirelessMode, 0, "8"

;; For WiFi test, 1: WiFi Config and 0: Performance Config
HKR,Ndi\params\WiFiConfg,        ParamDesc,  0, "WiFi Config"
HKR,Ndi\params\WiFiConfg,        type,       0, "enum"
HKR,Ndi\params\WiFiConfg,        default,    0, "0"
HKR,Ndi\params\WiFiConfg\enum,   "0",        0, "Performance"
HKR,Ndi\params\WiFiConfg\enum,   "1",        0, "WiFi"
HKR,defaults,WiFiConfg,0,"0"
HKR,,WiFiConfg,0,"0"
HKR,,WiFiConfg,,"0"

HKR,defaults,RxReorder,0,"1"
HKR,,RxReorder,0,"1"

HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""

;Leisure Power Save
HKR,defaults,bLeisurePs,0,"2"
HKR,,bLeisurePs,0,"2"

;Fw Control LPS
HKR,defaults,bFwCtrlLPS,0,"1"
HKR,,bFwCtrlLPS,0,"1"

;; LPS Interval
;HKR,defaults,LPSIntvl,0,"5"
HKR,,LPSIntvl,0,"5"

;BTmode
HKR,,bBTMode,0,"1"

; Reset Tx Hang
HKR,defaults,USBResetTxHang,0,"1"
HKR,,USBResetTxHang,0,"1"

HKR,,WEPinNmode,0,"0"

; OS protocol offload detection and decision
HKR,,ProtocolOffloadDecision,0,"1"

; Win8 FSS mode detection mechanism
HKR,,FSSDetection,0,"1"

;-------------------------------------------------------------------------------
;	Some function ability setting
;-------------------------------------------------------------------------------
HKR,defaults,UPDMEnable,0,"1"
HKR,,UPDMEnable,0,"1"

HKR,defaults,LinkSpeedLevel,0,"0"
HKR,,LinkSpeedLevel,0,"0"

HKR,defaults,AutoConnect,0,"1"
HKR,,AutoConnect,0,"1"

HKR,defaults,RWRetry,0,"0"
HKR,,RWRetry,0,"0"

HKR,defaults,MultiMode,0,"1"
HKR,,MultiMode,0,"1"

HKR,defaults,TxMode,0,"0"
HKR,,TxMode,0,"0"

HKR,defaults,PwrTblSel,0,"0"
HKR,,PwrTblSel,0,"0"
HKR,defaults,PwrByRate,0,"0"
HKR,,PwrByRate,0,"0"
HKR,defaults,PwrRaTbl1,0,"0"
HKR,,PwrRaTbl1,0,"0"
HKR,defaults,PwrRaTbl2,0,"0"
HKR,,PwrRaTbl2,0,"0"
HKR,defaults,PwrRaTbl3,0,"0"
HKR,,PwrRaTbl3,0,"0"
HKR,defaults,PwrRaTbl4,0,"0"
HKR,,PwrRaTbl4,0,"0"
HKR,defaults,PwrRaTbl5,0,"0"
HKR,,PwrRaTbl5,0,"0"
HKR,defaults,PwrRaTbl6,0,"0"
HKR,,PwrRaTbl6,0,"0"
HKR,defaults,PwrRaTbl7,0,"0"
HKR,,PwrRaTbl7,0,"0"
HKR,defaults,PwrRaTbl8,0,"0"
HKR,,PwrRaTbl8,0,"0"
HKR,defaults,PwrRaTbl9,0,"0"
HKR,,PwrRaTbl9,0,"0"
HKR,defaults,PwrRaTbl10,0,"0"
HKR,,PwrRaTbl10,0,"0"
HKR,defaults,PwrRaTbl11,0,"0"
HKR,,PwrRaTbl11,0,"0"
HKR,defaults,PwrRaTbl12,0,"0"
HKR,,PwrRaTbl12,0,"0"
HKR,defaults,PwrRaTbl13,0,"0"
HKR,,PwrRaTbl13,0,"0"
HKR,defaults,PwrRaTbl14,0,"0"
HKR,,PwrRaTbl14,0,"0"
HKR,defaults,PwrRaTbl15,0,"0"
HKR,,PwrRaTbl15,0,"0"
HKR,defaults,PwrRaTbl16,0,"0"
HKR,,PwrRaTbl16,0,"0"

HKR,defaults,GainOffsetFCCLow,0,"0"
HKR,,GainOffsetFCCLow,0,"0"
HKR,defaults,GainOffsetFCC,0,"0"
HKR,,GainOffsetFCC,0,"0"
HKR,defaults,GainOffsetFCCHigh,0,"0"
HKR,,GainOffsetFCCHigh,0,"0"

HKR,defaults,GainOffsetMKKLow,0,"0"
HKR,,GainOffsetMKKLow,0,"0"
HKR,defaults,GainOffsetMKK,0,"0"
HKR,,GainOffsetMKK,0,"0"
HKR,defaults,GainOffsetMKKHigh,0,"0"
HKR,,GainOffsetMKKHigh,0,"0"

HKR,defaults,GainOffsetETSILow,0,"0"
HKR,,GainOffsetETSILow,0,"0"
HKR,defaults,GainOffsetETSI,0,"0"
HKR,,GainOffsetETSI,0,"0"
HKR,defaults,GainOffsetETSIHigh,0,"0"
HKR,,GainOffsetETSIHigh,0,"0"

HKR,defaults,RxSC,0,"0"
HKR,,RxSC,0,"0"

HKR,defaults,TxSC,0,"0"
HKR,,TxSC,0,"0"

;Dynamic batch indication
HKR,defaults,DynamicBatchEnable,0,"1"
HKR,,DynamicBatchEnable,0,"1"

HKR,defaults,BINumber,0,"10"
HKR,,BINumber,0,"10"

[Ndis5Set.reg]
HKR,Ndi\params\PSPXlinkMode,			ParamDesc,  0, %PSP_XLINK_STR%
HKR,Ndi\params\PSPXlinkMode,			type,       0, "enum"
HKR,Ndi\params\PSPXlinkMode,			default,    0, "0"
HKR,Ndi\params\PSPXlinkMode\enum,		"0",        0, %DISABLE_STR%
HKR,Ndi\params\PSPXlinkMode\enum,		"1",        0, %ENABLE_STR%
HKR,defaults,PSPXlinkMode,0,"0"
HKR,,PSPXlinkMode,0,"0"

; Hw Beacon Max Error
HKR,,bBcnMaxErrorRegEnable,0,"0"

;Inactive Power Save
HKR,defaults,InactivePs,0,"0"
HKR,,InactivePs,0,"0"

HKR,defaults,AggDMEnable,0,"0"
HKR,,AggDMEnable,0,"0"

[Ndis6Set.reg]
;Inactive Power Save
HKR,defaults,InactivePs,0,"2"
HKR,,InactivePs,0,"2"

HKR,defaults,AggDMEnable,0,"1"
HKR,,AggDMEnable,0,"1"

; /****************************************************************************
; ** IHV Service Reg for CCX
; ****************************************************************************/
[CIHVS.reg]
HKR, Ndi\IHVExtensions, ExtensibilityDLL,       0,  "%SystemRoot%\system32\Rtlihvs.dll"
HKR, Ndi\IHVExtensions, UIExtensibilityCLSID,   0,  "{6C2A8CCA-B2A2-4d81-A3B2-4E15F445C312}"
HKR, Ndi\IHVExtensions, GroupName,              0,  "Realtek CCX SDK IHV Service"
HKR, Ndi\IHVExtensions, AdapterOUI,             0x00010001, 0x00e04c

;;----------------------------------------------------------------------------
;; Belkin WLAN NIC parameters
;;----------------------------------------------------------------------------
[Belkin.reg]
HKR,Ndi\params\RFOff,			ParamDesc,  0, "Radio"
HKR,Ndi\params\RFOff,			type,       0, "enum"
HKR,Ndi\params\RFOff,			default,    0, "0"
HKR,Ndi\params\RFOff\enum,		"0",        0, "On"
HKR,Ndi\params\RFOff\enum,		"1",        0, "Off"
HKR,defaults,RFOff,0,"0"
HKR,,RFOff,0,"0"

;;----------------------------------------------------------------------------
;; Wireless mode option parameters
;;----------------------------------------------------------------------------
[11gWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,defaults,WirelessMode, 0, "4"
HKR,,WirelessMode, 0, "4"

[11nWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %IEEE_802_11BGN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

[11acWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "64"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"16", 		0, %IEEE_802_11BGN_STR%
HKR,Ndi\params\WirelessMode\enum, 	"64", 		0, %IEEE_802_11ANAC_STR%
HKR,defaults,WirelessMode, 0, "64"
HKR,,WirelessMode, 0, "64"

HKR,defaults,BW40MHz,0,"1"
HKR,,BW40MHz,0,"1"

HKR,defaults,BW80MHz,0,"1"
HKR,,BW80MHz,0,"1"


;;----------------------------------------------------------------------------
;; Wake on Wlan mode option parameters
;;----------------------------------------------------------------------------
[WoWModeOnn.reg]
;;HKR,Ndi\params\WoWLANMode, 		ParamDesc, 	0, %WOW_MODE_STR%
;;HKR,Ndi\params\WoWLANMode, 		type, 		0, "enum"
;;HKR,Ndi\params\WoWLANMode, 		default, 	0, "1"
;;HKR,Ndi\params\WoWLANMode\enum, 	"0", 		0, %WOW_DISABLE%
;;HKR,Ndi\params\WoWLANMode\enum, 	"1", 		0, %WOW_ENABLE_MAGIC_PKT%
;;HKR,Ndi\params\WoWLANMode\enum, 	"2", 		0, %WOW_ENABLE_PATTERN_PKT%
;;HKR,Ndi\params\WoWLANMode\enum, 	"3", 		0, %WOW_ENABLE_MAGIC_PATTERN_PKT%
HKR,defaults,WoWLANMode, 0, "1"
HKR,,WoWLANMode, 0, "1"

; ARP Offload
HKR,,ARPOffloadEnable, 0, "1"

; GTK Offload
HKR,,GTKOffloadEnable, 0, "1"

[WoWModeOff.reg]
;;HKR,Ndi\params\WoWLANMode, 		ParamDesc, 	0, %WOW_MODE_STR%
;;HKR,Ndi\params\WoWLANMode, 		type, 		0, "enum"
;;HKR,Ndi\params\WoWLANMode, 		default, 	0, "0"
;;HKR,Ndi\params\WoWLANMode\enum, 	"0", 		0, %WOW_DISABLE%
;;HKR,Ndi\params\WoWLANMode\enum, 	"1", 		0, %WOW_ENABLE_MAGIC_PKT%
;;HKR,Ndi\params\WoWLANMode\enum, 	"2", 		0, %WOW_ENABLE_PATTERN_PKT%
;;HKR,Ndi\params\WoWLANMode\enum, 	"3", 		0, %WOW_ENABLE_MAGIC_PATTERN_PKT%
HKR,defaults,WoWLANMode, 0, "0"
HKR,,WoWLANMode, 0, "0"


;;----------------------------------------------------------------------------
;; Usb selective suspend parameters
;;----------------------------------------------------------------------------
[NdisSS.reg]
HKR,Ndi\params\*SelectiveSuspend,	    ParamDesc,  0, %SelectiveSuspend%
HKR,Ndi\params\*SelectiveSuspend,	    default,    0, "1"
HKR,Ndi\params\*SelectiveSuspend,	    type,       0, "enum"
HKR,Ndi\params\*SelectiveSuspend\enum,   "0",        0, "Disabled"
HKR,Ndi\params\*SelectiveSuspend\enum,   "1",        0, "Enabled"

HKR,Ndi\params\*SSIdleTimeout,	    ParamDesc,  0, %SSIdleTimeout%
HKR,Ndi\params\*SSIdleTimeout,	    type,       0, "int"
HKR,Ndi\params\*SSIdleTimeout,	    default,    0, "30"
HKR,Ndi\Params\*SSIdleTimeout,      Max,        0, "60"
HKR,Ndi\Params\*SSIdleTimeout,      Min,        0, "5"
HKR,Ndi\Params\*SSIdleTimeout,      Step,       0, "1"


;*******************************************************************************
; Two STA Concurrent Mode Reg
;*******************************************************************************
[ConcurrentMode.reg]
HKR,Ndi\params\TwoStaConcurrentMode,		ParamDesc,  0, %TWO_STA_CONCURRENT_MODE%
HKR,Ndi\params\TwoStaConcurrentMode,		type,       0, "enum"
HKR,Ndi\params\TwoStaConcurrentMode,			default,    0, "1"
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"0",        0, %SECONDARY_DISABLE%
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"1",        0, %SECONDARY_ENABLE%
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"2",        0, %SECONDARY_AUTO%
HKR,defaults,TwoStaConcurrentMode,0,"0"
HKR,,TwoStaConcurrentMode,0,"0"

;*******************************************************************************
; bandwidth setting
;*******************************************************************************
[2G40MHzAnd5G40MHz.reg]
HKR,Ndi\params\BW40MHzFor2G,        ParamDesc,  0, "Bandwidth_2.4G"
HKR,Ndi\params\BW40MHzFor2G,        type,       0, "enum"
HKR,Ndi\params\BW40MHzFor2G,        default,    0, "1"
HKR,Ndi\params\BW40MHzFor2G\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor2G\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHzFor2G,0,"1"
HKR,,BW40MHzFor2G,0,"1"
HKR,,BW40MHzFor2G,,"1"

HKR,Ndi\params\BW40MHzFor5G,        ParamDesc,  0, "Bandwidth_5G"
HKR,Ndi\params\BW40MHzFor5G,        type,       0, "enum"
HKR,Ndi\params\BW40MHzFor5G,        default,    0, "1"
HKR,Ndi\params\BW40MHzFor5G\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor5G\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,,"1"

[2G20MHzAnd5G40MHz.reg]
HKR,defaults,BW40MHzFor2G,0,"0"
HKR,,BW40MHzFor2G,0,"0"

HKR,Ndi\params\BW40MHzFor5G,        ParamDesc,  0, "Bandwidth_5G"
HKR,Ndi\params\BW40MHzFor5G,        type,       0, "enum"
HKR,Ndi\params\BW40MHzFor5G,        default,    0, "1"
HKR,Ndi\params\BW40MHzFor5G\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor5G\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,,"1"

[2G20MHzAnd5G20MHz.reg]
HKR,defaults,BW40MHzFor2G,0,"0"
HKR,,BW40MHzFor2G,0,"0"

HKR,defaults,BW40MHzFor5G,0,"0"
HKR,,BW40MHzFor5G,0,"0"

[BandWidthSetting.reg]
;; 40MHz Support in 11n
HKR,Ndi\params\BW40MHz,        ParamDesc,  0, "Bandwidth"
HKR,Ndi\params\BW40MHz,        type,       0, "enum"
HKR,Ndi\params\BW40MHz,        default,    0, "1"
HKR,Ndi\params\BW40MHz\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHz\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHz,0,"1"
HKR,,BW40MHz,0,"1"
HKR,,BW40MHz,,"1"

[BelkinCustomId.reg]
HKR,,CustomerID,0,"21"
HKR,,CustomerID,,"21"

[BandSet.reg]
HKR,Ndi\params\WirelessBand,			ParamDesc,  0, "Disable Bands"
HKR,Ndi\params\WirelessBand,			type,       0, "enum"
HKR,Ndi\params\WirelessBand,			default,    0, "0"
HKR,Ndi\params\WirelessBand\enum,		"0",        0, "Disable 11A"
HKR,Ndi\params\WirelessBand\enum,		"1",        0, "Disable 11B/G"
HKR,Ndi\params\WirelessBand\enum,		"2",        0, "None"
HKR,defaults,WirelessBand,0,"2"
HKR,,WirelessBand,0,"2"


[BandOnly5G.reg]
HKR,defaults,WirelessBand,0,"1"
HKR,,WirelessBand,0,"1"
;*******************************************************************************
; Destination Directory
;*******************************************************************************
[RTWlanU.CopyFiles]
RTWlanU.sys,,,2

[DestinationDirs]
DefaultDestDir     	= 11
RTWlanU.CopyFiles	= 12


;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksFiles]
RTWlanU.sys = 1

[SourceDisksNames]
1=%DISKNAME%,,,


;*******************************************************************************
; Strings
;*******************************************************************************
[Strings]
SSID_STR					= "SSID"
CHANNEL_STR					= "Channel"
NETWORK_TYPE_STR			= "Network Type"
LED_CONTROL_STR				= "LED Control" 
POWER_SAVE_STR				= "Power Save Mode"
WIFI_IBSS_STR				= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR			= "Rate Adaptive"
QOS_STR						= "QoS"
WiFiConfg_STR	  			= "WiFiConfg"
WMM_APSD					= "WMM APSD"
CCX_RM_STR					= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line Measurement (0: unlimited)"
FORCE_PRIORITY_STR			= "Forced Priority"
HW_PARA_STR					= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR						= "Transmit Power Control"
TPC_POLARITY_STR			= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "PSP XLink Mode"
DISABLE_STR					= "Disable"
ENABLE_STR					= "Enable"
AD_HOC_STR					= "Ad Hoc"
INFRASTRUCTURE_STR			= "Infrastructure"
AUTO_SELECT					= "Auto select"
WL_MODE_STR					= "Wireless Mode"
RX_REORDER_STR				= "Rx Reorder"
CAM_STR						= "CAM"
MAX_PSP_STR					= "MAX_PSP"
Fast_PSP_STR				= "Fast_PSP"
NO_AC_STR					= "No AC (Disable)"
ALL_AC_STR					= "ALL AC"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
SelectiveSuspend               		= "Selective suspend"
SSIdleTimeout                  		= "Selective suspend Timeout"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation strings
;-------------------------------------------------------------------------------
RX_AGG_MODE_STR				= "Rx Aggregation Mode"
RX_AGG_MODE_BLOCK_STR		= "Rx Agg USB Block Mode"
RX_AGG_MODE_PAGE_STR		= "Rx Agg DMA Page Mode"
RX_AGG_MODE_MIXED_STR		= "Rx Agg USB and Page Mixed Mode"
RX_AGG_USB_BLOCK_STR		= "Rx Agg USB Block Threshold"
RX_AGG_USB_TIMEOUT_STR		= "Rx Agg USB Timeout"
RX_AGG_DMA_PAGE_STR			= "Rx Agg DMA Page Threshold"
RX_AGG_DMA_TIMEOUT_STR		= "Rx Agg DMA Timeout"
TX_AGG_MODE_STR				= "Tx Aggregation Mode"
TX_AGG_DESC_PER_OUT_STR		= "Tx Agg Number of descriptor per bulk out"

;-------------------------------------------------------------------------------
;	Two STA Concurrent Mode
;-------------------------------------------------------------------------------
TWO_STA_CONCURRENT_MODE		= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"

;*******************************************************************************
; manufacture description
;*******************************************************************************
Realtek					= "Realtek Semiconductor Corp."
PCI             		= "PLANEX COMMUNICATIONS INC"
Sitecom         		= "Sitecom Europe B.V."
EDIMAX         			= "EDIMAX"
Abocom					= "AboCom System, Inc."
Amigo					= "Amigo Technology Inc"
Hercules				= "Guillemot Corporation S.A"
DLink					= "D-Link Corporation"
Belkin					= "Belkin International, Inc."
Zyxel					= "ZyXEL"
ATKK					= "Allied Telesis K.K."
TRENDnet				= "TRENDnet"
Feixun					= "Shanghai Feixun Communication Co.,Ltd"
NetweeN					= "NetweeN"
XAVI					= "XAVI Technologies Corp."
Netgear					= "NETGEAR Inc."
Oar_Inc					= "Oar Inc."
ASUS					= "ASUSTeK Computer Inc."
HAWKING					= "Hawking Technologies Inc."
Compare					= "Compare Electronics CO.,LTD"
IO_DATA					= "I-O DATA DEVICE, INC"
Logitec					= "Logitec Japan"
TPLINK					= "TP-LINK Technologies Co."
Actiontec				= "Actiontec"

;*******************************************************************************
;	Source disk name
;*******************************************************************************
;DISKNAME							= "Realtek RTL8192CU Wireless LAN 802.11n USB 2.0 Network Adapter Driver Disk"
DISKNAME							= "Realtek Wireless LAN 802.11n USB 2.0 Network Adapter Driver Disk"
RtlWlanu.DeviceDesc 				= "Realtek Wireless LAN 802.11n USB 2.0 Network Adapter"
RtlWlanu.DeviceDesc.DispName		= "Realtek Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8192cu.DeviceDesc 				= "Realtek RTL8192CU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8192cu.DeviceDesc.DispName		= "Realtek RTL8192CU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188cu.DeviceDesc 				= "Realtek RTL8188CU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188cu.DeviceDesc.DispName		= "Realtek RTL8188CU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188cu_G.DeviceDesc 				= "Realtek RTL8188CU Wireless LAN 802.11 USB 2.0 Network Adapter"
RTL8188cu_G.DeviceDesc.DispName		= "Realtek RTL8188CU Wireless LAN 802.11 USB 2.0 Network Adapter"
RTL8188ce_vau.DeviceDesc 			= "Realtek RTL8188CE-VAU Wireless LAN 802.11n USB minicard"
RTL8188ce_vau.DeviceDesc.DispName	= "Realtek RTL8188CE-VAU Wireless LAN 802.11n USB minicard"
RTL8188ce_vau_G.DeviceDesc 			= "Realtek RTL8188CE-VAU Wireless LAN 802.11 USB minicard"
RTL8188ce_vau_G.DeviceDesc.DispName	= "Realtek RTL8188CE-VAU Wireless LAN 802.11 USB minicard"
RTL8192ce_vau.DeviceDesc 			= "Realtek RTL8192CE-VAU Wireless LAN 802.11n USB minicard"
RTL8192ce_vau.DeviceDesc.DispName	= "Realtek RTL8192CE-VAU Wireless LAN 802.11n USB minicard"
RTL8188cu_slim_solo.DeviceDesc				= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
RTL8188cu_slim_solo.DeviceDesc.DispName		= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
RTL8188cu_slim_solo_lc.DeviceDesc			= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
RTL8188cu_slim_solo_lc.DeviceDesc.DispName	= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
RTL8188cu_slim_combo.DeviceDesc				= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Combo"
RTL8188cu_slim_combo.DeviceDesc.DispName	= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Combo"
RTL8188ru.DeviceDesc 				= "Realtek RTL8188RU Wireless LAN 802.11n USB High Power Dongle"
RTL8188ru.DeviceDesc.DispName		= "Realtek RTL8188RU Wireless LAN 802.11n USB High Power Dongle"
RTL8188cus_vl.DeviceDesc 			= "Realtek RTL8188CUS-VL Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188cus_vl.DeviceDesc.DispName	= "Realtek RTL8188CUS-VL Wireless LAN 802.11n USB 2.0 Network Adapter"
RTK_AZ88vau.DeviceDesc				= "Realtek RTL8188CE-VAU Wireless LAN 802.11n USB minicard"
RTK_AZ88vau.DeviceDesc.DispName		= "Realtek RTL8188CE-VAU Wireless LAN 802.11n USB minicard"
RTK_AZ88vau_G.DeviceDesc			= "Realtek RTL8188CE-VAU Wireless LAN 802.11 USB minicard"
RTK_AZ88vau_G.DeviceDesc.DispName	= "Realtek RTL8188CE-VAU Wireless LAN 802.11 USB minicard"
RTK_AZ88cus.DeviceDesc				= "Wireless USB Card"
RTK_AZ88cus.DeviceDesc.DispName		= "Wireless USB Card"
RTL8188ctv.DeviceDesc				= "Realtek RTL8188CTV Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188ctv.DeviceDesc.DispName		= "Realtek RTL8188CTV Wireless LAN 802.11n USB 2.0 Network Adapter"
PCI.DeviceDesc 						= "GW-USValue-EZ"
PCI.DeviceDesc.DispName				= "GW-USValue-EZ"
PCI-2.DeviceDesc 					= "GW-USLight"
PCI-2.DeviceDesc.DispName			= "GW-USLight"
PCI_Abocom88cu.DeviceDesc 			= "GW-USNano2"
PCI_Abocom88cu.DeviceDesc.DispName	= "GW-USNano2"
PCI_Abocom92cu.DeviceDesc 			= "GW-USEco300"
PCI_Abocom92cu.DeviceDesc.DispName	= "GW-USEco300"
PCI_Vencer.DeviceDesc 				= "BT-Micro3H2X Wireless LAN"
PCI_Vencer.DeviceDesc.DispName		= "BT-Micro3H2X Wireless LAN"
Sitecom.DeviceDesc 					= "Sitecom Wireless Ultra Nano USB Adapter 150N X1 WL-365"
Sitecom.DeviceDesc.DispName			= "Sitecom Wireless Ultra Nano USB Adapter 150N X1 WL-365"
Sitecom_UN.DeviceDesc 				= "Wireless Ultra Nano Network Adapter 150N"
Sitecom_UN.DeviceDesc.DispName		= "Wireless Ultra Nano Network Adapter 150N"
Sitecom_HG.DeviceDesc 				= "Wireless High-gain Network adapter 300N WLA-4001"
Sitecom_HG.DeviceDesc.DispName		= "Wireless High-gain Network adapter 300N WLA-4001"
Sitecom_0070.DeviceDesc 				= "WiFi USB adapter N300"
Sitecom_0070.DeviceDesc.DispName			= "WiFi USB adapter N300"
EDIMAX.DeviceDesc 					= "150Mbps Wireless 802.11b/g/n Nano USB Adapter"
EDIMAX.DeviceDesc.DispName			= "150Mbps Wireless 802.11b/g/n Nano USB Adapter"
EDIMAX300.DeviceDesc 				= "Edimax 300Mbps wireless 802.11b/g/n USB adapter"
EDIMAX300.DeviceDesc.DispName		= "Edimax 300Mbps wireless 802.11b/g/n USB adapter"
Abocom.DeviceDesc 					= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Abocom.DeviceDesc.DispName			= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Abocom92cu.DeviceDesc				= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Abocom92cu.DeviceDesc.DispName		= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Amigo.DeviceDesc 					= "Wireless USB Card"
Amigo.DeviceDesc.DispName			= "Wireless USB Card"
Hercules.DeviceDesc 				= "Hercules Wireless N Pico USB "
Hercules.DeviceDesc.DispName		= "Hercules Wireless N Pico USB "
Hercules-E035.DeviceDesc 			= "Hercules Wireless N Mini v2 USB Key"
Hercules-E035.DeviceDesc.DispName	= "Hercules Wireless N Mini v2 USB Key"
DLink-1.DeviceDesc 					= "D-Link DWA-133 Wireless N USB Adapter"
DLink-1.DeviceDesc.DispName			= "D-Link DWA-133 Wireless N USB Adapter"
DLink-2.DeviceDesc 					= "D-Link DWA-135 Wireless N USB Adapter"
DLink-2.DeviceDesc.DispName			= "D-Link DWA-135 Wireless N USB Adapter"
DLink-3.DeviceDesc 					= "D-Link DWA-121 Wireless N USB Adapter"
DLink-3.DeviceDesc.DispName			= "D-Link DWA-121 Wireless N USB Adapter"
DLink-4.DeviceDesc 					= "D-Link DWA-130 Wireless N USB Adapter(rev.F1)"
DLink-4.DeviceDesc.DispName			= "D-Link DWA-130 Wireless N USB Adapter(rev.F1)"
DLink-5.DeviceDesc 					= "D-Link DWA-123 Wireless N 150 USB Adapter(rev.C)"
DLink-5.DeviceDesc.DispName			= "D-Link DWA-123 Wireless N 150 USB Adapter(rev.C)"
Belkin.DeviceDesc 					= "Surf Wireless Micro USB Adapter"
Belkin.DeviceDesc.DispName			= "Surf Wireless Micro USB Adapter"
Belkin-2.DeviceDesc 				= "Belkin Surf & Share Wireless USB Adapter"
Belkin-2.DeviceDesc.DispName		= "Belkin Surf & Share Wireless USB Adapter"
Belkin-3.DeviceDesc 				= "N300 USB Network Adapter"
Belkin-3.DeviceDesc.DispName		= "N300 USB Network Adapter"
Belkin-4.DeviceDesc 				= "Belkin Wireless Adapter"
Belkin-4.DeviceDesc.DispName		= "Belkin Wireless Adapter"
ZyXEL.DeviceDesc 					= "ZyXEL Wireless LAN 802.11n USB 2.0 Network Adapter"
ZyXEL.DeviceDesc.DispName			= "ZyXEL Wireless LAN 802.11n USB 2.0 Network Adapter"
ATKK.DeviceDesc						= "Corega CG-WLUSB300NS"
ATKK.DeviceDesc.DispName			= "Corega CG-WLUSB300NS"
TRENDnet.DeviceDesc					= "TRENDnet 150Mbps Micro Wireless N USB Adapter"
TRENDnet.DeviceDesc.DispName		= "TRENDnet 150Mbps Micro Wireless N USB Adapter"
TRENDnet_2.DeviceDesc				= "TRENDnet 300Mbps Mini Wireless N USB Adapter"
TRENDnet_2.DeviceDesc.DispName		= "TRENDnet 300Mbps Mini Wireless N USB Adapter"
Feixun.DeviceDesc 					= "FEIXUN Wireless LAN 802.11n USB 2.0 Network Adaptor"
Feixun.DeviceDesc.DispName			= "FEIXUN Wireless LAN 802.11n USB 2.0 Network Adaptor"
NetweeN.DeviceDesc 					= "NetweeN Wireless LAN 802.11n USB 2.0 Network Adaptor"
NetweeN.DeviceDesc.DispName			= "NetweeN Wireless LAN 802.11n USB 2.0 Network Adaptor"
XAVI.DeviceDesc 					= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
XAVI.DeviceDesc.DispName			= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
XAVI88cusc.DeviceDesc 				= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Combo"
XAVI88cusc.DeviceDesc.DispName		= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Combo"
Netgear.DeviceDesc 					= "NETGEAR WNA1000M N150 Wireless USB Micro Adapter"
Netgear.DeviceDesc.DispName			= "NETGEAR WNA1000M N150 Wireless USB Micro Adapter"
Oar_Inc.DeviceDesc 					= "SW-WF02-AD15"
Oar_Inc.DeviceDesc.DispName			= "SW-WF02-AD15"
ASUS.DeviceDesc 					= "ASUS USB-N13 300Mbps 11n Wireless USB dongle"
ASUS.DeviceDesc.DispName			= "ASUS USB-N13 300Mbps 11n Wireless USB dongle"
ASUS-2.DeviceDesc 					= "ASUS USB-N10 150Mbps 11n Wireless USB dongle"
ASUS-2.DeviceDesc.DispName			= "ASUS USB-N10 150Mbps 11n Wireless USB dongle"
ASUS-17C0.DeviceDesc 				= "ASUS USB-N10E 150Mbps Wireless-N Adapter"
ASUS-17C0.DeviceDesc.DispName		= "ASUS USB-N10E 150Mbps Wireless-N Adapter"
Hawking-1.DeviceDesc 				= "Hawking HWDN3 Wls-N Dish Adapter"
Hawking-1.DeviceDesc.DispName		= "Hawking HWDN3 Wls-N Dish Adapter"
Hawking-2.DeviceDesc 				= "Hawking HWUN4 Wls-300N Adapter"
Hawking-2.DeviceDesc.DispName		= "Hawking HWUN4 Wls-300N Adapter"
Compare-1.DeviceDesc 				= "Compare Wireless LAN 802.11n USB 2.0 Network Adapter"
Compare-1.DeviceDesc.DispName		= "Compare Wireless LAN 802.11n USB 2.0 Network Adapter"
IO_DATA_094c.DeviceDesc				= "I-O DATA WN-G150UM Wireless LAN Adapter"
IO_DATA_094c.DeviceDesc.DispName	= "I-O DATA WN-G150UM Wireless LAN Adapter"
IO_DATA_0950.DeviceDesc				= "I-O DATA WN-G300UA Wireless LAN Adapter"
IO_DATA_0950.DeviceDesc.DispName	= "I-O DATA WN-G300UA Wireless LAN Adapter"
TPLINK-0100.DeviceDesc				= "300Mbps Wireless High Power USB Adapter"
TPLINK-0100.DeviceDesc.DispName		= "300Mbps Wireless High Power USB Adapter"

;*******************************************************************************
; RTL8192DU Device description
;*******************************************************************************
RTL8192du.DeviceDesc 				= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8192du.DeviceDesc.DispName		= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8192du0.DeviceDesc 				= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC0"
RTL8192du0.DeviceDesc.DispName		= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC0"
RTL8192du1.DeviceDesc 				= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC1"
RTL8192du1.DeviceDesc.DispName		= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC1"
RTL8192du2.DeviceDesc           	= "Realtek RTL8192DU Wireless LAN 802.11N USB 2.0 Network Adapter MAC0"
RTL8192du2.DeviceDesc.DispName		= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC0"
RTL8192du3.DeviceDesc           	= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC1"
RTL8192du3.DeviceDesc.DispName		= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC1"
PCI_Abocom_du0.DeviceDesc 			= "GW-USDual300 MAC0"
PCI_Abocom_du0.DeviceDesc.DispName	= "GW-USDual300 MAC0"
PCI_Abocom_du1.DeviceDesc 			= "GW-USDual300 MAC1"
PCI_Abocom_du1.DeviceDesc.DispName	= "GW-USDual300 MAC1"
PCI_3_du0.DeviceDesc 				= "GW-USFang300 MAC0"
PCI_3_du0.DeviceDesc.DispName		= "GW-USFang300 MAC0"
PCI_3_du1.DeviceDesc 				= "GW-USFang300 MAC1"
PCI_3_du1.DeviceDesc.DispName		= "GW-USFang300 MAC1"
PCI_4_du0.DeviceDesc 				= "GW-USUltra300 MAC0"
PCI_4_du0.DeviceDesc.DispName		= "GW-USUltra300 MAC0"
PCI_4_du1.DeviceDesc 				= "GW-USUltra300 MAC1"
PCI_4_du1.DeviceDesc.DispName		= "GW-USUltra300 MAC1"
PCIWIDI_92DU.DeviceDesc 			= "MZK-WD300DH"
PCIWIDI_92DU.DeviceDesc.DispName	= "MZK-WD300DH"
Abocom_92DU0.DeviceDesc				= "802.11 a/b/g/n Wireless LAN USB 2.0 Network Adapter MAC0"
Abocom_92DU0.DeviceDesc.DispName	= "802.11 a/b/g/n Wireless LAN USB 2.0 Network Adapter MAC0"
Abocom_92DU1.DeviceDesc				= "802.11 a/b/g/n Wireless LAN USB 2.0 Network Adapter MAC1"
Abocom_92DU1.DeviceDesc.DispName	= "802.11 a/b/g/n Wireless LAN USB 2.0 Network Adapter MAC1"
Belkin-N600DB.DeviceDesc			= "Belkin Wireless Adapter"
Belkin-N600DB.DeviceDesc.DispName	= "Belkin Wireless Adapter"
Belkin-N450DB.DeviceDesc			= "Belkin Wireless Adapter"
Belkin-N450DB.DeviceDesc.DispName	= "Belkin Wireless Adapter"
Belkin-N300DB.DeviceDesc			= "Belkin Wireless Adapter"
Belkin-N300DB.DeviceDesc.DispName	= "Belkin Wireless Adapter"
DLink-DWA151.DeviceDesc                 = "D-Link DWA-151 Wireless N 150 dual band USB Adapter"   
DLink-DWA151.DeviceDesc.DispName        = "D-Link DWA-151 Wireless N 150 dual band USB Adapter"  
TRENDnet_3_du.DeviceDesc			= "TRENDnet 300Mbps Dual Band Wireless N USB Adapter"
TRENDnet_3_du.DeviceDesc.DispName	= "TRENDnet 300Mbps Dual Band Wireless N USB Adapter"
Logitec.DeviceDesc			= "150N 5GHz USB Dongle"
Logitec.DeviceDesc.DispName		= "150N 5GHz USB Dongle"
Actiontec.DeviceDesc			= "Actiontec ScreenBeam USB Transmitter"
Actiontec.DeviceDesc.DispName		= "Actiontec ScreenBeam USB Transmitter"
EDIMAX5G.DeviceDesc			= "Realtek RTL8192DU Wireless LAN 802.11a/n 5G USB 2.0 Network Adapter"
EDIMAX5G.DeviceDesc.DispName		= "Realtek RTL8192DU Wireless LAN 802.11a/n 5G USB 2.0 Network Adapter"

;*******************************************************************************
; RTL8723au Device description
;*******************************************************************************
RTL8723au.DeviceDesc 				= "Realtek RTL8723A Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8723au.DeviceDesc.DispName		= "Realtek RTL8723A Wireless LAN 802.11n USB 2.0 Network Adapter"
;*******************************************************************************
; RTL8188EU Device description
;*******************************************************************************
RTL8188eu.DeviceDesc 				= "Realtek RTL8188EU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188eu.DeviceDesc.DispName		= "Realtek RTL8188EU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188ee_vau.DeviceDesc 			= "Realtek RTL8188EE-VAU Wireless LAN 802.11n USB minicard"
RTL8188ee_vau.DeviceDesc.DispName	= "Realtek RTL8188EE-VAU Wireless LAN 802.11n USB minicard"
