
CONEXANT Tiki USB Audio Device Firmware Programming Guide


Rev1.0

1. Insert Conexnat Tiki USB device in system USB slot.


2. Open UpgradeFirmware-1.0.47.0-Somic.exe, below dialog will show:



3. Press “Browse” button, the open dialog will show to ask for firmware file selection.



4. Press “Upgrade” button and press “OK” button of the warning dialog to program the selected firmware into the attached USB device.



5. Plug out the device and re-plug it in the USB slot, check if the new device’s VID/PID is the right one matching with the firmware from “Device Manager”.