12. Product Specification

| Note: | • Specification values vary slightly from printers with different models with different functions ,and product specifications vary from different countries and regions. • These values are based on the initial data. For more information about the latest specifications, please visit: www.pantum.com.

12.1. Specification Overview

Product Size (W*D*H) | 337mm*220mm*178mm
Product weight (excluding the cartridge) | 4kg
Print Environment | Optimal Printing Temp Range: 10-32℃
Relative humidity range: 20%~80%RH
Power Voltage | 220V Model：AC220~240V,50Hz/60Hz,3A
Noise (acoustic pressure level) | Print: 52dB(A)
Standby: 30dB(A)
Enter network standby time: | 1 minutes
Power Consumption
Printing: average 370W
Ready: 38W
Sleep: <2W
Operating System | Microsoft Windows XP/ Windows Vista/Windows 7/Windows 8/Windows 8.1/ Windows 10/ Windows Server2003/2008/2012（32/64Bit）
macOS 10.7/10.8/10.9/10.10/10.11/10.12/10.13/10.14/10.15
Linux(Ubuntu 12.04~18.04)
iOS 7.0-14.0
Android 4.4-10.0
Communication interface | USB 2.0(High Speed)
IEEE802.11b/g/n interface

12.2. Print Specifications

Print Speed | Please see Chapter 1.1.
Print Time of First Page | ≤7.8S
Print Language | GDI

Supplier's Declaration of Conformity 47 CFR § 2.1077 Compliance Information Unique Identifier Trade Name: Pantum Model No.: P221**/P251**(* could be A-Z, a-z, 0-9 or blank) Responsible Party – U.S. Contact Information Company Name: PANTUM (USA) CO.,LTD Office address:13875 Ramona Ave.,Chino, CA 91710 TEL: 626-965-6662 FCC Compliance Statement This device complies with Part 15 of the FCC Rules. Operation is subject to the following two conditions: (1) This device may not cause harmful interference, and (2) this device must accept any interference received, including interference that may cause undesired operation. USA Only