SUMO
Simulation of Urban MObility

- Home
- Download
- Documentation
- Wiki
- Trac
- Blog
- Contact
- SF-Project

# Tutorials/OSMActivityGen/eichstaett.osm

eichstaett.osm

Map of the German city Eichstätt in the OpenStreetMap format. After the map had been exported from OpenStreetMap, a detail was cut out, unnecessary objects were deleted and the map has been improved for traffic simulation and for the conversion with netconvert. The steps are described in Tutorials/Import from OpenStreetMap. As a final step, the XML identifiers were renumbered to positive numbers. This way, JOSM thinks there are no changes necessary for upload.

You can use this file if you need a road network of a town with about 13,000 inhabitants. All roads were verified to have the right highway type, speed limit and one-way attribute. All traffic lights of cars (not all pedestrian lights) were also verified. You can find a corresponding SUMO network file at Tutorials/OSMActivityGen/eichstaett.net.xml.

Author | W. Bamberger
Date | 2011-02-17
Source | Map data © OpenStreetMap contributors, CC-BY-SA
History | This file is located in the SUMO Subversion repository. See the log there.
License | This work is licensed under a Creative Commons Attribution-ShareAlike 3.0 Unported License. The authors are listed in the history.

This page was last modified on 4 October 2012, at 12:47.