SUMO
Simulation of Urban MObility

- Home
- Download
- Documentation
- Wiki
- Trac
- Blog
- Contact
- SF-Project

# Networks/Import

NETCONVERT allows to import road networks from different formats. By now, the following formats are supported:

- OpenStreetMap databases, see Networks/Import/OpenStreetMap
- PTV VISUM (a macroscopic traffic simulation package), see Networks/Import/VISUM
- PTV VISSIM (a microscopic traffic simulation package), see Networks/Import/Vissim
- openDRIVE networks, see Networks/Import/openDRIVE
- MATsim networks, see Networks/Import/MATsim
- SUMO networks, see Networks/Import/SUMO Road Networks
- ArcView-data base files, see Importing ArcView networks (shapefiles)
- Elmar Brockfelds unsplitted and splitted NavTeq-data, see Networks/Import/DlrNavteq
- RoboCup Rescue League folders, see Networks/Import/RoboCup

In most of these cases, NETCONVERT needs only two parameter: the option named as the source application/format followed by the name of the file to convert and the name of the output file (using the --output-file option). In the case, a VISUM network shall be imported, the following code will convert it into a SUMO-network:

    netconvert --visum=MyVisumNet.inp --output-file=MySUMONet.net.xml

The import can be influenced using further NETCONVERT options.

This page was last modified on 12 September 2011, at 07:17.