SUMO
Simulation of Urban MObility

- Home
- Download
- Documentation
- Wiki
- Trac
- Blog
- Contact
- SF-Project

# Topics/V2X

# State of the Art

Missing:
Describe "state of the art", here.

# V2X simulations in SUMO

SUMO is usually coupled to a communication network simulator using a middleware.

## Coupling to network simulators

Coupling Middlewares Overview

Name | Used Network Simulator | Under Development
--- | --- | ---
TraNS | ns2 | no
Veins | Focused on OMNeT++/MiXiM with an extendable, modular framework (ports exist for INET, INETMANET, and JiST/SWANS) | yes
iTETRIS | ns3 | yes
VSimRTI | ns3, JiST/SWANS or OMNeT++ (extendable) | yes

### TraNS

TraNS is an extension of ns2

### Veins

See the Veins Homepage for a short overview, download links, beginner's tutorial, full publication list, and documentation.

### iTETRIS

### VSimRTI

The V2X Simulation Runtime Infrastructure (VSimRTI) is a framework which enables the preparation and execution of V2X simulations. The easy integration and exchange of simulators enables the substitution of the most relevant simulators for a realistic presentation of vehicle traffic, emissions, wireless communication, and the execution of V2X applications. For immediate use, a set of simulators is already coupled with VSimRTI. For example, the traffic simulators VISSIM and SUMO, the communication simulators ns3, JiST/SWANS and OMNeT++, the application simulator VSimRTI_App, and several visualization and analysis tools are prepared for VSimRTI. For more information see VSimRTI Homepage.

# References

This page was last modified on 5 December 2012, at 15:39.