SUMO
Simulation of Urban MObility

- Home
- Download
- Documentation
- Wiki
- Trac
- Blog
- Contact
- SF-Project

# TraCI/Route Value Retrieval

## Command 0xa6: Get Route Variable

ubyte | string
Variable | Route ID
--- | ---

Asks for the value of a certain variable of the named route.

The following variable values can be retrieved, the type of the return value is also shown in the table.

Overview Retrievable Route Variables
Variable | ValueType | Description
--- | --- | ---
id list (0x00) | stringList | Returns a list of ids of all currently loaded routes (the given route ID is ignored)
count (0x01) | int | Returns the number of currently loaded routes (the given route ID is ignored)
edges (0x54) | stringList | Returns the ids of the edges this route covers

### Response 0xb6: Route Variable

ubyte | string | ubyte | <return_type>
Variable | Induction Loop ID | Return type of the variable | <VARIABLE_VALUE>
--- | --- | --- | ---

The respond to a "Command Get Route Variable".

This page was last modified on 13 July 2011, at 14:01.