SUMO
Simulation of Urban MObility

- Home
- Download
- Documentation
- Wiki
- Trac
- Blog
- Contact
- SF-Project

# Data/Networks

You should read the main page on NETCONVERT before reading this.

# OpenStreetMap-project

  URL: http://www.openstreetmap.org/
  Area: the complete world :-)
  Demand data: not available
  Extraction:
    1. OpenStreetMapDownload explains how to obtain OSM-data.
    2. Networks/Import/OpenStreetMap explains how to create Sumo-networks from OSM-data using NETCONVERT.
  Comments: A great source of networks and man-made infrastucture. However, infrastructure data and definitions are still changing which complicates import.
  See also: Data/Scenarios/TAPASCologne - a complete scenario based on OSM and TAPAS

# Frida-project

  URL: http://frida.intevation.org/
  Area: city of Osnabrück
  Demand data: not available
  Extraction: netconvert --shapefile strassen -o frida2.net.xml --shapefile.street-id strShapeID -t frida.typ.xml --shapefile.type-id strTypID -v --proj "+proj=utm +ellps=bessel +units=m"
  Comments: Not really applicable because the streets lack information about the number of lanes and the direction. Especially the second makes the converted network quite useless. Trying to use the option --shapefile.all-bidi solves the problem for inner-city roads but makes highway on/offramps bidirectional, too. The projection might be wrong as well, give --proj.utm a try.
  See also:
  Networks/Import/ArcView - (notes on) importing ArcView networks (shapefiles)

This page was last modified on 12 September 2011, at 07:42.