SUMO
Simulation of Urban MObility

- Home
- Download
- Documentation
- Wiki
- Trac
- Blog
- Contact
- SF-Project

# Networks/Import/openDRIVE

For reading openDRIVE networks, give NETCONVERT the option --opendrive-files <FILE>[,<FILE>]* or --opendrive <FILE>[,<FILE>]* for short.

    netconvert --opendrive myOpenDriveNetwork.xodr -o mySUMOnetwork.net.xml

Lanes are imported by their type, as listed in the following table

Lane types NETCONVERT interprets as driving lanes

type@lane | interpreted as
--- | ---
shoulder | -
none | -
driving | allowed for all
restricted | -
stop | allowed for all
mwyEntry | allowed for all
mwyExit | allowed for all
special1 | allowed for all
parking | allowed for all
sidewalk | -
border | -

This page was last modified on 31 October 2012, at 09:51.