#	How to use	#
1. Copy content of copy_to_sd_root folder to the root of your SD card
2. Power on phone holding power button to access magldr menu
3. Select "USB Flasher" option
4. Run DAF.exe and go through installer to set required partition layout
5. After reboot repeat step 2 to access menu again
6. Select "Boot AD SD" and recovery will load
