;****************************************************************************************
;
; RT61.inf
;
;   This installation script supports Windows 98,Me,2000 & XP for the
;   Ralink RT2561 & RT2661 series Wireless LAN Card.
;
;   Copyright (c)2002-2006, Ralink Technology Corp., All Rights Reserved
;   All Rights Reserved.
;   Developed by RaLink Technology, Corp. -- http://www.ralinktech.com
;
;****************************************************************************************

[Version]
Signature       = "$Chicago$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %Ralink%
Compatible      = 1
DriverVer       = 09/07/2006, 1.01.03.0000
CatalogFile     = RT61.CAT            

[ControlFlags]
;ExcludeFromSelect = PCI\VEN_1814&DEV_0301

[Manufacturer]
%Ralink%        = Ralink
%Gigabyte%      = Gigabyte
%Edimax%        = Edimax
%Sitecom%       = Sitecom
%Delta%         = Delta
%Hawking%       = Hawking
%Billionton%    = Billionton
%Asus%          = ASUS
%ZINWELL%       = ZINWELL
%AMIT%          = AMIT
%CASTLENET%     = CASTLENET
%ACCTON%        = ACCTON
%Surecom%       = Surecom
%VTech%         = VTech
%Siemens%       = Siemens
%Conceptronic%  = Conceptronic
%SMC%           = SMC
%CNet%          = CNet
%Corega%        = Corega
%Amigo%         = Amigo

[Ralink]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Ralink_0301.DeviceDesc%    = RALINK_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_25611814
%Ralink_0302.DeviceDesc%    = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_25611814
%Ralink_0401.DeviceDesc%    = RALINK_0401.ndi,      PCI\VEN_1814&DEV_0401&SUBSYS_26611814
; MSI
%M61_B833T.DeviceDesc%      = RALINK_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_B8331462
%M61_B834T.DeviceDesc%      = RALINK_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_B8341462
%M61_B835T.DeviceDesc%      = RALINK_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_B8351462
%M61_B833.DeviceDesc%       = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_B8331462
%M61_B834.DeviceDesc%       = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_B8341462
%M61_B835.DeviceDesc%       = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_B8351462
; Winstron
%WLANm.DeviceDesc%          = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_12A0185F
%WLANc.DeviceDesc%          = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_22A0185F
; Amigo
%AMIGO.DeviceDesc1%         = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_914016EF&REV_01
%AMIGO.DeviceDesc2%         = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_922016EF&REV_01
%AMIGO.DeviceDesc3%         = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_923016EF&REV_01
; CNet
%CNetPCI.DeviceDesc%        = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_00251371
%CNetMPCI.DeviceDesc%       = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_00261371
%CNetCardbus.DeviceDesc%    = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_00271371
; Qcom
%Qcom.DeviceDesc%           = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_619418E8

[Gigabyte]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%GigabyteWM01GS.DeviceDesc% = GIGABYTE1.ndi,        PCI\VEN_1814&DEV_0301&SUBSYS_E8321458
%GigabyteWI01GS.DeviceDesc% = GIGABYTE1.ndi,        PCI\VEN_1814&DEV_0301&SUBSYS_E9331458
%GigabyteWP01GS.DeviceDesc% = GIGABYTE1.ndi,        PCI\VEN_1814&DEV_0301&SUBSYS_E9341458
%GigabyteWM02GS.DeviceDesc% = GIGABYTE2.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_E8321458
%GigabyteWI02GS.DeviceDesc% = GIGABYTE2.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_E9331458
%GigabyteWP02GS.DeviceDesc% = GIGABYTE2.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_E9341458
%GigabyteWI02GM.DeviceDesc% = GIGABYTE3.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_E9351458
%GigabyteWM01GM.DeviceDesc% = GIGABYTE3.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_E8331458
%GigabyteWP01GM.DeviceDesc% = GIGABYTE3.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_E9361458

[Edimax]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%EW-7108.DeviceDesc%        = Edimax.ndi,           PCI\VEN_1814&DEV_0302&SUBSYS_71081432
%EW-7128.DeviceDesc%        = Edimax.ndi,           PCI\VEN_1814&DEV_0302&SUBSYS_71281432

[Sitecom]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Sitecom_WL112V2.DeviceDesc% = SITECOM_0301.ndi,         PCI\VEN_1814&DEV_0301&SUBSYS_9072182D
%Sitecom_WL115V2.DeviceDesc% = SITECOM_0301.ndi,         PCI\VEN_1814&DEV_0301&SUBSYS_9074182D
%Sitecom_WL150.DeviceDesc%  = SITECOM_0401.ndi,          PCI\VEN_1814&DEV_0401&SUBSYS_9096182D
%Sitecom_WL151.DeviceDesc%  = SITECOM_0401.ndi,          PCI\VEN_1814&DEV_0401&SUBSYS_9097182D

[Delta]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%DeltaPCI.DeviceDesc%       = DELTA.ndi,            PCI\VEN_1814&DEV_0301&SUBSYS_701C4033
%DeltaCB.DeviceDesc%        = DELTA.ndi,            PCI\VEN_1814&DEV_0301&SUBSYS_701B4033

[Hawking]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Hawking0C54.DeviceDesc%    = HAWKING.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_0C541432
%Hawking0B54.DeviceDesc%    = HAWKING.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_0B541432

[Billionton]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%GMIWLGRL2-B.DeviceDesc%   = BILLIONTON.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_020514CB
%GMIWLGRL2-N.DeviceDesc%   = BILLIONTON.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_020614CB

[ASUS]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%ASUS.DeviceDesc%           = ASUS.ndi,             PCI\VEN_1814&DEV_0302&SUBSYS_107F1043
%ASUS.DeviceDesc%           = ASUS.ndi,             PCI\VEN_1814&DEV_0302&SUBSYS_127F1043
%ASUS.DeviceDesc%           = ASUS.ndi,             PCI\VEN_1814&DEV_0302&SUBSYS_130F1043
%ASUS.DeviceDesc%           = ASUS.ndi,             PCI\VEN_1814&DEV_0302&SUBSYS_137F1043
%ASUSGEN.DeviceDesc%        = ASUS.ndi,             PCI\VEN_1814&DEV_0302&SUBSYS_137E1043

[ZINWELL]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%ZINWELLPCI.DeviceDesc%     = ZINWELL.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_03615A57
%ZINWELLMPCI.DeviceDesc%    = ZINWELL.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_03605A57
%ZINWELLCARD.DeviceDesc%    = ZINWELL.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_01605A57
%ZINWELLOEM1.DeviceDesc%    = ZINWELL.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_300918A3
%ZINWELLOEM2.DeviceDesc%    = ZINWELL.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_301018A3

[AMIT]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%AMIT.DeviceDesc%           = AMIT_0302.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_531018EB
%AMITMINI.DeviceDesc%       = AMIT_0302.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_531118EB
%AMITPCI.DeviceDesc%        = AMIT_0302.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_531218EB
%AMIT0100.DeviceDesc%       = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_010018EB
%AMIT0200.DeviceDesc%       = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_020018EB
%AMIT0300.DeviceDesc%       = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_030018EB
%AMIT0202.DeviceDesc%       = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_020218EB
%AMIT0302.DeviceDesc%       = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_030218EB
%AMIT0203.DeviceDesc%       = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_020318EB
%AMIT0303.DeviceDesc%       = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_030318EB
%AMIT0204.DeviceDesc%       = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_020418EB
%AMIT0304.DeviceDesc%       = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_030418EB
%AMITCG.DeviceDesc%         = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_C11E1259

[CASTLENET]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%CASTLENET.DeviceDesc%      = CASTLENET.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_12801688

[ACCTON]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%WN4306A.DeviceDesc%        = WN4306A.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_43061113

[Surecom]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%SurecomPCI.DeviceDesc%     = SURECOM.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_13F310BD
%SurecomCardbus.DeviceDesc% = SURECOM.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_14F310BD

[VTech]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%VTechPCI.DeviceDesc%       = VTECH.ndi,            PCI\VEN_1814&DEV_0302&SUBSYS_301118A3
%VTechCARD.DeviceDesc%      = VTECH.ndi,            PCI\VEN_1814&DEV_0302&SUBSYS_301318A3

[Siemens]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Siemens.DeviceDesc%        = SIEMENS.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_3C800681

[Conceptronic]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Conceptronic_PCCard.DeviceDesc% = CONCEPTRONIC.ndi,  PCI\VEN_1814&DEV_0302&SUBSYS_3C231948
%Conceptronic_PCICard.DeviceDesc% = CONCEPTRONIC.ndi, PCI\VEN_1814&DEV_0302&SUBSYS_3C241948

[SMC]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%SMC_EE04.DeviceDesc%       = SMC.ndi,              PCI\VEN_1814&DEV_0401&SUBSYS_EE041113
%SMC_EE05.DeviceDesc%       = SMC.ndi,              PCI\VEN_1814&DEV_0401&SUBSYS_EE051113

[CNet]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%CNet_6221.DeviceDesc%      = CNET_0301.ndi,        PCI\VEN_1814&DEV_0301&SUBSYS_62211371
%CNet_7221.DeviceDesc%      = CNET_0301.ndi,        PCI\VEN_1814&DEV_0301&SUBSYS_72211371
%CNet_8221.DeviceDesc%      = CNET_0301.ndi,        PCI\VEN_1814&DEV_0301&SUBSYS_82211371
%CNet_6121.DeviceDesc%      = CNET_0302.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_61211371
%CNet_7121.DeviceDesc%      = CNET_0302.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_71211371
%CNet_8121.DeviceDesc%      = CNET_0302.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_81211371
%CNet_6321.DeviceDesc%      = CNET_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_63211371
%CNet_7321.DeviceDesc%      = CNET_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_73211371
%CNet_8321.DeviceDesc%      = CNET_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_83211371

[Corega]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Corega.DeviceDesc%         = Corega.ndi,           PCI\VEN_1814&DEV_0401&SUBSYS_C11D1259

[Amigo]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Amigo_9141.DeviceDesc%     = AMIGO_9141.ndi,       PCI\VEN_1814&DEV_0302&SUBSYS_914116EF
%Amigo_9221.DeviceDesc%     = AMIGO_9221.ndi,       PCI\VEN_1814&DEV_0302&SUBSYS_922116EF
%Amigo_9261.DeviceDesc%     = AMIGO_9261.ndi,       PCI\VEN_1814&DEV_0302&SUBSYS_926116EF

;*******************************************************************************************
; Windows 9X specific entries
;*******************************************************************************************

[RALINK_0301.ndi]
AddReg                  = PCI0301.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[RALINK_0302.ndi]
AddReg                  = PCI0302.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[RALINK_0401.ndi]
AddReg                  = PCI0401.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[GIGABYTE1.ndi]
AddReg                  = PCI0301.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[GIGABYTE2.ndi]
AddReg                  = PCI0302.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[GIGABYTE3.ndi]
AddReg                  = PCI0401.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[Edimax.ndi]
AddReg                  = PCI0302.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[SITECOM_0301.ndi]
AddReg                  = PCI0301.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[SITECOM_0401.ndi]
AddReg                  = PCI0401.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[DELTA.ndi]
AddReg                  = PCI0301.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[HAWKING.ndi]
AddReg                  = PCI0302.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[BILLIONTON.ndi]
AddReg                  = PCI0302.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[ASUS.ndi]
AddReg                  = PCI0302.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[ZINWELL.ndi]
AddReg                  = PCI0302.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[AMIT_0302.ndi]
AddReg                  = PCI0302.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[AMIT_0401.ndi]
AddReg                  = PCI0401.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[CASTLENET.ndi]
AddReg                  = PCI0302.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[WN4306A.ndi]
AddReg                  = PCI0302.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[SURECOM.ndi]
AddReg                  = PCI0302.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[VTECH.ndi]
AddReg                  = PCI0302.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[SIEMENS.ndi]
AddReg                  = PCI0302.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[CONCEPTRONIC.ndi]
AddReg                  = PCI0302.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[SMC.ndi]
AddReg                  = PCI0401.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[CNET_0301.ndi]
AddReg                  = PCI0301.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[CNET_0302.ndi]
AddReg                  = PCI0302.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[CNET_0401.ndi]
AddReg                  = PCI0401.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[Corega.ndi]
AddReg                  = PCI0401.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[AMIGO_9141.ndi]
AddReg                  = PCI0302.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[AMIGO_9221.ndi]
AddReg                  = PCI0302.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

[AMIGO_9261.ndi]
AddReg                  = PCI0302.ndi.reg, RT619X.ndi.reg, Common.reg
CopyFiles               = win9x.CopyFiles

;*******************************************************************************************
; NT specific entries
;*******************************************************************************************

[RALINK_0301.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[RALINK_0302.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[RALINK_0401.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[GIGABYTE1.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[GIGABYTE2.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[GIGABYTE3.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Edimax.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[SITECOM_0301.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[SITECOM_0401.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[DELTA.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[HAWKING.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[BILLIONTON.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[ASUS.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[ZINWELL.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[AMIT_0302.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[AMIT_0401.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[CASTLENET.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[WN4306A.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[SURECOM.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[VTECH.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[SIEMENS.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[CONCEPTRONIC.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[SMC.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[CNET_0301.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[CNET_0302.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[CNET_0401.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Corega.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[AMIGO_9141.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[AMIGO_9221.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[AMIGO_9261.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

; NT services sections
[RALINK_0301.ndi.NT.Services]
AddService              = RT61, 2, RALINK.Service, common.EventLog

[RALINK_0302.ndi.NT.Services]
AddService              = RT61, 2, RALINK.Service, common.EventLog

[RALINK_0401.ndi.NT.Services]
AddService              = RT61, 2, RALINK.Service, common.EventLog

[GIGABYTE1.ndi.NT.Services]
AddService              = RT61, 2, GIGABYTE.Service, common.EventLog

[GIGABYTE2.ndi.NT.Services]
AddService              = RT61, 2, GIGABYTE.Service, common.EventLog

[GIGABYTE3.ndi.NT.Services]
AddService              = RT61, 2, GIGABYTE.Service, common.EventLog

[Edimax.ndi.NT.Services]
AddService              = RT61, 2, Edimax.Service, common.EventLog

[SITECOM_0301.ndi.NT.Services]
AddService              = RT61, 2, SITECOM.Service, common.EventLog

[SITECOM_0401.ndi.NT.Services]
AddService              = RT61, 2, SITECOM.Service, common.EventLog

[DELTA.ndi.NT.Services]
AddService              = RT61, 2, DELTA.Service, common.EventLog

[HAWKING.ndi.NT.Services]
AddService              = RT61, 2, HAWKING.Service, common.EventLog

[BILLIONTON.ndi.NT.Services]
AddService              = RT61, 2, BILLIONTON.Service, common.EventLog

[ASUS.ndi.NT.Services]
AddService              = RT61, 2, ASUS.Service, common.EventLog

[ZINWELL.ndi.NT.Services]
AddService              = RT61, 2, ZINWELL.Service, common.EventLog

[AMIT_0302.ndi.NT.Services]
AddService              = RT61, 2, AMIT.Service, common.EventLog

[AMIT_0401.ndi.NT.Services]
AddService              = RT61, 2, AMIT.Service, common.EventLog

[CASTLENET.ndi.NT.Services]
AddService              = RT61, 2, CASTLENET.Service, common.EventLog

[WN4306A.ndi.NT.Services]
AddService              = RT61, 2, WN4306A.Service, common.EventLog

[SURECOM.ndi.NT.Services]
AddService              = RT61, 2, SURECOM.Service, common.EventLog

[VTECH.ndi.NT.Services]
AddService              = RT61, 2, VTECH.Service, common.EventLog

[SIEMENS.ndi.NT.Services]
AddService              = RT61, 2, SIEMENS.Service, common.EventLog

[CONCEPTRONIC.ndi.NT.Services]
AddService              = RT61, 2, CONCEPTRONIC.Service, common.EventLog

[SMC.ndi.NT.Services]
AddService              = RT61, 2, SMC.Service, common.EventLog

[CNET_0301.ndi.NT.Services]
AddService              = RT61, 2, CNET.Service, common.EventLog

[CNET_0302.ndi.NT.Services]
AddService              = RT61, 2, CNET.Service, common.EventLog

[CNET_0401.ndi.NT.Services]
AddService              = RT61, 2, CNET.Service, common.EventLog

[Corega.ndi.NT.Services]
AddService              = RT61, 2, COREGA.Service, common.EventLog

[AMIGO_9141.ndi.NT.Services]
AddService              = RT61, 2, AMIGO.Service, common.EventLog

[AMIGO_9221.ndi.NT.Services]
AddService              = RT61, 2, AMIGO.Service, common.EventLog

[AMIGO_9261.ndi.NT.Services]
AddService              = RT61, 2, AMIGO.Service, common.EventLog

;*******************************************************************************************
; common regs for NT and W9x
;*******************************************************************************************

[Common.reg]
;*******************************************************************************************
; System Level Property

;
; Current Profile
;
HKR, ,                    CurProfile,      0,""
HKR, Default,             CurProfile,      0,""

;
; Radio On/Off
;
HKR, ,                            Radio,           0, "0"
HKR, NDI\params\Radio,            ParamDesc,       0, "Radio On/Off"
HKR, NDI\params\Radio,            type,            0, "enum"
HKR, NDI\params\Radio,            default,         0, "0"
HKR, NDI\params\Radio\enum,       1,               0, "Disable"
HKR, NDI\params\Radio\enum,       0,               0, "Enable"

;
; Auto Reconnect Mode
;
HKR, ,                                  AutoReconnect,      0, "1"
HKR, NDI\params\AutoReconnect,          ParamDesc,          0, "Auto Reconnect Mode"
HKR, NDI\params\AutoReconnect,          type,               0, "enum"
HKR, NDI\params\AutoReconnect,          default,            0, "1"
HKR, NDI\params\AutoReconnect\enum,     0,                  0, "Disable"
HKR, NDI\params\AutoReconnect\enum,     1,                  0, "Enable"

;
; Show Hidden SSID in Site Survey Page
;
HKR, ,                                  ShowHiddenSSID,     0, "0"   ; 0=disable(default), 1=enable

;
; Country Region G Band
;
HKR, ,                                 CountryRegion,      0, "0"
HKR, NDI\params\CountryRegion,         ParamDesc,          0, "Country Region 11G"
HKR, NDI\params\CountryRegion,         type,               0, "enum"
HKR, NDI\params\CountryRegion,         default,            0, "0"
HKR, NDI\params\CountryRegion\enum,    0,                  0, "(Channel 1 - 11)"
HKR, NDI\params\CountryRegion\enum,    1,                  0, "(Channel 1 - 13)"
HKR, NDI\params\CountryRegion\enum,    2,                  0, "(Channel 10 - 11)"
HKR, NDI\params\CountryRegion\enum,    3,                  0, "(Channel 10 - 13)"
HKR, NDI\params\CountryRegion\enum,    4,                  0, "(Channel 14)"
HKR, NDI\params\CountryRegion\enum,    5,                  0, "(Channel 1 - 14)"
HKR, NDI\params\CountryRegion\enum,    6,                  0, "(Channel 3 - 9)"
HKR, NDI\params\CountryRegion\enum,    7,                  0, "(Channel 5 - 13)"

;
; Country Region A Band
;
HKR, ,                                 CountryRegionABand, 0, "7"
HKR, NDI\params\CountryRegionABand,    ParamDesc,          0, "Country Region 11A"
HKR, NDI\params\CountryRegionABand,    type,               0, "enum"
HKR, NDI\params\CountryRegionABand,    default,            0, "7"
HKR, NDI\params\CountryRegionABand\enum,0,                 0, "Ch(36 - 64,149 - 165)"
HKR, NDI\params\CountryRegionABand\enum,1,                 0, "Ch(36 - 140)"
HKR, NDI\params\CountryRegionABand\enum,2,                 0, "Ch(36 - 64)"
HKR, NDI\params\CountryRegionABand\enum,3,                 0, "Ch(52 - 64,149 - 161)"
HKR, NDI\params\CountryRegionABand\enum,4,                 0, "Ch(149 - 165)"
HKR, NDI\params\CountryRegionABand\enum,5,                 0, "Ch(149 - 161)"
HKR, NDI\params\CountryRegionABand\enum,6,                 0, "Ch(36 - 48)"
HKR, NDI\params\CountryRegionABand\enum,7,                 0, "Ch(36 - 165)"
HKR, NDI\params\CountryRegionABand\enum,8,                 0, "Ch(52 - 64)"
HKR, NDI\params\CountryRegionABand\enum,9,                 0, "Ch(34 - 46)"
HKR, NDI\params\CountryRegionABand\enum,10,                0, "Ch(34 - 64)"

;*******************************************************************************************
; Advance Page

;
; OpMode
;
HKR, ,                            OpMode,          0, "0"

;
; WirelessMode
;
HKR, ,                            WirelessMode,    0, "3"

;
; Enable TX Burst
;
HKR, ,                            TXBurst,         0, "0"

;
; Use Short Slot Time
;
HKR, ,                            ShortSlot,       0, "1"

;
; Use Turbo rate
;
HKR, ,                            TurboRate,       0, "0"

;
; Use Ofdm rate in adhoc mode
;
HKR, ,                            AdhocOfdm,       0, "0"
HKR, NDI\params\AdhocOfdm,              ParamDesc, 0, "Adhoc Wireless Mode"
HKR, NDI\params\AdhocOfdm,              type,      0, "enum"
HKR, NDI\params\AdhocOfdm,              default,   0, "0"
HKR, NDI\params\AdhocOfdm\enum,         0,         0, "802.11 B Only"
HKR, NDI\params\AdhocOfdm\enum,         1,         0, "802.11 B/G Mix"
HKR, NDI\params\AdhocOfdm\enum,         2,         0, "802.11 G Only"
HKR, NDI\params\AdhocOfdm\enum,         3,         0, "802.11 A Only"
HKR, NDI\params\AdhocOfdm\enum,         4,         0, "802.11 A/B/G Mix"

;
; Use BG Protection
;
HKR, ,                            BGProtection,    0, "0"
HKR, NDI\params\BGProtection,           ParamDesc, 0, "B/G Protection"
HKR, NDI\params\BGProtection,           type,      0, "enum"
HKR, NDI\params\BGProtection,           default,   0, "0"
HKR, NDI\params\BGProtection\enum,      0,         0, "Auto"
HKR, NDI\params\BGProtection\enum,      1,         0, "On"
HKR, NDI\params\BGProtection\enum,      2,         0, "Off"

;
; FrameAggregation
;
HKR, ,                            FrameAggregation,0, "1"
HKR, NDI\params\FrameAggregation,       ParamDesc, 0, "Frame Aggregation"
HKR, NDI\params\FrameAggregation,       type,      0, "enum"
HKR, NDI\params\FrameAggregation,       default,   0, "1"
HKR, NDI\params\FrameAggregation\enum,  0,         0, "Disable"
HKR, NDI\params\FrameAggregation\enum,  1,         0, "Enable"

;
; IEEE80211H
;
HKR, ,                            IEEE80211H,      0, "0"
HKR, NDI\params\IEEE80211H,       ParamDesc,       0, "IEEE802.11h"
HKR, NDI\params\IEEE80211H,       type,            0, "enum"
HKR, NDI\params\IEEE80211H,       default,         0, "0"
HKR, NDI\params\IEEE80211H\enum,  0,               0, "Disable"
HKR, NDI\params\IEEE80211H\enum,  1,               0, "Enable"

;
; AutoChannelSelect
;
HKR, ,                            AutoChannelSelect,      0, "0"
HKR, NDI\params\AutoChannelSelect,       ParamDesc,0, "Auto Channel Select"
HKR, NDI\params\AutoChannelSelect,       type,     0, "enum"
HKR, NDI\params\AutoChannelSelect,       default,  0, "0"
HKR, NDI\params\AutoChannelSelect\enum,  0,        0, "Disable"
HKR, NDI\params\AutoChannelSelect\enum,  1,        0, "Enable"

;
; WMMCapable
;
HKR, ,                            WMMCapable,      0, "0"
HKR, NDI\params\WMMCapable,             ParamDesc, 0, "WMM Capable"
HKR, NDI\params\WMMCapable,             type,      0, "enum"
HKR, NDI\params\WMMCapable,             default,   0, "0"
HKR, NDI\params\WMMCapable\enum,        0,         0, "Disable"
HKR, NDI\params\WMMCapable\enum,        1,         0, "Enable"

;
; APSDCapable
;
HKR, ,                            APSDCapable,     0, "0"
HKR, NDI\params\APSDCapable,            ParamDesc, 0, "APSD Capable"
HKR, NDI\params\APSDCapable,            type,      0, "enum"
HKR, NDI\params\APSDCapable,            default,   0, "0"
HKR, NDI\params\APSDCapable\enum,       0,         0, "Disable"
HKR, NDI\params\APSDCapable\enum,       1,         0, "Enable"

;
; APSDAC_BE
;
HKR, ,                            APSDAC_BE,       0, "0"
HKR, NDI\params\APSDAC_BE,              ParamDesc, 0, "AC_BE support APSD"
HKR, NDI\params\APSDAC_BE,              type,      0, "enum"
HKR, NDI\params\APSDAC_BE,              default,   0, "0"
HKR, NDI\params\APSDAC_BE\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_BE\enum,         1,         0, "Enable"

;
; APSDAC_BK
;
HKR, ,                            APSDAC_BK,       0, "0"
HKR, NDI\params\APSDAC_BK,              ParamDesc, 0, "AC_BK support APSD"
HKR, NDI\params\APSDAC_BK,              type,      0, "enum"
HKR, NDI\params\APSDAC_BK,              default,   0, "0"
HKR, NDI\params\APSDAC_BK\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_BK\enum,         1,         0, "Enable"

;
; APSDAC_VI
;
HKR, ,                            APSDAC_VI,       0, "0"
HKR, NDI\params\APSDAC_VI,              ParamDesc, 0, "AC_VI support APSD"
HKR, NDI\params\APSDAC_VI,              type,      0, "enum"
HKR, NDI\params\APSDAC_VI,              default,   0, "0"
HKR, NDI\params\APSDAC_VI\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_VI\enum,         1,         0, "Enable"

;
; APSDAC_VO
;
HKR, ,                            APSDAC_VO,       0, "0"
HKR, NDI\params\APSDAC_VO,              ParamDesc, 0, "AC_VO support APSD"
HKR, NDI\params\APSDAC_VO,              type,      0, "enum"
HKR, NDI\params\APSDAC_VO,              default,   0, "0"
HKR, NDI\params\APSDAC_VO\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_VO\enum,         1,         0, "Enable"

;
; MaxSPLength
;
HKR, ,                            MaxSPLength,     0, "0"
HKR, Default,                     MaxSPLength,     0, "0"
HKR, NDI\params\MaxSPLength,      ParamDesc,       0, "Max Service Period Length"
HKR, NDI\params\MaxSPLength,      type,            0, "int"
HKR, NDI\params\MaxSPLength,      default,         0, "0"
HKR, NDI\params\MaxSPLength,      min,             0, "0"
HKR, NDI\params\MaxSPLength,      max,             0, "3"
HKR, NDI\params\MaxSPLength,      step,            0, "1"
HKR, NDI\params\MaxSPLength,      optional,        0, "0"

;
; DLSCapable
;
HKR, ,                            DLSCapable,      0, "0"
HKR, NDI\params\DLSCapable,             ParamDesc, 0, "DLS Capable"
HKR, NDI\params\DLSCapable,             type,      0, "enum"
HKR, NDI\params\DLSCapable,             default,   0, "0"
HKR, NDI\params\DLSCapable\enum,        0,         0, "Disable"
HKR, NDI\params\DLSCapable\enum,        1,         0, "Enable"

;
; PSP XLink mode
;
HKR, ,                            PSPXlink,        0, "0"
HKR, NDI\params\PSPXlink,         ParamDesc,       0, "PSP Xlink Mode"
HKR, NDI\params\PSPXlink,         type,            0, "enum"
HKR, NDI\params\PSPXlink,         default,         0, "0"
HKR, NDI\params\PSPXlink\enum,    0,               0, "Disable"
HKR, NDI\params\PSPXlink\enum,    1,               0, "Enable"

;
; CCX2 control
;
HKR, ,                            CCX2Control,     0x00010001, 0x00fa4600

;
; Vendor Description
;
HKR, ,                            VendorDesc,      0, %VENDOR_DESC_DEF_STR%
HKR, Default,                     VendorDesc,      0, %VENDOR_DESC_DEF_STR%

;*******************************************************************************************
; Profile

;
; SSID
;
HKR, ,                            SSID,            0, %SSID_DEF_STR%
HKR, Default,                     SSID,            0, %SSID_DEF_STR%
HKR, NDI\params\SSID,             ParamDesc,       0, "SSID"
HKR, NDI\params\SSID,             type,            0, "edit"
HKR, NDI\params\SSID,             limitText,       0, "32"
HKR, NDI\params\SSID,             default,         0, %SSID_DEF_STR%

;
; Network Type
;
HKR, ,                            NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, Default,                     NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType,      ParamDesc,       0, "Network Type"
HKR, NDI\params\NetworkType,      type,            0, "enum"
HKR, NDI\params\NetworkType,      default,         0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType\enum, 0,               0, "802.11 Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1,               0, "Infrastructure"

;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%


;*******************************************************************************************
; System Configuration Page

;
; Local Administration MAC Network Address
;
HKR, ,                            NetworkAddress,  0, ""
HKR, Default,                     NetworkAddress,  0, ""
HKR, NDI\params\NetworkAddress,   ParamDesc,       0, "Local Administration MAC Network Address"
HKR, NDI\params\NetworkAddress,   type,            0, "edit"
HKR, NDI\params\NetworkAddress,   limitText,       0, "12"
HKR, NDI\params\NetworkAddress,   default,         0, ""

;
; Power Saving Mode
;
HKR, ,                            PSMode,          0, "0"
HKR, Default,                     PSMode,          0, "0"
HKR, NDI\params\PSMode,           ParamDesc,       0, "Power Saving Mode"
HKR, NDI\params\PSMode,           type,            0, "enum"
HKR, NDI\params\PSMode,           default,         0, "0"
HKR, NDI\params\PSMode\enum,      0,               0, "CAM (Constantly Awake Mode)"
;HKR, NDI\params\PSMode\enum,      1,               0, "Max_PSP (Max Power Savings)"
HKR, NDI\params\PSMode\enum,      2,               0, "Fast_PSP (Power Save Mode)"

;
; CAM when AC Power
;
;HKR, ,                            ACPowerCam,      0, "0"
;HKR, Default,                     ACPowerCam,      0, "0"
;HKR, NDI\params\ACPowerCam,       ParamDesc,       0, "CAM when AC Power"
;HKR, NDI\params\ACPowerCam,       type,            0, "enum"
;HKR, NDI\params\ACPowerCam,       default,         0, "0"
;HKR, NDI\params\ACPowerCam\enum,  0,               0, "Disable"
;HKR, NDI\params\ACPowerCam\enum,  1,               0, "Enable"

;
; Preamble Type
;
HKR, ,                            PreambleType,    0, "0"
HKR, Default,                     PreambleType,    0, "0"

;
; RTS Threshold
;
HKR, ,                            RTSThresh,       0, "2347"
HKR, Default,                     RTSThresh,       0, "2347"
HKR, NDI\params\RTSThresh,        ParamDesc,       0, "RTS Threshold"
HKR, NDI\params\RTSThresh,        type,            0, "int"
HKR, Ndi\params\RTSThresh,        default,         0, "2347"
HKR, NDI\params\RTSThresh,        min,             0, "0"
HKR, NDI\params\RTSThresh,        max,             0, "2347"
HKR, NDI\params\RTSThresh,        step,            0, "32"
HKR, NDI\params\RTSThresh,        optional,        0, "0"

;
; Fragment Threshold
;
HKR, ,                            FragThresh,      0, "2346"
HKR, Default,                     FragThresh,      0, "2346"
HKR, NDI\params\FragThresh,       ParamDesc,       0, "Fragment Threshold"
HKR, NDI\params\FragThresh,       type,            0, "int"
HKR, Ndi\params\FragThresh,       default,         0, "2346"
HKR, NDI\params\FragThresh,       min,             0, "256"
HKR, NDI\params\FragThresh,       max,             0, "2346"
HKR, NDI\params\FragThresh,       step,            0, "32"
HKR, NDI\params\FragThresh,       optional,        0, "0"

;*******************************************************************************************
; Authentication & Security Page

;
; Authentication Type
;
HKR, ,                AuthenType,      0, "0" ; Open System
HKR, Default,         AuthenType,      0, "0"

;
; Encryption
;
HKR, ,                Encryption,      0, "1" ; Disable
HKR, Default,         Encryption,      0, "1"

;
; WEP Keys Length
;
HKR, ,                WEPKeyLen,       0, "0"
HKR, Default,         WEPKeyLen,       0, "0"

;
; WEP Key to use
;
HKR, ,                WEPKeyUse,       0,"1"
HKR, Default,         WEPKeyUse,       0,"1"

;
; WEP Key1
;
HKR, ,                WEPKey1,         0,""
HKR, Default,         WEPKey1,         0,""

;
; WEP Key2
;
HKR, ,                WEPKey2,         0,""
HKR, Default,         WEPKey2,         0,""

;
; WEP Key3
;
HKR, ,                WEPKey3,         0,""
HKR, Default,         WEPKey3,         0,""

;
; WEP Key4
;
HKR, ,                WEPKey4,         0,""
HKR, Default,         WEPKey4,         0,""

[PCI0301.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "PCI\VEN_1814&DEV_0301"

[PCI0302.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "PCI\VEN_1814&DEV_0302"

[PCI0401.ndi.reg]
HKR, Ndi,                         DeviceID,         0, "PCI\VEN_1814&DEV_0401"

[RT619X.ndi.reg]
HKR, ,                            NTMPDriver,       0, RT619x.sys

HKR, ,                            BusType,          0, 5
HKR, NDI,                         CardType,         0, "PCI"

HKR, ,                            RunningWin9X,     0, "1"
HKR, ,                            DevLoader,        0, "*ndis"
HKR, ,                            DeviceVxDs,       0, "RT619x.sys"
HKR, ,                            EnumPropPages,    0, "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,              DefUpper,         0, "ndis3"
HKR, Ndi\Interfaces,              DefLower,         0, "ethernet"
HKR, Ndi\Interfaces,              UpperRange,       0, "ndis3"
HKR, Ndi\Interfaces,              LowerRange,       0, "ethernet"

HKR, NDIS,                        LogDriverName,    0, "RT619X"
HKR, NDIS,                        MajorNdisVersion, 1, 03
HKR, NDIS,                        MinorNdisVersion, 1, 0A

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************

[DestinationDirs]
NT.CopyFiles            = 12    ; system32\drivers subdirectory on NT
XP.CopyFiles            = 12    ; system32\drivers subdirectory on Windows XP
win9x.CopyFiles         = 11    ; system subdirectory on win9x

[NT.CopyFiles]
rt61.sys                        ; NT Installation

[XP.CopyFiles]
rt61.sys                        ; XP Installation

[win9x.CopyFiles]
rt619x.sys                      ; Win9x Installation

[SourceDisksNames]
1                       = %INSTALL_DISK_STR%,,,

[SourceDisksFiles] 
rt61.sys                = 1
rt619x.sys              = 1

;*******************************************************************************************
; NT specific
;*******************************************************************************************
[RT61.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "RT61"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[RALINK.Service]
DisplayName                 = %RALINK.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[GIGABYTE.Service]
DisplayName                 = %GIGABYTE.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[Edimax.Service]
DisplayName                 = %EDIMAX.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[SITECOM.Service]
DisplayName                 = %SITECOM.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[DELTA.Service]
DisplayName                 = %DELTA.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[HAWKING.Service]
DisplayName                 = %HAWKING.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[BILLIONTON.Service]
DisplayName                 = %BILLIONTON.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[ASUS.Service]
DisplayName                 = %ASUS.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[ZINWELL.Service]
DisplayName                 = %ZINWELL.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[AMIT.Service]
DisplayName                 = %AMIT.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[CASTLENET.Service]
DisplayName                 = %CASTLENET.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[WN4306A.Service]
DisplayName                 = %WN4306A.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[SURECOM.Service]
DisplayName                 = %Surecom.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[VTECH.Service]
DisplayName                 = %VTECH.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[SIEMENS.Service]
DisplayName                 = %SIEMENS.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[CONCEPTRONIC.Service]
DisplayName                 = %CONCEPTRONIC.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[SMC.Service]
DisplayName                 = %SMC.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[CNET.Service]
DisplayName                 = %CNET.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[COREGA.Service]
DisplayName                 = %COREGA.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[AMIGO.Service]
DisplayName                 = %AMIGO.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[common.EventLog]
AddReg=common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\RT61.sys"
HKR, , TypesSupported,   0x00010001, 7

;*******************************************************************************************
; Strings
;*******************************************************************************************
[Strings]
Ralink                      = "Ralink Technology, Inc."
Gigabyte                    = "Gigabyte Technology Corp."
Edimax                      = "Edimax Technology Co., Ltd."
Sitecom                     = "Sitecom Europe BV"
Billionton                  = "Billionton Systems Inc."
Delta                       = "Delta Networks, Inc."
Hawking                     = "Hawking Technologies, Inc."
Asus                        = "ASUSTeK Computer Inc."
ZINWELL                     = "ZINWELL Technology, Inc."
AMIT                        = "AMIT Technology, Inc."
CASTLENET                   = "CastleNet Technology, Inc."
ACCTON                      = "Accton Technology Corporation"
Surecom                     = "SURECOM Technology Corp."
VTech                       = "VTech Telecommunications Ltd"
Siemens                     = "Siemens"
Conceptronic                = "2L (Conceptronic)"
SMC                         = "SMC Networks Inc."
CNet                        = "CNet Technology Inc."
Corega                      = "Corega Components"
Amigo                       = "AMIGO TECHNOLOGY LTD"

;*******************************************************************************************
; Device description
;*******************************************************************************************
Ralink_0301.DeviceDesc      = "Ralink Turbo Wireless LAN Card"
Ralink_0302.DeviceDesc      = "Ralink Wireless LAN Card V2"
Ralink_0401.DeviceDesc      = "Ralink MIMO Wireless LAN Card"

GigabyteWM01GS.DeviceDesc   = "Gigabyte GN-WM01GS Cardbus WLAN Card(Turbo)"
GigabyteWI01GS.DeviceDesc   = "Gigabyte GN-WI01GS mini PCI WLAN Card(Turbo)"
GigabyteWP01GS.DeviceDesc   = "Gigabyte GN-WP01GS PCI WLAN Card(Turbo)"
GigabyteWM02GS.DeviceDesc   = "Gigabyte GN-WM01GS Cardbus WLAN Card"
GigabyteWI02GS.DeviceDesc   = "Gigabyte GN-WI01GS mini PCI WLAN Card"
GigabyteWP02GS.DeviceDesc   = "Gigabyte GN-WP01GS PCI WLAN Card"
GigabyteWI02GM.DeviceDesc   = "Gigabyte GN-WI02GM mini PCI MIMO WLAN Card"
GigabyteWM01GM.DeviceDesc   = "Gigabyte GN-WM01GM Cardbus MIMO WLAN Card"
GigabyteWP01GM.DeviceDesc   = "Gigabyte GN-WP01GM PCI MIMO WLAN Card"

EW-7108.DeviceDesc          = "Edimax EW-7108 Series 802.11g Wireless LAN PC Card"
EW-7128.DeviceDesc          = "Edimax EW-7128 Series 802.11g Wireless LAN PCI Card"

GMIWLGRL2-B.DeviceDesc      = "Billionton mini PCI Wireless Lan 11B/G card"
GMIWLGRL2-N.DeviceDesc      = "mini PCI Wireless Lan 11B/G card"

Sitecom_WL112V2.DeviceDesc  = "Sitecom Wireless Network PC Card 54G WL-112v2"
Sitecom_WL115V2.DeviceDesc  = "Sitecom Wireless Network PCI Adapter 54G WL-115v2"
Sitecom_WL150.DeviceDesc    = "Sitecom Wirless Network PC Card MiMoXR WL-150"
Sitecom_WL151.DeviceDesc    = "Sitecom Wireless Network PCI Adapter MiMoXR WL-151"

DeltaPCI.DeviceDesc         = "IEEE 802.11g Wireless PCI Adapter"
DeltaCB.DeviceDesc          = "IEEE 802.11g Wireless PC Card"

Hawking0C54.DeviceDesc      = "Hawking HWC54GR Hi-Speed Wireless-G CardBus Card"
Hawking0B54.DeviceDesc      = "Hawking HWP54GR Hi-Speed Wireless-G PCI Card"

ASUS.DeviceDesc             = "ASUS 802.11b/g Wireless LAN Card"
ASUSGEN.DeviceDesc          = "802.11b/g Wireless LAN Card"

ZINWELLPCI.DeviceDesc       = "802.11g WLAN PCI Adapter"
ZINWELLMPCI.DeviceDesc      = "802.11g WLAN mini-PCI Adapter"
ZINWELLCARD.DeviceDesc      = "802.11g WLAN CardBus Adapter"
ZINWELLOEM1.DeviceDesc      = "AT&T Plug&Share 54 Mbps Wireless PCI Adapter"
ZINWELLOEM2.DeviceDesc      = "AT&T Plug&Share 54 Mbps Wireless Cardbus Adapter"

AMIT.DeviceDesc             = "AMIT 802.11 g Wireless LAN PC Card"
AMITMINI.DeviceDesc         = "AMIT MINI 802.11 g Wireless LAN PC Card"
AMITPCI.DeviceDesc          = "AMIT PCI 802.11 g Wireless LAN PC Card"
AMIT0100.DeviceDesc         = "802.11g MIMO Wireless Mini-PCI Adapter"
AMIT0200.DeviceDesc         = "802.11g MIMO Wireless Cardbus Adapter"
AMIT0300.DeviceDesc         = "802.11g MIMO Wireless PCI Adapter"
AMIT0202.DeviceDesc         = "AirLive MIMO-G Wireless Cardbus Adapter"
AMIT0302.DeviceDesc         = "AirLive MIMO-G Wireless PCI Adapter"
AMIT0203.DeviceDesc         = "802.11g MIMO Wireless Cardbus Adapter"
AMIT0303.DeviceDesc         = "802.11g MIMO Wireless PCI Adapter"
AMIT0204.DeviceDesc         = "802.11g MIMO Wireless Cardbus Adapter"
AMIT0304.DeviceDesc         = "802.11g MIMO Wireless PCI Adapter"
AMITCG.DeviceDesc           = "CG-WLCBGMO, corega MISO Wireless Cardbus Adapter"

CASTLENET.DeviceDesc        = "CastleNet WP1280 802.11 g Wireless LAN Card"

WN4306A.DeviceDesc          = "802.11g 54Mbps Wireless PC Card SE"

SurecomPCI.DeviceDesc       = "802.11g Wireless LAN PCI Adapter"
SurecomCardbus.DeviceDesc   = "802.11g 54M Wireless CardBus Adapter"

VTechPCI.DeviceDesc         = "VTech Wireless 802.11g PCI Adapter"
VTechCARD.DeviceDesc        = "VTech Wireless 802.11g PCMCIA Adapter"

Siemens.DeviceDesc          = "Siemens 802.11g PC Card Wireless Network Adapter"

Qcom.DeviceDesc             = "Ralink Wireless LAN Card V2"

M61_B833T.DeviceDesc        = "802.11g MiniPCI Turbo Wireless Adapter"
M61_B834T.DeviceDesc        = "802.11g PCI Turbo Wireless Adapter"
M61_B835T.DeviceDesc        = "802.11g CardBus Turbo Wireless Adapter"
M61_B833.DeviceDesc         = "802.11g MiniPCI Wireless Adapter"
M61_B834.DeviceDesc         = "802.11g PCI Wireless Adapter"
M61_B835.DeviceDesc         = "802.11g CardBus Wireless Adapter"

WLANm.DeviceDesc            = "WLAN 802.11g miniPCI module"
WLANc.DeviceDesc            = "WLAN 802.11g Cardbus module"

AMIGO.DeviceDesc1           = "Wireless PC Card"
AMIGO.DeviceDesc2           = "Wireless miniPCI Adapter"
AMIGO.DeviceDesc3           = "Wireless PCI Adapter"

CNetPCI.DeviceDesc          = "802.11a/g Wireless LAN PCI"
CNetMPCI.DeviceDesc         = "802.11a/g Wireless LAN Mini-PCI"
CNetCardbus.DeviceDesc      = "802.11a/g Wireless LAN CardBus"

Conceptronic_PCCard.DeviceDesc = "Conceptronic 54g Wireless PC-Card"
Conceptronic_PCICard.DeviceDesc = "Conceptronic 54g Wireless PCI Card"

SMC_EE04.DeviceDesc         = "SMC SMCWCB-GM EZ Connect TM 802.11g Wireless Cardbus Adapter with MIMO Technology"
SMC_EE05.DeviceDesc         = "SMC SMCWPCI-GM EZ Connect TM 802.11g Wireless PCI Adapter with MIMO Technology"

CNet_6221.DeviceDesc        = "CNet Turbo Wireless-G PCI Adapter"
CNet_7221.DeviceDesc        = "CNet Turbo Wireless-G miniPCI Adapter"
CNet_8221.DeviceDesc        = "CNet Turbo Wireless-G Cardbus Adapter"
CNet_6121.DeviceDesc        = "CNet Wireless-G PCI Adapter"
CNet_7121.DeviceDesc        = "CNet Wireless-G miniPCI Adapter"
CNet_8121.DeviceDesc        = "CNet Wireless-G Cardbus Adapter"
CNet_6321.DeviceDesc        = "CNet Wireless-G PCI Adapter"
CNet_7321.DeviceDesc        = "CNet Wireless-G miniPCI Adapter"
CNet_8321.DeviceDesc        = "CNet Wireless-G Cardbus Adapter"

Corega.DeviceDesc           = "CG-WLCB54AGM"

Amigo_9141.DeviceDesc       = "Wireless PC Card"
Amigo_9221.DeviceDesc       = "Wireless miniPCI Adapter"
Amigo_9261.DeviceDesc       = "Wireless PCI Adapter"

INSTALL_DISK_STR            = "Ralink Wireless LAN Installation Disk"

RALINK.Service.DispName     = "Ralink RT61 Wireless Driver"
GIGABYTE.Service.DispName   = "Gigabyte RT61 Wireless Driver"
EDIMAX.Service.DispName     = "Edimax RT61 Wireless Driver"
SITECOM.Service.DispName    = "Sitecom RT61 Wireless Network Driver"
DELTA.Service.DispName      = "Delta Networks RT61 Wireless Driver"
HAWKING.Service.DispName    = "Hawking RT61 Wireless Driver"
BILLIONTON.Service.DispName = "Billionton RT61 Wireless Driver"
ASUS.Service.DispName       = "AsusTek RT61 Wireless Driver"
ZINWELL.Service.DispName    = "ZINWELL RT61 Wireless Driver"
AMIT.Service.DispName       = "AMIT RT61 Wireless Driver"
CASTLENET.Service.DispName  = "CastleNet RT61 Wireless Driver"
WN4306A.Service.DispName    = "RT61 802.11g 54Mbps Wireless PC Card SE Driver"
Surecom.Service.DispName    = "Surecom RT61 Wireless Driver"
VTECH.Service.DispName      = "VTech RT61 802.11g Wireless Driver"
SIEMENS.Service.DispName    = "Siemens RT61 Wireless 802.11b/g Driver(RT61)"
Conceptronic.Service.DispName = "Conceptronic RT61 54g Wireless Driver"
SMC.Service.DispName        = "SMC RT61 Wireless Driver"
CNET.Service.DispName       = "CNET RT61 Wireless Driver"
COREGA.Service.DispName     = "COREGA Wireless Driver"
AMIGO.Service.DispName      = "Amigo RT61 Wireless Driver"

; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = "IEEE 802.11g Wireless Card."
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"

