;/*++
;
;Copyright (c) 2004 3Com Corporation , Incorporated All Rights Reserved
;
;Module Name:
;
;    3C154A72.inf
;
;Abstract:
;    INF file for installing  Wireless Network Adapter
;
;    Installs 3C154A72.sys (NDIS 5/5.1 driver) on NT platforms (2000, XP and greater)
;    Installs 3c154A9x.sys (NDIS 5 driver) on 9x platforms 
;
;--*/

[Version]
Signature   = "$CHICAGO$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Vendor%
Compatible  = 1
DriverVer   = 04/07/2004,3.0.0.46
Catalogfile = 3C154A72.cat

[Manufacturer]
%Vendor%     = DeviceList

[ControlFlags]
ExcludeFromSelect = *

[DeviceList]
%DeviceList.DeviceDesc%      = NIC1,        PCI\VEN_168C&DEV_0013&SUBSYS_600210B7
; Windows 9X specific entries

[NIC1]
AddReg          = NIC1.id.reg, NIC1.common.reg, NIC1.win.reg, NIC1.abg.reg
CopyFiles       = NIC1.win.CopyFiles,NETRWCCU.Apps, DEFAULTDESTDIRS
DelFiles        = NIC1.DelIniFiles

; Windows NT specific entries

[NIC1.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = NIC1.common.reg, NIC1.reg, NIC1.common.reg, NIC1.abg.reg
CopyFiles       = NIC1.CopyFiles.nt,NETRWCCU.Apps, DEFAULTDESTDIRS
DelFiles        = NIC1.DelIniFiles

[NIC1.NT.Services]
AddService      = 3C154A72, 2, NIC1.Service, common.EventLog

[NIC1.NT.CoInstallers]
 CopyFiles      = NETRWCoInstallFile
 AddReg         = NETRWCCU.CoInstallers_AddReg


;----------------------------------------------------------------------------
; Win9x id registry sections
; These are not needed by NT

[NIC1.id.reg]
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\RunOnce, "3C154A72",, "%11%\CCUA72.exe"
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_600210B7"

;
; 5211 Enumerated Types
;

[NIC1.abg.reg]
HKR, ,                                  NetBand,                        0x00002,  "29"
HKR, CustomParams\Configurations,       NicType,                        0x10003,  1
HKR, ,                                  radioEnable,                    0x00002,  "0"
;-----------------------------------------------------------------------------

;
; 5211 common
;

[NIC1.common.reg]

HKR, Ndi\params\MapRegisters,           ParamDesc,                      0,  %MapRegisters%
HKR, Ndi\params\MapRegisters,           default,                        0,  "256"
HKR, Ndi\params\MapRegisters,           min,                            0,  "32"
HKR, Ndi\params\MapRegisters,           max,                            0,  "512"
HKR, Ndi\params\MapRegisters,           step,                           0,  "8"
HKR, Ndi\params\MapRegisters,           base,                           0,  "10"
HKR, Ndi\params\MapRegisters,           type,                           0,  "int"

HKR, Ndi\params\NetworkAddress,         ParamDesc,                      0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,         default,                        0,  ""
HKR, Ndi\params\NetworkAddress,         LimitText,                      0,  "12"
HKR, Ndi\params\NetworkAddress,         UpperCase,                      0,  "1"
HKR, Ndi\params\NetworkAddress,         optional,                       0,  "1"
HKR, Ndi\params\NetworkAddress,         type,                           0,  "edit"

HKR, Ndi\params\sleepMode,              ParamDesc,                      0,  %sleepMode%
HKR, Ndi\params\sleepMode,              Base,                           0,  "10"
HKR, Ndi\params\sleepMode,              default,                        0,  "2"
HKR, Ndi\params\sleepMode,              type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,         "0",                            0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,         "2",                            0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,         "1",                            0,  %sleepModeMax%

HKR, Ndi\params\tpc,                    ParamDesc,                      0,  %tpc%
HKR, Ndi\params\tpc,                    Base,                           0,  "10"
HKR, Ndi\params\tpc,                    default,                        0,  "0"
HKR, Ndi\params\tpc,                    type,                           0,  "enum"
HKR, Ndi\params\tpc\enum,               "0",                            0,  %tpc100%
HKR, Ndi\params\tpc\enum,               "1",                            0,  %tpc50%
HKR, Ndi\params\tpc\enum,               "2",                            0,  %tpc25%
HKR, Ndi\params\tpc\enum,               "3",                            0,  %tpc12%
HKR, Ndi\params\tpc\enum,               "4",                            0,  %tpcLowest%

HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  "1"
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,  %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,  "10"
HKR, Ndi\params\radioEnable,            default,                        0,  "1"
HKR, Ndi\params\radioEnable,            type,                           0,  "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,  %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,  %radioEnableOff%

HKR, Ndi\params\authTypeUseOnly,               ParamDesc,                      0,  %authTypeUseOnly%
HKR, Ndi\params\authTypeUseOnly,               Base,                           0,  "10"
HKR, Ndi\params\authTypeUseOnly,               default,                        0,  "0"
HKR, Ndi\params\authTypeUseOnly,               type,                           0,  "enum"
HKR, Ndi\params\authTypeUseOnly\enum,          "0",                            0,  %authAuto%
HKR, Ndi\params\authTypeUseOnly\enum,          "1",                            0,  %authOpen%
HKR, Ndi\params\authTypeUseOnly\enum,          "2",                            0,  %authShared%

HKR, ,                                  AdHocBand,                      0x00002,  "0"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"
HKR, ,                                  beaconInterval,                 0x00002,  "100"
HKR, ,                                  bkScanEnable,                   0x00002,  "1"
HKR, ,                                  bssType,                        0x00002,  "1"
HKR, ,                                  ccode,                          0x00002,  "JP"
HKR, ,                                  clist,                          0x00002,  ""
HKR, ,                                  defaultKey,                     0x00002,  "0"
HKR, ,                                  EncryptionAlg,                  0x00002,  "2"
HKR, ,                                  FragThreshold,                  0x00002,  "2346"
HKR, ,                                  HwTxRetries,                    0x00002,  "4"
HKR, ,                                  privacyInvoked,                 0x00002,  "0"
HKR, ,                                  QoS,                            0x00002,  "0"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                                  RTSThreshold,                   0x00002,  "2346"
HKR, ,                                  scanType,                       0x00002,  "2"
HKR, ,                                  SwTxRetryScale,                 0x00002,  "6"
HKR, ,                                  SmeEnable,                      0x00002,  "1"

HKR, CustomParams\Configurations,       MajorVersion,                   0x10003,  2
HKR, CustomParams\Configurations,       MinorVersion,                   0x10003,  0

HKR, CustomParams\Configurations,       SelectedConfigurationIndex,     0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationName,      0x00002,  "Default"


;-----------------------------------------------------------------------------
; NT specific
;

[NIC1.reg]
HKR, Ndi,             Service,      0, "3C154A72"
HKR, Ndi\Interfaces,  UpperRange,   0, "ndis5"
HKR, Ndi\Interfaces,  LowerRange,   0, "ethernet"
HKR, ,                aifs,         0, "2"
HKR, ,                cwmin,        0, "15"


[NIC1.Service]
DisplayName     = %NIC1.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\3C154A72.sys
LoadOrderGroup  = NDIS

;-----------------------------------------------------------------------------
; NT/XP common
;
[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, ,                  EventMessageFile,   0x00020000,   "%%SystemRoot%%\System32\netevent.dll"
HKR, ,                  TypesSupported,     0x00010001,   7

;----------------------------------------------------------------------------
; Win9x specific
;
[NIC1.win.reg]
HKR, ,                  DevLoader,          0,    "*ndis"
HKR, ,                  DeviceVxDs,         0,    "3C154A9x.sys"
HKR, ,                  EnumPropPages,      0,    "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,    DefUpper,           0,    "ndis3"
HKR, Ndi\Interfaces,    DefLower,           0,    "ethernet"
HKR, Ndi\Interfaces,    UpperRange,         0,    "ndis3"
HKR, Ndi\Interfaces,    LowerRange,         0,    "ethernet"


HKR, NDIS,              LogDriverName,      0,    "3C154A9x"
HKR, NDIS,              MajorNdisVersion,   1,    03
HKR, NDIS,              MinorNdisVersion,   1,    0A
HKR, ,                  aifs,               0,    "2"
HKR, ,                  cwmin,              0,    "15"

HKR, Ndi\Install,       ndis3,              0,    "3Com.install"

[NETRWCCU.CoInstallers_AddReg]
HKR,,CoInstallers32,0x10000,"CCUA72.dll, CoCCU"

[NETRWCoInstallFile]
CCUA72.dll,,,2

[NETRWCCU.Apps]
CCUA72.exe,,,2

;----------------------------------------------------------------------------
; Win9x Files to Copy
[NIC1.win.CopyFiles]
3C154A9X.sys,,,2
;----------------------------------------------------------------------------
; NT Files to Copy
[NIC1.CopyFiles.nt]
3C154A72.sys,,,2

[NIC1.DelIniFiles]
Athnic.ini,,,1

[SourceDisksNames]
;
; diskid = description[, [tagfile] [, <unused>, subdir]]
;
1 = %3Com_Disk%,,,

;----------------------------------------------------------------------------
; Source Files
[SourceDisksFiles]
3C154A9X.sys                   = 1,, ; on distribution disk 1
3C154A72.sys                   = 1,, ; on distribution disk 1
CCUA72.dll 		       = 1
CCUA72.exe 		       = 1

[DestinationDirs]
NIC1.CopyFiles.nt             = 12
NIC1.win.CopyFiles            = 11 ; %SystemRoot%\system\drivers 
NIC1.DelIniFiles              = 10,system32\drivers ; %SystemRoot%\system32\drivers 
DefaultDestDir                = 11
NETRWCCU.Apps                 = 11
NETRWCoInstallFile            = 11

[DEFAULTDESTDIRS]
;


[Strings]
Vendor                       = "3Com Corporation."
authTypeUseOnly              = "802.11 Authentication Type"
authAuto                     = "Auto"
authOpen                     = "Open"
authShared                   = "Shared"
MapRegisters                 = "Map Registers"
NetworkAddress               = "Network Address"
sleepMode                    = "Power Save Mode"
sleepModeOff                 = "Off"
sleepModeNormal              = "Normal"
sleepModeMax                 = "Maximum"
tpc                          = "Transmit Power"
tpcLowest                    = "Lowest"
tpc12                        = "12.5%"
tpc25                        = "25%"
tpc50                        = "50%"
tpc100                       = "100%"
shortPreamble                = "802.11b Preamble"
shortPreambleEnable          = "Long and Short"
shortPreambleDisable         = "Long only"
radioEnable                  = "Radio On/Off"
radioEnableOn                = "On"
radioEnableOff               = "Off"

3Com_Disk                    = "3Com Driver Disk 1"
DeviceList.DeviceDesc        = "3Com OfficeConnect Wireless a/b/g PC Card (3CRWE154A72)"
NIC1.Service.DispName        = "3Com OfficeConnect Wireless a/b/g PC Card (3CRWE154A72) Service"
