;****************************************************************************************
;
; rt73.inf
;
;   This installation script supports Windows 98,Me,2000 & XP for the
;   Ralink RT73 series USB Wireless LAN Card.
;
;   Copyright (c)2006 , Ralink Technology Corp., All Rights Reserved
;   All Rights Reserved.
;   Developed by RaLink Technology, Corp. -- http://www.ralinktech.com
;
;****************************************************************************************

[Version]
Signature       = "$Chicago$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %Provider%
Compatible      = 1
DriverVer       = 09/07/2006, 1.01.03.0000
CatalogFile     = rt73.cat            ;for WHQL certified

[ControlFlags]
;***********Ralink 802.11g board  ***********
;ExcludeFromSelect = USB\VID_148F&PID_2573

[Manufacturer]
%Ralink%        = Ralink
%Qcom%          = Qcom
%Gigabyte%      = Gigabyte
%Conceptronic%  = Conceptronic
%Surecom%       = Surecom
%Asus%          = ASUS
%Amit%          = AMIT
%CNet%          = CNet
%Huawei-3Com%   = Huawei-3Com
%Askey%         = Askey
%Amigo%         = Amigo

[Ralink]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Ralink.DeviceDesc%         = Ralink.ndi,           USB\VID_148F&PID_2573
%Ralink.DeviceDesc%         = Ralink_2671.ndi,      USB\VID_148F&PID_2671
; MSI
%M6877.DeviceDesc%          = M6877.ndi,            USB\VID_0DB0&PID_6877
%MA874.DeviceDesc%          = MA874.ndi,            USB\VID_0DB0&PID_A874
%M6874.DeviceDesc%          = M6874.ndi,            USB\VID_0DB0&PID_6874
%MA861.DeviceDesc%          = MA861.ndi,            USB\VID_0DB0&PID_A861
;
%GMEWLGRL.DeviceDesc%       = GMEWLGRL.ndi,         USB\VID_1631&PID_C019

[Qcom]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Qcom.DeviceDesc%           = Qcom.ndi,             USB\VID_18E8&PID_6196
%Qcom.DeviceDesc%           = Qcom2.ndi,            USB\VID_18E8&PID_6229

[Gigabyte]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Gigabyte.DeviceDesc%       = Gigabyte.ndi,         USB\VID_1044&PID_8008
%Gigabyte2.DeviceDesc%      = Gigabyte2.ndi,        USB\VID_1044&PID_800A

[Conceptronic]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Conceptronic.DeviceDesc%   = Conceptronic.ndi,     USB\VID_14B2&PID_3C22

[Surecom]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Surecom.DeviceDesc%        = Surecom.ndi,          USB\VID_0769&PID_31F3

[ASUS]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%ASUS.DeviceDesc%           = ASUS.ndi,             USB\VID_0B05&PID_1723
%ASUSGEN.DeviceDesc%        = ASUSGEN.ndi,          USB\VID_0B05&PID_1724

[AMIT]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%AMIT.DeviceDesc%           = AMIT.ndi,             USB\VID_18C5&PID_0002

[CNet]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%CNet.DeviceDesc%           = CNET.ndi,             USB\VID_1371&PID_9032

[Huawei-3Com]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Huawei-3Com.DeviceDesc%    = HUAWEI.ndi,           USB\VID_1472&PID_0009

[Askey]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Askey.DeviceDesc%          = Askey.ndi,            USB\VID_1690&PID_0722

[Amigo]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Amigo1.DeviceDesc%         = Amigo1.ndi,           USB\VID_148F&PID_9021
%Amigo2.DeviceDesc%         = Amigo2.ndi,           USB\VID_0EB0&PID_9021

;*******************************************************************************************
; Windows 9X specific entries
;*******************************************************************************************

[Ralink.ndi]
AddReg                  = USB_148F_2573.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Ralink_2671.ndi]
AddReg                  = USB_148F_2671.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[M6877.ndi]
AddReg                  = USB_0DB0_6877.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[MA874.ndi]
AddReg                  = USB_0DB0_A874.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[M6874.ndi]
AddReg                  = USB_0DB0_6874.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[MA861.ndi]
AddReg                  = USB_0DB0_A861.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[GMEWLGRL.ndi]
AddReg                  = USB_1631_C019.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Qcom.ndi]
AddReg                  = USB_18E8_6196.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Qcom2.ndi]
AddReg                  = USB_18E8_6229.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Gigabyte.ndi]
AddReg                  = USB_1044_8008.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Gigabyte2.ndi]
AddReg                  = USB_1044_800A.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Conceptronic.ndi]
AddReg                  = USB_14B2_3C22.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Surecom.ndi]
AddReg                  = USB_0769_11F3.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[ASUS.ndi]
AddReg                  = USB_0B05_1723.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[ASUSGEN.ndi]
AddReg                  = USB_0B05_1724.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[AMIT.ndi]
AddReg                  = USB_18C5_0002.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[CNET.ndi]
AddReg                  = USB_1371_9032.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[HUAWEI.ndi]
AddReg                  = USB_1472_0009.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Askey.ndi]
AddReg                  = USB_1690_0722.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Amigo1.ndi]
AddReg                  = USB_148F_9021.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[Amigo2.ndi]
AddReg                  = USB_0EB0_9021.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

;*******************************************************************************************
; NT specific entries
;*******************************************************************************************

[Ralink.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Ralink_2671.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[M6877.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[MA874.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[M6874.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[MA861.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[GMEWLGRL.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Qcom.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Qcom2.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Gigabyte.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Gigabyte2.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Conceptronic.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Surecom.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[ASUS.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[ASUSGEN.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[AMIT.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[CNET.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[HUAWEI.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Askey.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Amigo1.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[Amigo2.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

; NT services sections
[Ralink.ndi.NT.Services]
AddService              = RT73, 2, Ralink.Service, common.EventLog

[Ralink_2671.ndi.NT.Services]
AddService              = RT73, 2, Ralink.Service, common.EventLog

[M6877.ndi.NT.Services]
AddService              = RT73, 2, Ralink.Service, common.EventLog

[MA874.ndi.NT.Services]
AddService              = RT73, 2, Ralink.Service, common.EventLog

[M6874.ndi.NT.Services]
AddService              = RT73, 2, Ralink.Service, common.EventLog

[MA861.ndi.NT.Services]
AddService              = RT73, 2, Ralink.Service, common.EventLog

[GMEWLGRL.ndi.NT.Services]
AddService              = RT73, 2, Ralink.Service, common.EventLog

[Qcom.ndi.NT.Services]
AddService              = RT73, 2, Qcom.Service, common.EventLog

[Qcom2.ndi.NT.Services]
AddService              = RT73, 2, Qcom.Service, common.EventLog

[Gigabyte.ndi.NT.Services]
AddService              = RT73, 2, Gigabyte.Service, common.EventLog

[Gigabyte2.ndi.NT.Services]
AddService              = RT73, 2, Gigabyte.Service, common.EventLog

[Conceptronic.ndi.NT.Services]
AddService              = RT73, 2, Conceptronic.Service, common.EventLog

[Surecom.ndi.NT.Services]
AddService              = RT73, 2, Surecom.Service, common.EventLog

[ASUS.ndi.NT.Services]
AddService              = RT73, 2, ASUS.Service, common.EventLog

[ASUSGEN.ndi.NT.Services]
AddService              = RT73, 2, ASUS.Service, common.EventLog

[AMIT.ndi.NT.Services]
AddService              = RT73, 2, AMIT.Service, common.EventLog

[CNET.ndi.NT.Services]
AddService              = RT73, 2, CNET.Service, common.EventLog

[HUAWEI.ndi.NT.Services]
AddService              = RT73, 2, HUAWEI.Service, common.EventLog

[Askey.ndi.NT.Services]
AddService              = RT73, 2, Askey.Service, common.EventLog

[Amigo1.ndi.NT.Services]
AddService              = RT73, 2, Amigo.Service, common.EventLog

[Amigo2.ndi.NT.Services]
AddService              = RT73, 2, Amigo.Service, common.EventLog

;*******************************************************************************************
; common regs for NT and W9x
;*******************************************************************************************

[Common.reg]
;*******************************************************************************************
; System Level Property

;
; Current Profile
;
HKR, ,                    CurProfile,      0,""
HKR, Default,             CurProfile,      0,""

;
; Radio On/Off
;
HKR, ,                            Radio,           0, "0"
HKR, NDI\params\Radio,            ParamDesc,       0, "Radio On/Off"
HKR, NDI\params\Radio,            type,            0, "enum"
HKR, NDI\params\Radio,            default,         0, "0"
HKR, NDI\params\Radio\enum,       1,               0, "Disable"
HKR, NDI\params\Radio\enum,       0,               0, "Enable"

;
; Auto Reconnect Mode
;
HKR, ,                                  AutoReconnect,      0, "1"
HKR, NDI\params\AutoReconnect,          ParamDesc,          0, "Auto Reconnect Mode"
HKR, NDI\params\AutoReconnect,          type,               0, "enum"
HKR, NDI\params\AutoReconnect,          default,            0, "1"
HKR, NDI\params\AutoReconnect\enum,     0,                  0, "Disable"
HKR, NDI\params\AutoReconnect\enum,     1,                  0, "Enable"

;
; Show Hidden SSID in Site Survey Page
;
HKR, ,                                  ShowHiddenSSID,     0, "0"   ; 0=disable(default), 1=enable

;
; Country Region G Band
;
HKR, ,                                 CountryRegion,      0, "0"
HKR, NDI\params\CountryRegion,         ParamDesc,          0, "Country Region 11G"
HKR, NDI\params\CountryRegion,         type,               0, "enum"
HKR, NDI\params\CountryRegion,         default,            0, "0"
HKR, NDI\params\CountryRegion\enum,    0,                  0, "(Channel 1 - 11)"
HKR, NDI\params\CountryRegion\enum,    1,                  0, "(Channel 1 - 13)"
HKR, NDI\params\CountryRegion\enum,    2,                  0, "(Channel 10 - 11)"
HKR, NDI\params\CountryRegion\enum,    3,                  0, "(Channel 10 - 13)"
HKR, NDI\params\CountryRegion\enum,    4,                  0, "(Channel 14)"
HKR, NDI\params\CountryRegion\enum,    5,                  0, "(Channel 1 - 14)"
HKR, NDI\params\CountryRegion\enum,    6,                  0, "(Channel 3 - 9)"
HKR, NDI\params\CountryRegion\enum,    7,                  0, "(Channel 5 - 13)"

;
; Country Region A Band
;
HKR, ,                                 CountryRegionABand, 0, "7"
HKR, NDI\params\CountryRegionABand,    ParamDesc,          0, "Country Region 11A"
HKR, NDI\params\CountryRegionABand,    type,               0, "enum"
HKR, NDI\params\CountryRegionABand,    default,            0, "7"
HKR, NDI\params\CountryRegionABand\enum,0,                 0, "Ch(36 - 64,149 - 165)"
HKR, NDI\params\CountryRegionABand\enum,1,                 0, "Ch(36 - 140)"
HKR, NDI\params\CountryRegionABand\enum,2,                 0, "Ch(36 - 64)"
HKR, NDI\params\CountryRegionABand\enum,3,                 0, "Ch(52 - 64,149 - 161)"
HKR, NDI\params\CountryRegionABand\enum,4,                 0, "Ch(149 - 165)"
HKR, NDI\params\CountryRegionABand\enum,5,                 0, "Ch(149 - 161)"
HKR, NDI\params\CountryRegionABand\enum,6,                 0, "Ch(36 - 48)"
HKR, NDI\params\CountryRegionABand\enum,7,                 0, "Ch(36 - 165)"
HKR, NDI\params\CountryRegionABand\enum,8,                 0, "Ch(52 - 64)"
HKR, NDI\params\CountryRegionABand\enum,9,                 0, "Ch(34 - 46)"
HKR, NDI\params\CountryRegionABand\enum,10,                0, "Ch(34 - 64)"

;*******************************************************************************************
; Advance Page

;
; OpMode
;
HKR, ,                            OpMode,          0, "0"

;
; WirelessMode
;
HKR, ,                            WirelessMode,    0, "3"

;
; Enable TX Burst
;
HKR, ,                            TXBurst,         0, "0"

;
; Use Short Slot Time
;
HKR, ,                            ShortSlot,       0, "1"

;
; Use Turbo rate
;
HKR, ,                            TurboRate,       0, "0"

;
; Use Ofdm rate in adhoc mode
;
HKR, ,                            AdhocOfdm,       0, "0"
HKR, NDI\params\AdhocOfdm,              ParamDesc, 0, "Adhoc Wireless Mode"
HKR, NDI\params\AdhocOfdm,              type,      0, "enum"
HKR, NDI\params\AdhocOfdm,              default,   0, "0"
HKR, NDI\params\AdhocOfdm\enum,         0,         0, "802.11 B Only"
HKR, NDI\params\AdhocOfdm\enum,         1,         0, "802.11 B/G Mix"
HKR, NDI\params\AdhocOfdm\enum,         2,         0, "802.11 G Only"
HKR, NDI\params\AdhocOfdm\enum,         3,         0, "802.11 A Only"
HKR, NDI\params\AdhocOfdm\enum,         4,         0, "802.11 A/B/G Mix"

;
; Use BG Protection
;
HKR, ,                            BGProtection,    0, "0"
HKR, NDI\params\BGProtection,           ParamDesc, 0, "B/G Protection"
HKR, NDI\params\BGProtection,           type,      0, "enum"
HKR, NDI\params\BGProtection,           default,   0, "0"
HKR, NDI\params\BGProtection\enum,      0,         0, "Auto"
HKR, NDI\params\BGProtection\enum,      1,         0, "On"
HKR, NDI\params\BGProtection\enum,      2,         0, "Off"

;
; FrameAggregation
;
HKR, ,                            FrameAggregation,0, "1"
HKR, NDI\params\FrameAggregation,       ParamDesc, 0, "Frame Aggregation"
HKR, NDI\params\FrameAggregation,       type,      0, "enum"
HKR, NDI\params\FrameAggregation,       default,   0, "1"
HKR, NDI\params\FrameAggregation\enum,  0,         0, "Disable"
HKR, NDI\params\FrameAggregation\enum,  1,         0, "Enable"

;
; IEEE80211H
;
HKR, ,                            IEEE80211H,      0, "0"
HKR, NDI\params\IEEE80211H,       ParamDesc,       0, "IEEE802.11h"
HKR, NDI\params\IEEE80211H,       type,            0, "enum"
HKR, NDI\params\IEEE80211H,       default,         0, "0"
HKR, NDI\params\IEEE80211H\enum,  0,               0, "Disable"
HKR, NDI\params\IEEE80211H\enum,  1,               0, "Enable"

;
; AutoChannelSelect
;
HKR, ,                            AutoChannelSelect,      0, "0"
HKR, NDI\params\AutoChannelSelect,       ParamDesc,0, "Auto Channel Select"
HKR, NDI\params\AutoChannelSelect,       type,     0, "enum"
HKR, NDI\params\AutoChannelSelect,       default,  0, "0"
HKR, NDI\params\AutoChannelSelect\enum,  0,        0, "Disable"
HKR, NDI\params\AutoChannelSelect\enum,  1,        0, "Enable"

;
; WMMCapable
;
HKR, ,                            WMMCapable,      0, "0"
HKR, NDI\params\WMMCapable,             ParamDesc, 0, "WMM Capable"
HKR, NDI\params\WMMCapable,             type,      0, "enum"
HKR, NDI\params\WMMCapable,             default,   0, "0"
HKR, NDI\params\WMMCapable\enum,        0,         0, "Disable"
HKR, NDI\params\WMMCapable\enum,        1,         0, "Enable"

;
; APSDCapable
;
HKR, ,                            APSDCapable,     0, "0"
HKR, NDI\params\APSDCapable,            ParamDesc, 0, "APSD Capable"
HKR, NDI\params\APSDCapable,            type,      0, "enum"
HKR, NDI\params\APSDCapable,            default,   0, "0"
HKR, NDI\params\APSDCapable\enum,       0,         0, "Disable"
HKR, NDI\params\APSDCapable\enum,       1,         0, "Enable"

;
; APSDAC_BE
;
HKR, ,                            APSDAC_BE,       0, "0"
HKR, NDI\params\APSDAC_BE,              ParamDesc, 0, "AC_BE support APSD"
HKR, NDI\params\APSDAC_BE,              type,      0, "enum"
HKR, NDI\params\APSDAC_BE,              default,   0, "0"
HKR, NDI\params\APSDAC_BE\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_BE\enum,         1,         0, "Enable"

;
; APSDAC_BK
;
HKR, ,                            APSDAC_BK,       0, "0"
HKR, NDI\params\APSDAC_BK,              ParamDesc, 0, "AC_BK support APSD"
HKR, NDI\params\APSDAC_BK,              type,      0, "enum"
HKR, NDI\params\APSDAC_BK,              default,   0, "0"
HKR, NDI\params\APSDAC_BK\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_BK\enum,         1,         0, "Enable"

;
; APSDAC_VI
;
HKR, ,                            APSDAC_VI,       0, "0"
HKR, NDI\params\APSDAC_VI,              ParamDesc, 0, "AC_VI support APSD"
HKR, NDI\params\APSDAC_VI,              type,      0, "enum"
HKR, NDI\params\APSDAC_VI,              default,   0, "0"
HKR, NDI\params\APSDAC_VI\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_VI\enum,         1,         0, "Enable"

;
; APSDAC_VO
;
HKR, ,                            APSDAC_VO,       0, "0"
HKR, NDI\params\APSDAC_VO,              ParamDesc, 0, "AC_VO support APSD"
HKR, NDI\params\APSDAC_VO,              type,      0, "enum"
HKR, NDI\params\APSDAC_VO,              default,   0, "0"
HKR, NDI\params\APSDAC_VO\enum,         0,         0, "Disable"
HKR, NDI\params\APSDAC_VO\enum,         1,         0, "Enable"

;
; MaxSPLength
;
HKR, ,                            MaxSPLength,     0, "0"
HKR, Default,                     MaxSPLength,     0, "0"
HKR, NDI\params\MaxSPLength,      ParamDesc,       0, "Max Service Period Length"
HKR, NDI\params\MaxSPLength,      type,            0, "int"
HKR, Ndi\params\MaxSPLength,      default,         0, "0"
HKR, NDI\params\MaxSPLength,      min,             0, "0"
HKR, NDI\params\MaxSPLength,      max,             0, "3"
HKR, NDI\params\MaxSPLength,      step,            0, "1"
HKR, NDI\params\MaxSPLength,      optional,        0, "0"

;
; DLSCapable
;
HKR, ,                            DLSCapable,      0, "0"
HKR, NDI\params\DLSCapable,             ParamDesc, 0, "DLS Capable"
HKR, NDI\params\DLSCapable,             type,      0, "enum"
HKR, NDI\params\DLSCapable,             default,   0, "0"
HKR, NDI\params\DLSCapable\enum,        0,         0, "Disable"
HKR, NDI\params\DLSCapable\enum,        1,         0, "Enable"

;
; PSP XLink mode
;
HKR, ,                            PSPXlink,        0, "0"
HKR, NDI\params\PSPXlink,         ParamDesc,       0, "PSP Xlink Mode"
HKR, NDI\params\PSPXlink,         type,            0, "enum"
HKR, NDI\params\PSPXlink,         default,         0, "0"
HKR, NDI\params\PSPXlink\enum,    0,               0, "Disable"
HKR, NDI\params\PSPXlink\enum,    1,               0, "Enable"

;
; CCX2 control
;
HKR, ,                            CCX2Control,     0x00010001, 0x00fa4600

;
; Vendor Description
;
HKR, ,                            VendorDesc,      0, %VENDOR_DESC_DEF_STR%
HKR, Default,                     VendorDesc,      0, %VENDOR_DESC_DEF_STR%

;*******************************************************************************************
; Profile

;
; SSID
;
HKR, ,                            SSID,            0, %SSID_DEF_STR%
HKR, Default,                     SSID,            0, %SSID_DEF_STR%
HKR, NDI\params\SSID,             ParamDesc,       0, "SSID"
HKR, NDI\params\SSID,             type,            0, "edit"
HKR, NDI\params\SSID,             limitText,       0, "32"
HKR, NDI\params\SSID,             default,         0, %SSID_DEF_STR%

;
; Network Type
;
HKR, ,                            NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, Default,                     NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType,      ParamDesc,       0, "Network Type"
HKR, NDI\params\NetworkType,      type,            0, "enum"
HKR, NDI\params\NetworkType,      default,         0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType\enum, 0,               0, "802.11 Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1,               0, "Infrastructure"

;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%


;*******************************************************************************************
; System Configuration Page

;
; Local Administration MAC Network Address
;
HKR, ,                            NetworkAddress,  0, ""
HKR, Default,                     NetworkAddress,  0, ""
HKR, NDI\params\NetworkAddress,   ParamDesc,       0, "Local Administration MAC Network Address"
HKR, NDI\params\NetworkAddress,   type,            0, "edit"
HKR, NDI\params\NetworkAddress,   limitText,       0, "12"
HKR, NDI\params\NetworkAddress,   default,         0, ""

;
; Power Saving Mode
;
HKR, ,                            PSMode,          0, "0"
HKR, Default,                     PSMode,          0, "0"
HKR, NDI\params\PSMode,           ParamDesc,       0, "Power Saving Mode"
HKR, NDI\params\PSMode,           type,            0, "enum"
HKR, NDI\params\PSMode,           default,         0, "0"
HKR, NDI\params\PSMode\enum,      0,               0, "CAM (Constantly Awake Mode)"
;HKR, NDI\params\PSMode\enum,      1,               0, "Max_PSP (Max Power Savings)"
HKR, NDI\params\PSMode\enum,      2,               0, "Fast_PSP (Power Save Mode)"

;
; CAM when AC Power
;
;HKR, ,                            ACPowerCam,      0, "0"
;HKR, Default,                     ACPowerCam,      0, "0"
;HKR, NDI\params\ACPowerCam,       ParamDesc,       0, "CAM when AC Power"
;HKR, NDI\params\ACPowerCam,       type,            0, "enum"
;HKR, NDI\params\ACPowerCam,       default,         0, "0"
;HKR, NDI\params\ACPowerCam\enum,  0,               0, "Disable"
;HKR, NDI\params\ACPowerCam\enum,  1,               0, "Enable"

;
; Preamble Type
;
HKR, ,                            PreambleType,    0, "0"
HKR, Default,                     PreambleType,    0, "0"

;
; RTS Threshold
;
HKR, ,                            RTSThresh,       0, "2347"
HKR, Default,                     RTSThresh,       0, "2347"
HKR, NDI\params\RTSThresh,        ParamDesc,       0, "RTS Threshold"
HKR, NDI\params\RTSThresh,        type,            0, "int"
HKR, Ndi\params\RTSThresh,        default,         0, "2347"
HKR, NDI\params\RTSThresh,        min,             0, "0"
HKR, NDI\params\RTSThresh,        max,             0, "2347"
HKR, NDI\params\RTSThresh,        step,            0, "32"
HKR, NDI\params\RTSThresh,        optional,        0, "0"

;
; Fragment Threshold
;
HKR, ,                            FragThresh,      0, "2346"
HKR, Default,                     FragThresh,      0, "2346"
HKR, NDI\params\FragThresh,       ParamDesc,       0, "Fragment Threshold"
HKR, NDI\params\FragThresh,       type,            0, "int"
HKR, Ndi\params\FragThresh,       default,         0, "2346"
HKR, NDI\params\FragThresh,       min,             0, "256"
HKR, NDI\params\FragThresh,       max,             0, "2346"
HKR, NDI\params\FragThresh,       step,            0, "32"
HKR, NDI\params\FragThresh,       optional,        0, "0"

;*******************************************************************************************
; Authentication & Security Page

;
; Authentication Type
;
HKR, ,                AuthenType,      0, "0" ; Open System
HKR, Default,         AuthenType,      0, "0"

;
; Encryption
;
HKR, ,                Encryption,      0, "1" ; Disable
HKR, Default,         Encryption,      0, "1"

;
; WEP Keys Length
;
HKR, ,                WEPKeyLen,       0, "0"
HKR, Default,         WEPKeyLen,       0, "0"

;
; WEP Key to use
;
HKR, ,                WEPKeyUse,       0,"1"
HKR, Default,         WEPKeyUse,       0,"1"

;
; WEP Key1
;
HKR, ,                WEPKey1,         0,""
HKR, Default,         WEPKey1,         0,""

;
; WEP Key2
;
HKR, ,                WEPKey2,         0,""
HKR, Default,         WEPKey2,         0,""

;
; WEP Key3
;
HKR, ,                WEPKey3,         0,""
HKR, Default,         WEPKey3,         0,""

;
; WEP Key4
;
HKR, ,                WEPKey4,         0,""
HKR, Default,         WEPKey4,         0,""

;*******************************************************************************************
; DeviceID for Win9X 
;*******************************************************************************************
[USB_148F_2573.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_148F&PID_2573"

[USB_148F_2671.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_148F&PID_2671"

[USB_0DB0_6877.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_0DB0&PID_6877"

[USB_0DB0_A874.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_0DB0&PID_A874"

[USB_0DB0_6874.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_0DB0&PID_6874"

[USB_0DB0_A861.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_0DB0&PID_A861"

[USB_1631_C019.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_1631&PID_C019"

[USB_18E8_6196.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_18E8&PID_6196"

[USB_18E8_6229.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_18E8&PID_6229"

[USB_1044_8008.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_1044&PID_8008"

[USB_1044_800A.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_1044&PID_800A"

[USB_14B2_3C22.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_14B2&PID_3C22"

[USB_0769_31F3.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_0769&PID_31F3"

[USB_0B05_1723.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_0B05&PID_1723"

[USB_0B05_1724.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_0B05&PID_1724"

[USB_18C5_0002.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_18C5&PID_0002"

[USB_1371_9032.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_1371&PID_9032"

[USB_1472_0009.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_1472&PID_0009"

[USB_1690_0722.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_1690&PID_0722"

[USB_148F_9021.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_148F&PID_9021"

[USB_0EB0_9021.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_0EB0&PID_9021"

[USB9X.ndi.reg]
HKR, ,                            NTMPDriver,       0, rt73u98.sys

HKR, ,                            BusType,          0, 15
HKR, NDI,                         CardType,         0, "PNP"

HKR, ,                            RunningWin9X,     0, "1"
HKR, ,                            DevLoader,        0, "*ndis"
HKR, ,                            DeviceVxDs,       0, "rt73u98.sys"
HKR, ,                            EnumPropPages,    0, "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,              DefUpper,         0, "ndis3"
HKR, Ndi\Interfaces,              DefLower,         0, "ethernet"
HKR, Ndi\Interfaces,              UpperRange,       0, "ndis3"
HKR, Ndi\Interfaces,              LowerRange,       0, "ethernet"

HKR, NDIS,                        LogDriverName,    0, "rt73u98"
HKR, NDIS,                        MajorNdisVersion, 1, 03
HKR, NDIS,                        MinorNdisVersion, 1, 0A

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************

[DestinationDirs]
NT.CopyFiles            = 12    ; system32\drivers subdirectory on NT
win9x.CopyFiles         = 11    ; system32 subdirectory on win9x

[NT.CopyFiles]
rt73.sys                   ; NT Installation

[win9x.CopyFiles]
rt73u98.sys                     ;  Win9x Installation

[SourceDisksNames]
1                       = %INSTALL_DISK_STR%,,,

[SourceDisksFiles] 
rt73.sys                = 1
rt73u98.sys             = 1

;*******************************************************************************************
; NT specific
;*******************************************************************************************
[RTUSB.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "rt73"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[Ralink.Service]
DisplayName                 = %Ralink.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt73.sys
LoadOrderGroup              = NDIS

[Qcom.Service]
DisplayName                 = %Qcom.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt73.sys
LoadOrderGroup              = NDIS

[Gigabyte.Service]
DisplayName                 = %Gigabyte.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt73.sys
LoadOrderGroup              = NDIS

[Conceptronic.Service]
DisplayName                 = %Conceptronic.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt73.sys
LoadOrderGroup              = NDIS

[Surecom.Service]
DisplayName                 = %Surecom.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt73.sys
LoadOrderGroup              = NDIS

[ASUS.Service]
DisplayName                 = %ASUS.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt73.sys
LoadOrderGroup              = NDIS

[AMIT.Service]
DisplayName                 = %AMIT.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt73.sys
LoadOrderGroup              = NDIS

[CNET.Service]
DisplayName                 = %CNET.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt73.sys
LoadOrderGroup              = NDIS

[HUAWEI.Service]
DisplayName                 = %HUAWEI.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt73.sys
LoadOrderGroup              = NDIS

[Askey.Service]
DisplayName                 = %Askey.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt73.sys
LoadOrderGroup              = NDIS

[Amigo.Service]
DisplayName                 = %Amigo.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt73.sys
LoadOrderGroup              = NDIS

[common.EventLog]
AddReg=common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\rt73.sys"
HKR, , TypesSupported,   0x00010001, 7



;*******************************************************************************************
; Strings
;*******************************************************************************************
[strings]
Provider                    = "Ralink"
Ralink                      = "Ralink Technology Corp."
Qcom                        = "Qcom Technology Inc."
Gigabyte                    = "Gigabyte Technology Corp."
Conceptronic                = "2L (Conceptronic)"
Surecom                     = "SURECOM Technology Corp."
Asus                        = "ASUSTeK Computer Inc."
Amit                        = "AMIT Technology, Inc."
CNet                        = "CNet Technology Inc."
Huawei-3Com                 = "Huawei-3Com Technology Co., Ltd."
Askey                       = "WLAN"
Amigo                       = "AMIGO TECHNOLOGY LTD"

Ralink.DeviceDesc           = "RT73 USB Wireless LAN Card"
Qcom.DeviceDesc             = "RT73 USB Wireless LAN Card"
Gigabyte.DeviceDesc         = "Gigabyte GN-WB01GS USB WLAN Card"
Gigabyte2.DeviceDesc        = "Gigabyte GN-WI05GS mini WLAN Card"
Conceptronic.DeviceDesc     = "Conceptronic 54Mbps USB adapter"
M6877.DeviceDesc            = "802.11g Mini Card Wireless Adapter"
MA874.DeviceDesc            = "802.11g MiniUSB 2.0 Wireless Bluetooth Combo"
M6874.DeviceDesc            = "802.11g MiniUSB 2.0 Wireless Bluetooth Combo"
MA861.DeviceDesc            = "802.11g USB 2.0 Stick"
GMEWLGRL.DeviceDesc         = "RT73 USB Wireless LAN Card"
Surecom.DeviceDesc          = "802.11g 54M Wireless LAN USB Adapter"
ASUS.DeviceDesc             = "ASUS USB Wireless Network Adapter"
ASUSGEN.DeviceDesc          = "802.11b/g USB Wireless Network Adapter"
AMIT.DeviceDesc             = "CG-WLUSB2GO, corega Wireless USB Adapter"
CNet.DeviceDesc             = "CNet Wireless USB dongle"
Huawei-3Com.DeviceDesc      = "Aolynk WUB320g USB Wireless LAN Card"
Askey.DeviceDesc            = "WLAN USB Wireless LAN Stick"
Amigo1.DeviceDesc           = "Wireless USB Card"
Amigo2.DeviceDesc           = "IEEE 802.11g Wireless Pocket USB"

INSTALL_DISK_STR            = "Wireless 11g USB Installation Disk"

Ralink.Service.DispName     = "RT73 USB Wireless LAN Card Driver"
Qcom.Service.DispName       = "RT73 USB Wireless LAN Card Driver"
Gigabyte.Service.DispName   = "Gigabyte RT73 Wireless Driver"
Conceptronic.Service.DispName = "Conceptronic RT73 Wireles Driver"
Surecom.Service.DispName    = "Surecom RT73 Wireles Driver"
ASUS.Service.DispName       = "ASUS USB Wireless LAN Card Driver"
AMIT.Service.DispName       = "CG-WLUSB2GO RT73 Wireles Driver"
CNET.Service.DispName       = "CNet RT73 Wireless Driver"
HUAWEI.Service.DispName     = "Huawei-3Com RT73 Wireless Driver"
Askey.Service.DispName      = "Askey RT73 Wireless Driver"
Amigo.Service.DispName      = "Amigo RT73 Wireless Driver"

;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = "IEEE 802.11g Wireless Card."
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"

