;===========================================================================
; 
; Windows XP, 2000 NDIS driver INF for Libertas 802.11b/g Wireless
; Copyright (C) 2004 Marvell Semiconductor, Inc.
;
;=========================================================================== 
 
 
[Version] 
Signature = "$Windows NT$" 
Compatible  = 1
Class=Net
ClassGUID={4D36E972-E325-11CE-BFC1-08002BE10318} 
Provider=%MRVL% 
CatalogFile=mrv8335.cat
DriverVer=02/22/2005,3.1.1.7

;===========================================================================
; Source Media Information Sections
;===========================================================================
[SourceDisksNames]
1 = "Marvell installation disk 1",,,

[SourceDisksFiles]
; On Marvell installation disk 1 
MRV8335XP.sys = 1
MRV8335NT.sys = 1

[DestinationDirs]
W8335PCI.XP.CopyFiles  = 12 
W8335PCI.2K.CopyFiles  = 12 
DefaultDestDirs        = 11

[Manufacturer] 
%MRVL%=Marvell,NT.5.1

[Marvell]
%W8335PCI.DeviceDesc% = W8335PCI.ndi.NT, PCI\VEN_11AB&DEV_1FAA
%W8335PXPCI.DeviceDesc% = W8335PCI.ndi.NT, PCI\VEN_11AB&DEV_1FAB

[Marvell.NT.5.1]
%W8335PCI.DeviceDesc% = W8335PCIXP.ndi, PCI\VEN_11AB&DEV_1FAA
%W8335PXPCI.DeviceDesc% = W8335PCIXP.ndi, PCI\VEN_11AB&DEV_1FAB

;===========================================================================
; ControlFlags section
;===========================================================================
[ControlFlags]
ExcludeFromSelect = *

;***************************************************************************
;**         
;**          Win XP DDInstall section
;**          
;***************************************************************************
;***************************************************************************
[W8335PCIXP.ndi]
; "Characteristics" is (NCF_PHYSICAL | NCF_HAS_UI)
Characteristics = 0x84 
; "BusType" is PCI or CardBus
BusType         = 5 
AddReg          = W8335PCI.reg, W8335PCIXP.reg, W8335PCIXP.zerocfg
CopyFiles       = W8335PCI.XP.CopyFiles

[W8335PCIXP.ndi.Services]
AddService = W8335XP, 2, W8335PCIXP.Service, CommonXP.EventLog

;===========================================================================
; W8335 PCI WinXP registers
;===========================================================================
[W8335PCIXP.reg]
HKR, Ndi,            Service,    0, "W8335XP"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"


[W8335PCI.XP.CopyFiles]
MRV8335XP.sys,,,2 

[W8335PCIXP.Service]
DisplayName    = %W8335PCIXP.Service.DispName%
ServiceType    = 1 ;%SERVICE_KERNEL_DRIVER%
StartType      = 3 ;%SERVICE_DEMAND_START%
ErrorControl   = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\MRV8335XP.sys
LoadOrderGroup = NDIS


[CommonXP.EventLog]
AddReg = CommonXP.AddEventLog.reg

[CommonXP.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7



;***************************************************************************
;***************************************************************************
;**         
;**          Win 2K DDInstall section
;**          
;***************************************************************************
;***************************************************************************

[W8335PCI.ndi.NT]
; "Characteristics" is (NCF_PHYSICAL | NCF_HAS_UI)
Characteristics = 0x84 
; "BusType" is PCI or CardBus
BusType         = 5 
AddReg          = W8335PCI.reg, W8335PCI2K.reg, W8335PCI.devID.reg
CopyFiles       = W8335PCI.2K.CopyFiles 

DeviceID = "PCI\VEN_11AB&DEV_1FAA"

[W8335PCI.ndi.NT.Services]
AddService = W8335PCI, 2, W8335PCI2K.Service, Common.EventLog

;===========================================================================
; W8335 PCI Win2K registers
;===========================================================================
[W8335PCI2K.reg]
HKR, Ndi,            Service,    0, "W8335PCI"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

[W8335PCI.2K.CopyFiles]
MRV8335NT.sys,,,2 


[W8335PCI2K.Service]
DisplayName    = %W8335PCI2K.Service.DispName%
ServiceType    = 1 ;%SERVICE_KERNEL_DRIVER%
StartType      = 3 ;%SERVICE_DEMAND_START%
ErrorControl   = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\MRV8335NT.sys
LoadOrderGroup = NDIS

[Common.EventLog]
AddReg = Common.AddEventLog.reg

[Common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

[W8335PCI.devID.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_11AB&DEV_1FAA"

;===========================================================================
; W8335 PCI common, MIB can be defined here
;===========================================================================
[W8335PCI.reg]
HKR, Ndi\params\FragThsd,  ParamDesc,0 , "%FragThsd%"
HKR, Ndi\params\FragThsd,  default, 0 , "2346"
HKR, Ndi\params\FragThsd,  min, 0 , "256"
HKR, Ndi\params\FragThsd,  max, 0 , "2346"
HKR, Ndi\params\FragThsd,  step, 0 , "1"
HKR, Ndi\params\FragThsd,  Base, 0 , "10"
HKR, Ndi\params\FragThsd,  type, 0 ,"dword"

HKR, Ndi\params\RTSThsd,  ParamDesc, 0, "%RTSThsd%"
HKR, Ndi\params\RTSThsd,  default, 0, "2346"
HKR, Ndi\params\RTSThsd,  min, 0, "0"
HKR, Ndi\params\RTSThsd,  max, 0, "2346"
HKR, Ndi\params\RTSThsd,  step, 0, "1"
HKR, Ndi\params\RTSThsd,  Base, 0, "10"
HKR, Ndi\params\RTSThsd,  type, 0, "dword"

HKR, Ndi\params\PowerMode,ParamDesc,,"%PowerMode%"
HKR, Ndi\params\PowerMode,default,,"0"
HKR, Ndi\params\PowerMode,type,,enum
HKR, Ndi\params\PowerMode\enum,"0",,"CAM-Constantly Awake Mode"
HKR, Ndi\params\PowerMode\enum,"1",,"MaxPSP-Max Power Savings"
;HKR, Ndi\params\PowerMode\enum,"2",,"FastPSP-Fast Power Savings"

HKR, Ndi\params\Preamble,ParamDesc,,"%PreambleStr%"
HKR, Ndi\params\Preamble,default,,"3"
HKR, Ndi\params\Preamble,type,,enum 
HKR, Ndi\params\Preamble\enum,"1",,"Auto"
HKR, Ndi\params\Preamble\enum,"2",,"Short Preamble" 
HKR, Ndi\params\Preamble\enum,"3",,"Long Preamble"

HKR, Ndi\params\AdhocGMode,ParamDesc,,"%AdhocGMode%"
HKR, Ndi\params\AdhocGMode,default,,"1"
HKR, Ndi\params\AdhocGMode,type,,enum
HKR, Ndi\params\AdhocGMode\enum,"0",,"Adhoc G Mode"
HKR, Ndi\params\AdhocGMode\enum,"1",,"Adhoc B Mode only" 

HKR, Ndi\params\DesiredSSID,ParamDesc,,"%SSID%"
HKR, Ndi\params\DesiredSSID,default,,"MarvellAP3x"
HKR, Ndi\params\DesiredSSID,type,,"edit" 
HKR, Ndi\params\DesiredSSID,LimitText,,"32"
HKR, Ndi\params\DesiredSSID,UpperCase,,"0" 
HKR, Ndi\params\DesiredSSID,Optional,,"0" 

HKR, Ndi\xparams\AuthMode,ParamDesc,,"%AuthMode%"
HKR, Ndi\xparams\AuthMode,default,,"0"
HKR, Ndi\xparams\AuthMode,type,,enum
HKR, Ndi\xparams\AuthMode\enum,"0",,"Open"
HKR, Ndi\xparams\AuthMode\enum,"1",,"Shared"

HKR, Ndi\xparams\NetworkMode,ParamDesc,,"%NetworkMode%"
HKR, Ndi\xparams\NetworkMode,default,,"1"
HKR, Ndi\xparams\NetworkMode,type,,enum
HKR, Ndi\xparams\NetworkMode\enum,"0",,"Ad Hoc"
HKR, Ndi\xparams\NetworkMode\enum,"1",,"Infrastructure"

;HKR, Ndi\xparams\Wireless,ParamDesc,,"%WirelessM%"
;HKR, Ndi\xparams\Wireless,default,,"0"
;HKR, Ndi\xparams\Wireless,type,,enum
;HKR, Ndi\xparams\Wireless\enum,"0",,"Auto"
;HKR, Ndi\xparams\Wireless\enum,"1",,"B rates only"
 

HKR, Ndi\xparams\Channel,  ParamDesc,0 , "%Channel%"
HKR, Ndi\xparams\Channel,  default, 0 , "1"
HKR, Ndi\xparams\Channel,  min, 0 , "0"
HKR, Ndi\xparams\Channel,  max, 0 , "14"
HKR, Ndi\xparams\Channel,  step, 0 , "1"
HKR, Ndi\xparams\Channel,  Base, 0 , "16"
HKR, Ndi\xparams\Channel,  type, 0 ,"dword"

HKR, Ndi\xparams\TxAntenna,  ParamDesc,0 , "%TxAntennaStr%"
HKR, Ndi\xparams\TxAntenna,  default, 0 , "2"
HKR, Ndi\xparams\TxAntenna,  min, 0 , "1"
HKR, Ndi\xparams\TxAntenna,  max, 0 , "ffff"
HKR, Ndi\xparams\TxAntenna,  step, 0 , "1"
HKR, Ndi\xparams\TxAntenna,  Base, 0 , "16"
HKR, Ndi\xparams\TxAntenna,  type, 0 ,"dword"

HKR, Ndi\xparams\RxAntenna,  ParamDesc,0 , "%RxAntennaStr%"
HKR, Ndi\xparams\RxAntenna,  default, 0 , "ffff"
HKR, Ndi\xparams\RxAntenna,  min, 0 , "1"
HKR, Ndi\xparams\RxAntenna,  max, 0 , "ffff"
HKR, Ndi\xparams\RxAntenna,  step, 0 , "1"
HKR, Ndi\xparams\RxAntenna,  Base, 0 , "16"
HKR, Ndi\xparams\RxAntenna,  type, 0 ,"dword"

;
; LED Control
;
HKR,, LED0PowerOn, 2,"30001"
HKR,, LED1PowerOn, 2,"fe0101"
HKR,, LED0PowerOff, 2,"fe0000"
HKR,, LED1PowerOff, 2,"fe0100"
HKR,, LED0Scan, 2,"ff0002"
HKR,, LED1Scan, 2,"40102"
HKR,, LED0Associated, 2,"ff0005"
HKR,, LED1Associated, 2,"fe0105"
HKR,, LED0Joined, 2,"ff0006"
HKR,, LED1Joined, 2,"ff0106"
HKR,, LED0Started, 2,"ff0007"
HKR,, LED1Started, 2,"ff0107"
HKR,, LED0Tx, 2,"ff0008"
HKR,, LED1Tx, 2,"30108"
HKR,, LED0Rx, 2,"ff0009"
HKR,, LED1Rx, 2,"30109"
HKR,, LED0TxHigh, 2,"ff000c"
HKR,, LED1TxHigh, 2,"2010c"
HKR,, LED0RxHigh, 2,"ff000d"
HKR,, LED1RxHigh, 2,"2010d"

HKR, Ndi\xparams\LED0PowerOn,ParamDesc,,"%LED0PowerOnStr%"
HKR, Ndi\xparams\LED0PowerOn,default,,"ff0001"
HKR, Ndi\xparams\LED0PowerOn,type,,enum
HKR, Ndi\xparams\LED0PowerOn\enum,"ff0001",,"LED Stays On"
HKR, Ndi\xparams\LED0PowerOn\enum,"fe0001",,"LED Stays Off"
HKR, Ndi\xparams\LED0PowerOn\enum,"fd0001",,"No Change"
HKR, Ndi\xparams\LED0PowerOn\enum,"40001",,"Slow blink"
HKR, Ndi\xparams\LED0PowerOn\enum,"30001",,"Regular blink"
HKR, Ndi\xparams\LED0PowerOn\enum,"20001",,"Fast blink" 

HKR, Ndi\xparams\LED1PowerOn,ParamDesc,,"%LED1PowerOnStr%"
HKR, Ndi\xparams\LED1PowerOn,default,,"fe0101"
HKR, Ndi\xparams\LED1PowerOn,type,,enum
HKR, Ndi\xparams\LED1PowerOn\enum,"ff0101",,"LED Stays On"
HKR, Ndi\xparams\LED1PowerOn\enum,"fe0101",,"LED Stays Off"
HKR, Ndi\xparams\LED1PowerOn\enum,"fd0101",,"No Change"
HKR, Ndi\xparams\LED1PowerOn\enum,"40101",,"Slow blink"
HKR, Ndi\xparams\LED1PowerOn\enum,"30101",,"Regular blink"
HKR, Ndi\xparams\LED1PowerOn\enum,"20101",,"Fast blink" 

HKR, Ndi\xparams\LED0PowerOff,ParamDesc,,"%LED0PowerOffStr%"
HKR, Ndi\xparams\LED0PowerOff,default,,"fe0001"
HKR, Ndi\xparams\LED0PowerOff,type,,enum
HKR, Ndi\xparams\LED0PowerOff\enum,"ff0001",,"LED Stays On"
HKR, Ndi\xparams\LED0PowerOff\enum,"fe0001",,"LED Stays Off"
HKR, Ndi\xparams\LED0PowerOff\enum,"fd0001",,"No Change"
HKR, Ndi\xparams\LED0PowerOff\enum,"40001",,"Slow blink"
HKR, Ndi\xparams\LED0PowerOff\enum,"30001",,"Regular blink"
HKR, Ndi\xparams\LED0PowerOff\enum,"20001",,"Fast blink" 

HKR, Ndi\xparams\LED1PowerOff,ParamDesc,,"%LED1PowerOffStr%"
HKR, Ndi\xparams\LED1PowerOff,default,,"fe0101"
HKR, Ndi\xparams\LED1PowerOff,type,,enum
HKR, Ndi\xparams\LED1PowerOff\enum,"ff0101",,"LED Stays On"
HKR, Ndi\xparams\LED1PowerOff\enum,"fe0101",,"LED Stays Off"
HKR, Ndi\xparams\LED1PowerOff\enum,"fd0101",,"No Change"
HKR, Ndi\xparams\LED1PowerOff\enum,"40101",,"Slow blink"
HKR, Ndi\xparams\LED1PowerOff\enum,"30101",,"Regular blink"
HKR, Ndi\xparams\LED1PowerOff\enum,"20101",,"Fast blink" 

HKR, Ndi\xparams\LED0Scan,ParamDesc,,"%LED0ScanStr%"
HKR, Ndi\xparams\LED0Scan,default,,"ff0001"
HKR, Ndi\xparams\LED0Scan,type,,enum
HKR, Ndi\xparams\LED0Scan\enum,"ff0001",,"LED Stays On"
HKR, Ndi\xparams\LED0Scan\enum,"fe0001",,"LED Stays Off"
HKR, Ndi\xparams\LED0Scan\enum,"fd0001",,"No Change"
HKR, Ndi\xparams\LED0Scan\enum,"40001",,"Slow blink"
HKR, Ndi\xparams\LED0Scan\enum,"30001",,"Regular blink"
HKR, Ndi\xparams\LED0Scan\enum,"20001",,"Fast blink" 

HKR, Ndi\xparams\LED1Scan,ParamDesc,,"%LED1ScanStr%"
HKR, Ndi\xparams\LED1Scan,default,,"40101"
HKR, Ndi\xparams\LED1Scan,type,,enum
HKR, Ndi\xparams\LED1Scan\enum,"ff0101",,"LED Stays On"
HKR, Ndi\xparams\LED1Scan\enum,"fe0101",,"LED Stays Off"
HKR, Ndi\xparams\LED1Scan\enum,"fd0101",,"No Change"
HKR, Ndi\xparams\LED1Scan\enum,"40101",,"Slow blink"
HKR, Ndi\xparams\LED1Scan\enum,"30101",,"Regular blink"
HKR, Ndi\xparams\LED1Scan\enum,"20101",,"Fast blink" 

HKR, Ndi\xparams\LED0Associated,ParamDesc,,"%LED0AssociatedStr%"
HKR, Ndi\xparams\LED0Associated,default,,"ff0001"
HKR, Ndi\xparams\LED0Associated,type,,enum
HKR, Ndi\xparams\LED0Associated\enum,"ff0001",,"LED Stays On"
HKR, Ndi\xparams\LED0Associated\enum,"fe0001",,"LED Stays Off"
HKR, Ndi\xparams\LED0Associated\enum,"fd0001",,"No Change"
HKR, Ndi\xparams\LED0Associated\enum,"40001",,"Slow blink"
HKR, Ndi\xparams\LED0Associated\enum,"30001",,"Regular blink"
HKR, Ndi\xparams\LED0Associated\enum,"20001",,"Fast blink" 

HKR, Ndi\xparams\LED1Associated,ParamDesc,,"%LED1AssociatedStr%"
HKR, Ndi\xparams\LED1Associated,default,,"ff0101"
HKR, Ndi\xparams\LED1Associated,type,,enum
HKR, Ndi\xparams\LED1Associated\enum,"ff0101",,"LED Stays On"
HKR, Ndi\xparams\LED1Associated\enum,"fe0101",,"LED Stays Off"
HKR, Ndi\xparams\LED1Associated\enum,"fd0101",,"No Change"
HKR, Ndi\xparams\LED1Associated\enum,"40101",,"Slow blink"
HKR, Ndi\xparams\LED1Associated\enum,"30101",,"Regular blink"
HKR, Ndi\xparams\LED1Associated\enum,"20101",,"Fast blink" 

HKR, Ndi\xparams\LED0Joined,ParamDesc,,"%LED0JoinedStr%"
HKR, Ndi\xparams\LED0Joined,default,,"ff0001"
HKR, Ndi\xparams\LED0Joined,type,,enum
HKR, Ndi\xparams\LED0Joined\enum,"ff0001",,"LED Stays On"
HKR, Ndi\xparams\LED0Joined\enum,"fe0001",,"LED Stays Off"
HKR, Ndi\xparams\LED0Joined\enum,"fd0001",,"No Change"
HKR, Ndi\xparams\LED0Joined\enum,"40001",,"Slow blink"
HKR, Ndi\xparams\LED0Joined\enum,"30001",,"Regular blink"
HKR, Ndi\xparams\LED0Joined\enum,"20001",,"Fast blink" 

HKR, Ndi\xparams\LED1Joined,ParamDesc,,"%LED1JoinedStr%"
HKR, Ndi\xparams\LED1Joined,default,,"ff0101"
HKR, Ndi\xparams\LED1Joined,type,,enum
HKR, Ndi\xparams\LED1Joined\enum,"ff0101",,"LED Stays On"
HKR, Ndi\xparams\LED1Joined\enum,"fe0101",,"LED Stays Off"
HKR, Ndi\xparams\LED1Joined\enum,"fd0101",,"No Change"
HKR, Ndi\xparams\LED1Joined\enum,"40101",,"Slow blink"
HKR, Ndi\xparams\LED1Joined\enum,"30101",,"Regular blink"
HKR, Ndi\xparams\LED1Joined\enum,"20101",,"Fast blink" 

HKR, Ndi\xparams\LED0Started,ParamDesc,,"%LED0StartedStr%"
HKR, Ndi\xparams\LED0Started,default,,"ff0001"
HKR, Ndi\xparams\LED0Started,type,,enum
HKR, Ndi\xparams\LED0Started\enum,"ff0001",,"LED Stays On"
HKR, Ndi\xparams\LED0Started\enum,"fe0001",,"LED Stays Off"
HKR, Ndi\xparams\LED0Started\enum,"fd0001",,"No Change"
HKR, Ndi\xparams\LED0Started\enum,"40001",,"Slow blink"
HKR, Ndi\xparams\LED0Started\enum,"30001",,"Regular blink"
HKR, Ndi\xparams\LED0Started\enum,"20001",,"Fast blink" 

HKR, Ndi\xparams\LED1Started,ParamDesc,,"%LED1StartedStr%"
HKR, Ndi\xparams\LED1Started,default,,"ff0101"
HKR, Ndi\xparams\LED1Started,type,,enum
HKR, Ndi\xparams\LED1Started\enum,"ff0101",,"LED Stays On"
HKR, Ndi\xparams\LED1Started\enum,"fe0101",,"LED Stays Off"
HKR, Ndi\xparams\LED1Started\enum,"fd0101",,"No Change"
HKR, Ndi\xparams\LED1Started\enum,"40101",,"Slow blink"
HKR, Ndi\xparams\LED1Started\enum,"30101",,"Regular blink"
HKR, Ndi\xparams\LED1Started\enum,"20101",,"Fast blink" 

HKR, Ndi\xparams\LED0Tx,ParamDesc,,"%LED0TxStr%"
HKR, Ndi\xparams\LED0Tx,default,,"ff0001"
HKR, Ndi\xparams\LED0Tx,type,,enum
HKR, Ndi\xparams\LED0Tx\enum,"ff0001",,"LED Stays On"
HKR, Ndi\xparams\LED0Tx\enum,"fe0001",,"LED Stays Off"
HKR, Ndi\xparams\LED0Tx\enum,"fd0001",,"No Change"
HKR, Ndi\xparams\LED0Tx\enum,"40001",,"Slow blink"
HKR, Ndi\xparams\LED0Tx\enum,"30001",,"Regular blink"
HKR, Ndi\xparams\LED0Tx\enum,"20001",,"Fast blink" 

HKR, Ndi\xparams\LED1Tx,ParamDesc,,"%LED1TxStr%"
HKR, Ndi\xparams\LED1Tx,default,,"30101"
HKR, Ndi\xparams\LED1Tx,type,,enum
HKR, Ndi\xparams\LED1Tx\enum,"ff0101",,"LED Stays On"
HKR, Ndi\xparams\LED1Tx\enum,"fe0101",,"LED Stays Off"
HKR, Ndi\xparams\LED1Tx\enum,"fd0101",,"No Change"
HKR, Ndi\xparams\LED1Tx\enum,"40101",,"Slow blink"
HKR, Ndi\xparams\LED1Tx\enum,"30101",,"Regular blink"
HKR, Ndi\xparams\LED1Tx\enum,"20101",,"Fast blink" 

HKR, Ndi\xparams\LED0Rx,ParamDesc,,"%LED0RxStr%"
HKR, Ndi\xparams\LED0Rx,default,,"ff0001"
HKR, Ndi\xparams\LED0Rx,type,,enum
HKR, Ndi\xparams\LED0Rx\enum,"ff0001",,"LED Stays On"
HKR, Ndi\xparams\LED0Rx\enum,"fe0001",,"LED Stays Off"
HKR, Ndi\xparams\LED0Rx\enum,"fd0001",,"No Change"
HKR, Ndi\xparams\LED0Rx\enum,"40001",,"Slow blink"
HKR, Ndi\xparams\LED0Rx\enum,"30001",,"Regular blink"
HKR, Ndi\xparams\LED0Rx\enum,"20001",,"Fast blink" 

HKR, Ndi\xparams\LED1Rx,ParamDesc,,"%LED1RxStr%"
HKR, Ndi\xparams\LED1Rx,default,,"30101"
HKR, Ndi\xparams\LED1Rx,type,,enum
HKR, Ndi\xparams\LED1Rx\enum,"ff0101",,"LED Stays On"
HKR, Ndi\xparams\LED1Rx\enum,"fe0101",,"LED Stays Off"
HKR, Ndi\xparams\LED1Rx\enum,"fd0101",,"No Change"
HKR, Ndi\xparams\LED1Rx\enum,"40101",,"Slow blink"
HKR, Ndi\xparams\LED1Rx\enum,"30101",,"Regular blink"
HKR, Ndi\xparams\LED1Rx\enum,"20101",,"Fast blink" 

HKR, Ndi\xparams\LED0TxHigh,ParamDesc,,"%LED0TxHighStr%"
HKR, Ndi\xparams\LED0TxHigh,default,,"ff0001"
HKR, Ndi\xparams\LED0TxHigh,type,,enum
HKR, Ndi\xparams\LED0TxHigh\enum,"ff0001",,"LED Stays On"
HKR, Ndi\xparams\LED0TxHigh\enum,"fe0001",,"LED Stays Off"
HKR, Ndi\xparams\LED0TxHigh\enum,"fd0001",,"No Change"
HKR, Ndi\xparams\LED0TxHigh\enum,"40001",,"Slow blink"
HKR, Ndi\xparams\LED0TxHigh\enum,"30001",,"Regular blink"
HKR, Ndi\xparams\LED0TxHigh\enum,"20001",,"Fast blink" 

HKR, Ndi\xparams\LED1TxHigh,ParamDesc,,"%LED1TxHighStr%"
HKR, Ndi\xparams\LED1TxHigh,default,,"20101"
HKR, Ndi\xparams\LED1TxHigh,type,,enum
HKR, Ndi\xparams\LED1TxHigh\enum,"ff0101",,"LED Stays On"
HKR, Ndi\xparams\LED1TxHigh\enum,"fe0101",,"LED Stays Off"
HKR, Ndi\xparams\LED1TxHigh\enum,"fd0101",,"No Change"
HKR, Ndi\xparams\LED1TxHigh\enum,"40101",,"Slow blink"
HKR, Ndi\xparams\LED1TxHigh\enum,"30101",,"Regular blink"
HKR, Ndi\xparams\LED1TxHigh\enum,"20101",,"Fast blink" 

HKR, Ndi\xparams\LED0RxHigh,ParamDesc,,"%LED0RxHighStr%"
HKR, Ndi\xparams\LED0RxHigh,default,,"ff0001"
HKR, Ndi\xparams\LED0RxHigh,type,,enum
HKR, Ndi\xparams\LED0RxHigh\enum,"ff0001",,"LED Stays On"
HKR, Ndi\xparams\LED0RxHigh\enum,"fe0001",,"LED Stays Off"
HKR, Ndi\xparams\LED0RxHigh\enum,"fd0001",,"No Change"
HKR, Ndi\xparams\LED0RxHigh\enum,"40001",,"Slow blink"
HKR, Ndi\xparams\LED0RxHigh\enum,"30001",,"Regular blink"
HKR, Ndi\xparams\LED0RxHigh\enum,"20001",,"Fast blink" 

HKR, Ndi\xparams\LED1RxHigh,ParamDesc,,"%LED1RxHighStr%"
HKR, Ndi\xparams\LED1RxHigh,default,,"20101"
HKR, Ndi\xparams\LED1RxHigh,type,,enum
HKR, Ndi\xparams\LED1RxHigh\enum,"ff0101",,"LED Stays On"
HKR, Ndi\xparams\LED1RxHigh\enum,"fe0101",,"LED Stays Off"
HKR, Ndi\xparams\LED1RxHigh\enum,"fd0101",,"No Change"
HKR, Ndi\xparams\LED1RxHigh\enum,"40101",,"Slow blink"
HKR, Ndi\xparams\LED1RxHigh\enum,"30101",,"Regular blink"
HKR, Ndi\xparams\LED1RxHigh\enum,"20101",,"Fast blink" 

HKR,, LEDOffAfterRadioOff, 2, "1" 

HKR, Ndi\xparams\DataRate,ParamDesc,,"%DataRate%"
HKR, Ndi\xparams\DataRate,default,,"FF"
HKR, Ndi\xparams\DataRate,type,,enum
HKR, Ndi\xparams\DataRate\enum,"FF",,"Auto"
HKR, Ndi\xparams\DataRate\enum,"2",,"1 Mbps"
HKR, Ndi\xparams\DataRate\enum,"4",,"2 Mbps"
HKR, Ndi\xparams\DataRate\enum,"b",,"5.5 Mbps"
HKR, Ndi\xparams\DataRate\enum,"16",,"11 Mbps"
;HKR, Ndi\xparams\DataRate\enum,"2C",,"22 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"C",,"6 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"12",,"9 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"18",,"12 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"24",,"18 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"30",,"24 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"48",,"36 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"60",,"48 Mbps" 
HKR, Ndi\xparams\DataRate\enum,"6C",,"54 Mbps"

HKR, Ndi\xparams\WepStatus,ParamDesc,,"%WepStatus%"
HKR, Ndi\xparams\WepStatus,default,,"1"
HKR, Ndi\xparams\WepStatus,type,,enum
HKR, Ndi\xparams\WepStatus\enum,"0",,"Enabled"
HKR, Ndi\xparams\WepStatus\enum,"1",,"Disabled"

HKR,, TxWepKey, 2, "" 
HKR,, WepKey1, 2, "" 
HKR,, WepKey2, 2, "" 
HKR,, WepKey3, 2, "" 
HKR,, WepKey4, 2, "" 

;HKR,, DriverVer, 2, "3.1.1.4"
HKR,, DriverRel, 2, "01/31/2005"


;Special for Driver on WinXP OS.
[W8335PCIXP.zerocfg]
 
;===========================================================================
; Strings section
;===========================================================================
[Strings]
MRVL = "Marvell"

TxAntennaStr = "Tx Antenna Select"
RxAntennaStr = "Rx Antenna Select" 
Channel = "Channel"
FragThsd = "Fragamentation Threshold"
DataRate = "Data Rate"
RTSThsd = "RTS Threshold"
AuthMode = "Authentication Mode"
;WirelessM = "Wireless Mode"
NetworkMode = "Operation Mode"
WepStatus = "WEP Status"
SSID = "SSID"
PreambleStr = "Preamble Select"
PowerMode = "Power Save Mode"
AdhocGMode = "Adhoc Mode"

LED0PowerOnStr    = "LED 0 Power On"
LED0PowerOffStr   = "LED 0 Power Off"
LED0ScanStr       = "LED 0 Site Survey"
LED0AssociatedStr = "LED 0 Associated"
LED0JoinedStr     = "LED 0 IBSS Joined"
LED0StartedStr    = "LED 0 IBSS Started"
LED0TxStr         = "LED 0 Tx"
LED0RxStr         = "LED 0 Rx"
LED0TxHighStr     = "LED 0 Tx High Traffic"
LED0RxHighStr     = "LED 0 Rx High Traffic"

LED1PowerOnStr    = "LED 1 Power On"
LED1PowerOffStr   = "LED 1 Power Off"
LED1ScanStr       = "LED 1 Site Survey"
LED1AssociatedStr = "LED 1 Associated"
LED1JoinedStr     = "LED 1 IBSS Joined"
LED1StartedStr    = "LED 1 IBSS Started"
LED1TxStr         = "LED 1 Tx"
LED1RxStr         = "LED 1 Rx"
LED1TxHighStr     = "LED 1 Tx High Traffic"
LED1RxHighStr     = "LED 1 Rx High Traffic"

W8335PCI.DeviceDesc     = "Marvell Libertas 802.11b/g Wireless (8335)"
W8335PXPCI.DeviceDesc     = "Marvell Libertas 802.11b/g Wireless (8335 PX)"
W8335PCIXP.Service.DispName = "Marvell Libertas 802.11b/g Driver for Windows XP (8335)"
W8335PCI2K.Service.DispName = "Marvell Libertas 802.11b/g Driver for Windows 2K (8335)" 










 






