;+-----------------------------------------------------------------------+
;| Device name    : ZD1211B USB 802.11 b+g Wireless LAN card. (ZD1211B)  |
;| Platform	  : Microsoft Windows 98 / Me / 2000 / XP                |
;| Host interface : USB                                                  |
;|                                                                       |
;| Copyright (c) 2000-2003 ZyDAS Technology Corporation.                 |
;| All Rights Reserved.                                                  |
;+-----------------------------------------------------------------------+

;-------------------------------------------------------------------------
[Version]
Signature		= "$Chicago$"
Compatible		= 1
Class			= Net
ClassGUID		= {4d36e972-e325-11ce-bfc1-08002be10318}
MillenniumPreferred	= .ME
Provider		= %INFProvider%
;CatalogFile		= zd1211Bu.cat			; for WHQL certified
CatalogFile.NT		= zd1211Bu.cat			; for WHQL certified
DriverVer		= 06/27/2006,6.17.0.0


[Manufacturer]
%Manufacturer%	= ZyDAS, NT.5.1, ntamd64


[ControlFlags]


[ZyDAS]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------
%ZD1211B_50U_DESC%       = ZD1211B_50U.ndi,   USB\VID_0ACE&PID_1215
%ZD1211B_50U_DESC%       = ZD1211B_50U.ndi,   USB\VID_0053&PID_5301
%ZD1211B_50U_DESC%       = ZD1211B_50U.ndi,   USB\VID_0053&PID_5302
%ZD1211B_50U_DESC%       = ZD1211B_50U.ndi,   USB\VID_0105&PID_145F
%ZD1211B_50U_DESC%       = ZD1211B_50U.ndi,   USB\VID_050D&PID_4050
%ZD1211B_50U_DESC%       = ZD1211B_50U.ndi,   USB\VID_050D&PID_705C
%ZD1211B_50U_DESC%       = ZD1211B_50U.ndi,   USB\VID_0586&PID_340F
%ZD1211B_50U_DESC%       = ZD1211B_50U.ndi,   USB\VID_079B&PID_0062
%ZD1211B_50U_DESC%       = ZD1211B_50U.ndi,   USB\VID_083A&PID_4505
%ZD1211B_50U_DESC%       = ZD1211B_50U.ndi,   USB\VID_083A&PID_E501
%ZD1211B_50U_DESC%       = ZD1211B_50U.ndi,   USB\VID_0BAF&PID_0121
%ZD1211B_50U_DESC%       = ZD1211B_50U.ndi,   USB\VID_0CDE&PID_001A
%ZD1211B_50U_DESC%       = ZD1211B_50U.ndi,   USB\VID_0DF6&PID_9071
%ZD1211B_50U_DESC%       = ZD1211B_50U.ndi,   USB\VID_0DF6&PID_9075
%ZD1211B_50U_DESC%       = ZD1211B_50U.ndi,   USB\VID_0F88&PID_3014
%ZD1211B_50U_DESC%       = ZD1211B_50U.ndi,   USB\VID_1233&PID_0471
%ZD1211B_50U_DESC%       = ZD1211B_50U.ndi,   USB\VID_1582&PID_6003

[ZyDAS.NT.5.1]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ndi, USB\VID_0ACE&PID_1215
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ndi, USB\VID_0053&PID_5301
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ndi, USB\VID_0053&PID_5302
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ndi, USB\VID_0105&PID_145F
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ndi, USB\VID_050D&PID_4050
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ndi, USB\VID_050D&PID_705C
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ndi, USB\VID_0586&PID_340F
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ndi, USB\VID_079B&PID_0062
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ndi, USB\VID_083A&PID_4505
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ndi, USB\VID_083A&PID_E501
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ndi, USB\VID_0BAF&PID_0121
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ndi, USB\VID_0CDE&PID_001A
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ndi, USB\VID_0DF6&PID_9071
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ndi, USB\VID_0DF6&PID_9075
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ndi, USB\VID_0F88&PID_3014
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ndi, USB\VID_1233&PID_0471
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ndi, USB\VID_1582&PID_6003

[ZyDAS.ntamd64]
;DisplayName              Section           Hardware ID
;-----------              -------           --------------------------
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ntamd64, USB\VID_0ACE&PID_1215
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ntamd64, USB\VID_0053&PID_5301
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ntamd64, USB\VID_0053&PID_5302
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ntamd64, USB\VID_0105&PID_145F
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ntamd64, USB\VID_050D&PID_4050
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ntamd64, USB\VID_050D&PID_705C
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ntamd64, USB\VID_0586&PID_340F
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ntamd64, USB\VID_079B&PID_0062
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ntamd64, USB\VID_083A&PID_4505
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ntamd64, USB\VID_083A&PID_E501
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ntamd64, USB\VID_0BAF&PID_0121
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ntamd64, USB\VID_0CDE&PID_001A
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ntamd64, USB\VID_0DF6&PID_9071
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ntamd64, USB\VID_0DF6&PID_9075
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ntamd64, USB\VID_0F88&PID_3014
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ntamd64, USB\VID_1233&PID_0471
%ZD1211B_50U_DESC%       = ZD1211BXP50U.ntamd64, USB\VID_1582&PID_6003

;*********************************************************************
;   Microsoft Windows 98 section
;*********************************************************************
;---------- 5.0 volt ----------
[ZD1211B_50U.ndi]
AddReg		= ZD1211B_Win9x.reg, ZD1211B_Common.reg, UnZDRegistryUSB.reg
CopyFiles       = ZD1211B.CopyFiles98
DriverVer	= 06/27/2006,6.17.0.0


[ZD1211B_Win9x.reg]
HKR,NDI,              DeviceID,           0, %ZD1211B_50U_PNP%
HKR,NDI,              CardType,           0, %CardType%
HKR,,                 DevLoader,          0, "*ndis"
HKR,,                 DeviceVxDs,         0, %DriverFileName%

; NDIS Info
HKR,NDIS,             MajorNdisVersion,   1, 03
HKR,NDIS,             MinorNdisVersion,   1, 0A
HKR,NDIS,             LogDriverName,      0, %CustomServiceName%(%Manufacturer%)

; Interfaces Info
HKR,NDI\Interfaces,   DefUpper,           0, "ndis3"
HKR,NDI\Interfaces,   DefLower,           0, "ethernet"
HKR,NDI\Interfaces,   UpperRange,         0, "ndis3"
HKR,NDI\Interfaces,   LowerRange,         0, "ethernet"

; Other Info
HKR,,                 BusType,            0, 15
HKR,,                 IOBaseAddress,      1, 02,00,00,00
HKR,,                 InterruptNumber,    1, 04,00,00,00
HKR,,                 EnumPropPages,      0, "netdi.dll,EnumPropPages"

; Install Sections
HKR,NDI\Install,      ndis3,              0, "ZD1211B.ndis3"

HKR,,                 VendorDesc,         0, %VendorDesc%


[ZD1211B.CopyFiles98]
ZD1211BU.sys,ZD11BU98.sys,,2


;*********************************************************************
;   Microsoft Windows Me section
;*********************************************************************
;---------- 5.0 volt ----------
[ZD1211B_50U.ndi.ME]
Characteristics = 0x84
BusType         = 15
AddReg		= ZD1211B_WinMe.reg, ZD1211B_Common.reg, UnZDRegistryUSB.reg
CopyFiles       = ZD1211B.CopyFilesMe


[ZD1211B_50U.ndi.ME.Services]
AddService = %CustomServiceName%(%Manufacturer%), 2, ZD1211BU_ME.Service, ZD1211BU.EventLog


[ZD1211B_WinMe.reg]
HKR,NDI,              Service,            0, %CustomServiceName%(%Manufacturer%)
HKR,,                 DevLoader,          0, "*ndis"
HKR,,                 DeviceVxDs,         0, %DriverFileName%
HKR,,                 EnumPropPages,      0, "netdi.dll,EnumPropPages"

; NDIS Info
HKR,NDIS,             MajorNdisVersion,   1, 05
HKR,NDIS,             MinorNdisVersion,   1, 00
HKR,NDIS,             LogDriverName,      0, %CustomServiceName%(%Manufacturer%)

; Interfaces Info
HKR,NDI\Interfaces,   DefUpper,           0, "ndis5"
HKR,NDI\Interfaces,   DefLower,           0, "ethernet"
HKR,NDI\Interfaces,   UpperRange,         0, "ndis5"
HKR,NDI\Interfaces,   LowerRange,         0, "ethernet"

; Install Sections
HKR,NDI\Install,      ndis3,              0, "ZD1211B.ndis5me"

HKR,,                 VendorDesc,         0, %VendorDesc%


[ZD1211B.ndis5me]
CopyFiles       = ZD1211B.CopyFilesMe


[ZD1211B.CopyFilesMe]
ZD1211BU.sys,ZD11BUME.sys,,2


[ZD1211BU_ME.Service]
DisplayName     = %ZD1211BU.Service.DispName%(%Manufacturer%)
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %11%\%DriverFileName%		; %11%\zd1211Bu.sys
LoadOrderGroup  = NDIS


;*********************************************************************
;   Microsoft Windows 2000 section
;*********************************************************************
;---------- 5.0 volt ----------
[ZD1211B_50U.ndi.NTx86]
Characteristics = 0x84
BusType         = 15
AddReg		= ZD1211B_Win2K.reg, ZD1211B_Common.reg
CopyFiles       = ZD1211B.CopyFiles2K

[ZD1211B_50U.ndi.NTx86.Services]
AddService = %CustomServiceName%(%Manufacturer%), 2, ZD1211BU_NT.Service, ZD1211BU.EventLog

[ZD1211B_Win2K.reg]
; Interfaces Info
HKR,NDI\Interfaces,   UpperRange,         0, "ndis5"
HKR,NDI\Interfaces,   LowerRange,         0, "ethernet"
HKR,NDI,              Service,            0, %CustomServiceName%(%Manufacturer%)

HKR,,                 VendorDesc,         0, %VendorDesc%


[ZD1211B.CopyFiles2K]
ZD1211BU.sys,ZD11BU2K.sys,,2


;*********************************************************************
;   Microsoft Windows XP section
;*********************************************************************
;---------- 5.0 volt ----------
[ZD1211BXP50U.ndi.NTx86]
Characteristics = 0x84
BusType         = 15
AddReg		= ZD1211B_WinXP.reg, ZD1211B_Common.reg
CopyFiles       = ZD1211B.CopyFilesXP


[ZD1211BXP50U.ndi.NTx86.Services]
AddService = %CustomServiceName%(%Manufacturer%), 2, ZD1211BU_NT.Service, ZD1211BU.EventLog

[ZD1211BXP50U.ntamd64]
Characteristics = 0x84
BusType         = 15
AddReg		= ZD1211B_WinXP.reg, ZD1211B_Common.reg
CopyFiles       = ZD1211B.CopyFilesXP64

[ZD1211BXP50U.ntamd64.Services]
AddService = %CustomServiceName%(%Manufacturer%), 2, ZD1211BU_NT.Service, ZD1211BU.EventLog

[ZD1211B_WinXP.reg]
; Interfaces Info
HKR,NDI\Interfaces,   UpperRange,         0, "ndis5"
HKR,NDI\Interfaces,   LowerRange,         0, "ethernet"
HKR,NDI,              Service,            0, %CustomServiceName%(%Manufacturer%)
HKR,,                 VendorDesc,         0, %VendorDesc%


[ZD1211B.CopyFilesXP]
ZD1211BU.sys,ZD11BUXP.sys,,2

[ZD1211B.CopyFilesXP64]
ZD1211BU.sys,ZD11BU64.sys,,2

;*********************************************************************
;   Microsoft Windows 2000/XP Common Section
;*********************************************************************
;---------- 5.0 volt ----------
[ZD1211BU_NT.Service]
DisplayName     = %ZD1211BU.Service.DispName%(%Manufacturer%)
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\%DriverFileName%		; %12%\%DriverFileName%
LoadOrderGroup  = NDIS


;*********************************************************************
;   Microsoft Windows ME/2000/XP Common Section
;*********************************************************************
;---------- 5.0 volt ----------
[ZD1211BU.EventLog]
Addreg = ZD1211BU.AddEventLog.reg

[ZD1211BU.AddEventLog.reg]
HKR,,                               EventMessageFile,  0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR,,                               TypesSupported,    0x00010001, 7


;*********************************************************************
;   Destination Directories
;*********************************************************************
[DestinationDirs]
ZD1211B.CopyFiles98	= 11			; system subdirectory on Win 98
ZD1211B.CopyFilesMe	= 11			; system subdirectory on Win Me
ZD1211B.CopyFiles2K	= 12			; system32\drivers subdirectory on Win NT/2000
ZD1211B.CopyFilesXP	= 12			; system32\drivers subdirectory on Win XP
ZD1211B.CopyFilesXP64	= 12			; system32\drivers subdirectory on Win XP


[PreCopySection]
HKR,,NoSetupUI,,1


[SourceDisksNames]
1=%DISKNAME%,,,


[SourceDisksFiles]
ZD11BU98.sys = 1
ZD11BUME.sys = 1
ZD11BU2K.sys = 1
ZD11BUXP.sys = 1
ZD11BU64.sys = 1



;******************************************************************************
[ZD1211B_Common.reg]
HKR, Ndi\params\NumRfd,         ParamDesc,  	0, "%ReceiveFrameDescriptors%"
HKR, Ndi\params\NumRfd,         default,    	0, "32"
HKR, Ndi\params\NumRfd,         min,        	0, "1"
HKR, Ndi\params\NumRfd,         max,        	0, "00001024"
HKR, Ndi\params\NumRfd,         step,       	0, "1"
HKR, Ndi\params\NumRfd,         Base,       	0, "10"
HKR, Ndi\params\NumRfd,         type,       	0, "int"
HKR, Ndi\params\NumRfd,         flag, 		1, 20,00,00,00

HKR, Ndi\params\NumTcb,         ParamDesc,  	0, "%TransmitControlBlocks%"
HKR, Ndi\params\NumTcb,         default,    	0, "32"
HKR, Ndi\params\NumTcb,         min,        	0, "1"
HKR, Ndi\params\NumTcb,         max,        	0, "00000064"
HKR, Ndi\params\NumTcb,         step,       	0, "1"
HKR, Ndi\params\NumTcb,         Base,       	0, "10"
HKR, Ndi\params\NumTcb,         type,		0, "int"
HKR, Ndi\params\NumTcb,         flag,		1, 20,00,00,00

HKR, Ndi\params\NumCoalesce,    ParamDesc,  	0, "%CoalesceBuffers%"
HKR, Ndi\params\NumCoalesce,    default,    	0, "128"
HKR, Ndi\params\NumCoalesce,    min,        	0, "1"
HKR, Ndi\params\NumCoalesce,    max,        	0, "00000128"
HKR, Ndi\params\NumCoalesce,    step,       	0, "1"
HKR, Ndi\params\NumCoalesce,    Base,       	0, "10"
HKR, Ndi\params\NumCoalesce,    type,       	0, "int"
HKR, Ndi\params\NumCoalesce,    flag, 		1, 20,00,00,00

HKR,,                           	PreambleMode,   0, "0"
HKR,NDI\params\PreambleMode,    	ParamDesc,      0, "PreambleMode"
HKR,NDI\params\PreambleMode,       	type,           0, "enum"
HKR,NDI\params\PreambleMode,           	flag,           1, 30,00,00,00
HKR,Ndi\params\PreambleMode,           	default,        0, "3"
HKR,NDI\params\PreambleMode\enum,      	1,              0, "Long"
HKR,NDI\params\PreambleMode\enum,      	2,              0, "Short"
HKR,NDI\params\PreambleMode\enum,      	3,              0, "Auto"

;HKR,,                           	IBSS_G_Mode,    0, "0"
;HKR,NDI\params\IBSS_G_Mode,    	        ParamDesc,      0, "IBSS_G_Mode"
;HKR,NDI\params\IBSS_G_Mode,       	type,           0, "enum"
;HKR,NDI\params\IBSS_G_Mode,           	flag,           1, 30,00,00,00
;HKR,Ndi\params\IBSS_G_Mode,           	default,        0, "0"
;HKR,NDI\params\IBSS_G_Mode\enum,      	0,              0, "Disable"
;HKR,NDI\params\IBSS_G_Mode\enum,      	1,              0, "Enable"

;HKR,,                           	IBSS_PureG_Mode,0, "0"
;HKR,NDI\params\IBSS_PureG_Mode,    	ParamDesc,      0, "IBSS_PureG_Mode"
;HKR,NDI\params\IBSS_PureG_Mode,       	type,           0, "enum"
;HKR,NDI\params\IBSS_PureG_Mode,         flag,           1, 30,00,00,00
;HKR,Ndi\params\IBSS_PureG_Mode,         default,        0, "0"
;HKR,NDI\params\IBSS_PureG_Mode\enum,    0,              0, "Disable"
;HKR,NDI\params\IBSS_PureG_Mode\enum,    1,              0, "Enable"

HKR,,                           		IBSS Wireless Mode,   0, "0"
HKR,NDI\params\IBSS Wireless Mode,    		ParamDesc,      0, "IBSS Wireless Mode"
HKR,NDI\params\IBSS Wireless Mode,       	type,           0, "enum"
HKR,NDI\params\IBSS Wireless Mode,           	flag,           1, 30,00,00,00
HKR,Ndi\params\IBSS Wireless Mode,           	default,        0, "0"
HKR,NDI\params\IBSS Wireless Mode\enum,      	0,              0, "IBSS B Mode"
HKR,NDI\params\IBSS Wireless Mode\enum,      	1,              0, "IBSS G Mode"

HKR,,                           	IBSS Protection Mode,0, "0"
HKR,NDI\params\IBSS Protection Mode,    	ParamDesc,      0, "IBSS Protection Mode"
HKR,NDI\params\IBSS Protection Mode,       	type,           0, "enum"
HKR,NDI\params\IBSS Protection Mode,         flag,           1, 30,00,00,00
HKR,Ndi\params\IBSS Protection Mode,         default,        0, "0"
HKR,NDI\params\IBSS Protection Mode\enum,    0,              0, "Disable"
HKR,NDI\params\IBSS Protection Mode\enum,    1,              0, "Enable"

HKR,,                           	             Use_G_Mode_in_Usb1.1,0, "0"
HKR,NDI\params\Use_G_Mode_in_Usb1.1,    	     ParamDesc,      0, "Use_G_Mode_in_Usb1.1"
HKR,NDI\params\Use_G_Mode_in_Usb1.1,             type,           0, "enum"
HKR,NDI\params\Use_G_Mode_in_Usb1.1,             flag,           1, 30,00,00,00
HKR,Ndi\params\Use_G_Mode_in_Usb1.1,             default,        0, "0"
HKR,NDI\params\Use_G_Mode_in_Usb1.1\enum,        0,              0, "Disable"
HKR,NDI\params\Use_G_Mode_in_Usb1.1\enum,        1,              0, "Enable"

HKR,,                           	PSPXLinkMode,   0, "0"
HKR,NDI\params\PSPXLinkMode,    	        ParamDesc,      0, "PSPXLinkMode"
HKR,NDI\params\PSPXLinkMode,       	type,           0, "enum"
HKR,NDI\params\PSPXLinkMode,           	flag,           1, 30,00,00,00
HKR,Ndi\params\PSPXLinkMode,           	default,        0, "0"
HKR,NDI\params\PSPXLinkMode\enum,      	0,              0, "Disable"
HKR,NDI\params\PSPXLinkMode\enum,      	1,              0, "Enable"

HKR,,                           	QosTagPolicy,   0, "0"
HKR,NDI\params\QosTagPolicy,    	ParamDesc,      0, "QosTagPolicy"
HKR,NDI\params\QosTagPolicy,       	type,           0, "enum"
HKR,NDI\params\QosTagPolicy,           	flag,           1, 30,00,00,00
HKR,Ndi\params\QosTagPolicy,           	default,        0, "0"
HKR,NDI\params\QosTagPolicy\enum,      	0,              0, "Auto"
HKR,NDI\params\QosTagPolicy\enum,      	1,              0, "802.1Q Tag"
HKR,NDI\params\QosTagPolicy\enum,      	2,              0, "DSCP Tag"

HKR,,                           	WMMQosSupport,   0, "0"
HKR,NDI\params\WMMQosSupport,    	ParamDesc,       0, "WMMQosSupport"
HKR,NDI\params\WMMQosSupport,       	type,            0, "enum"
HKR,NDI\params\WMMQosSupport,           flag,            1, 30,00,00,00
HKR,Ndi\params\WMMQosSupport,           default,         0, "0"
HKR,NDI\params\WMMQosSupport\enum,      0,               0, "Disable"
HKR,NDI\params\WMMQosSupport\enum,      1,               0, "Enable"

HKR,,                           PHY_A_6M_Setpoint_Value,	0x10001, 0x28
HKR,,                           PHY_A_6M_CR128_Value,	0x10001, 0x17
HKR,,                           PHY_A_1dBm_Value,	0x10001, 0x08

;HKR,,                           FirmwareName,	0, %FirmwareFileName%
HKR,,                           EnableAntennaDiversity, 0, "0"
HKR,,                           DefaultAntenna, 0, "0"
HKR,,                           DefaultWirelessMode, 0, "0"
HKR,,                           SaveDefaultConnection, 0, "1"
HKR,,                           RFSwitch, 0, "0"
; FastRoaming: 1000(1sec) <= value <= 4000(4 sec)
HKR,,                           FastRoaming, 0, "4000" 
HKR,,                           EnableFastRoaming, 0, "0" 
HKR,,                           FwRadio, 0, "0" 
;*********************************************************************
[UnZDRegistryUSB.reg]
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Uninstall\UNZD1211B%InterfaceType%,DEL_HKR_0000,0,"ENUM\"%ZD1211B_50U_PNP%


;*********************************************************************
[Strings]
INFProvider	= "ZyDAS"
Manufacturer	= "ZyDAS"

DISKNAME	= "ZyDAS ZD1211B IEEE 802.11 b+g Wireless LAN Driver (USB) Installation Disk"

DriverFileName	= "zd1211Bu.sys"
InterfaceType	= "USB"
CardType	= "PNP"
VendorDesc	= "ZyDAS ZD1211B 802.11 b+g Wireless LAN"
CustomServiceName = "ZD1211BU"

ZD1211B_50U_DESC	= "(ZD1211B)IEEE 802.11 b+g USB Adapter"
ZD1211B_50U_PNP  = "USB\VID_0ACE&PID_1215"

ReceiveFrameDescriptors = "ReceiveFrameDescriptors"
TransmitControlBlocks = "TransmitControlBlocks"
CoalesceBuffers = "CoalesceBuffers"


ZD1211BU.Service.DispName = "ZyDAS ZD1211B IEEE 802.11 b+g Wireless LAN Driver (USB)"
