; Installation inf for Atheros Predator USB board
;


[Version]
Signature="$CHICAGO$"
Class=USB
ClassGUID={36FC9E60-C465-11CF-8056-444553540000}
provider=%ATHR%
DriverVer=12/05/2003,1.00.001
;Catalogfile = athfmwdl.cat

[SourceDisksNames]
1=%Disk_Description%,,,

[SourceDisksFiles]
ATHFMWDL.sys = 1

[Manufacturer]
%MfgName%=Atheros

[Atheros]
%USB\VID_0CF3&PID_0002.DeviceDesc%=ATHFMWDL.Dev, USB\VID_0CF3&PID_0002
%USB\VID_0CF3&PID_0002.DeviceDesc%=ATHFMWDL.Dev, USB\VID_168C&PID_0002
%USB\VID_0CF3&PID_0002.DeviceDesc%=ATHFMWDL.Dev, USB\VID_0CF3&PID_0004
%USB\VID_0CF3&PID_0002.DeviceDesc%=ATHFMWDL.Dev, USB\VID_0CF3&PID_0006

[DestinationDirs]
ATHFMWDL.Files.Ext = 10,System32\Drivers

[ATHFMWDL.Dev.NT]
CopyFiles=ATHFMWDL.Files.Ext

[ATHFMWDL.Dev.NT.Services]
Addservice = ATHFMWDL, 0x00000002, ATHFMWDL.AddService

[ATHFMWDL.AddService]
DisplayName    = %ATHFMWDL.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\ATHFMWDL.sys
AddReg         = ATHFMWDL.AddReg
LoadOrderGroup = Base

[ATHFMWDL.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,ATHFMWDL.sys
HKR,"Parameters","MaximumTransferSize",0x10001,4096
HKR,"Parameters","DebugLevel",0x10001,3
HKR,"Parameters","AthUsbEnable",0x10001,0

[ATHFMWDL.Files.Ext]
Athfmwdl.sys

;---------------------------------------------------------------;

[Strings]
ATHR="Atheros"
MfgName="Atheros"
Disk_Description="AthUsb Installation Disk"
USB\VID_0CF3&PID_0002.DeviceDesc="Atheros USB 2.0 Wireless Adapter Bootloader Download"
ATHFMWDL.SvcDesc="Atheros USB Wireless Adapter Bootloader driver"
