;;*******************************************************************
;; This INF file is for DigitalChina DCN-530TX Fast Ethernet Adapter
;;
;; Copyright (C) 2002 Digitalchina Networks Limited.
;;*******************************************************************

[version]
LayoutFile  = layout.inf
Signature   = "$WINDOWS 95$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %DCN%
DriverVer   = 04/27/2002, 1.00.0427.2002

[Manufacturer]
%DCN%    = DCN

[DCN]
%DCN530T.DeviceDesc%  = DCN530T.ndi, PCI\VEN_1113&DEV_1216&SUBSYS_00011113

;;****************************************************************************
;; Windows 95
;;****************************************************************************
[DCN530T.ndi]
AddReg          = DCN530T.id.reg, DCN530.common.reg.1207F, DCN530.win.reg, DCN530.pci.reg
CopyFiles       = DCN530.sys.CopyFiles, DCN530.inf.CopyFiles


[DCN530.sys.CopyFiles]
DCN530N3.sys,,,2
[DCN530.inf.CopyFiles]
NETDC530.INF,,,2

;;----------------------------------------------------------------------------
;; DCN530 Parameters
;;----------------------------------------------------------------------------
;;****************************************************************************
;; Windows 95 parameters
;;****************************************************************************
[DCN530T.id.reg]
HKR, Ndi,       DeviceID,       0,      "PCI\VEN_1113&DEV_1216&SUBSYS_00011113"


[DCN530.pci.reg]
HKR, ,                                      AdapterType,    0, "5"
HKR,,TxPacketDesc,,"160"      ; 
HKR,,RxPacketDesc,,"120"      ; 0x78
HKR,,TxDmaDesc,,"320"         ; 0x258
HKR,,RxDmaDesc,,"40"          ; 0x28
HKR,,PacketsPerTxInt,,"10"    ; 0x0a
HKR,,PacketsPerRxInd,,"10"    ; 0x0a
HKR,,BurstLength,,"0"         ; 0 (Unlimited), 1 DW, 2 DW, 3 DW, ...

[DCN530.win.reg]
;; key,subkey,valuname,type,value
HKR, ,  AdapterCFID,     ,      12161113
HKR, ,  DriverDesc,     0,      "DigitalChina DCN-530TX Fast Ethernet Adapter"
HKR, ,  DevLoader,      0,      *ndis
HKR, ,  DeviceVxDs,     0,      DCN530N3.sys
HKR, ,  EnumPropPages,  0,      netdi.dll,      EnumPropPages

;;params
HKR, ,  MediaType,      0,      1
HKR, ,  AdapterType,    0,      5
HKR, ,  BusType,        0,      5

;; NDIS Info
HKR, NDIS,              MajorNdisVersion,       1,      03
HKR, NDIS,              MinorNdisVersion,       1,      0a
HKR, NDIS,              LogDriverName,          0,      "DCN530N3"

;; Interfaces
HKR, Ndi\Interfaces,    DefLower,               ,       "ethernet"
HKR, Ndi\Interfaces,    LowerRange,             ,       "ethernet"
HKR, Ndi\Interfaces,    DefUpper,               ,       "ndis3"
HKR, Ndi\Interfaces,    UpperRange,             ,       "ndis3"

;; Install sections
;HKR, Ndi\Install,       ndis3,                 0,       "DCN530.ndis3"

;;****************************************************************************
;; DCN530 common parameters
;;****************************************************************************
[DCN530.common.reg.1207F]
HKR,Ndi\Params\MediaType,ParamDesc,,"1.Media Type"
HKR,Ndi\Params\MediaType,default,,"0"
HKR,Ndi\Params\MediaType,type,,"enum"
HKR,Ndi\Params\MediaType\enum,0,,"AutoSense"
HKR,Ndi\Params\MediaType\enum,1,,"10BaseT"
HKR,Ndi\Params\MediaType\enum,2,,"10BaseT Full_Duplex"
HKR,Ndi\Params\MediaType\enum,3,,"100BaseTX"
HKR,Ndi\Params\MediaType\enum,4,,"100BaseTX Full_Duplex"
HKR,Ndi\Params\MediaType,flag,1,"20","00","00","00"

[DCN530.common.reg.CardBus]
HKR,Ndi\Params\MediaType,ParamDesc,,"1.Media Type"
HKR,Ndi\Params\MediaType,default,,"0"
HKR,Ndi\Params\MediaType,type,,"enum"
HKR,Ndi\Params\MediaType\enum,0,,"AutoSense"
HKR,Ndi\Params\MediaType\enum,1,,"10BaseT"
HKR,Ndi\Params\MediaType\enum,2,,"10BaseT Full_Duplex"
HKR,Ndi\Params\MediaType\enum,3,,"100BaseTX"
HKR,Ndi\Params\MediaType\enum,4,,"100BaseTX Full_Duplex"
HKR,Ndi\Params\MediaType,flag,1,"20","00","00","00"

[DCN530.common.reg.MiniPCI]
HKR,Ndi\Params\MediaType,ParamDesc,,"1.Media Type"
HKR,Ndi\Params\MediaType,default,,"0"
HKR,Ndi\Params\MediaType,type,,"enum"
HKR,Ndi\Params\MediaType\enum,0,,"AutoSense"
HKR,Ndi\Params\MediaType\enum,1,,"10BaseT"
HKR,Ndi\Params\MediaType\enum,2,,"10BaseT Full_Duplex"
HKR,Ndi\Params\MediaType\enum,3,,"100BaseTX"
HKR,Ndi\Params\MediaType\enum,4,,"100BaseTX Full_Duplex"
HKR,Ndi\Params\MediaType,flag,1,"20","00","00","00"

;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
DCN530.sys.CopyFiles          = 11
DCN530.inf.CopyFiles          = 17

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
DCN530N3.sys=1
NETDC530.INF=1

;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
DCN                    = "Digitalchina Networks Limited"

DISKNAME = "DigitalChina DCN-530TX Fast Ethernet Adapter Driver Diskette"

DCN530T.DeviceDesc      = "DigitalChina DCN-530TX Fast Ethernet Adapter"
