;*******************************************************
;****************************************************************************************
;
;    Copyright (c) 1998-2001 D-Link Corporation
;    All Rights Reserved.
;
;    $Logfile:  $
;    $Revision:  $
;    $Date:  $
;    $Author:  $
;
;    FILE:
;            netvusb.inf
;
;    DESCRIPTION:
;            D-Link DWL120 Wireless USB Adapter inf file.
;
;    COMMENTS:
;            INF file for the NDIS driver under Windows XP
;            
; 
;
; 
;



[Version]
Signature  = "$Windows NT$"
Class      = Net
ClassGUID  = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider   = %D-Link%
;CatalogFile = netvusba.cat
DriverVer  = 09/25/2001,1.1.2.22

[Manufacturer]
%D-Link%   = D-Link

[ControlFlags]
ExcludeFromSelect = VID_03eb&PID_7603
          
                                                             
[D-Link]
%USBFVNETA.DeviceDesc% = USBFVNETA.Ndi,USB\VID_03eb&PID_7603

;*******************************************************************************
; Win XP main sections
;*******************************************************************************


[USBFVNETA.Ndi.NT]
Characteristics = 0x84 	; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 15 	; USB
AddReg          = USBFVNETA.NT.Reg, USBFVNETA.Params
CopyFiles       = CopyFile.NT.Sys
DriverVer  = 09/25/2001,1.1.2.22

[USBFVNETA.Ndi.NT.Services]
AddService = USBFVNETA, 2, USBFVNETA.Service, Common.EventLog

;*******************************************************************************
; Driver parameters
;*******************************************************************************

[USBFVNETA.Params]

HKR, Ndi,                              	NetworkAddress, 	0, "000000000000"

HKR, Ndi\params\PreambleType,	      	ParamDesc,     		0, "Preamble Type"
HKR, Ndi\params\PreambleType,		default,		0, "0"
HKR, Ndi\params\PreambleType,	      	type,			0, "enum"
HKR, Ndi\params\PreambleType\enum,	0,			0, "Long"
HKR, Ndi\params\PreambleType\enum,	1,			0, "Short"
HKR, ,                                	PreambleType,   	0, "0"

HKR, Ndi\params\Rate,	      		ParamDesc,     		0, "Rate (Mbps)"
HKR, Ndi\params\Rate,			default,		0, "3"
HKR, Ndi\params\Rate,	      		type,			0, "enum"
HKR, Ndi\params\Rate\enum,		0,			0, "1"
HKR, Ndi\params\Rate\enum,		1,			0, "2"
HKR, Ndi\params\Rate\enum,		2,			0, "5.5"
HKR, Ndi\params\Rate\enum,		3,			0, "11"
HKR, Ndi\params\Rate\enum,		4,			0, "Auto"
HKR, ,                                	Rate,    		0, "3"

HKR, Ndi\params\RTS_Threshold,	      	ParamDesc,     		0, "RTS Threshold"
HKR, Ndi\params\RTS_Threshold,		default,		0, "2347"
HKR, Ndi\params\RTS_Threshold,	      	type,			0, "int"
HKR, Ndi\params\RTS_Threshold,		min,			0, "0"
HKR, Ndi\params\RTS_Threshold,		max,			0, "2347"
HKR, Ndi\params\RTS_Threshold,		step,			0, "1"
HKR, ,                                	RTS_Threshold,  	0, "2347"

HKR, Ndi\params\Frag_Threshold,	      	ParamDesc,     		0, "Fragmentation Threshold"
HKR, Ndi\params\Frag_Threshold,		default,		0, "2346"
HKR, Ndi\params\Frag_Threshold,	      	type,			0, "int"
HKR, Ndi\params\Frag_Threshold,		min,			0, "256"
HKR, Ndi\params\Frag_Threshold,		max,			0, "2346"
HKR, Ndi\params\Frag_Threshold,		step,			0, "1"
HKR, ,                                	Frag_Threshold, 	0, "2346"



;*******************************************************************************
; Install section for Windows XP
;*******************************************************************************

[USBFVNETA.NT.Reg]
; Interfaces
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi,            Service,    0, "USBFVNETA"

[USBFVNETA.Service]
DisplayName    = %USBFVNETA.DisplayName%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\vnetusba.sys
LoadOrderGroup = NDIS


[Common.EventLog]
AddReg = Common.AddEventLog.Reg

[Common.AddEventLog.Reg]
HKR, , EventMessageFile, 0x00020000, %%SystemRoot%%\System32\netevent.dll, %%SystemRoot%%\System32\drivers\vnetusba.sys
HKR, , TypesSupported  , 0x00010001, 7


[CopyFile.NT.Sys]
vnetusba.sys,,,2

;*******************************************************************************
; Destination directories
;*******************************************************************************

[DestinationDirs]
DefaultDestDir   = 12 ; Drivers directory
CopyFile.Sys     = 11
CopyFile.NT.Sys  = 12


[SourceDisksNames]
50=%DriverDisketteName%,,

[SourceDisksFiles]
vnetusba.sys=50,.,vnetusba.sys,10000
netvusba.inf=50,.,netvusba.inf,10000

;*******************************************************************************
; Localizable strings
;*******************************************************************************

[Strings]
D-Link = "D-Link"
USBFVNETA.DeviceDesc = "D-LINK DWL-120 WIRELESS USB ADAPTER"
USBFVNETA.DisplayName = "D-LINK DWL-120 WIRELESS USB ADAPTER"
DriverDisketteName      = "D-Link Air USB Driver Disk"
Help_Text = "The D-Link Air Wireless USB Adapter lets you set up and operate a Wireless LAN compliant with the IEEE 802.11b Standard. It operates in the license free 2.4 GHz ISM band and achieves a peak data rate of 11 Mbs."
