; 
; IEEE 802.11g Wireless Cardbus/PCI Adapter
;
; Supported OS:Win98/WinME/Win2k/WinXP 
;
;
; This file is for direct installation without Install Shield


[Version]
;;CatalogFile=tnet1130.cat
Signature = "$Windows NT$"
Provider  = %TI%
Class     = Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
DriverVer=06/17/2004,6.0.5.30

[Manufacturer]
%TI% = TexasInstruments,NT.5.1

; pnp cards should be excluded from select
[ControlFlags]
ExcludeFromSelect = PCI\VEN_104C&DEV_9066	

;For WinXP
[TexasInstruments.NT.5.1]
%TIACX.DeviceDesc% = TIACXXP, PCI\VEN_104C&DEV_9066	; B & G

; For Win98,ME,2K
[TexasInstruments]
%TIACX.DeviceDesc% = TIACX, PCI\VEN_104C&DEV_9066       ; B & G

;~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
;~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~   Windows XP   ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
;~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

;******************************   Windows XP B & G ******************************
[TIACXXP]
BusType         = 5
AddReg          =TIACXXP.ndi.reg.NT, TI.Param.Reg, BG.Param.Reg
Characteristics = 0x84
CopyFiles       =TIACXXP.CopyFiles

[TIACXXP.ndi.reg.NT]
HKR, Ndi,               Service,    0,  "TNET1130"
HKR, Ndi\Interfaces,    LowerRange, 0,  "ethernet"
HKR, Ndi\Interfaces,    UpperRange, 0,  "ndis5"

[TIACXXP.Services]
AddService = TNET1130, 2, TIACXLNXP.Service, TIACXLNXP.EventLog

[TIACXXP.CopyFiles]
FwRad16.bin
FwRad17.bin
TNET1130.sys

;******************************   Windows XP A & G ******************************
[TIACXAGXP]
BusType         = 5
AddReg          =TIACXAGXP.ndi.reg.NT, TI.Param.Reg, AG.Param.Reg
Characteristics = 0x84
CopyFiles       =TIACXAGXP.CopyFiles

[TIACXAGXP.ndi.reg.NT]
HKR, Ndi,               Service,    0,  "TNET1130"
HKR, Ndi\Interfaces,    LowerRange, 0,  "ethernet"
HKR, Ndi\Interfaces,    UpperRange, 0,  "ndis5"

[TIACXAGXP.Services]
AddService = TNET1130, 2, TIACXLNXP.Service, TIACXLNXP.EventLog


[TIACXAGXP.CopyFiles]
FwRad16.bin
FwRad17.bin
TNET1130.sys

;******************************   Windows XP Common A & B & G **************************

[TIACXLNXP.Service]
DisplayName     = %TIACXLN.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\tnet1130.sys
LoadOrderGroup  = NDIS

[TIACXLNXP.EventLog]
AddReg = TIACXLNXP.AddEventLog.reg

[TIACXLNXP.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


;~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
;~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~   End of Windows XP   ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
;~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
;~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~   Windows 2k/ME   ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
;~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

;******************************   Windows 2k/ME   B & G   ******************************
[TIACX.NT]
BusType         = 5
AddReg          =TIACX.ndi.reg.NT, TI.Param.Reg, BG.Param.Reg
Characteristics = 0x84
CopyFiles       =TIACX.CopyFiles.NT, TIACX.BinFiles.NT

[TIACX.ndi.reg.NT]
HKR, Ndi,               Service,    0,  "TNET1130"
HKR, Ndi\Interfaces,    LowerRange, 0,  "ethernet"
HKR, Ndi\Interfaces,    UpperRange, 0,  "ndis5"

[TIACX.NT.Services]
AddService = TNET1130, 2, TIACXLN.Service, TIACXLN.EventLog

[TIACX.CopyFiles.NT]
FwRad16.bin
FwRad17.bin
TNET1130.sys

;
; Copy tiacxsn.bin to system directory for ME
;
[TIACX.BinFiles.NT]
FwRad16.bin
FwRad17.bin

;******************************   Windows 2k/ME   A & G   ******************************
[TIACXAG.NT]
BusType         = 5
AddReg          =TIACXAG.ndi.reg.NT, TI.Param.Reg, AG.Param.Reg
Characteristics = 0x84
CopyFiles       =TIACXAG.CopyFiles.NT, TIACXAG.BinFiles.NT

[TIACXAG.ndi.reg.NT]
HKR, Ndi,               Service,    0,  "TNET1130"
HKR, Ndi\Interfaces,    LowerRange, 0,  "ethernet"
HKR, Ndi\Interfaces,    UpperRange, 0,  "ndis5"

[TIACXAG.NT.Services]
AddService = TNET1130, 2, TIACXLN.Service, TIACXLN.EventLog

[TIACXAG.CopyFiles.NT]
FwRad16.bin
FwRad17.bin
TNET1130.sys

;
; Copy tiacxsn.bin to system directory for ME
;
[TIACXAG.BinFiles.NT]
FwRad16.bin
FwRad17.bin

;******************************   Windows 2K/ME Common A & B & G **************************

[TIACXLN.Service]
DisplayName     = %TIACXLN.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\tnet1130.sys
LoadOrderGroup  = NDIS

[TIACXLN.EventLog]
AddReg = TIACXLN.AddEventLog.reg

[TIACXLN.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

;~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
;~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~   End of Windows 2k/ME  ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
;~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
;~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~   Windows 98   ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
;~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

;*********************************   Windows 98 B & G  ********************************

[TIACX]
AddReg=TIACX.ndi.reg, TI.Param.Reg, TIACX.Install, BG.Param.Reg

[TIACX.Copy]
CopyFiles=TIACX.CopyFiles

[TIACX.Install]
HKR,Ndi\Install,,,"TIACX.Copy"
HKR,Ndi\Remove,,,"TIACX.Remove"

[TIACX.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_104C&DEV_9066"

HKR,Ndi,HelpText,0,%WLANAdapterHelpText%

; key,subkey,valuname,type,value
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,TNET1130.sys
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"

; NDIS Info
HKR, NDIS, LogDriverName, , "TNET1130"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,Ndi\Interfaces,DefUpper,,"ndis3,ndis4,ndis5"
HKR,Ndi\Interfaces,UpperRange,,"ndis3,ndis4,ndis5"


[TIACX.CopyFiles]
FwRad16.bin
FwRad17.bin
TNET1130.sys

;*********************************   Windows 98 A & G  ********************************

[TIACXAG]
AddReg=TIACXAG.ndi.reg, TI.Param.Reg, TIACXAG.Install, AG.Param.Reg

[TIACXAG.Copy]
CopyFiles=TIACX.CopyFiles

[TIACXAG.Install]
HKR,Ndi\Install,,,"TIACX.Copy"
HKR,Ndi\Remove,,,"TIACX.Remove"

[TIACXAG.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_104C&DEV_9066"

HKR,Ndi,HelpText,0,%WLANAdapterHelpText%

; key,subkey,valuname,type,value
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,TNET1130.sys
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"

; NDIS Info
HKR, NDIS, LogDriverName, , "TNET1130"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,Ndi\Interfaces,DefUpper,,"ndis3,ndis4,ndis5"
HKR,Ndi\Interfaces,UpperRange,,"ndis3,ndis4,ndis5"


[TIACXAG.CopyFiles]
FwRad16.bin
FwRad17.bin
TNET1130.sys


;~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
;~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~   End of Windows  98   ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
;~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

;***********************************   B & G All OSes ***********************************

[BG.Param.Reg]


HKR, ,dot11NetworkType,, "3"


;************************************   A & G All OSes ************************************

[AG.Param.Reg]

HKR, ,dot11NetworkType,, "4"


;******************************  Common Registry Settings  ******************************

[TI.Param.Reg]


; GlobalMaxTcpWindowSize - TCP Window size
HKLM,System\CurrentControlSet\Services\Tcpip\Parameters, TcpWindowSize, ,40320

HKR,NDI\params\dot11DesiredBSSType,ParamDesc,,"Network Type"
HKR,NDI\params\dot11DesiredBSSType,type,,"enum"
HKR,NDI\params\dot11DesiredBSSType,default,,"1"
HKR,NDI\params\dot11DesiredBSSType\enum,"0",,"802.11 Ad-hoc"
HKR,NDI\params\dot11DesiredBSSType\enum,"1",,"Infrastructure"


HKR, Ndi\Params\dot11DesiredSSID, ParamDesc, ,"SSID"
HKR, Ndi\Params\dot11DesiredSSID, Type, ,"edit"
HKR, Ndi\Params\dot11DesiredSSID, LimitText, ,"32"
HKR, Ndi\Params\dot11DesiredSSID, Default,,""
HKR, Ndi\Params\dot11DesiredSSID, UpperCase,,"0"

; Desired Tx Rate 
HKR,NDI\params\dot11DesiredTxRate,ParamDesc,, "Desired Tx Rate"
HKR,NDI\params\dot11DesiredTxRate,type,,"enum"
HKR,NDI\params\dot11DesiredTxRate,default,,"0"
HKR,NDI\params\dot11DesiredTxRate\enum,"0",,"Auto"
HKR,NDI\params\dot11DesiredTxRate\enum,"1",,"1 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"2",,"2 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"3",,"5.5 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"4",,"6 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"5",,"9 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"6",,"11 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"7",,"12 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"8",,"18 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"9",,"22 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"10",,"24 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"11",,"36 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"12",,"48 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"13",,"54 Mbps"


; Rate Adaptation
HKR, ,Mode4x,, "0"
HKR, ,dot11DesiredBSSType,, "1"
HKR, ,dot11BasicRateMask,, "1"
HKR, ,dot11SupportedRateMask,, "8"
HKR, ,dot11AuthenticationMode,, "2"
HKR, ,FBLongInterval,, "100"
HKR, ,FBShortInterval,, "2000"
HKR, ,LnaRestoreTime,, "600"
HKR, ,LnaFftBadCorrCountThresh,, "100"
HKR, ,LnaAgcHighThresh,, "55"
HKR, ,LnaAgcLowThresh,, "60"
HKR, ,PrivacyMode,, "2"
HKR, ,WiFiAdhoc,, "1"

;******************************   Common Misc Settings ******************************

[DestinationDirs]
DefaultDestDir  =     12 ; Windows\System32\Drivers
TIACXXP.CopyFiles =   12 ; Winnt\System32\Drivers Directory ; WinXP
TIACXAGXP.CopyFiles = 12 ; Winnt\System32\Drivers Directory ; WinXP
TIACX.CopyFiles =     11 ; Windows\System or Winnt\System32 Directory ; Win98/ME
TIACX.BinFiles.NT =   10,system
TIACXAG.CopyFiles =   11 ; Windows\System or Winnt\System32 Directory ; Win98/ME
TIACXAG.BinFiles.NT = 10,system

;TIACX.CopyFiles.NT = 12 ; Winnt\System32\Drivers Directory ; Win2k


[SourceDisksNames]
1 = %DiskName%,,

[SourceDisksFiles]
FwRad16.bin   = 1
FwRad17.bin   = 1
TNET1130.sys  = 1


[Strings]
TI="OEM"
TIACX.DeviceDesc ="IEEE 802.11g Wireless Cardbus/PCI Adapter"
TIACXLN.Service.DispName  ="IEEE 802.11g Wireless Cardbus/PCI Adapter"
WLANAdapterHelpText= "A WLAN Adapter provides high speed connection to the Internet through 802.11g technology"
DiskName="IEEE 802.11g Wireless Cardbus/PCI Adapter Driver Disk"
