;; NETGA311.INF (WindowsXP inf for NDIS5.1 driver)
;;
;; NETGEAR GA311 Gigabit Adapter NDIS Driver
;;
;; Copyright 2003, NETGEAR

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %NETGEAR%                                
CatalogFile = GA311NXP.CAT
DriverVer   = 10/09/2003,5.608.1009.2003

[Manufacturer]
%NETGEAR%   = NETGEAR

[ControlFlags]
;;ExcludeFromSelect = PCI\VEN_10EC&DEV_8169

[NETGEAR]
; DisplayName		Section		   DeviceID
; -----------		-------		   --------
;;%GA311.DeviceDesc%	= GA311.ndi,	   PCI\VEN_10EC&DEV_8169
%GA311.DeviceDesc%	= GA311.ndi,     PCI\VEN_10EC&DEV_8169&SUBSYS_311A1385

;;****************************************************************************
;; Windows XP
;;****************************************************************************
[GA311.ndi.NT]
Characteristics = 0x84
BusType         = 5
AddReg          = GA311.common.reg, RTL8023.reg
CopyFiles       = Rtlnic.CopyFiles

[GA311.ndi.NT.Services]
AddService = RTL8023, 2, rtsnt.Service, common.EventLog

[Rtlnic.CopyFiles]
GA311ND5.SYS,,,2

;;****************************************************************************
;; common parameters
;;****************************************************************************
[GA311.common.reg]
HKR, Ndi\params\DuplexMode,       ParamDesc,  0, %SpeedDuplexMode%
HKR, Ndi\params\DuplexMode,       type,       0, "enum"
HKR, Ndi\params\DuplexMode,       default,    0, "1"
HKR, Ndi\params\DuplexMode\enum,  1,          0, %auto_nego%
HKR, Ndi\params\DuplexMode\enum,  2,          0, %sd10half%
HKR, Ndi\params\DuplexMode\enum,  3,          0, %sd10full%
HKR, Ndi\params\DuplexMode\enum,  4,          0, %sd100half%
HKR, Ndi\params\DuplexMode\enum,  5,          0, %sd100full%
HKR, Ndi\params\DuplexMode\enum,  6,          0, %sd1000full%

HKR,Ndi\params\NetworkAddress,    ParamDesc,  0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,    type,       0, "edit"
HKR,Ndi\params\NetworkAddress,    default,    0, "000000000000"
HKR,Ndi\params\NetworkAddress,    LimitText,  0, "12"
HKR,Ndi\params\NetworkAddress,    UpperCase,  0, "1"
HKR,Ndi\params\NetworkAddress,    Optional,   0, "1"

;;HKR,Ndi\Params\NumTxDesc,         ParamDesc,  0, %TxDescNumber%
;;HKR,Ndi\Params\NumTxDesc,         Type,       0, "int"
;;HKR,Ndi\Params\NumTxDesc,         Default,    0, "256"
;;HKR,Ndi\Params\NumTxDesc,         Min,        0, "64"
;;HKR,Ndi\Params\NumTxDesc,         Max,        0, "512"
;;HKR,Ndi\Params\NumTxDesc,         Step,       0, "1"
;;HKR,Ndi\Params\NumTxDesc,         Base,       0, "10"

;;HKR,Ndi\Params\NumRxDesc,         ParamDesc,  0, %RxDescNumber%
;;HKR,Ndi\Params\NumRxDesc,         Type,       0, "int"
;;HKR,Ndi\Params\NumRxDesc,         Default,    0, "256"
;;HKR,Ndi\Params\NumRxDesc,         Min,        0, "64"
;;HKR,Ndi\Params\NumRxDesc,         Max,        0, "512"
;;HKR,Ndi\Params\NumRxDesc,         Step,       0, "1"
;;HKR,Ndi\Params\NumRxDesc,         Base,       0, "10"

;;HKR,Ndi\Params\NumTxDescHPQ,      ParamDesc,  0, %TxHPQDescNumber%
;;HKR,Ndi\Params\NumTxDescHPQ,      Type,       0, "int"
;;HKR,Ndi\Params\NumTxDescHPQ,      Default,    0, "128"
;;HKR,Ndi\Params\NumTxDescHPQ,      Min,        0, "64"
;;HKR,Ndi\Params\NumTxDescHPQ,      Max,        0, "256"
;;HKR,Ndi\Params\NumTxDescHPQ,      Step,       0, "1"
;;HKR,Ndi\Params\NumTxDescHPQ,      Base,       0, "10"

HKR,Ndi\params\WakeUpFrame,       ParamDesc,  0, %WOLCapability%
HKR,Ndi\params\WakeUpFrame,       default,    0, "1"
HKR,Ndi\params\WakeUpFrame,       type,       0, "enum"
HKR,Ndi\params\WakeUpFrame\enum,  "0",        0, "Disable"
HKR,Ndi\params\WakeUpFrame\enum,  "1",        0, "Enable"

HKR,Ndi\params\CksOffload,        ParamDesc,  0, %ChecksumOffload%
HKR,Ndi\params\CksOffload,        default,    0, "1"
HKR,Ndi\params\CksOffload,        type,       0, "enum"
HKR,Ndi\params\CksOffload\enum,   "0",        0, "Disable"
HKR,Ndi\params\CksOffload\enum,   "1",        0, "Tx/Rx Checksum"
HKR,Ndi\params\CksOffload\enum,   "3",        0, "Rx Checksum"
HKR,Ndi\params\CksOffload\enum,   "4",        0, "Tx Checksum"

HKR,Ndi\params\Largesend,         ParamDesc,  0, %LargesendOffload%
HKR,Ndi\params\Largesend,         default,    0, "0"
HKR,Ndi\params\Largesend,         type,       0, "enum"
HKR,Ndi\params\Largesend\enum,    "1",        0, "Enable"
HKR,Ndi\params\Largesend\enum,    "0",        0, "Disable"

HKR,Ndi\params\Support8021p,      ParamDesc,  0, %VLanTagging%
HKR,Ndi\params\Support8021p,      default,    0, "0"
HKR,Ndi\params\Support8021p,      type,       0, "enum"
HKR,Ndi\params\Support8021p\enum, "0",        0, "Disable"
HKR,Ndi\params\Support8021p\enum, "1",        0, "Enable"

HKR,Ndi\Params\RegVlanid,   ParamDesc,  0, %VLanID%
HKR,Ndi\Params\RegVlanid,   Type,       0, "int"
HKR,Ndi\Params\RegVlanid,   Default,    0, "1"
HKR,Ndi\Params\RegVlanid,   Min,        0, "1"
HKR,Ndi\Params\RegVlanid,   Max,        0, "4094"
HKR,Ndi\Params\RegVlanid,   Step,       0, "1"
HKR,Ndi\Params\RegVlanid,   Base,       0, "10"

HKR,Ndi\params\Jumboframe,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\Jumboframe,        default,    0, "0"
HKR,Ndi\params\Jumboframe,        type,       0, "enum"
HKR,Ndi\params\Jumboframe\enum,   "0",        0, "Disable"
HKR,Ndi\params\Jumboframe\enum,   "6",        0, "Enable"

HKR,,WakeUpFrame,0,"1" 
HKR,,CksOffload,0,"1" 
HKR,,Largesend,0,"0" 

;;****************************************************************************
;; NT 5.0 parameters
;;****************************************************************************
[RTL8023.reg]
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi,            Service,    0, "RTL8023"

[rtsnt.Service]
DisplayName     = %Rtlnic.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\GA311ND5.SYS
LoadOrderGroup  = NDIS

[common.EventLog]
Addreg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
Rtlnic.CopyFiles           = 12
DefaultDestDir             = 11        ; LDID_SYS

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
GA311ND5.SYS  = 1

;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
NETGEAR			= "NETGEAR"
VLanTagging		= "802.1Q/1p VLAN Tagging"
VLanID			= "802.1Q VLAN ID"
ChecksumOffload		= "Offload Checksum"
LargesendOffload	= "Offload TCP_LargeSend"
SpeedDuplexMode		= "Link Speed/Duplex Mode"
auto_nego		= "Auto Negotiation"
sd10half		= "10Mbps/Half Duplex"
sd10full		= "10Mbps/Full Duplex"
sd100half		= "100Mbps/Half Duplex"
sd100full		= "100Mbps/Full Duplex"
sd1000full		= "1000Mbps/Full Duplex"
NetworkAddress		= "Network Address"
JumboFrame		= "Jumbo Frame"
EarlyTxThreshold	= "Early Tx Threshold"
TxDescNumber		= "Number of Tx Descriptor"
RxDescNumber		= "Number of Rx Descriptor"
TxHPQDescNumber		= "Number of High Priority Tx Descriptor"
WOLCapability		= "WakeUp on ARP/PING"
WOLLinkChange		= "WakeUp on Link Change"
LDPSCapability		= "Link Down Power Saving"

;;Source disk name
DISKNAME = "NETGEAR GA311 Gigabit Adapter NDIS Driver"

GA311.DeviceDesc      = "NETGEAR GA311 Gigabit Adapter"

;;NT service name
Rtlnic.Service.DispName = "NETGEAR GA311 Gigabit Adapter NDIS Driver"
