;***********************************************************************
;
; wlanCIG.INF
;
;   This installation script supports Windows 98SE, ME, 2000, XP for the
;   Wireless LAN Adapters.
;
;   Copyright (c) 2005
;   All Rights Reserved.
;
;***********************************************************************

[Version]
 DriverVer                      = 04/19/2005, 3.3.21.0
 Signature			= "$Chicago$"
 Compatible			= 1
 Class				= Net
 ClassGUID			= {4d36e972-e325-11ce-bfc1-08002be10318}
 Provider			= %VER_VENDOR_STR%
 CatalogFile.NT			= wlanCIG.cat

;[ControlFlags]
;Exclude all PNP adapters from user selection
; ExcludeFromSelect   = *

[Manufacturer]
 %VER_VENDOR_NAME_STR% = DeviceList,NTx86.5.1

[DeviceList.NTx86.5.1]
 %DCB_DESC_STR_XG301_CARDBUS%		= WLAN_DCB1.XP,        PCI\VEN_1260&DEV_3890&SUBSYS_001417CF
 %DCB_DESC_STR_XG601_MINIPCI%		= WLAN_DCB2.XP,        PCI\VEN_1260&DEV_3890&SUBSYS_001517CF
 %DCB_DESC_STR_XG901_PCI%		= WLAN_DCB3.XP,        PCI\VEN_1260&DEV_3890&SUBSYS_002017CF
 %DCB_DESC_STR_XG302_CARDBUS%		= WLAN_DCB4.XP,        PCI\VEN_1260&DEV_3886&SUBSYS_003517CF
 %DCB_DESC_STR_XG602_MINIPCI%		= WLAN_DCB5.XP,        PCI\VEN_1260&DEV_3886&SUBSYS_003617CF
 %DCB_DESC_STR_XG902_PCI%		= WLAN_DCB6.XP,        PCI\VEN_1260&DEV_3886&SUBSYS_003717CF

[DeviceList]
 %DCB_DESC_STR_XG301_CARDBUS%		= WLAN_DCB1,        PCI\VEN_1260&DEV_3890&SUBSYS_001417CF
 %DCB_DESC_STR_XG601_MINIPCI%		= WLAN_DCB2,        PCI\VEN_1260&DEV_3890&SUBSYS_001517CF
 %DCB_DESC_STR_XG901_PCI%		= WLAN_DCB3,        PCI\VEN_1260&DEV_3890&SUBSYS_002017CF
 %DCB_DESC_STR_XG302_CARDBUS%		= WLAN_DCB4,        PCI\VEN_1260&DEV_3886&SUBSYS_003517CF
 %DCB_DESC_STR_XG602_MINIPCI%		= WLAN_DCB5,        PCI\VEN_1260&DEV_3886&SUBSYS_003617CF
 %DCB_DESC_STR_XG902_PCI%		= WLAN_DCB6,        PCI\VEN_1260&DEV_3886&SUBSYS_003717CF
 
;==========================================
;WINXP
;###############################################################################
[WLAN_DCB1.XP.NT]    
 AddReg         = WLAN_DCB1.XP.reg, WLAN_RegNDIS_NT, WLAN_RegParams
 CopyFiles      = WLAN_DRIVER_copy_NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
 
[WLAN_DCB1.XP.NT.Services]
 AddService     = "NBXG3021", 2, WLAN_DRIVER_DCB.Service, WLAN_DRIVER.EventLog

[WLAN_DCB1.XP.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_001417CF"
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR_XG301_CARDBUS%
 ;==================================================================================
 [WLAN_DCB2.XP.NT]    
 AddReg         = WLAN_DCB2.XP.reg, WLAN_RegNDIS_NT, WLAN_RegParams
 CopyFiles      = WLAN_DRIVER_copy_NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
 
[WLAN_DCB2.XP.NT.Services]
 AddService     = "NBXG3021", 2, WLAN_DRIVER_DCB.Service, WLAN_DRIVER.EventLog

[WLAN_DCB2.XP.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_001517CF"
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR_XG601_MINIPCI% 
 ;====================================================================================
 [WLAN_DCB3.XP.NT]   
 AddReg         = WLAN_DCB3.XP.reg, WLAN_RegNDIS_NT, WLAN_RegParams
 CopyFiles      = WLAN_DRIVER_copy_NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
 
[WLAN_DCB3.XP.NT.Services]
 AddService     = "NBXG3021", 2, WLAN_DRIVER_DCB.Service, WLAN_DRIVER.EventLog

[WLAN_DCB3.XP.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_002017CF"
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR_XG901_PCI%
 ;=======================================================================================
 [WLAN_DCB4.XP.NT]   
 AddReg         = WLAN_DCB4.XP.reg, WLAN_RegNDIS_NT, WLAN_RegParams
 CopyFiles      = WLAN_DRIVER_copy_NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
 
[WLAN_DCB4.XP.NT.Services]
 AddService     = "NBXG3021", 2, WLAN_DRIVER_DCB.Service, WLAN_DRIVER.EventLog

[WLAN_DCB4.XP.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3886&SUBSYS_003517CF"
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR_XG302_CARDBUS%
 ;===============================================================================

 [WLAN_DCB5.XP.NT]   
 AddReg         = WLAN_DCB5.XP.reg, WLAN_RegNDIS_NT, WLAN_RegParams
 CopyFiles      = WLAN_DRIVER_copy_NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
 
[WLAN_DCB5.XP.NT.Services]
 AddService     = "NBXG3021", 2, WLAN_DRIVER_DCB.Service, WLAN_DRIVER.EventLog

[WLAN_DCB5.XP.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3886&SUBSYS_003617CF"
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR_XG602_MINIPCI%
 ;====================================================================================
 [WLAN_DCB6.XP.NT]   
 AddReg         = WLAN_DCB6.XP.reg, WLAN_RegNDIS_NT, WLAN_RegParams
 CopyFiles      = WLAN_DRIVER_copy_NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
 
[WLAN_DCB6.XP.NT.Services]
 AddService     = "NBXG3021", 2, WLAN_DRIVER_DCB.Service, WLAN_DRIVER.EventLog

[WLAN_DCB6.XP.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3886&SUBSYS_003717CF"
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR_XG902_PCI%
 ;======================================================================================
 ;########################### WIN2000 ###################################################
 ;======================================================================================
 [WLAN_DCB1.NT]    ; Win2k
 AddReg         = WLAN_DCB1.2K.reg, WLAN_RegNDIS_NT, WLAN_RegParams
 CopyFiles      = WLAN_DRIVER_copy_NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
 
[WLAN_DCB1.NT.Services]
 AddService     = "NBXG3021", 2, WLAN_DRIVER_DCB.Service, WLAN_DRIVER.EventLog

[WLAN_DCB1.2K.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_001417CF"
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR_XG301_CARDBUS%
 ;========================================================================================
 [WLAN_DCB2.NT]    ; Win2k
 AddReg         = WLAN_DCB2.2K.reg, WLAN_RegNDIS_NT, WLAN_RegParams
 CopyFiles      = WLAN_DRIVER_copy_NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
 
[WLAN_DCB2.NT.Services]
 AddService     = "NBXG3021", 2, WLAN_DRIVER_DCB.Service, WLAN_DRIVER.EventLog

[WLAN_DCB2.2K.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_001517CF"
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR_XG601_MINIPCI% 
 
;========================================================================================

[WLAN_DCB3.NT]    ; Win2k
 AddReg         = WLAN_DCB3.2K.reg, WLAN_RegNDIS_NT, WLAN_RegParams
 CopyFiles      = WLAN_DRIVER_copy_NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
 
[WLAN_DCB3.NT.Services]
 AddService     = "NBXG3021", 2, WLAN_DRIVER_DCB.Service, WLAN_DRIVER.EventLog

[WLAN_DCB3.2K.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_002017CF"
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR_XG901_PCI%
 
;======================================================================================
[WLAN_DCB4.NT]    ; Win2k
 AddReg         = WLAN_DCB4.2K.reg, WLAN_RegNDIS_NT, WLAN_RegParams
 CopyFiles      = WLAN_DRIVER_copy_NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
 
[WLAN_DCB4.NT.Services]
 AddService     = "NBXG3021", 2, WLAN_DRIVER_DCB.Service, WLAN_DRIVER.EventLog

[WLAN_DCB4.2K.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3886&SUBSYS_003517CF"
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR_XG302_CARDBUS%
 ;==========================================================================================
 [WLAN_DCB5.NT]    
 AddReg         = WLAN_DCB5.2K.reg, WLAN_RegNDIS_NT, WLAN_RegParams
 CopyFiles      = WLAN_DRIVER_copy_NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
 
[WLAN_DCB5.NT.Services]
 AddService     = "NBXG3021", 2, WLAN_DRIVER_DCB.Service, WLAN_DRIVER.EventLog

[WLAN_DCB5.2K.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3886&SUBSYS_003617CF"
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR_XG602_MINIPCI%
 ;=====================================================================================
 [WLAN_DCB6.NT]    ; Win2k
 AddReg         = WLAN_DCB6.2K.reg, WLAN_RegNDIS_NT, WLAN_RegParams
 CopyFiles      = WLAN_DRIVER_copy_NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
 
[WLAN_DCB6.NT.Services]
 AddService     = "NBXG3021", 2, WLAN_DRIVER_DCB.Service, WLAN_DRIVER.EventLog

[WLAN_DCB6.2K.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3886&SUBSYS_003717CF"
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR_XG902_PCI%
 ;=====================================================================================
 ;###########################   WIN2000 && XP COMMON  ##################################
 ;======================================================================================
 [WLAN_DRIVER_DCB.Service]
 DisplayName    = %WLAN_SERVICE_DISPLAY_DCB%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\wlanCIG.sys
 LoadOrderGroup = NDIS
 
[WLAN_DRIVER.EventLog]
 AddReg         = WLAN_DRIVER.EventLog.reg

[WLAN_DRIVER.EventLog.reg]
 HKR,           			,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           			,TypesSupported         ,0x00010001     ,7

[WLAN_RegNDIS_NT]
 HKR, NDI				,Service               	,0      	,"NBXG3021"
 HKR,                   		,BusType               	,0		,"5"
 HKR, NDI\Interfaces			,UpperRange            	,0		,"ndis5"
 HKR, NDI\Interfaces			,LowerRange            	,0		,"ethernet"
 HKR,                   		,DeviceVxDs            	,0      	,"wlanCIG.sys"
 ;####################################################################################################
 ;############################## WIN 98 && ME ########################################################
 ;####################################################################################################

[WLAN_DCB1]       ; Win9x
 AddReg         = WLAN_DCB1.reg, WLAN_RegNDIS_9x, WLAN_RegParams
 CopyFiles      = WLAN_DRIVER_copy_9x
 
[WLAN_DCB1.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_001417CF"
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR_XG301_CARDBUS%
 
;==========================================

[WLAN_DCB2]       ; Win9x
 AddReg         = WLAN_DCB2.reg, WLAN_RegNDIS_9x, WLAN_RegParams
 CopyFiles      = WLAN_DRIVER_copy_9x

[WLAN_DCB2.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_001517CF"
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR_XG601_MINIPCI% 
 
;==========================================

[WLAN_DCB3]       ; Win9x
 AddReg         = WLAN_DCB3.reg, WLAN_RegNDIS_9x, WLAN_RegParams
 CopyFiles      = WLAN_DRIVER_copy_9x

[WLAN_DCB3.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_002017CF"
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR_XG901_PCI%
 
;==========================================

[WLAN_DCB4]       ; Win9x
 AddReg         = WLAN_DCB4.reg, WLAN_RegNDIS_9x, WLAN_RegParams
 CopyFiles      = WLAN_DRIVER_copy_9x
 
[WLAN_DCB4.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3886&SUBSYS_003517CF"
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR_XG302_CARDBUS%
 
;==========================================

[WLAN_DCB5]       ; Win9x
 AddReg         = WLAN_DCB5.reg, WLAN_RegNDIS_9x, WLAN_RegParams
 CopyFiles      = WLAN_DRIVER_copy_9x
 
[WLAN_DCB5.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3886&SUBSYS_003617CF"
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR_XG602_MINIPCI%
 
;==========================================

[WLAN_DCB6]       ; Win9x
 AddReg         = WLAN_DCB6.reg, WLAN_RegNDIS_9x, WLAN_RegParams
 CopyFiles      = WLAN_DRIVER_copy_9x
 
[WLAN_DCB6.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3886&SUBSYS_003717CF"
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%DCB_DESC_STR_XG902_PCI%
;###############################################################################
 
;###############   WIN98 && ME COMMON   ########################################

;###############################################################################

[WLAN_RegNDIS_9x]
 HKR,                   		,RunningWin9X           ,0      	,"1"
 HKR, NDI                		,Service                ,0      	,"wlanCI9X"
 HKR,                   		,BusType                ,0      	,"5"
 HKR,                   		,DevLoader              ,0      	,"*ndis"
 HKR,                   		,EnumPropPages          ,0      	,"netdi.dll,EnumPropPages"
 HKR, NDI\Interfaces     		,UpperRange             ,0      	,"ndis3"
 HKR, NDI\Interfaces     		,LowerRange             ,0      	,"ethernet"
 HKR, NDI\Interfaces     		,DefUpper               ,0      	,"ndis3"
 HKR, NDI\Interfaces     		,DefLower               ,0      	,"ethernet"
 HKR, NDIS               		,LogDriverName          ,0      	,"WLANCI9X"
 HKR, NDIS               		,MajorNdisVersion       ,1      	,04
 HKR, NDIS               		,MinorNdisVersion       ,1      	,00
 HKR,                   		,DeviceVxDs            	,0      	,"wlanCI9X.sys"
;##################################################################################
;###############     COMMON  ########################################################
;####################################################################################


[WLAN_RegParams]
;for utility

 HKR,                   		,WLANIOC		,0      	,"XG-300"
 HKR,                   		,SilentInstall          ,0      	,"1"
;Uncomment the line above to install without user interface prompts
 HKR,                    		,CardBusBridgeLatencyTimer  		,0  		,"32"
 HKR,                    		,CardBusBridgeCacheLineSize 		,0  		,"8"
 
 HKR,  					,RTSThresh		,0		,2347
 HKR,  					,FragThresh		,0		,2346
 HKR,                   		,SSID                   ,0      	,"ANY"
 HKR,  					,NetworkType		,0		,1
 HKR,  					,LongPreamble		,0		,1
 HKR,  					,NitroMode		,0		,1
 HKR,					,NitroTime		,0		,1400
 HKR,  					,ShortRetryLimit	,0		,7
 HKR,  					,LongRetryLimit		,0		,4
 HKR,  					,PSMode			,0		,1
 HKR, 					,ConfigProfile		,0		,256

;For Default Value
 HKR, defaults				,RTSThresh		,0		,2347
 HKR, defaults				,FragThresh		,0		,2346
 HKR, defaults				,SSID			,0		,"ANY"
 HKR, defaults				,NetworkType		,0		,1
 HKR, defaults				,LongPreamble		,0		,1
 HKR, defaults				,NitroMode		,0		,1
 HKR, defaults				,NitroTime		,0		,1400
 HKR, defaults				,ShortRetryLimit	,0		,7
 HKR, defaults				,LongRetryLimit		,0		,4
 HKR, defaults				,PSMode			,0		,1
 HKR, defaults				,ConfigProfile		,0		,256
 
 
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,0,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,0,"enum"
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
 HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
 HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
 HKR,NDI\params\PSMode\enum,4,,%POWER_SAVE_DYNALWAYS_STR%
 HKR,NDI\params\PSMode\enum,5,,%POWER_SAVE_MAXALWAYS_STR%


 HKR,NDI\params\ConfigProfile,default,0,256
 HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
 HKR,NDI\params\ConfigProfile,type,0,"enum"
 HKR,NDI\params\ConfigProfile,flag,1,30,00,00,00
 HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
 HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
 HKR,NDI\params\ConfigProfile\enum,2,,%CONFIG_PROF_MIXED_LONG%
 HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
 HKR,NDI\params\ConfigProfile\enum,4,,%CONFIG_PROF_TEST%
 HKR,NDI\params\ConfigProfile\enum,5,,%CONFIG_PROF_B_WIFI%
 HKR,NDI\params\ConfigProfile\enum,6,,%CONFIG_PROF_MIXED_SHORT%
 HKR,NDI\params\ConfigProfile\enum,256,,%CONFIG_PROF_WIFI_SPEC%

 HKR,NDI\params\NitroMode,default,0,1
 HKR,NDI\params\NitroMode,ParamDesc,,%NITRO_MODE%
 HKR,NDI\params\NitroMode,type,,enum
 HKR,NDI\params\NitroMode,flag,1,30,00,00,00
 HKR,NDI\params\NitroMode\enum,0,,%OFF_STR%
 HKR,NDI\params\NitroMode\enum,1,,%ON_STR%

 HKR, NDI\params\NitroTime,default,0,1400
 HKR, NDI\params\NitroTime,ParamDesc,0,%NITRO_TIME%
 HKR, NDI\params\NitroTime,type	,0,int
 HKR, NDI\params\NitroTime,flag,1,20,00,00,00
 HKR, NDI\params\NitroTime,min	,0,0
 HKR, NDI\params\NitroTime,max	,0,5000
 HKR, NDI\params\NitroTime,step	,0,10

 HKR,Ndi\params\RTSThresh,default,0,2347
 HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
 HKR,NDI\params\RTSThresh,type,0,int
 HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
 HKR,NDI\params\RTSThresh,min,0,0
 HKR,NDI\params\RTSThresh,max,0,2347
 HKR,NDI\params\RTSThresh,step,0,1


 HKR,Ndi\params\FragThresh,default,0,2346
 HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
 HKR,NDI\params\FragThresh,type,0,int
 HKR,NDI\params\FragThresh,flag,1,20,00,00,00
 HKR,NDI\params\FragThresh,min,0,256
 HKR,NDI\params\FragThresh,max,0,2346
 HKR,NDI\params\FragThresh,step,0,2

 HKR,NDI\params\PpePdlpEnable,default,0,0
 HKR,NDI\params\PpePdlpEnable,ParamDesc,,%PPE_PDLP%
 HKR,NDI\params\PpePdlpEnable,type,,enum
 HKR,NDI\params\PpePdlpEnable,flag,1,30,00,00,00
 HKR,NDI\params\PpePdlpEnable\enum,0,,%OFF_STR%
 HKR,NDI\params\PpePdlpEnable\enum,1,,%ON_STR%

 HKR,NDI\params\PpeCompressEnable,default,0,0
 HKR,NDI\params\PpeCompressEnable,ParamDesc,,%PPE_COMPRESS%
 HKR,NDI\params\PpeCompressEnable,type,,enum
 HKR,NDI\params\PpeCompressEnable,flag,1,30,00,00,00
 HKR,NDI\params\PpeCompressEnable\enum,0,,%OFF_STR%
 HKR,NDI\params\PpeCompressEnable\enum,1,,%ON_STR%

 HKR,NDI\params\PpeConcatEnable,default,0,0
 HKR,NDI\params\PpeConcatEnable,ParamDesc,,%PPE_CONCAT%
 HKR,NDI\params\PpeConcatEnable,type,,enum
 HKR,NDI\params\PpeConcatEnable,flag,1,30,00,00,00
 HKR,NDI\params\PpeConcatEnable\enum,0,,%OFF_STR%
 HKR,NDI\params\PpeConcatEnable\enum,1,,%ON_STR%

 HKR,NDI\params\PpePiggyBackEnable,default,0,0
 HKR,NDI\params\PpePiggyBackEnable,ParamDesc,,%PPE_PIGGYBACK%
 HKR,NDI\params\PpePiggyBackEnable,type,,enum
 HKR,NDI\params\PpePiggyBackEnable,flag,1,30,00,00,00
 HKR,NDI\params\PpePiggyBackEnable\enum,0,,%OFF_STR%
 HKR,NDI\params\PpePiggyBackEnable\enum,1,,%ON_STR%

 ;11d Mode
 HKR, Ndi\params\11dMode,default,0,2 
 HKR, Ndi\params\11dMode,ParamDesc,0,%11D_MODE%
 HKR, Ndi\params\11dMode,type,0	,"enum"
 HKR, Ndi\params\11dMode\enum,0	,0,"Disabled"
 HKR, Ndi\params\11dMode\enum,1	,0,"Strict"
 HKR, Ndi\params\11dMode\enum,2	,0,"Flexible"
 
 ;Roaming Profile
 HKR,NDI\params\RoamingProfile,default,0,1
 HKR,NDI\params\RoamingProfile,ParamDesc,0,%ROAM_PROFILE_STR%
 HKR,NDI\params\RoamingProfile,type,0,"enum"
 HKR,NDI\params\RoamingProfile,flag,1,30,00,00,00
 HKR,NDI\params\RoamingProfile\enum,0,,%ROAM_PROFILE_SOHO%
 HKR,NDI\params\RoamingProfile\enum,1,,%ROAM_PROFILE_HIGH%
 HKR,NDI\params\RoamingProfile\enum,2,,%ROAM_PROFILE_MEDIUM%
 HKR,NDI\params\RoamingProfile\enum,3,,%ROAM_PROFILE_LOW%
;###############################################################################
[DestinationDirs]
;CopyFiles Section       = Destination Directory ID -- see layout.inf
;-----------------         ------------------------
 DefaultDestDir          = 11 ; Win9x=%windir%\system Win2k=%windir%\system32
 WLAN_DRIVER_copy_NT     = 12 ; Win2k=%windir%\system32\drivers
 WLAN_DRIVER_copy_9x     = 11 ; Win9x=%windir%\system Win2k=%windir%\system32

[WLAN_DRIVER_copy_NT]
 wlanCIG.sys
 
[WLAN_DRIVER_copy_9x]
 wlanCI9X.sys
  
[SourceDisksNames]
;Source Disk ID           = Disk Name
;--------------             ---------
 1                        = %INSTALL_DISK_STR%,,,
 
[SourceDisksFiles]
;File Name                = Source Disk ID
;---------                --------------
 wlanCIG.sys              = 1
 wlanCI9X.sys             = 1

;###############################################################################
[Strings]
;String ID                = String Text
;---------                -----------
 VER_VENDOR_STR           = " "
 VER_VENDOR_NAME_STR      = " "

 
 WLAN_SERVICE_DISPLAY_DCB 		= "NB 802.11g XG302 SP1 Driver"
 
 INSTALL_DISK_STR         		= "NB 802.11g Wireless LAN Install Disk"

 DCB_DESC_STR_XG301_CARDBUS		= "NB 802.11g Wireless LAN Cardbus Adapter(3890)"
 DCB_DESC_STR_XG601_MINIPCI		= "NB 802.11g Wireless LAN MiniPCI Adapter(3890)"
 DCB_DESC_STR_XG901_PCI			= "NB 802.11g Wireless LAN PCI Adapter(3890)"
 DCB_DESC_STR_XG302_CARDBUS		= "NB 802.11g Wireless LAN Cardbus Adapter(3886)"
 DCB_DESC_STR_XG602_MINIPCI		= "NB 802.11g Wireless LAN MiniPCI Adapter(3886)"
 DCB_DESC_STR_XG902_PCI			= "NB 802.11g Wireless LAN PCI Adapter(3886)"

 POWER_SAVE_STR          = "Power Save Mode"
 POWER_SAVE_OFF_STR      = "Disabled"
 POWER_SAVE_DYN_STR      = "Dynamic (Auto)"
 POWER_SAVE_MAX_STR      = "Maximum (Auto)"
 POWER_SAVE_DYNALWAYS_STR= "Dynamic"
 POWER_SAVE_MAXALWAYS_STR= "Maximum"

 RTSTHRESH_STR           = "RTS Threshold"
 FRAGTHRESH_STR          = "Fragmentation Threshold"
 ON_STR                  = "On"
 OFF_STR                 = "Off"
 CONFIG_PROFILE          = "Configuration Profile"
 CONFIG_PROF_B_ONLY      = "B only"
 CONFIG_PROF_MIXED       = "Mixed"
 CONFIG_PROF_MIXED_LONG  = "Mixed Long"
 CONFIG_PROF_G_ONLY      = "G only"
 CONFIG_PROF_TEST        = "Test"
 CONFIG_PROF_B_WIFI      = "B WiFi"
 CONFIG_PROF_MIXED_SHORT = "Mixed Short"
 CONFIG_PROF_WIFI_SPEC   = "WiFi Spec"
 NITRO_MODE              = "Nitro Mode"
 NITRO_TIME		 = "NitroTime"
 PPE_PDLP                = "Direct Link"
 PPE_COMPRESS            = "Compression"
 PPE_CONCAT              = "Concatenation"
 PPE_PIGGYBACK           = "PiggyBack"
 11D_MODE		 = "11D Mode"
 ROAM_PROFILE_STR        = "Roaming Profile"
 ROAM_PROFILE_SOHO       = "Single AP"
 ROAM_PROFILE_HIGH       = "High Density"
 ROAM_PROFILE_MEDIUM     = "Medium Density"
 ROAM_PROFILE_LOW        = "Low Density"